SPDX-FileCopyrightText: 1991-2024 kernel.org contributors
SPDX-FileCopyrightText: 2023-2024 Open Enterprise Linux Association <kernel-lts@openela.org>

SPDX-License-Identifier: GPL-2.0-only

Patch kernel up to 4.14.341-openela

REUSE-IgnoreStart

diff --git Documentation/ABI/testing/sysfs-class-net-queues Documentation/ABI/testing/sysfs-class-net-queues
index 0c0df91b1516..2734cd9ee43c 100644
--- linux-4.14.336/Documentation/ABI/testing/sysfs-class-net-queues
+++ linux-4.14.336/Documentation/ABI/testing/sysfs-class-net-queues
@@ -1,4 +1,4 @@
-What:		/sys/class/<iface>/queues/rx-<queue>/rps_cpus
+What:		/sys/class/net/<iface>/queues/rx-<queue>/rps_cpus
 Date:		March 2010
 KernelVersion:	2.6.35
 Contact:	netdev@vger.kernel.org
@@ -8,7 +8,7 @@ Description:
 		network device queue. Possible values depend on the number
 		of available CPU(s) in the system.
 
-What:		/sys/class/<iface>/queues/rx-<queue>/rps_flow_cnt
+What:		/sys/class/net/<iface>/queues/rx-<queue>/rps_flow_cnt
 Date:		April 2010
 KernelVersion:	2.6.35
 Contact:	netdev@vger.kernel.org
@@ -16,7 +16,7 @@ Description:
 		Number of Receive Packet Steering flows being currently
 		processed by this particular network device receive queue.
 
-What:		/sys/class/<iface>/queues/tx-<queue>/tx_timeout
+What:		/sys/class/net/<iface>/queues/tx-<queue>/tx_timeout
 Date:		November 2011
 KernelVersion:	3.3
 Contact:	netdev@vger.kernel.org
@@ -24,7 +24,7 @@ Description:
 		Indicates the number of transmit timeout events seen by this
 		network interface transmit queue.
 
-What:		/sys/class/<iface>/queues/tx-<queue>/tx_maxrate
+What:		/sys/class/net/<iface>/queues/tx-<queue>/tx_maxrate
 Date:		March 2015
 KernelVersion:	4.1
 Contact:	netdev@vger.kernel.org
@@ -32,7 +32,7 @@ Description:
 		A Mbps max-rate set for the queue, a value of zero means disabled,
 		default is disabled.
 
-What:		/sys/class/<iface>/queues/tx-<queue>/xps_cpus
+What:		/sys/class/net/<iface>/queues/tx-<queue>/xps_cpus
 Date:		November 2010
 KernelVersion:	2.6.38
 Contact:	netdev@vger.kernel.org
@@ -42,7 +42,7 @@ Description:
 		network device transmit queue. Possible vaules depend on the
 		number of available CPU(s) in the system.
 
-What:		/sys/class/<iface>/queues/tx-<queue>/byte_queue_limits/hold_time
+What:		/sys/class/net/<iface>/queues/tx-<queue>/byte_queue_limits/hold_time
 Date:		November 2011
 KernelVersion:	3.3
 Contact:	netdev@vger.kernel.org
@@ -51,7 +51,7 @@ Description:
 		of this particular network device transmit queue.
 		Default value is 1000.
 
-What:		/sys/class/<iface>/queues/tx-<queue>/byte_queue_limits/inflight
+What:		/sys/class/net/<iface>/queues/tx-<queue>/byte_queue_limits/inflight
 Date:		November 2011
 KernelVersion:	3.3
 Contact:	netdev@vger.kernel.org
@@ -59,7 +59,7 @@ Description:
 		Indicates the number of bytes (objects) in flight on this
 		network device transmit queue.
 
-What:		/sys/class/<iface>/queues/tx-<queue>/byte_queue_limits/limit
+What:		/sys/class/net/<iface>/queues/tx-<queue>/byte_queue_limits/limit
 Date:		November 2011
 KernelVersion:	3.3
 Contact:	netdev@vger.kernel.org
@@ -68,7 +68,7 @@ Description:
 		on this network device transmit queue. This value is clamped
 		to be within the bounds defined by limit_max and limit_min.
 
-What:		/sys/class/<iface>/queues/tx-<queue>/byte_queue_limits/limit_max
+What:		/sys/class/net/<iface>/queues/tx-<queue>/byte_queue_limits/limit_max
 Date:		November 2011
 KernelVersion:	3.3
 Contact:	netdev@vger.kernel.org
@@ -77,7 +77,7 @@ Description:
 		queued on this network device transmit queue. See
 		include/linux/dynamic_queue_limits.h for the default value.
 
-What:		/sys/class/<iface>/queues/tx-<queue>/byte_queue_limits/limit_min
+What:		/sys/class/net/<iface>/queues/tx-<queue>/byte_queue_limits/limit_min
 Date:		November 2011
 KernelVersion:	3.3
 Contact:	netdev@vger.kernel.org
diff --git Documentation/ABI/testing/sysfs-class-net-statistics Documentation/ABI/testing/sysfs-class-net-statistics
index 397118de7b5e..53e508c6936a 100644
--- linux-4.14.336/Documentation/ABI/testing/sysfs-class-net-statistics
+++ linux-4.14.336/Documentation/ABI/testing/sysfs-class-net-statistics
@@ -1,4 +1,4 @@
-What:		/sys/class/<iface>/statistics/collisions
+What:		/sys/class/net/<iface>/statistics/collisions
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -6,7 +6,7 @@ Description:
 		Indicates the number of collisions seen by this network device.
 		This value might not be relevant with all MAC layers.
 
-What:		/sys/class/<iface>/statistics/multicast
+What:		/sys/class/net/<iface>/statistics/multicast
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -14,7 +14,7 @@ Description:
 		Indicates the number of multicast packets received by this
 		network device.
 
-What:		/sys/class/<iface>/statistics/rx_bytes
+What:		/sys/class/net/<iface>/statistics/rx_bytes
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -23,7 +23,7 @@ Description:
 		See the network driver for the exact meaning of when this
 		value is incremented.
 
-What:		/sys/class/<iface>/statistics/rx_compressed
+What:		/sys/class/net/<iface>/statistics/rx_compressed
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -32,7 +32,7 @@ Description:
 		network device. This value might only be relevant for interfaces
 		that support packet compression (e.g: PPP).
 
-What:		/sys/class/<iface>/statistics/rx_crc_errors
+What:		/sys/class/net/<iface>/statistics/rx_crc_errors
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -41,7 +41,7 @@ Description:
 		by this network device. Note that the specific meaning might
 		depend on the MAC layer used by the interface.
 
-What:		/sys/class/<iface>/statistics/rx_dropped
+What:		/sys/class/net/<iface>/statistics/rx_dropped
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -51,7 +51,15 @@ Description:
 		packet processing. See the network driver for the exact
 		meaning of this value.
 
-What:		/sys/class/<iface>/statistics/rx_fifo_errors
+What:		/sys/class/net/<iface>/statistics/rx_errors
+Date:		April 2005
+KernelVersion:	2.6.12
+Contact:	netdev@vger.kernel.org
+Description:
+		Indicates the number of receive errors on this network device.
+		See the network driver for the exact meaning of this value.
+
+What:		/sys/class/net/<iface>/statistics/rx_fifo_errors
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -60,7 +68,7 @@ Description:
 		network device. See the network driver for the exact
 		meaning of this value.
 
-What:		/sys/class/<iface>/statistics/rx_frame_errors
+What:		/sys/class/net/<iface>/statistics/rx_frame_errors
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -70,7 +78,7 @@ Description:
 		on the MAC layer protocol used. See the network driver for
 		the exact meaning of this value.
 
-What:		/sys/class/<iface>/statistics/rx_length_errors
+What:		/sys/class/net/<iface>/statistics/rx_length_errors
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -79,7 +87,7 @@ Description:
 		error, oversized or undersized. See the network driver for the
 		exact meaning of this value.
 
-What:		/sys/class/<iface>/statistics/rx_missed_errors
+What:		/sys/class/net/<iface>/statistics/rx_missed_errors
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -88,7 +96,15 @@ Description:
 		due to lack of capacity in the receive side. See the network
 		driver for the exact meaning of this value.
 
-What:		/sys/class/<iface>/statistics/rx_over_errors
+What:		/sys/class/net/<iface>/statistics/rx_nohandler
+Date:		February 2016
+KernelVersion:	4.6
+Contact:	netdev@vger.kernel.org
+Description:
+		Indicates the number of received packets that were dropped on
+		an inactive device by the network core.
+
+What:		/sys/class/net/<iface>/statistics/rx_over_errors
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -98,7 +114,7 @@ Description:
 		(e.g: larger than MTU). See the network driver for the exact
 		meaning of this value.
 
-What:		/sys/class/<iface>/statistics/rx_packets
+What:		/sys/class/net/<iface>/statistics/rx_packets
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -106,7 +122,7 @@ Description:
 		Indicates the total number of good packets received by this
 		network device.
 
-What:		/sys/class/<iface>/statistics/tx_aborted_errors
+What:		/sys/class/net/<iface>/statistics/tx_aborted_errors
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -116,7 +132,7 @@ Description:
 		a medium collision). See the network driver for the exact
 		meaning of this value.
 
-What:		/sys/class/<iface>/statistics/tx_bytes
+What:		/sys/class/net/<iface>/statistics/tx_bytes
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -127,7 +143,7 @@ Description:
 		transmitted packets or all packets that have been queued for
 		transmission.
 
-What:		/sys/class/<iface>/statistics/tx_carrier_errors
+What:		/sys/class/net/<iface>/statistics/tx_carrier_errors
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -136,7 +152,7 @@ Description:
 		because of carrier errors (e.g: physical link down). See the
 		network driver for the exact meaning of this value.
 
-What:		/sys/class/<iface>/statistics/tx_compressed
+What:		/sys/class/net/<iface>/statistics/tx_compressed
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -145,7 +161,7 @@ Description:
 		this might only be relevant for devices that support
 		compression (e.g: PPP).
 
-What:		/sys/class/<iface>/statistics/tx_dropped
+What:		/sys/class/net/<iface>/statistics/tx_dropped
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -154,7 +170,7 @@ Description:
 		See the driver for the exact reasons as to why the packets were
 		dropped.
 
-What:		/sys/class/<iface>/statistics/tx_errors
+What:		/sys/class/net/<iface>/statistics/tx_errors
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -163,7 +179,7 @@ Description:
 		a network device. See the driver for the exact reasons as to
 		why the packets were dropped.
 
-What:		/sys/class/<iface>/statistics/tx_fifo_errors
+What:		/sys/class/net/<iface>/statistics/tx_fifo_errors
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -172,7 +188,7 @@ Description:
 		FIFO error. See the driver for the exact reasons as to why the
 		packets were dropped.
 
-What:		/sys/class/<iface>/statistics/tx_heartbeat_errors
+What:		/sys/class/net/<iface>/statistics/tx_heartbeat_errors
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -181,7 +197,7 @@ Description:
 		reported as heartbeat errors. See the driver for the exact
 		reasons as to why the packets were dropped.
 
-What:		/sys/class/<iface>/statistics/tx_packets
+What:		/sys/class/net/<iface>/statistics/tx_packets
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
@@ -190,7 +206,7 @@ Description:
 		device. See the driver for whether this reports the number of all
 		attempted or successful transmissions.
 
-What:		/sys/class/<iface>/statistics/tx_window_errors
+What:		/sys/class/net/<iface>/statistics/tx_window_errors
 Date:		April 2005
 KernelVersion:	2.6.12
 Contact:	netdev@vger.kernel.org
diff --git Documentation/sound/soc/dapm.rst Documentation/sound/soc/dapm.rst
index 8e44107933ab..c3154ce6e1b2 100644
--- linux-4.14.336/Documentation/sound/soc/dapm.rst
+++ linux-4.14.336/Documentation/sound/soc/dapm.rst
@@ -234,7 +234,7 @@ corresponding soft power control. In this case it is necessary to create
 a virtual widget - a widget with no control bits e.g.
 ::
 
-  SND_SOC_DAPM_MIXER("AC97 Mixer", SND_SOC_DAPM_NOPM, 0, 0, NULL, 0),
+  SND_SOC_DAPM_MIXER("AC97 Mixer", SND_SOC_NOPM, 0, 0, NULL, 0),
 
 This can be used to merge to signal paths together in software.
 
diff --git Makefile Makefile
index 3e5a7d98a1e3..0a53d6d980f7 100644
--- linux-4.14.336/Makefile
+++ linux-4.14.336/Makefile
@@ -1,8 +1,8 @@
 # SPDX-License-Identifier: GPL-2.0
 VERSION = 4
 PATCHLEVEL = 14
-SUBLEVEL = 336
-EXTRAVERSION =
+SUBLEVEL = 341
+EXTRAVERSION = -openela
 NAME = Petit Gorille
 
 # *DOCUMENTATION*
diff --git arch/arc/kernel/signal.c arch/arc/kernel/signal.c
index 68901f6f18ba..c36e642eb1a0 100644
--- linux-4.14.336/arch/arc/kernel/signal.c
+++ linux-4.14.336/arch/arc/kernel/signal.c
@@ -64,7 +64,7 @@ struct rt_sigframe {
 	unsigned int sigret_magic;
 };
 
-static int save_arcv2_regs(struct sigcontext *mctx, struct pt_regs *regs)
+static int save_arcv2_regs(struct sigcontext __user *mctx, struct pt_regs *regs)
 {
 	int err = 0;
 #ifndef CONFIG_ISA_ARCOMPACT
@@ -77,12 +77,12 @@ static int save_arcv2_regs(struct sigcontext *mctx, struct pt_regs *regs)
 #else
 	v2abi.r58 = v2abi.r59 = 0;
 #endif
-	err = __copy_to_user(&mctx->v2abi, &v2abi, sizeof(v2abi));
+	err = __copy_to_user(&mctx->v2abi, (void const *)&v2abi, sizeof(v2abi));
 #endif
 	return err;
 }
 
-static int restore_arcv2_regs(struct sigcontext *mctx, struct pt_regs *regs)
+static int restore_arcv2_regs(struct sigcontext __user *mctx, struct pt_regs *regs)
 {
 	int err = 0;
 #ifndef CONFIG_ISA_ARCOMPACT
diff --git arch/arm/boot/dts/imx1-ads.dts arch/arm/boot/dts/imx1-ads.dts
index 5ea28ee07cf4..c2ee0a6b74ac 100644
--- linux-4.14.336/arch/arm/boot/dts/imx1-ads.dts
+++ linux-4.14.336/arch/arm/boot/dts/imx1-ads.dts
@@ -81,7 +81,7 @@
 	pinctrl-0 = <&pinctrl_weim>;
 	status = "okay";
 
-	nor: nor@0,0 {
+	nor: flash@0,0 {
 		compatible = "cfi-flash";
 		reg = <0 0x00000000 0x02000000>;
 		bank-width = <4>;
diff --git arch/arm/boot/dts/imx1-apf9328.dts arch/arm/boot/dts/imx1-apf9328.dts
index e8b4b52c2418..001984de53ff 100644
--- linux-4.14.336/arch/arm/boot/dts/imx1-apf9328.dts
+++ linux-4.14.336/arch/arm/boot/dts/imx1-apf9328.dts
@@ -50,7 +50,7 @@
 	pinctrl-0 = <&pinctrl_weim>;
 	status = "okay";
 
-	nor: nor@0,0 {
+	nor: flash@0,0 {
 		compatible = "cfi-flash";
 		reg = <0 0x00000000 0x02000000>;
 		bank-width = <2>;
diff --git arch/arm/boot/dts/imx1.dtsi arch/arm/boot/dts/imx1.dtsi
index 38d712be5685..65e27c86468a 100644
--- linux-4.14.336/arch/arm/boot/dts/imx1.dtsi
+++ linux-4.14.336/arch/arm/boot/dts/imx1.dtsi
@@ -269,9 +269,12 @@
 			status = "disabled";
 		};
 
-		esram: esram@00300000 {
+		esram: sram@300000 {
 			compatible = "mmio-sram";
 			reg = <0x00300000 0x20000>;
+			ranges = <0 0x00300000 0x20000>;
+			#address-cells = <1>;
+			#size-cells = <1>;
 		};
 	};
 };
diff --git arch/arm/boot/dts/imx23-sansa.dts arch/arm/boot/dts/imx23-sansa.dts
index 221fd55e967e..3e532f4c86a4 100644
--- linux-4.14.336/arch/arm/boot/dts/imx23-sansa.dts
+++ linux-4.14.336/arch/arm/boot/dts/imx23-sansa.dts
@@ -174,10 +174,8 @@
 		#address-cells = <1>;
 		#size-cells = <0>;
 		compatible = "i2c-gpio";
-		gpios = <
-			&gpio1 24 0		/* SDA */
-			&gpio1 22 0		/* SCL */
-		>;
+		sda-gpios = <&gpio1 24 0>;
+		scl-gpios = <&gpio1 22 0>;
 		i2c-gpio,delay-us = <2>;	/* ~100 kHz */
 	};
 
@@ -185,10 +183,8 @@
 		#address-cells = <1>;
 		#size-cells = <0>;
 		compatible = "i2c-gpio";
-		gpios = <
-			&gpio0 31 0		/* SDA */
-			&gpio0 30 0		/* SCL */
-		>;
+		sda-gpios = <&gpio0 31 0>;
+		scl-gpios = <&gpio0 30 0>;
 		i2c-gpio,delay-us = <2>;	/* ~100 kHz */
 
 		touch: touch@20 {
diff --git arch/arm/boot/dts/imx23.dtsi arch/arm/boot/dts/imx23.dtsi
index 10d57f9cbb42..7a1613258e6c 100644
--- linux-4.14.336/arch/arm/boot/dts/imx23.dtsi
+++ linux-4.14.336/arch/arm/boot/dts/imx23.dtsi
@@ -413,7 +413,7 @@
 				status = "disabled";
 			};
 
-			dma_apbx: dma-apbx@80024000 {
+			dma_apbx: dma-controller@80024000 {
 				compatible = "fsl,imx23-dma-apbx";
 				reg = <0x80024000 0x2000>;
 				interrupts = <7 5 9 26
diff --git arch/arm/boot/dts/imx25-eukrea-cpuimx25.dtsi arch/arm/boot/dts/imx25-eukrea-cpuimx25.dtsi
index d6f27641c0ef..8676a28f8b7a 100644
--- linux-4.14.336/arch/arm/boot/dts/imx25-eukrea-cpuimx25.dtsi
+++ linux-4.14.336/arch/arm/boot/dts/imx25-eukrea-cpuimx25.dtsi
@@ -34,7 +34,7 @@
 	pinctrl-0 = <&pinctrl_i2c1>;
 	status = "okay";
 
-	pcf8563@51 {
+	rtc@51 {
 		compatible = "nxp,pcf8563";
 		reg = <0x51>;
 	};
diff --git arch/arm/boot/dts/imx27-apf27dev.dts arch/arm/boot/dts/imx27-apf27dev.dts
index 5f84b598e0d0..167f21434fbf 100644
--- linux-4.14.336/arch/arm/boot/dts/imx27-apf27dev.dts
+++ linux-4.14.336/arch/arm/boot/dts/imx27-apf27dev.dts
@@ -53,7 +53,7 @@
 		pinctrl-names = "default";
 		pinctrl-0 = <&pinctrl_gpio_leds>;
 
-		user {
+		led-user {
 			label = "Heartbeat";
 			gpios = <&gpio6 14 GPIO_ACTIVE_HIGH>;
 			linux,default-trigger = "heartbeat";
diff --git arch/arm/boot/dts/imx27-eukrea-cpuimx27.dtsi arch/arm/boot/dts/imx27-eukrea-cpuimx27.dtsi
index 2cf896c505f9..546b0544f8c9 100644
--- linux-4.14.336/arch/arm/boot/dts/imx27-eukrea-cpuimx27.dtsi
+++ linux-4.14.336/arch/arm/boot/dts/imx27-eukrea-cpuimx27.dtsi
@@ -45,7 +45,7 @@
 	pinctrl-0 = <&pinctrl_i2c1>;
 	status = "okay";
 
-	pcf8563@51 {
+	rtc@51 {
 		compatible = "nxp,pcf8563";
 		reg = <0x51>;
 	};
@@ -102,7 +102,7 @@
 &weim {
 	status = "okay";
 
-	nor: nor@0,0 {
+	nor: flash@0,0 {
 		#address-cells = <1>;
 		#size-cells = <1>;
 		compatible = "cfi-flash";
diff --git arch/arm/boot/dts/imx27-phytec-phycore-som.dtsi arch/arm/boot/dts/imx27-phytec-phycore-som.dtsi
index c973c5d91875..1cd3251d21e1 100644
--- linux-4.14.336/arch/arm/boot/dts/imx27-phytec-phycore-som.dtsi
+++ linux-4.14.336/arch/arm/boot/dts/imx27-phytec-phycore-som.dtsi
@@ -326,7 +326,7 @@
 &weim {
 	status = "okay";
 
-	nor: nor@0,0 {
+	nor: flash@0,0 {
 		compatible = "cfi-flash";
 		reg = <0 0x00000000 0x02000000>;
 		bank-width = <2>;
diff --git arch/arm/boot/dts/imx27.dtsi arch/arm/boot/dts/imx27.dtsi
index 15d85f1f85fd..507159b5d1d4 100644
--- linux-4.14.336/arch/arm/boot/dts/imx27.dtsi
+++ linux-4.14.336/arch/arm/boot/dts/imx27.dtsi
@@ -600,6 +600,9 @@
 		iram: iram@ffff4c00 {
 			compatible = "mmio-sram";
 			reg = <0xffff4c00 0xb400>;
+			ranges = <0 0xffff4c00 0xb400>;
+			#address-cells = <1>;
+			#size-cells = <1>;
 		};
 	};
 };
diff --git arch/arm/boot/dts/imx28.dtsi arch/arm/boot/dts/imx28.dtsi
index 2f4ebe0318d3..e489c480f4c0 100644
--- linux-4.14.336/arch/arm/boot/dts/imx28.dtsi
+++ linux-4.14.336/arch/arm/boot/dts/imx28.dtsi
@@ -985,7 +985,7 @@
 				status = "disabled";
 			};
 
-			dma_apbx: dma-apbx@80024000 {
+			dma_apbx: dma-controller@80024000 {
 				compatible = "fsl,imx28-dma-apbx";
 				reg = <0x80024000 0x2000>;
 				interrupts = <78 79 66 0
diff --git arch/arm/boot/dts/imx7s.dtsi arch/arm/boot/dts/imx7s.dtsi
index 836550f2297a..1d158707b5de 100644
--- linux-4.14.336/arch/arm/boot/dts/imx7s.dtsi
+++ linux-4.14.336/arch/arm/boot/dts/imx7s.dtsi
@@ -674,7 +674,7 @@
 			};
 
 			lcdif: lcdif@30730000 {
-				compatible = "fsl,imx7d-lcdif", "fsl,imx28-lcdif";
+				compatible = "fsl,imx7d-lcdif", "fsl,imx6sx-lcdif";
 				reg = <0x30730000 0x10000>;
 				interrupts = <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>;
 				clocks = <&clks IMX7D_LCDIF_PIXEL_ROOT_CLK>,
@@ -1039,7 +1039,7 @@
 		gpmi: gpmi-nand@33002000{
 			compatible = "fsl,imx7d-gpmi-nand";
 			#address-cells = <1>;
-			#size-cells = <1>;
+			#size-cells = <0>;
 			reg = <0x33002000 0x2000>, <0x33004000 0x4000>;
 			reg-names = "gpmi-nand", "bch";
 			interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>;
diff --git arch/arm/boot/dts/rk3036.dtsi arch/arm/boot/dts/rk3036.dtsi
index 03cf0c84ac0a..b1ede7a1e8de 100644
--- linux-4.14.336/arch/arm/boot/dts/rk3036.dtsi
+++ linux-4.14.336/arch/arm/boot/dts/rk3036.dtsi
@@ -353,12 +353,20 @@
 		pinctrl-0 = <&hdmi_ctl>;
 		status = "disabled";
 
-		hdmi_in: port {
+		ports {
 			#address-cells = <1>;
 			#size-cells = <0>;
-			hdmi_in_vop: endpoint@0 {
+
+			hdmi_in: port@0 {
 				reg = <0>;
-				remote-endpoint = <&vop_out_hdmi>;
+
+				hdmi_in_vop: endpoint {
+					remote-endpoint = <&vop_out_hdmi>;
+				};
+			};
+
+			hdmi_out: port@1 {
+				reg = <1>;
 			};
 		};
 	};
diff --git arch/mips/alchemy/devboards/db1200.c arch/mips/alchemy/devboards/db1200.c
index ae81e05fcb2c..fe827f98ebf1 100644
--- linux-4.14.336/arch/mips/alchemy/devboards/db1200.c
+++ linux-4.14.336/arch/mips/alchemy/devboards/db1200.c
@@ -858,7 +858,7 @@ int __init db1200_dev_setup(void)
 	i2c_register_board_info(0, db1200_i2c_devs,
 				ARRAY_SIZE(db1200_i2c_devs));
 	spi_register_board_info(db1200_spi_devs,
-				ARRAY_SIZE(db1200_i2c_devs));
+				ARRAY_SIZE(db1200_spi_devs));
 
 	/* SWITCHES:	S6.8 I2C/SPI selector  (OFF=I2C	 ON=SPI)
 	 *		S6.7 AC97/I2S selector (OFF=AC97 ON=I2S)
diff --git arch/mips/alchemy/devboards/db1550.c arch/mips/alchemy/devboards/db1550.c
index 7d3dfaa10231..aaee46fe582f 100644
--- linux-4.14.336/arch/mips/alchemy/devboards/db1550.c
+++ linux-4.14.336/arch/mips/alchemy/devboards/db1550.c
@@ -581,7 +581,7 @@ int __init db1550_dev_setup(void)
 	i2c_register_board_info(0, db1550_i2c_devs,
 				ARRAY_SIZE(db1550_i2c_devs));
 	spi_register_board_info(db1550_spi_devs,
-				ARRAY_SIZE(db1550_i2c_devs));
+				ARRAY_SIZE(db1550_spi_devs));
 
 	c = clk_get(NULL, "psc0_intclk");
 	if (!IS_ERR(c)) {
diff --git arch/mips/include/asm/checksum.h arch/mips/include/asm/checksum.h
index 77cad232a1c6..d7f673a6ef6d 100644
--- linux-4.14.336/arch/mips/include/asm/checksum.h
+++ linux-4.14.336/arch/mips/include/asm/checksum.h
@@ -276,7 +276,8 @@ static __inline__ __sum16 csum_ipv6_magic(const struct in6_addr *saddr,
 	"	.set	pop"
 	: "=&r" (sum), "=&r" (tmp)
 	: "r" (saddr), "r" (daddr),
-	  "0" (htonl(len)), "r" (htonl(proto)), "r" (sum));
+	  "0" (htonl(len)), "r" (htonl(proto)), "r" (sum)
+	: "memory");
 
 	return csum_fold(sum);
 }
diff --git arch/mips/kernel/elf.c arch/mips/kernel/elf.c
index 731325a61a78..d7d0a4872389 100644
--- linux-4.14.336/arch/mips/kernel/elf.c
+++ linux-4.14.336/arch/mips/kernel/elf.c
@@ -15,6 +15,7 @@
 
 #include <asm/cpu-features.h>
 #include <asm/cpu-info.h>
+#include <asm/fpu.h>
 
 /* Whether to accept legacy-NaN and 2008-NaN user binaries.  */
 bool mips_use_nan_legacy;
@@ -311,6 +312,11 @@ void mips_set_personality_nan(struct arch_elf_state *state)
 	struct cpuinfo_mips *c = &boot_cpu_data;
 	struct task_struct *t = current;
 
+	/* Do this early so t->thread.fpu.fcr31 won't be clobbered in case
+	 * we are preempted before the lose_fpu(0) in start_thread.
+	 */
+	lose_fpu(0);
+
 	t->thread.fpu.fcr31 = c->fpu_csr31;
 	switch (state->nan_2008) {
 	case 0:
diff --git arch/parisc/kernel/firmware.c arch/parisc/kernel/firmware.c
index 906b7c882587..82f264621845 100644
--- linux-4.14.336/arch/parisc/kernel/firmware.c
+++ linux-4.14.336/arch/parisc/kernel/firmware.c
@@ -127,10 +127,10 @@ static unsigned long f_extend(unsigned long address)
 #ifdef CONFIG_64BIT
 	if(unlikely(parisc_narrow_firmware)) {
 		if((address & 0xff000000) == 0xf0000000)
-			return 0xf0f0f0f000000000UL | (u32)address;
+			return (0xfffffff0UL << 32) | (u32)address;
 
 		if((address & 0xf0000000) == 0xf0000000)
-			return 0xffffffff00000000UL | (u32)address;
+			return (0xffffffffUL << 32) | (u32)address;
 	}
 #endif
 	return address;
diff --git arch/powerpc/Kconfig arch/powerpc/Kconfig
index 3fcfa8534156..ff7a86090eac 100644
--- linux-4.14.336/arch/powerpc/Kconfig
+++ linux-4.14.336/arch/powerpc/Kconfig
@@ -281,12 +281,10 @@ config ARCH_MAY_HAVE_PC_FDC
 
 config PPC_UDBG_16550
 	bool
-	default n
 
 config GENERIC_TBSYNC
 	bool
 	default y if PPC32 && SMP
-	default n
 
 config AUDIT_ARCH
 	bool
@@ -305,13 +303,11 @@ config EPAPR_BOOT
 	bool
 	help
 	  Used to allow a board to specify it wants an ePAPR compliant wrapper.
-	default n
 
 config DEFAULT_UIMAGE
 	bool
 	help
 	  Used to allow a board to specify it wants a uImage built by default
-	default n
 
 config ARCH_HIBERNATION_POSSIBLE
 	bool
@@ -325,11 +321,9 @@ config ARCH_SUSPEND_POSSIBLE
 
 config PPC_DCR_NATIVE
 	bool
-	default n
 
 config PPC_DCR_MMIO
 	bool
-	default n
 
 config PPC_DCR
 	bool
@@ -340,7 +334,6 @@ config PPC_OF_PLATFORM_PCI
 	bool
 	depends on PCI
 	depends on PPC64 # not supported on 32 bits yet
-	default n
 
 config ARCH_SUPPORTS_DEBUG_PAGEALLOC
 	depends on PPC32 || PPC_STD_MMU_64
@@ -449,14 +442,12 @@ config PPC_TRANSACTIONAL_MEM
        depends on SMP
        select ALTIVEC
        select VSX
-       default n
        ---help---
          Support user-mode Transactional Memory on POWERPC.
 
 config LD_HEAD_STUB_CATCH
 	bool "Reserve 256 bytes to cope with linker stubs in HEAD text" if EXPERT
 	depends on PPC64
-	default n
 	help
 	  Very large kernels can cause linker branch stubs to be generated by
 	  code in head_64.S, which moves the head text sections out of their
@@ -583,7 +574,6 @@ config RELOCATABLE
 config RELOCATABLE_TEST
 	bool "Test relocatable kernel"
 	depends on (PPC64 && RELOCATABLE)
-	default n
 	help
 	  This runs the relocatable kernel at the address it was initially
 	  loaded at, which tends to be non-zero and therefore test the
@@ -797,7 +787,6 @@ config PPC_SUBPAGE_PROT
 
 config PPC_COPRO_BASE
 	bool
-	default n
 
 config SCHED_SMT
 	bool "SMT (Hyperthreading) scheduler support"
@@ -911,7 +900,6 @@ config PPC_INDIRECT_PCI
 	bool
 	depends on PCI
 	default y if 40x || 44x
-	default n
 
 config EISA
 	bool
@@ -1008,7 +996,6 @@ source "drivers/pcmcia/Kconfig"
 
 config HAS_RAPIDIO
 	bool
-	default n
 
 config RAPIDIO
 	tristate "RapidIO support"
@@ -1044,7 +1031,6 @@ endmenu
 
 config NONSTATIC_KERNEL
 	bool
-	default n
 
 menu "Advanced setup"
 	depends on PPC32
diff --git arch/powerpc/Kconfig.debug arch/powerpc/Kconfig.debug
index 6c60cc03a53c..a185e7c3fc9c 100644
--- linux-4.14.336/arch/powerpc/Kconfig.debug
+++ linux-4.14.336/arch/powerpc/Kconfig.debug
@@ -5,7 +5,6 @@ source "lib/Kconfig.debug"
 
 config PPC_DISABLE_WERROR
 	bool "Don't build arch/powerpc code with -Werror"
-	default n
 	help
 	  This option tells the compiler NOT to build the code under
 	  arch/powerpc with the -Werror flag (which means warnings
@@ -59,7 +58,6 @@ config PPC_EMULATED_STATS
 config CODE_PATCHING_SELFTEST
 	bool "Run self-tests of the code-patching code"
 	depends on DEBUG_KERNEL
-	default n
 
 config JUMP_LABEL_FEATURE_CHECKS
 	bool "Enable use of jump label for cpu/mmu_has_feature()"
@@ -73,7 +71,6 @@ config JUMP_LABEL_FEATURE_CHECKS
 config JUMP_LABEL_FEATURE_CHECK_DEBUG
 	bool "Do extra check on feature fixup calls"
 	depends on DEBUG_KERNEL && JUMP_LABEL_FEATURE_CHECKS
-	default n
 	help
 	  This tries to catch incorrect usage of cpu_has_feature() and
 	  mmu_has_feature() in the code.
@@ -83,12 +80,10 @@ config JUMP_LABEL_FEATURE_CHECK_DEBUG
 config FTR_FIXUP_SELFTEST
 	bool "Run self-tests of the feature-fixup code"
 	depends on DEBUG_KERNEL
-	default n
 
 config MSI_BITMAP_SELFTEST
 	bool "Run self-tests of the MSI bitmap code"
 	depends on DEBUG_KERNEL
-	default n
 
 config XMON
 	bool "Include xmon kernel debugger"
diff --git arch/powerpc/include/asm/mmu.h arch/powerpc/include/asm/mmu.h
index 6364f5c2cc3e..2cc99f5dd703 100644
--- linux-4.14.336/arch/powerpc/include/asm/mmu.h
+++ linux-4.14.336/arch/powerpc/include/asm/mmu.h
@@ -332,5 +332,9 @@ static inline void mmu_early_init_devtree(void) { }
 #  include <asm/mmu-8xx.h>
 #endif
 
+#if defined(CONFIG_FA_DUMP) || defined(CONFIG_PRESERVE_FA_DUMP)
+#define __HAVE_ARCH_RESERVED_KERNEL_PAGES
+#endif
+
 #endif /* __KERNEL__ */
 #endif /* _ASM_POWERPC_MMU_H_ */
diff --git arch/powerpc/include/asm/mmzone.h arch/powerpc/include/asm/mmzone.h
index 91c69ff53a8a..50c2198c2c76 100644
--- linux-4.14.336/arch/powerpc/include/asm/mmzone.h
+++ linux-4.14.336/arch/powerpc/include/asm/mmzone.h
@@ -42,9 +42,6 @@ u64 memory_hotplug_max(void);
 #else
 #define memory_hotplug_max() memblock_end_of_DRAM()
 #endif /* CONFIG_NEED_MULTIPLE_NODES */
-#ifdef CONFIG_FA_DUMP
-#define __HAVE_ARCH_RESERVED_KERNEL_PAGES
-#endif
 
 #endif /* __KERNEL__ */
 #endif /* _ASM_MMZONE_H_ */
diff --git arch/powerpc/kernel/traps.c arch/powerpc/kernel/traps.c
index a507a6874d42..f70799febec4 100644
--- linux-4.14.336/arch/powerpc/kernel/traps.c
+++ linux-4.14.336/arch/powerpc/kernel/traps.c
@@ -1070,10 +1070,12 @@ static int emulate_instruction(struct pt_regs *regs)
 	return -EINVAL;
 }
 
+#ifdef CONFIG_GENERIC_BUG
 int is_valid_bugaddr(unsigned long addr)
 {
 	return is_kernel_addr(addr);
 }
+#endif
 
 #ifdef CONFIG_MATH_EMULATION
 static int emulate_math(struct pt_regs *regs)
diff --git arch/powerpc/lib/Makefile arch/powerpc/lib/Makefile
index 00c34be4c604..41491eb517cc 100644
--- linux-4.14.336/arch/powerpc/lib/Makefile
+++ linux-4.14.336/arch/powerpc/lib/Makefile
@@ -21,8 +21,8 @@ obj-$(CONFIG_PPC32)	+= div64.o copy_32.o crtsavres.o
 # 64-bit linker creates .sfpr on demand for final link (vmlinux),
 # so it is only needed for modules, and only for older linkers which
 # do not support --save-restore-funcs
-ifeq ($(call ld-ifversion, -lt, 225000000, y),y)
-extra-$(CONFIG_PPC64)	+= crtsavres.o
+ifeq ($(call ld-ifversion, -lt, 225000000, y)$(CONFIG_PPC64),yy)
+always	+= crtsavres.o
 endif
 
 obj64-y	+= copypage_64.o copyuser_64.o mem_64.o hweight_64.o \
diff --git arch/powerpc/lib/sstep.c arch/powerpc/lib/sstep.c
index e9bfd9751246..331f3d0cbeb2 100644
--- linux-4.14.336/arch/powerpc/lib/sstep.c
+++ linux-4.14.336/arch/powerpc/lib/sstep.c
@@ -471,6 +471,8 @@ static int do_fp_load(struct instruction_op *op, unsigned long ea,
 	} u;
 
 	nb = GETSIZE(op->type);
+	if (nb > sizeof(u))
+		return -EINVAL;
 	if (!address_ok(regs, ea, nb))
 		return -EFAULT;
 	rn = op->reg;
@@ -521,6 +523,8 @@ static int do_fp_store(struct instruction_op *op, unsigned long ea,
 	} u;
 
 	nb = GETSIZE(op->type);
+	if (nb > sizeof(u))
+		return -EINVAL;
 	if (!address_ok(regs, ea, nb))
 		return -EFAULT;
 	rn = op->reg;
@@ -565,6 +569,9 @@ static nokprobe_inline int do_vec_load(int rn, unsigned long ea,
 		u8 b[sizeof(__vector128)];
 	} u = {};
 
+	if (size > sizeof(u))
+		return -EINVAL;
+
 	if (!address_ok(regs, ea & ~0xfUL, 16))
 		return -EFAULT;
 	/* align to multiple of size */
@@ -592,6 +599,9 @@ static nokprobe_inline int do_vec_store(int rn, unsigned long ea,
 		u8 b[sizeof(__vector128)];
 	} u;
 
+	if (size > sizeof(u))
+		return -EINVAL;
+
 	if (!address_ok(regs, ea & ~0xfUL, 16))
 		return -EFAULT;
 	/* align to multiple of size */
diff --git arch/powerpc/mm/init-common.c arch/powerpc/mm/init-common.c
index eb8c6c8c4851..c8515de5292e 100644
--- linux-4.14.336/arch/powerpc/mm/init-common.c
+++ linux-4.14.336/arch/powerpc/mm/init-common.c
@@ -65,7 +65,7 @@ void pgtable_cache_add(unsigned shift, void (*ctor)(void *))
 	 * as to leave enough 0 bits in the address to contain it. */
 	unsigned long minalign = max(MAX_PGTABLE_INDEX_SIZE + 1,
 				     HUGEPD_SHIFT_MASK + 1);
-	struct kmem_cache *new;
+	struct kmem_cache *new = NULL;
 
 	/* It would be nice if this was a BUILD_BUG_ON(), but at the
 	 * moment, gcc doesn't seem to recognize is_power_of_2 as a
@@ -78,7 +78,8 @@ void pgtable_cache_add(unsigned shift, void (*ctor)(void *))
 
 	align = max_t(unsigned long, align, minalign);
 	name = kasprintf(GFP_KERNEL, "pgtable-2^%d", shift);
-	new = kmem_cache_create(name, table_size, align, 0, ctor);
+	if (name)
+		new = kmem_cache_create(name, table_size, align, 0, ctor);
 	if (!new)
 		panic("Could not allocate pgtable cache for order %d", shift);
 
diff --git arch/powerpc/perf/imc-pmu.c arch/powerpc/perf/imc-pmu.c
index a0b4c22d963a..0b785c6bdbbf 100644
--- linux-4.14.336/arch/powerpc/perf/imc-pmu.c
+++ linux-4.14.336/arch/powerpc/perf/imc-pmu.c
@@ -246,6 +246,8 @@ static int update_events_in_group(struct device_node *node, struct imc_pmu *pmu)
 	attr_group->attrs = attrs;
 	do {
 		ev_val_str = kasprintf(GFP_KERNEL, "event=0x%x", pmu->events[i]->value);
+		if (!ev_val_str)
+			continue;
 		dev_str = device_str_attr_create(pmu->events[i]->name, ev_val_str);
 		if (!dev_str)
 			continue;
@@ -253,6 +255,8 @@ static int update_events_in_group(struct device_node *node, struct imc_pmu *pmu)
 		attrs[j++] = dev_str;
 		if (pmu->events[i]->scale) {
 			ev_scale_str = kasprintf(GFP_KERNEL, "%s.scale",pmu->events[i]->name);
+			if (!ev_scale_str)
+				continue;
 			dev_str = device_str_attr_create(ev_scale_str, pmu->events[i]->scale);
 			if (!dev_str)
 				continue;
@@ -262,6 +266,8 @@ static int update_events_in_group(struct device_node *node, struct imc_pmu *pmu)
 
 		if (pmu->events[i]->unit) {
 			ev_unit_str = kasprintf(GFP_KERNEL, "%s.unit",pmu->events[i]->name);
+			if (!ev_unit_str)
+				continue;
 			dev_str = device_str_attr_create(ev_unit_str, pmu->events[i]->unit);
 			if (!dev_str)
 				continue;
diff --git arch/powerpc/platforms/40x/Kconfig arch/powerpc/platforms/40x/Kconfig
index 60254a321a91..2a9d66254ffc 100644
--- linux-4.14.336/arch/powerpc/platforms/40x/Kconfig
+++ linux-4.14.336/arch/powerpc/platforms/40x/Kconfig
@@ -2,7 +2,6 @@
 config ACADIA
 	bool "Acadia"
 	depends on 40x
-	default n
 	select PPC40x_SIMPLE
 	select 405EZ
 	help
@@ -11,7 +10,6 @@ config ACADIA
 config EP405
 	bool "EP405/EP405PC"
 	depends on 40x
-	default n
 	select 405GP
 	select PCI
 	help
@@ -20,7 +18,6 @@ config EP405
 config HOTFOOT
         bool "Hotfoot"
 	depends on 40x
-	default n
 	select PPC40x_SIMPLE
 	select PCI
         help
@@ -29,7 +26,6 @@ config HOTFOOT
 config KILAUEA
 	bool "Kilauea"
 	depends on 40x
-	default n
 	select 405EX
 	select PPC40x_SIMPLE
 	select PPC4xx_PCI_EXPRESS
@@ -41,7 +37,6 @@ config KILAUEA
 config MAKALU
 	bool "Makalu"
 	depends on 40x
-	default n
 	select 405EX
 	select PCI
 	select PPC4xx_PCI_EXPRESS
@@ -62,7 +57,6 @@ config WALNUT
 config XILINX_VIRTEX_GENERIC_BOARD
 	bool "Generic Xilinx Virtex board"
 	depends on 40x
-	default n
 	select XILINX_VIRTEX_II_PRO
 	select XILINX_VIRTEX_4_FX
 	select XILINX_INTC
@@ -80,7 +74,6 @@ config XILINX_VIRTEX_GENERIC_BOARD
 config OBS600
 	bool "OpenBlockS 600"
 	depends on 40x
-	default n
 	select 405EX
 	select PPC40x_SIMPLE
 	help
@@ -90,7 +83,6 @@ config OBS600
 config PPC40x_SIMPLE
 	bool "Simple PowerPC 40x board support"
 	depends on 40x
-	default n
 	help
 	  This option enables the simple PowerPC 40x platform support.
 
@@ -156,7 +148,6 @@ config IBM405_ERR51
 config APM8018X
 	bool "APM8018X"
 	depends on 40x
-	default n
 	select PPC40x_SIMPLE
 	help
 	  This option enables support for the AppliedMicro APM8018X evaluation
diff --git arch/powerpc/platforms/44x/Kconfig arch/powerpc/platforms/44x/Kconfig
index a6011422b861..559577065af2 100644
--- linux-4.14.336/arch/powerpc/platforms/44x/Kconfig
+++ linux-4.14.336/arch/powerpc/platforms/44x/Kconfig
@@ -2,7 +2,6 @@
 config PPC_47x
 	bool "Support for 47x variant"
 	depends on 44x
-	default n
 	select MPIC
 	help
 	  This option enables support for the 47x family of processors and is
@@ -11,7 +10,6 @@ config PPC_47x
 config BAMBOO
 	bool "Bamboo"
 	depends on 44x
-	default n
 	select PPC44x_SIMPLE
 	select 440EP
 	select PCI
@@ -21,7 +19,6 @@ config BAMBOO
 config BLUESTONE
 	bool "Bluestone"
 	depends on 44x
-	default n
 	select PPC44x_SIMPLE
 	select APM821xx
 	select PCI_MSI
@@ -44,7 +41,6 @@ config EBONY
 config SAM440EP
         bool "Sam440ep"
 	depends on 44x
-        default n
         select 440EP
         select PCI
         help
@@ -53,7 +49,6 @@ config SAM440EP
 config SEQUOIA
 	bool "Sequoia"
 	depends on 44x
-	default n
 	select PPC44x_SIMPLE
 	select 440EPX
 	help
@@ -62,7 +57,6 @@ config SEQUOIA
 config TAISHAN
 	bool "Taishan"
 	depends on 44x
-	default n
 	select PPC44x_SIMPLE
 	select 440GX
 	select PCI
@@ -73,7 +67,6 @@ config TAISHAN
 config KATMAI
 	bool "Katmai"
 	depends on 44x
-	default n
 	select PPC44x_SIMPLE
 	select 440SPe
 	select PCI
@@ -86,7 +79,6 @@ config KATMAI
 config RAINIER
 	bool "Rainier"
 	depends on 44x
-	default n
 	select PPC44x_SIMPLE
 	select 440GRX
 	select PCI
@@ -96,7 +88,6 @@ config RAINIER
 config WARP
 	bool "PIKA Warp"
 	depends on 44x
-	default n
 	select 440EP
 	help
 	  This option enables support for the PIKA Warp(tm) Appliance. The Warp
@@ -109,7 +100,6 @@ config WARP
 config ARCHES
 	bool "Arches"
 	depends on 44x
-	default n
 	select PPC44x_SIMPLE
 	select 460EX # Odd since it uses 460GT but the effects are the same
 	select PCI
@@ -120,7 +110,6 @@ config ARCHES
 config CANYONLANDS
 	bool "Canyonlands"
 	depends on 44x
-	default n
 	select 460EX
 	select PCI
 	select PPC4xx_PCI_EXPRESS
@@ -134,7 +123,6 @@ config CANYONLANDS
 config GLACIER
 	bool "Glacier"
 	depends on 44x
-	default n
 	select PPC44x_SIMPLE
 	select 460EX # Odd since it uses 460GT but the effects are the same
 	select PCI
@@ -147,7 +135,6 @@ config GLACIER
 config REDWOOD
 	bool "Redwood"
 	depends on 44x
-	default n
 	select PPC44x_SIMPLE
 	select 460SX
 	select PCI
@@ -160,7 +147,6 @@ config REDWOOD
 config EIGER
 	bool "Eiger"
 	depends on 44x
-	default n
 	select PPC44x_SIMPLE
 	select 460SX
 	select PCI
@@ -172,7 +158,6 @@ config EIGER
 config YOSEMITE
 	bool "Yosemite"
 	depends on 44x
-	default n
 	select PPC44x_SIMPLE
 	select 440EP
 	select PCI
@@ -182,7 +167,6 @@ config YOSEMITE
 config ISS4xx
 	bool "ISS 4xx Simulator"
 	depends on (44x || 40x)
-	default n
 	select 405GP if 40x
 	select 440GP if 44x && !PPC_47x
 	select PPC_FPU
@@ -193,7 +177,7 @@ config ISS4xx
 config CURRITUCK
 	bool "IBM Currituck (476fpe) Support"
 	depends on PPC_47x
-	default n
+	select I2C
 	select SWIOTLB
 	select 476FPE
 	select PPC4xx_PCI_EXPRESS
@@ -203,7 +187,6 @@ config CURRITUCK
 config FSP2
 	bool "IBM FSP2 (476fpe) Support"
 	depends on PPC_47x
-	default n
 	select 476FPE
 	select IBM_EMAC_EMAC4 if IBM_EMAC
 	select IBM_EMAC_RGMII if IBM_EMAC
@@ -215,7 +198,6 @@ config FSP2
 config AKEBONO
 	bool "IBM Akebono (476gtr) Support"
 	depends on PPC_47x
-	default n
 	select SWIOTLB
 	select 476FPE
 	select PPC4xx_PCI_EXPRESS
@@ -241,7 +223,6 @@ config AKEBONO
 config ICON
 	bool "Icon"
 	depends on 44x
-	default n
 	select PPC44x_SIMPLE
 	select 440SPe
 	select PCI
@@ -252,7 +233,6 @@ config ICON
 config XILINX_VIRTEX440_GENERIC_BOARD
 	bool "Generic Xilinx Virtex 5 FXT board support"
 	depends on 44x
-	default n
 	select XILINX_VIRTEX_5_FXT
 	select XILINX_INTC
 	help
@@ -280,7 +260,6 @@ config XILINX_ML510
 config PPC44x_SIMPLE
 	bool "Simple PowerPC 44x board support"
 	depends on 44x
-	default n
 	help
 	  This option enables the simple PowerPC 44x platform support.
 
diff --git arch/powerpc/platforms/82xx/Kconfig arch/powerpc/platforms/82xx/Kconfig
index 6e04099361b9..1947a88bc69f 100644
--- linux-4.14.336/arch/powerpc/platforms/82xx/Kconfig
+++ linux-4.14.336/arch/powerpc/platforms/82xx/Kconfig
@@ -51,7 +51,6 @@ endif
 
 config PQ2ADS
 	bool
-	default n
 
 config 8260
 	bool
diff --git arch/powerpc/platforms/Kconfig arch/powerpc/platforms/Kconfig
index e06ccba35133..7cf557c1e1b0 100644
--- linux-4.14.336/arch/powerpc/platforms/Kconfig
+++ linux-4.14.336/arch/powerpc/platforms/Kconfig
@@ -23,7 +23,6 @@ source "arch/powerpc/platforms/amigaone/Kconfig"
 
 config KVM_GUEST
 	bool "KVM Guest support"
-	default n
 	select EPAPR_PARAVIRT
 	---help---
 	  This option enables various optimizations for running under the KVM
@@ -34,7 +33,6 @@ config KVM_GUEST
 
 config EPAPR_PARAVIRT
 	bool "ePAPR para-virtualization support"
-	default n
 	help
 	  Enables ePAPR para-virtualization support for guests.
 
@@ -74,7 +72,6 @@ config PPC_DT_CPU_FTRS
 config UDBG_RTAS_CONSOLE
 	bool "RTAS based debug console"
 	depends on PPC_RTAS
-	default n
 
 config PPC_SMP_MUXED_IPI
 	bool
@@ -86,16 +83,13 @@ config PPC_SMP_MUXED_IPI
 
 config IPIC
 	bool
-	default n
 
 config MPIC
 	bool
-	default n
 
 config MPIC_TIMER
 	bool "MPIC Global Timer"
 	depends on MPIC && FSL_SOC
-	default n
 	help
 	  The MPIC global timer is a hardware timer inside the
 	  Freescale PIC complying with OpenPIC standard. When the
@@ -107,7 +101,6 @@ config MPIC_TIMER
 config FSL_MPIC_TIMER_WAKEUP
 	tristate "Freescale MPIC global timer wakeup driver"
 	depends on FSL_SOC &&  MPIC_TIMER && PM
-	default n
 	help
 	  The driver provides a way to wake up the system by MPIC
 	  timer.
@@ -115,43 +108,35 @@ config FSL_MPIC_TIMER_WAKEUP
 
 config PPC_EPAPR_HV_PIC
 	bool
-	default n
 	select EPAPR_PARAVIRT
 
 config MPIC_WEIRD
 	bool
-	default n
 
 config MPIC_MSGR
 	bool "MPIC message register support"
 	depends on MPIC
-	default n
 	help
 	  Enables support for the MPIC message registers.  These
 	  registers are used for inter-processor communication.
 
 config PPC_I8259
 	bool
-	default n
 
 config U3_DART
 	bool
 	depends on PPC64
-	default n
 
 config PPC_RTAS
 	bool
-	default n
 
 config RTAS_ERROR_LOGGING
 	bool
 	depends on PPC_RTAS
-	default n
 
 config PPC_RTAS_DAEMON
 	bool
 	depends on PPC_RTAS
-	default n
 
 config RTAS_PROC
 	bool "Proc interface to RTAS"
@@ -164,11 +149,9 @@ config RTAS_FLASH
 
 config MMIO_NVRAM
 	bool
-	default n
 
 config MPIC_U3_HT_IRQS
 	bool
-	default n
 
 config MPIC_BROKEN_REGREAD
 	bool
@@ -187,15 +170,12 @@ config EEH
 
 config PPC_MPC106
 	bool
-	default n
 
 config PPC_970_NAP
 	bool
-	default n
 
 config PPC_P7_NAP
 	bool
-	default n
 
 config PPC_INDIRECT_PIO
 	bool
@@ -301,7 +281,6 @@ config AXON_RAM
 
 config FSL_ULI1575
 	bool
-	default n
 	select GENERIC_ISA_DMA
 	help
 	  Supports for the ULI1575 PCIe south bridge that exists on some
diff --git arch/powerpc/platforms/Kconfig.cputype arch/powerpc/platforms/Kconfig.cputype
index 3ce376b42330..267cc8f41cf1 100644
--- linux-4.14.336/arch/powerpc/platforms/Kconfig.cputype
+++ linux-4.14.336/arch/powerpc/platforms/Kconfig.cputype
@@ -1,7 +1,6 @@
 # SPDX-License-Identifier: GPL-2.0
 config PPC64
 	bool "64-bit kernel"
-	default n
 	select ZLIB_DEFLATE
 	help
 	  This option selects whether a 32-bit or a 64-bit kernel
@@ -326,7 +325,6 @@ config PPC_MM_SLICES
 	bool
 	default y if PPC_STD_MMU_64
 	default y if PPC_8xx && HUGETLB_PAGE
-	default n
 
 config PPC_HAVE_PMU_SUPPORT
        bool
@@ -340,7 +338,6 @@ config PPC_PERF_CTRS
 config FORCE_SMP
 	# Allow platforms to force SMP=y by selecting this
 	bool
-	default n
 	select SMP
 
 config SMP
@@ -381,7 +378,6 @@ config CHECK_CACHE_COHERENCY
 
 config PPC_DOORBELL
 	bool
-	default n
 
 endmenu
 
diff --git arch/powerpc/platforms/cell/Kconfig arch/powerpc/platforms/cell/Kconfig
index 741a8fa8a3e6..3ad42075f1f4 100644
--- linux-4.14.336/arch/powerpc/platforms/cell/Kconfig
+++ linux-4.14.336/arch/powerpc/platforms/cell/Kconfig
@@ -1,7 +1,6 @@
 # SPDX-License-Identifier: GPL-2.0
 config PPC_CELL
 	bool
-	default n
 
 config PPC_CELL_COMMON
 	bool
@@ -22,7 +21,6 @@ config PPC_CELL_NATIVE
 	select IBM_EMAC_RGMII if IBM_EMAC
 	select IBM_EMAC_ZMII if IBM_EMAC #test only
 	select IBM_EMAC_TAH if IBM_EMAC  #test only
-	default n
 
 config PPC_IBM_CELL_BLADE
 	bool "IBM Cell Blade"
@@ -55,7 +53,6 @@ config SPU_FS
 
 config SPU_BASE
 	bool
-	default n
 	select PPC_COPRO_BASE
 
 config CBE_RAS
diff --git arch/powerpc/platforms/maple/Kconfig arch/powerpc/platforms/maple/Kconfig
index 376d0be36b66..2601fac50354 100644
--- linux-4.14.336/arch/powerpc/platforms/maple/Kconfig
+++ linux-4.14.336/arch/powerpc/platforms/maple/Kconfig
@@ -13,7 +13,6 @@ config PPC_MAPLE
 	select PPC_RTAS
 	select MMIO_NVRAM
 	select ATA_NONSTANDARD if ATA
-	default n
 	help
           This option enables support for the Maple 970FX Evaluation Board.
 	  For more information, refer to <http://www.970eval.com>
diff --git arch/powerpc/platforms/pasemi/Kconfig arch/powerpc/platforms/pasemi/Kconfig
index d458a791d35b..98e3bc22bebc 100644
--- linux-4.14.336/arch/powerpc/platforms/pasemi/Kconfig
+++ linux-4.14.336/arch/powerpc/platforms/pasemi/Kconfig
@@ -2,7 +2,6 @@
 config PPC_PASEMI
 	depends on PPC64 && PPC_BOOK3S && CPU_BIG_ENDIAN
 	bool "PA Semi SoC-based platforms"
-	default n
 	select MPIC
 	select PCI
 	select PPC_UDBG_16550
diff --git arch/powerpc/platforms/powernv/Kconfig arch/powerpc/platforms/powernv/Kconfig
index f8dc98d3dc01..05ee7b65d40f 100644
--- linux-4.14.336/arch/powerpc/platforms/powernv/Kconfig
+++ linux-4.14.336/arch/powerpc/platforms/powernv/Kconfig
@@ -35,7 +35,6 @@ config OPAL_PRD
 config PPC_MEMTRACE
 	bool "Enable removal of RAM from kernel mappings for tracing"
 	depends on PPC_POWERNV && MEMORY_HOTREMOVE
-	default n
 	help
 	  Enabling this option allows for the removal of memory (RAM)
 	  from the kernel mappings to be used for hardware tracing.
diff --git arch/powerpc/platforms/powernv/opal-irqchip.c arch/powerpc/platforms/powernv/opal-irqchip.c
index ecdcba9d1220..bd37ff2d7bd2 100644
--- linux-4.14.336/arch/powerpc/platforms/powernv/opal-irqchip.c
+++ linux-4.14.336/arch/powerpc/platforms/powernv/opal-irqchip.c
@@ -253,6 +253,8 @@ int __init opal_event_init(void)
 		else
 			name = kasprintf(GFP_KERNEL, "opal");
 
+		if (!name)
+			continue;
 		/* Install interrupt handler */
 		rc = request_irq(virq, opal_interrupt, IRQF_TRIGGER_LOW,
 				 name, NULL);
diff --git arch/powerpc/platforms/ps3/Kconfig arch/powerpc/platforms/ps3/Kconfig
index 6f7525555b19..24864b8aaf5d 100644
--- linux-4.14.336/arch/powerpc/platforms/ps3/Kconfig
+++ linux-4.14.336/arch/powerpc/platforms/ps3/Kconfig
@@ -49,7 +49,6 @@ config PS3_HTAB_SIZE
 config PS3_DYNAMIC_DMA
 	depends on PPC_PS3
 	bool "PS3 Platform dynamic DMA page table management"
-	default n
 	help
 	  This option will enable kernel support to take advantage of the
 	  per device dynamic DMA page table management provided by the Cell
@@ -89,7 +88,6 @@ config PS3_SYS_MANAGER
 config PS3_REPOSITORY_WRITE
 	bool "PS3 Repository write support" if PS3_ADVANCED
 	depends on PPC_PS3
-	default n
 	help
 	  Enables support for writing to the PS3 System Repository.
 
diff --git arch/powerpc/platforms/pseries/Kconfig arch/powerpc/platforms/pseries/Kconfig
index 0c698fd6d491..39032d9b316c 100644
--- linux-4.14.336/arch/powerpc/platforms/pseries/Kconfig
+++ linux-4.14.336/arch/powerpc/platforms/pseries/Kconfig
@@ -28,7 +28,6 @@ config PPC_PSERIES
 config PPC_SPLPAR
 	depends on PPC_PSERIES
 	bool "Support for shared-processor logical partitions"
-	default n
 	help
 	  Enabling this option will make the kernel run more efficiently
 	  on logically-partitioned pSeries systems which use shared
@@ -99,7 +98,6 @@ config PPC_SMLPAR
 	bool "Support for shared-memory logical partitions"
 	depends on PPC_PSERIES
 	select LPARCFG
-	default n
 	help
 	  Select this option to enable shared memory partition support.
 	  With this option a system running in an LPAR can be given more
diff --git arch/powerpc/platforms/pseries/hotplug-memory.c arch/powerpc/platforms/pseries/hotplug-memory.c
index 1a3cffdaa1e8..318772785547 100644
--- linux-4.14.336/arch/powerpc/platforms/pseries/hotplug-memory.c
+++ linux-4.14.336/arch/powerpc/platforms/pseries/hotplug-memory.c
@@ -573,7 +573,7 @@ static int dlpar_memory_remove_by_index(u32 drc_index, struct property *prop)
 	int lmb_found;
 	int i, rc;
 
-	pr_info("Attempting to hot-remove LMB, drc index %x\n", drc_index);
+	pr_debug("Attempting to hot-remove LMB, drc index %x\n", drc_index);
 
 	p = prop->value;
 	num_lmbs = *p++;
@@ -591,14 +591,15 @@ static int dlpar_memory_remove_by_index(u32 drc_index, struct property *prop)
 		}
 	}
 
-	if (!lmb_found)
+	if (!lmb_found) {
+		pr_debug("Failed to look up LMB for drc index %x\n", drc_index);
 		rc = -EINVAL;
-
-	if (rc)
-		pr_info("Failed to hot-remove memory at %llx\n",
-			lmbs[i].base_addr);
-	else
-		pr_info("Memory at %llx was hot-removed\n", lmbs[i].base_addr);
+	} else if (rc) {
+		pr_debug("Failed to hot-remove memory at %llx\n",
+			 lmbs[i].base_addr);
+	} else {
+		pr_debug("Memory at %llx was hot-removed\n", lmbs[i].base_addr);
+	}
 
 	return rc;
 }
@@ -875,8 +876,8 @@ static int dlpar_memory_add_by_count(u32 lmbs_to_add, struct property *prop)
 			if (!lmbs[i].reserved)
 				continue;
 
-			pr_info("Memory at %llx (drc index %x) was hot-added\n",
-				lmbs[i].base_addr, lmbs[i].drc_index);
+			pr_debug("Memory at %llx (drc index %x) was hot-added\n",
+				 lmbs[i].base_addr, lmbs[i].drc_index);
 			lmbs[i].reserved = 0;
 		}
 		rc = 0;
diff --git arch/powerpc/sysdev/Kconfig arch/powerpc/sysdev/Kconfig
index bcef2ac56479..e0dbec780fe9 100644
--- linux-4.14.336/arch/powerpc/sysdev/Kconfig
+++ linux-4.14.336/arch/powerpc/sysdev/Kconfig
@@ -6,19 +6,16 @@
 config PPC4xx_PCI_EXPRESS
 	bool
 	depends on PCI && 4xx
-	default n
 
 config PPC4xx_HSTA_MSI
 	bool
 	depends on PCI_MSI
 	depends on PCI && 4xx
-	default n
 
 config PPC4xx_MSI
 	bool
 	depends on PCI_MSI
 	depends on PCI && 4xx
-	default n
 
 config PPC_MSI_BITMAP
 	bool
@@ -37,11 +34,9 @@ config PPC_SCOM
 config SCOM_DEBUGFS
 	bool "Expose SCOM controllers via debugfs"
 	depends on PPC_SCOM && DEBUG_FS
-	default n
 
 config GE_FPGA
 	bool
-	default n
 
 config FSL_CORENET_RCPM
 	bool
diff --git arch/powerpc/sysdev/xive/Kconfig arch/powerpc/sysdev/xive/Kconfig
index 70ee976e1de0..785c292d104b 100644
--- linux-4.14.336/arch/powerpc/sysdev/xive/Kconfig
+++ linux-4.14.336/arch/powerpc/sysdev/xive/Kconfig
@@ -1,17 +1,14 @@
 # SPDX-License-Identifier: GPL-2.0
 config PPC_XIVE
 	bool
-	default n
 	select PPC_SMP_MUXED_IPI
 	select HARDIRQS_SW_RESEND
 
 config PPC_XIVE_NATIVE
 	bool
-	default n
 	select PPC_XIVE
 	depends on PPC_POWERNV
 
 config PPC_XIVE_SPAPR
 	bool
-	default n
 	select PPC_XIVE
diff --git arch/s390/kernel/ptrace.c arch/s390/kernel/ptrace.c
index 7c635e4328b8..60050ba8fa1d 100644
--- linux-4.14.336/arch/s390/kernel/ptrace.c
+++ linux-4.14.336/arch/s390/kernel/ptrace.c
@@ -411,6 +411,7 @@ static int __poke_user(struct task_struct *child, addr_t addr, addr_t data)
 		/*
 		 * floating point control reg. is in the thread structure
 		 */
+		save_fpu_regs();
 		if ((unsigned int) data != 0 ||
 		    test_fp_ctl(data >> (BITS_PER_LONG - 32)))
 			return -EINVAL;
@@ -771,6 +772,7 @@ static int __poke_user_compat(struct task_struct *child,
 		/*
 		 * floating point control reg. is in the thread structure
 		 */
+		save_fpu_regs();
 		if (test_fp_ctl(tmp))
 			return -EINVAL;
 		child->thread.fpu.fpc = data;
@@ -999,9 +1001,7 @@ static int s390_fpregs_set(struct task_struct *target,
 	int rc = 0;
 	freg_t fprs[__NUM_FPRS];
 
-	if (target == current)
-		save_fpu_regs();
-
+	save_fpu_regs();
 	if (MACHINE_HAS_VX)
 		convert_vx_to_fp(fprs, target->thread.fpu.vxrs);
 	else
diff --git arch/s390/kvm/kvm-s390.c arch/s390/kvm/kvm-s390.c
index 05bd51752845..ee822b451eb2 100644
--- linux-4.14.336/arch/s390/kvm/kvm-s390.c
+++ linux-4.14.336/arch/s390/kvm/kvm-s390.c
@@ -2788,8 +2788,6 @@ int kvm_arch_vcpu_ioctl_get_sregs(struct kvm_vcpu *vcpu,
 
 int kvm_arch_vcpu_ioctl_set_fpu(struct kvm_vcpu *vcpu, struct kvm_fpu *fpu)
 {
-	if (test_fp_ctl(fpu->fpc))
-		return -EINVAL;
 	vcpu->run->s.regs.fpc = fpu->fpc;
 	if (MACHINE_HAS_VX)
 		convert_fp_to_vx((__vector128 *) vcpu->run->s.regs.vrs,
diff --git arch/s390/pci/pci.c arch/s390/pci/pci.c
index 960c4a362d8c..cf6a0af76c8f 100644
--- linux-4.14.336/arch/s390/pci/pci.c
+++ linux-4.14.336/arch/s390/pci/pci.c
@@ -272,7 +272,7 @@ resource_size_t pcibios_align_resource(void *data, const struct resource *res,
 /* combine single writes by using store-block insn */
 void __iowrite64_copy(void __iomem *to, const void *from, size_t count)
 {
-       zpci_memcpy_toio(to, from, count);
+	zpci_memcpy_toio(to, from, count * 8);
 }
 
 /* Create a virtual mapping cookie for a PCI BAR */
diff --git arch/um/drivers/net_kern.c arch/um/drivers/net_kern.c
index 1669240c7a25..f107c9598127 100644
--- linux-4.14.336/arch/um/drivers/net_kern.c
+++ linux-4.14.336/arch/um/drivers/net_kern.c
@@ -207,7 +207,7 @@ static int uml_net_close(struct net_device *dev)
 	return 0;
 }
 
-static int uml_net_start_xmit(struct sk_buff *skb, struct net_device *dev)
+static netdev_tx_t uml_net_start_xmit(struct sk_buff *skb, struct net_device *dev)
 {
 	struct uml_net_private *lp = netdev_priv(dev);
 	unsigned long flags;
diff --git arch/um/include/shared/kern_util.h arch/um/include/shared/kern_util.h
index 35ab97e4bb9b..f2da8347d5f5 100644
--- linux-4.14.336/arch/um/include/shared/kern_util.h
+++ linux-4.14.336/arch/um/include/shared/kern_util.h
@@ -49,7 +49,7 @@ extern void do_uml_exitcalls(void);
  * Are we disallowed to sleep? Used to choose between GFP_KERNEL and
  * GFP_ATOMIC.
  */
-extern int __cant_sleep(void);
+extern int __uml_cant_sleep(void);
 extern int get_current_pid(void);
 extern int copy_from_user_proc(void *to, void *from, int size);
 extern int cpu(void);
diff --git arch/um/kernel/process.c arch/um/kernel/process.c
index 691b83b10649..c9d09d04d19d 100644
--- linux-4.14.336/arch/um/kernel/process.c
+++ linux-4.14.336/arch/um/kernel/process.c
@@ -210,7 +210,7 @@ void arch_cpu_idle(void)
 	local_irq_enable();
 }
 
-int __cant_sleep(void) {
+int __uml_cant_sleep(void) {
 	return in_atomic() || irqs_disabled() || in_interrupt();
 	/* Is in_interrupt() really needed? */
 }
diff --git arch/um/os-Linux/helper.c arch/um/os-Linux/helper.c
index 3f02d4232812..53d450e4a53a 100644
--- linux-4.14.336/arch/um/os-Linux/helper.c
+++ linux-4.14.336/arch/um/os-Linux/helper.c
@@ -45,7 +45,7 @@ int run_helper(void (*pre_exec)(void *), void *pre_data, char **argv)
 	unsigned long stack, sp;
 	int pid, fds[2], ret, n;
 
-	stack = alloc_stack(0, __cant_sleep());
+	stack = alloc_stack(0, __uml_cant_sleep());
 	if (stack == 0)
 		return -ENOMEM;
 
@@ -69,7 +69,7 @@ int run_helper(void (*pre_exec)(void *), void *pre_data, char **argv)
 	data.pre_data = pre_data;
 	data.argv = argv;
 	data.fd = fds[1];
-	data.buf = __cant_sleep() ? uml_kmalloc(PATH_MAX, UM_GFP_ATOMIC) :
+	data.buf = __uml_cant_sleep() ? uml_kmalloc(PATH_MAX, UM_GFP_ATOMIC) :
 					uml_kmalloc(PATH_MAX, UM_GFP_KERNEL);
 	pid = clone(helper_child, (void *) sp, CLONE_VM, &data);
 	if (pid < 0) {
@@ -116,7 +116,7 @@ int run_helper_thread(int (*proc)(void *), void *arg, unsigned int flags,
 	unsigned long stack, sp;
 	int pid, status, err;
 
-	stack = alloc_stack(0, __cant_sleep());
+	stack = alloc_stack(0, __uml_cant_sleep());
 	if (stack == 0)
 		return -ENOMEM;
 
diff --git arch/um/os-Linux/util.c arch/um/os-Linux/util.c
index 8cc8b2617a67..0436cc9537e0 100644
--- linux-4.14.336/arch/um/os-Linux/util.c
+++ linux-4.14.336/arch/um/os-Linux/util.c
@@ -166,23 +166,38 @@ __uml_setup("quiet", quiet_cmd_param,
 "quiet\n"
 "    Turns off information messages during boot.\n\n");
 
+/*
+ * The os_info/os_warn functions will be called by helper threads. These
+ * have a very limited stack size and using the libc formatting functions
+ * may overflow the stack.
+ * So pull in the kernel vscnprintf and use that instead with a fixed
+ * on-stack buffer.
+ */
+int vscnprintf(char *buf, size_t size, const char *fmt, va_list args);
+
 void os_info(const char *fmt, ...)
 {
+	char buf[256];
 	va_list list;
+	int len;
 
 	if (quiet_info)
 		return;
 
 	va_start(list, fmt);
-	vfprintf(stderr, fmt, list);
+	len = vscnprintf(buf, sizeof(buf), fmt, list);
+	fwrite(buf, len, 1, stderr);
 	va_end(list);
 }
 
 void os_warn(const char *fmt, ...)
 {
+	char buf[256];
 	va_list list;
+	int len;
 
 	va_start(list, fmt);
-	vfprintf(stderr, fmt, list);
+	len = vscnprintf(buf, sizeof(buf), fmt, list);
+	fwrite(buf, len, 1, stderr);
 	va_end(list);
 }
diff --git arch/x86/kernel/cpu/amd.c arch/x86/kernel/cpu/amd.c
index 96305270c435..9ffb0cc5aa01 100644
--- linux-4.14.336/arch/x86/kernel/cpu/amd.c
+++ linux-4.14.336/arch/x86/kernel/cpu/amd.c
@@ -198,15 +198,6 @@ static void init_amd_k6(struct cpuinfo_x86 *c)
 		return;
 	}
 #endif
-	/*
-	 * Work around Erratum 1386.  The XSAVES instruction malfunctions in
-	 * certain circumstances on Zen1/2 uarch, and not all parts have had
-	 * updated microcode at the time of writing (March 2023).
-	 *
-	 * Affected parts all have no supervisor XSAVE states, meaning that
-	 * the XSAVEC instruction (which works fine) is equivalent.
-	 */
-	clear_cpu_cap(c, X86_FEATURE_XSAVES);
 }
 
 static void init_amd_k7(struct cpuinfo_x86 *c)
@@ -880,6 +871,17 @@ static void init_amd_zn(struct cpuinfo_x86 *c)
 		if (c->x86 == 0x19 && !cpu_has(c, X86_FEATURE_BTC_NO))
 			set_cpu_cap(c, X86_FEATURE_BTC_NO);
 	}
+
+	/*
+	 * Work around Erratum 1386.  The XSAVES instruction malfunctions in
+	 * certain circumstances on Zen1/2 uarch, and not all parts have had
+	 * updated microcode at the time of writing (March 2023).
+	 *
+	 * Affected parts all have no supervisor XSAVE states, meaning that
+	 * the XSAVEC instruction (which works fine) is equivalent.
+	 */
+	if (c->x86 == 0x17)
+		clear_cpu_cap(c, X86_FEATURE_XSAVES);
 }
 
 static void init_amd(struct cpuinfo_x86 *c)
diff --git arch/x86/lib/misc.c arch/x86/lib/misc.c
index a018ec4fba53..c97be9a1430a 100644
--- linux-4.14.336/arch/x86/lib/misc.c
+++ linux-4.14.336/arch/x86/lib/misc.c
@@ -6,7 +6,7 @@
  */
 int num_digits(int val)
 {
-	int m = 10;
+	long long m = 10;
 	int d = 1;
 
 	if (val < 0) {
diff --git arch/x86/mm/ident_map.c arch/x86/mm/ident_map.c
index 407fa1df470e..50c537a4554b 100644
--- linux-4.14.336/arch/x86/mm/ident_map.c
+++ linux-4.14.336/arch/x86/mm/ident_map.c
@@ -26,18 +26,31 @@ static int ident_pud_init(struct x86_mapping_info *info, pud_t *pud_page,
 	for (; addr < end; addr = next) {
 		pud_t *pud = pud_page + pud_index(addr);
 		pmd_t *pmd;
+		bool use_gbpage;
 
 		next = (addr & PUD_MASK) + PUD_SIZE;
 		if (next > end)
 			next = end;
 
-		if (info->direct_gbpages) {
-			pud_t pudval;
+		/* if this is already a gbpage, this portion is already mapped */
+		if (pud_large(*pud))
+			continue;
+
+		/* Is using a gbpage allowed? */
+		use_gbpage = info->direct_gbpages;
 
-			if (pud_present(*pud))
-				continue;
+		/* Don't use gbpage if it maps more than the requested region. */
+		/* at the begining: */
+		use_gbpage &= ((addr & ~PUD_MASK) == 0);
+		/* ... or at the end: */
+		use_gbpage &= ((next & ~PUD_MASK) == 0);
+
+		/* Never overwrite existing mappings */
+		use_gbpage &= !pud_present(*pud);
+
+		if (use_gbpage) {
+			pud_t pudval;
 
-			addr &= PUD_MASK;
 			pudval = __pud((addr - info->offset) | info->page_flag);
 			set_pud(pud, pudval);
 			continue;
diff --git block/bio.c block/bio.c
index 1eaf31976702..28e288243266 100644
--- linux-4.14.336/block/bio.c
+++ linux-4.14.336/block/bio.c
@@ -1723,7 +1723,7 @@ void bio_set_pages_dirty(struct bio *bio)
 	bio_for_each_segment_all(bvec, bio, i) {
 		struct page *page = bvec->bv_page;
 
-		if (page && !PageCompound(page))
+		if (page)
 			set_page_dirty_lock(page);
 	}
 }
@@ -1790,7 +1790,7 @@ void bio_check_pages_dirty(struct bio *bio)
 	bio_for_each_segment_all(bvec, bio, i) {
 		struct page *page = bvec->bv_page;
 
-		if (PageDirty(page) || PageCompound(page)) {
+		if (PageDirty(page)) {
 			put_page(page);
 			bvec->bv_page = NULL;
 		} else {
diff --git crypto/af_alg.c crypto/af_alg.c
index da000a256e91..24de37ac9d27 100644
--- linux-4.14.336/crypto/af_alg.c
+++ linux-4.14.336/crypto/af_alg.c
@@ -1060,9 +1060,13 @@ EXPORT_SYMBOL_GPL(af_alg_sendpage);
 void af_alg_free_resources(struct af_alg_async_req *areq)
 {
 	struct sock *sk = areq->sk;
+	struct af_alg_ctx *ctx;
 
 	af_alg_free_areq_sgls(areq);
 	sock_kfree_s(sk, areq, areq->areqlen);
+
+	ctx = alg_sk(sk)->private;
+	ctx->inflight = false;
 }
 EXPORT_SYMBOL_GPL(af_alg_free_resources);
 
@@ -1126,11 +1130,19 @@ EXPORT_SYMBOL_GPL(af_alg_poll);
 struct af_alg_async_req *af_alg_alloc_areq(struct sock *sk,
 					   unsigned int areqlen)
 {
-	struct af_alg_async_req *areq = sock_kmalloc(sk, areqlen, GFP_KERNEL);
+	struct af_alg_ctx *ctx = alg_sk(sk)->private;
+	struct af_alg_async_req *areq;
+
+	/* Only one AIO request can be in flight. */
+	if (ctx->inflight)
+		return ERR_PTR(-EBUSY);
 
+	areq = sock_kmalloc(sk, areqlen, GFP_KERNEL);
 	if (unlikely(!areq))
 		return ERR_PTR(-ENOMEM);
 
+	ctx->inflight = true;
+
 	areq->areqlen = areqlen;
 	areq->sk = sk;
 	areq->last_rsgl = NULL;
diff --git crypto/algapi.c crypto/algapi.c
index 603d2d637209..8557aff7fb35 100644
--- linux-4.14.336/crypto/algapi.c
+++ linux-4.14.336/crypto/algapi.c
@@ -222,6 +222,7 @@ static struct crypto_larval *__crypto_register_alg(struct crypto_alg *alg)
 		}
 
 		if (!strcmp(q->cra_driver_name, alg->cra_name) ||
+		    !strcmp(q->cra_driver_name, alg->cra_driver_name) ||
 		    !strcmp(q->cra_name, alg->cra_driver_name))
 			goto err;
 	}
diff --git crypto/scompress.c crypto/scompress.c
index 2075e2c4e7df..9baaf49f16bb 100644
--- linux-4.14.336/crypto/scompress.c
+++ linux-4.14.336/crypto/scompress.c
@@ -29,9 +29,17 @@
 #include <crypto/internal/scompress.h>
 #include "internal.h"
 
+struct scomp_scratch {
+	spinlock_t	lock;
+	void		*src;
+	void		*dst;
+};
+
+static DEFINE_PER_CPU(struct scomp_scratch, scomp_scratch) = {
+	.lock = __SPIN_LOCK_UNLOCKED(scomp_scratch.lock),
+};
+
 static const struct crypto_type crypto_scomp_type;
-static void * __percpu *scomp_src_scratches;
-static void * __percpu *scomp_dst_scratches;
 static int scomp_scratch_users;
 static DEFINE_MUTEX(scomp_lock);
 
@@ -65,76 +73,53 @@ static void crypto_scomp_show(struct seq_file *m, struct crypto_alg *alg)
 	seq_puts(m, "type         : scomp\n");
 }
 
-static void crypto_scomp_free_scratches(void * __percpu *scratches)
+static void crypto_scomp_free_scratches(void)
 {
+	struct scomp_scratch *scratch;
 	int i;
 
-	if (!scratches)
-		return;
-
-	for_each_possible_cpu(i)
-		vfree(*per_cpu_ptr(scratches, i));
+	for_each_possible_cpu(i) {
+		scratch = per_cpu_ptr(&scomp_scratch, i);
 
-	free_percpu(scratches);
+		vfree(scratch->src);
+		vfree(scratch->dst);
+		scratch->src = NULL;
+		scratch->dst = NULL;
+	}
 }
 
-static void * __percpu *crypto_scomp_alloc_scratches(void)
+static int crypto_scomp_alloc_scratches(void)
 {
-	void * __percpu *scratches;
+	struct scomp_scratch *scratch;
 	int i;
 
-	scratches = alloc_percpu(void *);
-	if (!scratches)
-		return NULL;
-
 	for_each_possible_cpu(i) {
-		void *scratch;
-
-		scratch = vmalloc_node(SCOMP_SCRATCH_SIZE, cpu_to_node(i));
-		if (!scratch)
-			goto error;
-		*per_cpu_ptr(scratches, i) = scratch;
-	}
+		void *mem;
 
-	return scratches;
+		scratch = per_cpu_ptr(&scomp_scratch, i);
 
-error:
-	crypto_scomp_free_scratches(scratches);
-	return NULL;
-}
-
-static void crypto_scomp_free_all_scratches(void)
-{
-	if (!--scomp_scratch_users) {
-		crypto_scomp_free_scratches(scomp_src_scratches);
-		crypto_scomp_free_scratches(scomp_dst_scratches);
-		scomp_src_scratches = NULL;
-		scomp_dst_scratches = NULL;
-	}
-}
-
-static int crypto_scomp_alloc_all_scratches(void)
-{
-	if (!scomp_scratch_users++) {
-		scomp_src_scratches = crypto_scomp_alloc_scratches();
-		if (!scomp_src_scratches)
-			return -ENOMEM;
-		scomp_dst_scratches = crypto_scomp_alloc_scratches();
-		if (!scomp_dst_scratches) {
-			crypto_scomp_free_scratches(scomp_src_scratches);
-			scomp_src_scratches = NULL;
-			return -ENOMEM;
-		}
+		mem = vmalloc_node(SCOMP_SCRATCH_SIZE, cpu_to_node(i));
+		if (!mem)
+			goto error;
+		scratch->src = mem;
+		mem = vmalloc_node(SCOMP_SCRATCH_SIZE, cpu_to_node(i));
+		if (!mem)
+			goto error;
+		scratch->dst = mem;
 	}
 	return 0;
+error:
+	crypto_scomp_free_scratches();
+	return -ENOMEM;
 }
 
 static int crypto_scomp_init_tfm(struct crypto_tfm *tfm)
 {
-	int ret;
+	int ret = 0;
 
 	mutex_lock(&scomp_lock);
-	ret = crypto_scomp_alloc_all_scratches();
+	if (!scomp_scratch_users++)
+		ret = crypto_scomp_alloc_scratches();
 	mutex_unlock(&scomp_lock);
 
 	return ret;
@@ -193,42 +178,47 @@ static int scomp_acomp_comp_decomp(struct acomp_req *req, int dir)
 	void **tfm_ctx = acomp_tfm_ctx(tfm);
 	struct crypto_scomp *scomp = *tfm_ctx;
 	void **ctx = acomp_request_ctx(req);
-	const int cpu = get_cpu();
-	u8 *scratch_src = *per_cpu_ptr(scomp_src_scratches, cpu);
-	u8 *scratch_dst = *per_cpu_ptr(scomp_dst_scratches, cpu);
+	struct scomp_scratch *scratch;
+	unsigned int dlen;
 	int ret;
 
-	if (!req->src || !req->slen || req->slen > SCOMP_SCRATCH_SIZE) {
-		ret = -EINVAL;
-		goto out;
-	}
+	if (!req->src || !req->slen || req->slen > SCOMP_SCRATCH_SIZE)
+		return -EINVAL;
 
-	if (req->dst && !req->dlen) {
-		ret = -EINVAL;
-		goto out;
-	}
+	if (req->dst && !req->dlen)
+		return -EINVAL;
 
 	if (!req->dlen || req->dlen > SCOMP_SCRATCH_SIZE)
 		req->dlen = SCOMP_SCRATCH_SIZE;
 
-	scatterwalk_map_and_copy(scratch_src, req->src, 0, req->slen, 0);
+	dlen = req->dlen;
+
+	scratch = raw_cpu_ptr(&scomp_scratch);
+	spin_lock(&scratch->lock);
+
+	scatterwalk_map_and_copy(scratch->src, req->src, 0, req->slen, 0);
 	if (dir)
-		ret = crypto_scomp_compress(scomp, scratch_src, req->slen,
-					    scratch_dst, &req->dlen, *ctx);
+		ret = crypto_scomp_compress(scomp, scratch->src, req->slen,
+					    scratch->dst, &req->dlen, *ctx);
 	else
-		ret = crypto_scomp_decompress(scomp, scratch_src, req->slen,
-					      scratch_dst, &req->dlen, *ctx);
+		ret = crypto_scomp_decompress(scomp, scratch->src, req->slen,
+					      scratch->dst, &req->dlen, *ctx);
 	if (!ret) {
 		if (!req->dst) {
 			req->dst = crypto_scomp_sg_alloc(req->dlen, GFP_ATOMIC);
-			if (!req->dst)
+			if (!req->dst) {
+				ret = -ENOMEM;
 				goto out;
+			}
+		} else if (req->dlen > dlen) {
+			ret = -ENOSPC;
+			goto out;
 		}
-		scatterwalk_map_and_copy(scratch_dst, req->dst, 0, req->dlen,
+		scatterwalk_map_and_copy(scratch->dst, req->dst, 0, req->dlen,
 					 1);
 	}
 out:
-	put_cpu();
+	spin_unlock(&scratch->lock);
 	return ret;
 }
 
@@ -249,7 +239,8 @@ static void crypto_exit_scomp_ops_async(struct crypto_tfm *tfm)
 	crypto_free_scomp(*ctx);
 
 	mutex_lock(&scomp_lock);
-	crypto_scomp_free_all_scratches();
+	if (!--scomp_scratch_users)
+		crypto_scomp_free_scratches();
 	mutex_unlock(&scomp_lock);
 }
 
diff --git drivers/acpi/acpi_extlog.c drivers/acpi/acpi_extlog.c
index e05309bc41cc..e148b0a28ec9 100644
--- linux-4.14.336/drivers/acpi/acpi_extlog.c
+++ linux-4.14.336/drivers/acpi/acpi_extlog.c
@@ -317,9 +317,10 @@ static void __exit extlog_exit(void)
 {
 	edac_set_report_status(old_edac_report_status);
 	mce_unregister_decode_chain(&extlog_mce_dec);
-	((struct extlog_l1_head *)extlog_l1_addr)->flags &= ~FLAG_OS_OPTIN;
-	if (extlog_l1_addr)
+	if (extlog_l1_addr) {
+		((struct extlog_l1_head *)extlog_l1_addr)->flags &= ~FLAG_OS_OPTIN;
 		acpi_os_unmap_iomem(extlog_l1_addr, l1_size);
+	}
 	if (elog_addr)
 		acpi_os_unmap_iomem(elog_addr, elog_size);
 	release_mem_region(elog_base, elog_size);
diff --git drivers/acpi/acpi_video.c drivers/acpi/acpi_video.c
index cc228e5ad2b3..d426ece23a70 100644
--- linux-4.14.336/drivers/acpi/acpi_video.c
+++ linux-4.14.336/drivers/acpi/acpi_video.c
@@ -581,6 +581,15 @@ static const struct dmi_system_id video_dmi_table[] = {
 		DMI_MATCH(DMI_PRODUCT_NAME, "Vostro 3350"),
 		},
 	},
+	{
+	 .callback = video_set_report_key_events,
+	 .driver_data = (void *)((uintptr_t)REPORT_BRIGHTNESS_KEY_EVENTS),
+	 .ident = "COLORFUL X15 AT 23",
+	 .matches = {
+		DMI_MATCH(DMI_SYS_VENDOR, "COLORFUL"),
+		DMI_MATCH(DMI_PRODUCT_NAME, "X15 AT 23"),
+		},
+	},
 	/*
 	 * Some machines change the brightness themselves when a brightness
 	 * hotkey gets pressed, despite us telling them not to. In this case
@@ -1796,12 +1805,12 @@ static void acpi_video_dev_register_backlight(struct acpi_video_device *device)
 		return;
 	count++;
 
-	acpi_get_parent(device->dev->handle, &acpi_parent);
-
-	pdev = acpi_get_pci_dev(acpi_parent);
-	if (pdev) {
-		parent = &pdev->dev;
-		pci_dev_put(pdev);
+	if (ACPI_SUCCESS(acpi_get_parent(device->dev->handle, &acpi_parent))) {
+		pdev = acpi_get_pci_dev(acpi_parent);
+		if (pdev) {
+			parent = &pdev->dev;
+			pci_dev_put(pdev);
+		}
 	}
 
 	memset(&props, 0, sizeof(struct backlight_properties));
diff --git drivers/android/binder_alloc.c drivers/android/binder_alloc.c
index f7f0b71c9f68..08f31fa30648 100644
--- linux-4.14.336/drivers/android/binder_alloc.c
+++ linux-4.14.336/drivers/android/binder_alloc.c
@@ -284,7 +284,7 @@ static int binder_update_page_range(struct binder_alloc *alloc, int allocate,
 	}
 	if (mm) {
 		up_write(&mm->mmap_sem);
-		mmput(mm);
+		mmput_async(mm);
 	}
 	return 0;
 
@@ -319,7 +319,7 @@ err_page_ptr_cleared:
 err_no_vma:
 	if (mm) {
 		up_write(&mm->mmap_sem);
-		mmput(mm);
+		mmput_async(mm);
 	}
 	return vma ? -ENOMEM : -ESRCH;
 }
@@ -389,17 +389,17 @@ struct binder_buffer *binder_alloc_new_buf_locked(struct binder_alloc *alloc,
 				alloc->pid, extra_buffers_size);
 		return ERR_PTR(-EINVAL);
 	}
-	if (is_async &&
-	    alloc->free_async_space < size + sizeof(struct binder_buffer)) {
+
+	/* Pad 0-size buffers so they get assigned unique addresses */
+	size = max(size, sizeof(void *));
+
+	if (is_async && alloc->free_async_space < size) {
 		binder_alloc_debug(BINDER_DEBUG_BUFFER_ALLOC,
 			     "%d: binder_alloc_buf size %zd failed, no async space left\n",
 			      alloc->pid, size);
 		return ERR_PTR(-ENOSPC);
 	}
 
-	/* Pad 0-size buffers so they get assigned unique addresses */
-	size = max(size, sizeof(void *));
-
 	while (n) {
 		buffer = rb_entry(n, struct binder_buffer, rb_node);
 		BUG_ON(!buffer->free);
@@ -496,7 +496,7 @@ struct binder_buffer *binder_alloc_new_buf_locked(struct binder_alloc *alloc,
 	buffer->async_transaction = is_async;
 	buffer->extra_buffers_size = extra_buffers_size;
 	if (is_async) {
-		alloc->free_async_space -= size + sizeof(struct binder_buffer);
+		alloc->free_async_space -= size;
 		binder_alloc_debug(BINDER_DEBUG_BUFFER_ALLOC_ASYNC,
 			     "%d: binder_alloc_buf size %zd async free %zd\n",
 			      alloc->pid, size, alloc->free_async_space);
@@ -523,7 +523,7 @@ err_alloc_buf_struct_failed:
  * is the sum of the three given sizes (each rounded up to
  * pointer-sized boundary)
  *
- * Return:	The allocated buffer or %NULL if error
+ * Return:	The allocated buffer or %ERR_PTR(-errno) if error
  */
 struct binder_buffer *binder_alloc_new_buf(struct binder_alloc *alloc,
 					   size_t data_size,
@@ -619,8 +619,7 @@ static void binder_free_buf_locked(struct binder_alloc *alloc,
 	BUG_ON(buffer->data > alloc->buffer + alloc->buffer_size);
 
 	if (buffer->async_transaction) {
-		alloc->free_async_space += buffer_size + sizeof(struct binder_buffer);
-
+		alloc->free_async_space += buffer_size;
 		binder_alloc_debug(BINDER_DEBUG_BUFFER_ALLOC_ASYNC,
 			     "%d: binder_free_buf size %zd async free %zd\n",
 			      alloc->pid, size, alloc->free_async_space);
diff --git drivers/ata/ahci.c drivers/ata/ahci.c
index 5b810a290b93..c2e5ef709acb 100644
--- linux-4.14.336/drivers/ata/ahci.c
+++ linux-4.14.336/drivers/ata/ahci.c
@@ -605,6 +605,11 @@ MODULE_PARM_DESC(marvell_enable, "Marvell SATA via AHCI (1 = enabled)");
 static void ahci_pci_save_initial_config(struct pci_dev *pdev,
 					 struct ahci_host_priv *hpriv)
 {
+	if (pdev->vendor == PCI_VENDOR_ID_ASMEDIA && pdev->device == 0x1166) {
+		dev_info(&pdev->dev, "ASM1166 has only six ports\n");
+		hpriv->saved_port_map = 0x3f;
+	}
+
 	if (pdev->vendor == PCI_VENDOR_ID_JMICRON && pdev->device == 0x2361) {
 		dev_info(&pdev->dev, "JMB361 has only one port\n");
 		hpriv->force_port_map = 1;
diff --git drivers/atm/idt77252.c drivers/atm/idt77252.c
index e7a6b4903f9c..c777973f0ff3 100644
--- linux-4.14.336/drivers/atm/idt77252.c
+++ linux-4.14.336/drivers/atm/idt77252.c
@@ -2933,6 +2933,8 @@ open_card_ubr0(struct idt77252_dev *card)
 	vc->scq = alloc_scq(card, vc->class);
 	if (!vc->scq) {
 		printk("%s: can't get SCQ.\n", card->name);
+		kfree(card->vcs[0]);
+		card->vcs[0] = NULL;
 		return -ENOMEM;
 	}
 
diff --git drivers/base/core.c drivers/base/core.c
index e834087448a4..4f1ac622df06 100644
--- linux-4.14.336/drivers/base/core.c
+++ linux-4.14.336/drivers/base/core.c
@@ -3075,6 +3075,50 @@ define_dev_printk_level(_dev_info, KERN_INFO);
 
 #endif
 
+/**
+ * dev_err_probe - probe error check and log helper
+ * @dev: the pointer to the struct device
+ * @err: error value to test
+ * @fmt: printf-style format string
+ * @...: arguments as specified in the format string
+ *
+ * This helper implements common pattern present in probe functions for error
+ * checking: print debug or error message depending if the error value is
+ * -EPROBE_DEFER and propagate error upwards.
+ * It replaces code sequence::
+ * 	if (err != -EPROBE_DEFER)
+ * 		dev_err(dev, ...);
+ * 	else
+ * 		dev_dbg(dev, ...);
+ * 	return err;
+ *
+ * with::
+ *
+ * 	return dev_err_probe(dev, err, ...);
+ *
+ * Returns @err.
+ *
+ */
+int dev_err_probe(const struct device *dev, int err, const char *fmt, ...)
+{
+	struct va_format vaf;
+	va_list args;
+
+	va_start(args, fmt);
+	vaf.fmt = fmt;
+	vaf.va = &args;
+
+	if (err != -EPROBE_DEFER)
+		dev_err(dev, "error %pe: %pV", ERR_PTR(err), &vaf);
+	else
+		dev_dbg(dev, "error %pe: %pV", ERR_PTR(err), &vaf);
+
+	va_end(args);
+
+	return err;
+}
+EXPORT_SYMBOL_GPL(dev_err_probe);
+
 static inline bool fwnode_is_primary(struct fwnode_handle *fwnode)
 {
 	return fwnode && !IS_ERR(fwnode->secondary);
diff --git drivers/base/power/domain.c drivers/base/power/domain.c
index 0f38df5856e1..a469fb4badf2 100644
--- linux-4.14.336/drivers/base/power/domain.c
+++ linux-4.14.336/drivers/base/power/domain.c
@@ -749,7 +749,7 @@ static int __init genpd_power_off_unused(void)
 
 	return 0;
 }
-late_initcall(genpd_power_off_unused);
+late_initcall_sync(genpd_power_off_unused);
 
 #if defined(CONFIG_PM_SLEEP) || defined(CONFIG_PM_GENERIC_DOMAINS_OF)
 
diff --git drivers/block/virtio_blk.c drivers/block/virtio_blk.c
index 7e8f58c2f65b..2d3484a83fd7 100644
--- linux-4.14.336/drivers/block/virtio_blk.c
+++ linux-4.14.336/drivers/block/virtio_blk.c
@@ -930,14 +930,15 @@ static int virtblk_freeze(struct virtio_device *vdev)
 {
 	struct virtio_blk *vblk = vdev->priv;
 
+	/* Ensure no requests in virtqueues before deleting vqs. */
+	blk_mq_freeze_queue(vblk->disk->queue);
+
 	/* Ensure we don't receive any more interrupts */
 	vdev->config->reset(vdev);
 
 	/* Make sure no work handler is accessing the device. */
 	flush_work(&vblk->config_work);
 
-	blk_mq_quiesce_queue(vblk->disk->queue);
-
 	vdev->config->del_vqs(vdev);
 	kfree(vblk->vqs);
 
@@ -955,7 +956,7 @@ static int virtblk_restore(struct virtio_device *vdev)
 
 	virtio_device_ready(vdev);
 
-	blk_mq_unquiesce_queue(vblk->disk->queue);
+	blk_mq_unfreeze_queue(vblk->disk->queue);
 	return 0;
 }
 #endif
diff --git drivers/char/hw_random/core.c drivers/char/hw_random/core.c
index 303fd55f9be0..a12561fdd2f0 100644
--- linux-4.14.336/drivers/char/hw_random/core.c
+++ linux-4.14.336/drivers/char/hw_random/core.c
@@ -24,10 +24,13 @@
 #include <linux/random.h>
 #include <linux/sched.h>
 #include <linux/slab.h>
+#include <linux/string.h>
 #include <linux/uaccess.h>
 
 #define RNG_MODULE_NAME		"hw_random"
 
+#define RNG_BUFFER_SIZE (SMP_CACHE_BYTES < 32 ? 32 : SMP_CACHE_BYTES)
+
 static struct hwrng *current_rng;
 /* the current rng has been explicitly chosen by user via sysfs */
 static int cur_rng_set_by_user;
@@ -59,7 +62,7 @@ static inline int rng_get_data(struct hwrng *rng, u8 *buffer, size_t size,
 
 static size_t rng_buffer_size(void)
 {
-	return SMP_CACHE_BYTES < 32 ? 32 : SMP_CACHE_BYTES;
+	return RNG_BUFFER_SIZE;
 }
 
 static void add_early_randomness(struct hwrng *rng)
@@ -202,6 +205,7 @@ static inline int rng_get_data(struct hwrng *rng, u8 *buffer, size_t size,
 static ssize_t rng_dev_read(struct file *filp, char __user *buf,
 			    size_t size, loff_t *offp)
 {
+	u8 buffer[RNG_BUFFER_SIZE];
 	ssize_t ret = 0;
 	int err = 0;
 	int bytes_read, len;
@@ -229,34 +233,37 @@ static ssize_t rng_dev_read(struct file *filp, char __user *buf,
 			if (bytes_read < 0) {
 				err = bytes_read;
 				goto out_unlock_reading;
+			} else if (bytes_read == 0 &&
+				   (filp->f_flags & O_NONBLOCK)) {
+				err = -EAGAIN;
+				goto out_unlock_reading;
 			}
+
 			data_avail = bytes_read;
 		}
 
-		if (!data_avail) {
-			if (filp->f_flags & O_NONBLOCK) {
-				err = -EAGAIN;
-				goto out_unlock_reading;
-			}
-		} else {
-			len = data_avail;
+		len = data_avail;
+		if (len) {
 			if (len > size)
 				len = size;
 
 			data_avail -= len;
 
-			if (copy_to_user(buf + ret, rng_buffer + data_avail,
-								len)) {
+			memcpy(buffer, rng_buffer + data_avail, len);
+		}
+		mutex_unlock(&reading_mutex);
+		put_rng(rng);
+
+		if (len) {
+			if (copy_to_user(buf + ret, buffer, len)) {
 				err = -EFAULT;
-				goto out_unlock_reading;
+				goto out;
 			}
 
 			size -= len;
 			ret += len;
 		}
 
-		mutex_unlock(&reading_mutex);
-		put_rng(rng);
 
 		if (need_resched())
 			schedule_timeout_interruptible(1);
@@ -267,6 +274,7 @@ static ssize_t rng_dev_read(struct file *filp, char __user *buf,
 		}
 	}
 out:
+	memzero_explicit(buffer, sizeof(buffer));
 	return ret ? : err;
 
 out_unlock_reading:
diff --git drivers/clk/hisilicon/clk-hi3620.c drivers/clk/hisilicon/clk-hi3620.c
index fa0fba653898..7f49c7067028 100644
--- linux-4.14.336/drivers/clk/hisilicon/clk-hi3620.c
+++ linux-4.14.336/drivers/clk/hisilicon/clk-hi3620.c
@@ -481,8 +481,10 @@ static void __init hi3620_mmc_clk_init(struct device_node *node)
 		return;
 
 	clk_data->clks = kcalloc(num, sizeof(*clk_data->clks), GFP_KERNEL);
-	if (!clk_data->clks)
+	if (!clk_data->clks) {
+		kfree(clk_data);
 		return;
+	}
 
 	for (i = 0; i < num; i++) {
 		struct hisi_mmc_clock *mmc_clk = &hi3620_mmc_clks[i];
diff --git drivers/clk/mmp/clk-of-pxa168.c drivers/clk/mmp/clk-of-pxa168.c
index f110c02e83cb..9674c6c06dca 100644
--- linux-4.14.336/drivers/clk/mmp/clk-of-pxa168.c
+++ linux-4.14.336/drivers/clk/mmp/clk-of-pxa168.c
@@ -258,18 +258,21 @@ static void __init pxa168_clk_init(struct device_node *np)
 	pxa_unit->mpmu_base = of_iomap(np, 0);
 	if (!pxa_unit->mpmu_base) {
 		pr_err("failed to map mpmu registers\n");
+		kfree(pxa_unit);
 		return;
 	}
 
 	pxa_unit->apmu_base = of_iomap(np, 1);
 	if (!pxa_unit->apmu_base) {
 		pr_err("failed to map apmu registers\n");
+		kfree(pxa_unit);
 		return;
 	}
 
 	pxa_unit->apbc_base = of_iomap(np, 2);
 	if (!pxa_unit->apbc_base) {
 		pr_err("failed to map apbc registers\n");
+		kfree(pxa_unit);
 		return;
 	}
 
diff --git drivers/clk/rockchip/clk-rk3128.c drivers/clk/rockchip/clk-rk3128.c
index 5970a50671b9..83c7eb18321f 100644
--- linux-4.14.336/drivers/clk/rockchip/clk-rk3128.c
+++ linux-4.14.336/drivers/clk/rockchip/clk-rk3128.c
@@ -497,7 +497,7 @@ static struct rockchip_clk_branch common_clk_branches[] __initdata = {
 	GATE(HCLK_I2S_2CH, "hclk_i2s_2ch", "hclk_peri", 0, RK2928_CLKGATE_CON(7), 2, GFLAGS),
 	GATE(0, "hclk_usb_peri", "hclk_peri", CLK_IGNORE_UNUSED, RK2928_CLKGATE_CON(9), 13, GFLAGS),
 	GATE(HCLK_HOST2, "hclk_host2", "hclk_peri", 0, RK2928_CLKGATE_CON(7), 3, GFLAGS),
-	GATE(HCLK_OTG, "hclk_otg", "hclk_peri", 0, RK2928_CLKGATE_CON(3), 13, GFLAGS),
+	GATE(HCLK_OTG, "hclk_otg", "hclk_peri", 0, RK2928_CLKGATE_CON(5), 13, GFLAGS),
 	GATE(0, "hclk_peri_ahb", "hclk_peri", CLK_IGNORE_UNUSED, RK2928_CLKGATE_CON(9), 14, GFLAGS),
 	GATE(HCLK_SPDIF, "hclk_spdif", "hclk_peri", 0, RK2928_CLKGATE_CON(10), 9, GFLAGS),
 	GATE(HCLK_TSP, "hclk_tsp", "hclk_peri", 0, RK2928_CLKGATE_CON(10), 12, GFLAGS),
diff --git drivers/crypto/ccp/ccp-ops.c drivers/crypto/ccp/ccp-ops.c
index 453d27d2a4ff..56c571370486 100644
--- linux-4.14.336/drivers/crypto/ccp/ccp-ops.c
+++ linux-4.14.336/drivers/crypto/ccp/ccp-ops.c
@@ -183,8 +183,11 @@ static int ccp_init_dm_workarea(struct ccp_dm_workarea *wa,
 
 		wa->dma.address = dma_map_single(wa->dev, wa->address, len,
 						 dir);
-		if (dma_mapping_error(wa->dev, wa->dma.address))
+		if (dma_mapping_error(wa->dev, wa->dma.address)) {
+			kfree(wa->address);
+			wa->address = NULL;
 			return -ENOMEM;
+		}
 
 		wa->dma.length = len;
 	}
diff --git drivers/crypto/sahara.c drivers/crypto/sahara.c
index 085c229eab1d..fdc9db6c0d5e 100644
--- linux-4.14.336/drivers/crypto/sahara.c
+++ linux-4.14.336/drivers/crypto/sahara.c
@@ -46,7 +46,6 @@
 #define FLAGS_MODE_MASK		0x000f
 #define FLAGS_ENCRYPT		BIT(0)
 #define FLAGS_CBC		BIT(1)
-#define FLAGS_NEW_KEY		BIT(3)
 
 #define SAHARA_HDR_BASE			0x00800000
 #define SAHARA_HDR_SKHA_ALG_AES	0
@@ -144,8 +143,6 @@ struct sahara_hw_link {
 };
 
 struct sahara_ctx {
-	unsigned long flags;
-
 	/* AES-specific context */
 	int keylen;
 	u8 key[AES_KEYSIZE_128];
@@ -448,27 +445,24 @@ static int sahara_hw_descriptor_create(struct sahara_dev *dev)
 	int ret;
 	int i, j;
 	int idx = 0;
+	u32 len;
 
-	/* Copy new key if necessary */
-	if (ctx->flags & FLAGS_NEW_KEY) {
-		memcpy(dev->key_base, ctx->key, ctx->keylen);
-		ctx->flags &= ~FLAGS_NEW_KEY;
+	memcpy(dev->key_base, ctx->key, ctx->keylen);
 
-		if (dev->flags & FLAGS_CBC) {
-			dev->hw_desc[idx]->len1 = AES_BLOCK_SIZE;
-			dev->hw_desc[idx]->p1 = dev->iv_phys_base;
-		} else {
-			dev->hw_desc[idx]->len1 = 0;
-			dev->hw_desc[idx]->p1 = 0;
-		}
-		dev->hw_desc[idx]->len2 = ctx->keylen;
-		dev->hw_desc[idx]->p2 = dev->key_phys_base;
-		dev->hw_desc[idx]->next = dev->hw_phys_desc[1];
+	if (dev->flags & FLAGS_CBC) {
+		dev->hw_desc[idx]->len1 = AES_BLOCK_SIZE;
+		dev->hw_desc[idx]->p1 = dev->iv_phys_base;
+	} else {
+		dev->hw_desc[idx]->len1 = 0;
+		dev->hw_desc[idx]->p1 = 0;
+	}
+	dev->hw_desc[idx]->len2 = ctx->keylen;
+	dev->hw_desc[idx]->p2 = dev->key_phys_base;
+	dev->hw_desc[idx]->next = dev->hw_phys_desc[1];
+	dev->hw_desc[idx]->hdr = sahara_aes_key_hdr(dev);
 
-		dev->hw_desc[idx]->hdr = sahara_aes_key_hdr(dev);
+	idx++;
 
-		idx++;
-	}
 
 	dev->nb_in_sg = sg_nents_for_len(dev->in_sg, dev->total);
 	if (dev->nb_in_sg < 0) {
@@ -490,24 +484,27 @@ static int sahara_hw_descriptor_create(struct sahara_dev *dev)
 			 DMA_TO_DEVICE);
 	if (ret != dev->nb_in_sg) {
 		dev_err(dev->device, "couldn't map in sg\n");
-		goto unmap_in;
+		return -EINVAL;
 	}
+
 	ret = dma_map_sg(dev->device, dev->out_sg, dev->nb_out_sg,
 			 DMA_FROM_DEVICE);
 	if (ret != dev->nb_out_sg) {
 		dev_err(dev->device, "couldn't map out sg\n");
-		goto unmap_out;
+		goto unmap_in;
 	}
 
 	/* Create input links */
 	dev->hw_desc[idx]->p1 = dev->hw_phys_link[0];
 	sg = dev->in_sg;
+	len = dev->total;
 	for (i = 0; i < dev->nb_in_sg; i++) {
-		dev->hw_link[i]->len = sg->length;
+		dev->hw_link[i]->len = min(len, sg->length);
 		dev->hw_link[i]->p = sg->dma_address;
 		if (i == (dev->nb_in_sg - 1)) {
 			dev->hw_link[i]->next = 0;
 		} else {
+			len -= min(len, sg->length);
 			dev->hw_link[i]->next = dev->hw_phys_link[i + 1];
 			sg = sg_next(sg);
 		}
@@ -516,12 +513,14 @@ static int sahara_hw_descriptor_create(struct sahara_dev *dev)
 	/* Create output links */
 	dev->hw_desc[idx]->p2 = dev->hw_phys_link[i];
 	sg = dev->out_sg;
+	len = dev->total;
 	for (j = i; j < dev->nb_out_sg + i; j++) {
-		dev->hw_link[j]->len = sg->length;
+		dev->hw_link[j]->len = min(len, sg->length);
 		dev->hw_link[j]->p = sg->dma_address;
 		if (j == (dev->nb_out_sg + i - 1)) {
 			dev->hw_link[j]->next = 0;
 		} else {
+			len -= min(len, sg->length);
 			dev->hw_link[j]->next = dev->hw_phys_link[j + 1];
 			sg = sg_next(sg);
 		}
@@ -540,9 +539,6 @@ static int sahara_hw_descriptor_create(struct sahara_dev *dev)
 
 	return 0;
 
-unmap_out:
-	dma_unmap_sg(dev->device, dev->out_sg, dev->nb_out_sg,
-		DMA_FROM_DEVICE);
 unmap_in:
 	dma_unmap_sg(dev->device, dev->in_sg, dev->nb_in_sg,
 		DMA_TO_DEVICE);
@@ -587,16 +583,17 @@ static int sahara_aes_process(struct ablkcipher_request *req)
 
 	timeout = wait_for_completion_timeout(&dev->dma_completion,
 				msecs_to_jiffies(SAHARA_TIMEOUT_MS));
-	if (!timeout) {
-		dev_err(dev->device, "AES timeout\n");
-		return -ETIMEDOUT;
-	}
 
 	dma_unmap_sg(dev->device, dev->out_sg, dev->nb_out_sg,
 		DMA_FROM_DEVICE);
 	dma_unmap_sg(dev->device, dev->in_sg, dev->nb_in_sg,
 		DMA_TO_DEVICE);
 
+	if (!timeout) {
+		dev_err(dev->device, "AES timeout\n");
+		return -ETIMEDOUT;
+	}
+
 	return 0;
 }
 
@@ -611,7 +608,6 @@ static int sahara_aes_setkey(struct crypto_ablkcipher *tfm, const u8 *key,
 	/* SAHARA only supports 128bit keys */
 	if (keylen == AES_KEYSIZE_128) {
 		memcpy(ctx->key, key, keylen);
-		ctx->flags |= FLAGS_NEW_KEY;
 		return 0;
 	}
 
@@ -800,6 +796,7 @@ static int sahara_sha_hw_links_create(struct sahara_dev *dev,
 				       int start)
 {
 	struct scatterlist *sg;
+	unsigned int len;
 	unsigned int i;
 	int ret;
 
@@ -821,12 +818,14 @@ static int sahara_sha_hw_links_create(struct sahara_dev *dev,
 	if (!ret)
 		return -EFAULT;
 
+	len = rctx->total;
 	for (i = start; i < dev->nb_in_sg + start; i++) {
-		dev->hw_link[i]->len = sg->length;
+		dev->hw_link[i]->len = min(len, sg->length);
 		dev->hw_link[i]->p = sg->dma_address;
 		if (i == (dev->nb_in_sg + start - 1)) {
 			dev->hw_link[i]->next = 0;
 		} else {
+			len -= min(len, sg->length);
 			dev->hw_link[i]->next = dev->hw_phys_link[i + 1];
 			sg = sg_next(sg);
 		}
@@ -907,24 +906,6 @@ static int sahara_sha_hw_context_descriptor_create(struct sahara_dev *dev,
 	return 0;
 }
 
-static int sahara_walk_and_recalc(struct scatterlist *sg, unsigned int nbytes)
-{
-	if (!sg || !sg->length)
-		return nbytes;
-
-	while (nbytes && sg) {
-		if (nbytes <= sg->length) {
-			sg->length = nbytes;
-			sg_mark_end(sg);
-			break;
-		}
-		nbytes -= sg->length;
-		sg = sg_next(sg);
-	}
-
-	return nbytes;
-}
-
 static int sahara_sha_prepare_request(struct ahash_request *req)
 {
 	struct crypto_ahash *tfm = crypto_ahash_reqtfm(req);
@@ -961,36 +942,20 @@ static int sahara_sha_prepare_request(struct ahash_request *req)
 					hash_later, 0);
 	}
 
-	/* nbytes should now be multiple of blocksize */
-	req->nbytes = req->nbytes - hash_later;
-
-	sahara_walk_and_recalc(req->src, req->nbytes);
-
+	rctx->total = len - hash_later;
 	/* have data from previous operation and current */
 	if (rctx->buf_cnt && req->nbytes) {
 		sg_init_table(rctx->in_sg_chain, 2);
 		sg_set_buf(rctx->in_sg_chain, rctx->rembuf, rctx->buf_cnt);
-
 		sg_chain(rctx->in_sg_chain, 2, req->src);
-
-		rctx->total = req->nbytes + rctx->buf_cnt;
 		rctx->in_sg = rctx->in_sg_chain;
-
-		req->src = rctx->in_sg_chain;
 	/* only data from previous operation */
 	} else if (rctx->buf_cnt) {
-		if (req->src)
-			rctx->in_sg = req->src;
-		else
-			rctx->in_sg = rctx->in_sg_chain;
-		/* buf was copied into rembuf above */
+		rctx->in_sg = rctx->in_sg_chain;
 		sg_init_one(rctx->in_sg, rctx->rembuf, rctx->buf_cnt);
-		rctx->total = rctx->buf_cnt;
 	/* no data from previous operation */
 	} else {
 		rctx->in_sg = req->src;
-		rctx->total = req->nbytes;
-		req->src = rctx->in_sg;
 	}
 
 	/* on next call, we only have the remaining data in the buffer */
@@ -1011,7 +976,10 @@ static int sahara_sha_process(struct ahash_request *req)
 		return ret;
 
 	if (rctx->first) {
-		sahara_sha_hw_data_descriptor_create(dev, rctx, req, 0);
+		ret = sahara_sha_hw_data_descriptor_create(dev, rctx, req, 0);
+		if (ret)
+			return ret;
+
 		dev->hw_desc[0]->next = 0;
 		rctx->first = 0;
 	} else {
@@ -1019,7 +987,10 @@ static int sahara_sha_process(struct ahash_request *req)
 
 		sahara_sha_hw_context_descriptor_create(dev, rctx, req, 0);
 		dev->hw_desc[0]->next = dev->hw_phys_desc[1];
-		sahara_sha_hw_data_descriptor_create(dev, rctx, req, 1);
+		ret = sahara_sha_hw_data_descriptor_create(dev, rctx, req, 1);
+		if (ret)
+			return ret;
+
 		dev->hw_desc[1]->next = 0;
 	}
 
@@ -1032,18 +1003,19 @@ static int sahara_sha_process(struct ahash_request *req)
 
 	timeout = wait_for_completion_timeout(&dev->dma_completion,
 				msecs_to_jiffies(SAHARA_TIMEOUT_MS));
-	if (!timeout) {
-		dev_err(dev->device, "SHA timeout\n");
-		return -ETIMEDOUT;
-	}
 
 	if (rctx->sg_in_idx)
 		dma_unmap_sg(dev->device, dev->in_sg, dev->nb_in_sg,
 			     DMA_TO_DEVICE);
 
+	if (!timeout) {
+		dev_err(dev->device, "SHA timeout\n");
+		return -ETIMEDOUT;
+	}
+
 	memcpy(rctx->context, dev->context_base, rctx->context_size);
 
-	if (req->result)
+	if (req->result && rctx->last)
 		memcpy(req->result, rctx->context, rctx->digest_size);
 
 	return 0;
@@ -1187,8 +1159,7 @@ static int sahara_sha_import(struct ahash_request *req, const void *in)
 static int sahara_sha_cra_init(struct crypto_tfm *tfm)
 {
 	crypto_ahash_set_reqsize(__crypto_ahash_cast(tfm),
-				 sizeof(struct sahara_sha_reqctx) +
-				 SHA_BUFFER_LEN + SHA256_BLOCK_SIZE);
+				 sizeof(struct sahara_sha_reqctx));
 
 	return 0;
 }
diff --git drivers/crypto/virtio/virtio_crypto_common.h drivers/crypto/virtio/virtio_crypto_common.h
index e976539a05d9..d8be210a07ec 100644
--- linux-4.14.336/drivers/crypto/virtio/virtio_crypto_common.h
+++ linux-4.14.336/drivers/crypto/virtio/virtio_crypto_common.h
@@ -22,6 +22,7 @@
 #include <linux/virtio.h>
 #include <linux/crypto.h>
 #include <linux/spinlock.h>
+#include <linux/interrupt.h>
 #include <crypto/aead.h>
 #include <crypto/aes.h>
 #include <crypto/authenc.h>
@@ -40,6 +41,7 @@ struct data_queue {
 	char name[32];
 
 	struct crypto_engine *engine;
+	struct tasklet_struct done_task;
 };
 
 struct virtio_crypto {
diff --git drivers/crypto/virtio/virtio_crypto_core.c drivers/crypto/virtio/virtio_crypto_core.c
index ff1410a32c2b..e21dd216989f 100644
--- linux-4.14.336/drivers/crypto/virtio/virtio_crypto_core.c
+++ linux-4.14.336/drivers/crypto/virtio/virtio_crypto_core.c
@@ -34,27 +34,28 @@ virtcrypto_clear_request(struct virtio_crypto_request *vc_req)
 	}
 }
 
-static void virtcrypto_dataq_callback(struct virtqueue *vq)
+static void virtcrypto_done_task(unsigned long data)
 {
-	struct virtio_crypto *vcrypto = vq->vdev->priv;
+	struct data_queue *data_vq = (struct data_queue *)data;
+	struct virtqueue *vq = data_vq->vq;
 	struct virtio_crypto_request *vc_req;
-	unsigned long flags;
 	unsigned int len;
-	unsigned int qid = vq->index;
 
-	spin_lock_irqsave(&vcrypto->data_vq[qid].lock, flags);
 	do {
 		virtqueue_disable_cb(vq);
 		while ((vc_req = virtqueue_get_buf(vq, &len)) != NULL) {
-			spin_unlock_irqrestore(
-				&vcrypto->data_vq[qid].lock, flags);
 			if (vc_req->alg_cb)
 				vc_req->alg_cb(vc_req, len);
-			spin_lock_irqsave(
-				&vcrypto->data_vq[qid].lock, flags);
 		}
 	} while (!virtqueue_enable_cb(vq));
-	spin_unlock_irqrestore(&vcrypto->data_vq[qid].lock, flags);
+}
+
+static void virtcrypto_dataq_callback(struct virtqueue *vq)
+{
+	struct virtio_crypto *vcrypto = vq->vdev->priv;
+	struct data_queue *dq = &vcrypto->data_vq[vq->index];
+
+	tasklet_schedule(&dq->done_task);
 }
 
 static int virtcrypto_find_vqs(struct virtio_crypto *vi)
@@ -114,6 +115,8 @@ static int virtcrypto_find_vqs(struct virtio_crypto *vi)
 
 		vi->data_vq[i].engine->cipher_one_request =
 			virtio_crypto_ablkcipher_crypt_req;
+		tasklet_init(&vi->data_vq[i].done_task, virtcrypto_done_task,
+				(unsigned long)&vi->data_vq[i]);
 	}
 
 	kfree(names);
@@ -417,11 +420,14 @@ static void virtcrypto_free_unused_reqs(struct virtio_crypto *vcrypto)
 static void virtcrypto_remove(struct virtio_device *vdev)
 {
 	struct virtio_crypto *vcrypto = vdev->priv;
+	int i;
 
 	dev_info(&vdev->dev, "Start virtcrypto_remove.\n");
 
 	if (virtcrypto_dev_started(vcrypto))
 		virtcrypto_dev_stop(vcrypto);
+	for (i = 0; i < vcrypto->max_data_queues; i++)
+		tasklet_kill(&vcrypto->data_vq[i].done_task);
 	vdev->config->reset(vdev);
 	virtcrypto_free_unused_reqs(vcrypto);
 	virtcrypto_clear_crypto_engines(vcrypto);
diff --git drivers/dma/sh/shdma.h drivers/dma/sh/shdma.h
index 2c0a969adc9f..35987a35a848 100644
--- linux-4.14.336/drivers/dma/sh/shdma.h
+++ linux-4.14.336/drivers/dma/sh/shdma.h
@@ -29,7 +29,7 @@ struct sh_dmae_chan {
 	const struct sh_dmae_slave_config *config; /* Slave DMA configuration */
 	int xmit_shift;			/* log_2(bytes_per_xfer) */
 	void __iomem *base;
-	char dev_id[16];		/* unique name per DMAC of channel */
+	char dev_id[32];		/* unique name per DMAC of channel */
 	int pm_error;
 	dma_addr_t slave_addr;
 };
diff --git drivers/edac/thunderx_edac.c drivers/edac/thunderx_edac.c
index dfefa39e9351..bc9ecc6c0573 100644
--- linux-4.14.336/drivers/edac/thunderx_edac.c
+++ linux-4.14.336/drivers/edac/thunderx_edac.c
@@ -1154,7 +1154,7 @@ static irqreturn_t thunderx_ocx_com_threaded_isr(int irq, void *irq_id)
 		decode_register(other, OCX_OTHER_SIZE,
 				ocx_com_errors, ctx->reg_com_int);
 
-		strncat(msg, other, OCX_MESSAGE_SIZE);
+		strlcat(msg, other, OCX_MESSAGE_SIZE);
 
 		for (lane = 0; lane < OCX_RX_LANES; lane++)
 			if (ctx->reg_com_int & BIT(lane)) {
@@ -1163,12 +1163,12 @@ static irqreturn_t thunderx_ocx_com_threaded_isr(int irq, void *irq_id)
 					 lane, ctx->reg_lane_int[lane],
 					 lane, ctx->reg_lane_stat11[lane]);
 
-				strncat(msg, other, OCX_MESSAGE_SIZE);
+				strlcat(msg, other, OCX_MESSAGE_SIZE);
 
 				decode_register(other, OCX_OTHER_SIZE,
 						ocx_lane_errors,
 						ctx->reg_lane_int[lane]);
-				strncat(msg, other, OCX_MESSAGE_SIZE);
+				strlcat(msg, other, OCX_MESSAGE_SIZE);
 			}
 
 		if (ctx->reg_com_int & OCX_COM_INT_CE)
@@ -1238,7 +1238,7 @@ static irqreturn_t thunderx_ocx_lnk_threaded_isr(int irq, void *irq_id)
 		decode_register(other, OCX_OTHER_SIZE,
 				ocx_com_link_errors, ctx->reg_com_link_int);
 
-		strncat(msg, other, OCX_MESSAGE_SIZE);
+		strlcat(msg, other, OCX_MESSAGE_SIZE);
 
 		if (ctx->reg_com_link_int & OCX_COM_LINK_INT_UE)
 			edac_device_handle_ue(ocx->edac_dev, 0, 0, msg);
@@ -1917,7 +1917,7 @@ static irqreturn_t thunderx_l2c_threaded_isr(int irq, void *irq_id)
 
 		decode_register(other, L2C_OTHER_SIZE, l2_errors, ctx->reg_int);
 
-		strncat(msg, other, L2C_MESSAGE_SIZE);
+		strlcat(msg, other, L2C_MESSAGE_SIZE);
 
 		if (ctx->reg_int & mask_ue)
 			edac_device_handle_ue(l2c->edac_dev, 0, 0, msg);
diff --git drivers/firewire/core-card.c drivers/firewire/core-card.c
index 11c634125c7d..0e6f96c0e395 100644
--- linux-4.14.336/drivers/firewire/core-card.c
+++ linux-4.14.336/drivers/firewire/core-card.c
@@ -442,7 +442,23 @@ static void bm_work(struct work_struct *work)
 	 */
 	card->bm_generation = generation;
 
-	if (root_device == NULL) {
+	if (card->gap_count == 0) {
+		/*
+		 * If self IDs have inconsistent gap counts, do a
+		 * bus reset ASAP. The config rom read might never
+		 * complete, so don't wait for it. However, still
+		 * send a PHY configuration packet prior to the
+		 * bus reset. The PHY configuration packet might
+		 * fail, but 1394-2008 8.4.5.2 explicitly permits
+		 * it in this case, so it should be safe to try.
+		 */
+		new_root_id = local_id;
+		/*
+		 * We must always send a bus reset if the gap count
+		 * is inconsistent, so bypass the 5-reset limit.
+		 */
+		card->bm_retries = 0;
+	} else if (root_device == NULL) {
 		/*
 		 * Either link_on is false, or we failed to read the
 		 * config rom.  In either case, pick another root.
diff --git drivers/firewire/core-device.c drivers/firewire/core-device.c
index a293b39fd4ce..25c5de074525 100644
--- linux-4.14.336/drivers/firewire/core-device.c
+++ linux-4.14.336/drivers/firewire/core-device.c
@@ -113,10 +113,9 @@ static int textual_leaf_to_string(const u32 *block, char *buf, size_t size)
  * @buf:	where to put the string
  * @size:	size of @buf, in bytes
  *
- * The string is taken from a minimal ASCII text descriptor leaf after
- * the immediate entry with @key.  The string is zero-terminated.
- * An overlong string is silently truncated such that it and the
- * zero byte fit into @size.
+ * The string is taken from a minimal ASCII text descriptor leaf just after the entry with the
+ * @key. The string is zero-terminated. An overlong string is silently truncated such that it
+ * and the zero byte fit into @size.
  *
  * Returns strlen(buf) or a negative error code.
  */
diff --git drivers/firmware/efi/capsule-loader.c drivers/firmware/efi/capsule-loader.c
index 539825a17959..fa36bbdb9ca7 100644
--- linux-4.14.336/drivers/firmware/efi/capsule-loader.c
+++ linux-4.14.336/drivers/firmware/efi/capsule-loader.c
@@ -287,7 +287,7 @@ static int efi_capsule_open(struct inode *inode, struct file *file)
 		return -ENOMEM;
 	}
 
-	cap_info->phys = kzalloc(sizeof(void *), GFP_KERNEL);
+	cap_info->phys = kzalloc(sizeof(phys_addr_t), GFP_KERNEL);
 	if (!cap_info->phys) {
 		kfree(cap_info->pages);
 		kfree(cap_info);
diff --git drivers/firmware/ti_sci.c drivers/firmware/ti_sci.c
index dd677fc4578a..7ac5a8bd05c4 100644
--- linux-4.14.336/drivers/firmware/ti_sci.c
+++ linux-4.14.336/drivers/firmware/ti_sci.c
@@ -184,7 +184,7 @@ static int ti_sci_debugfs_create(struct platform_device *pdev,
 {
 	struct device *dev = &pdev->dev;
 	struct resource *res;
-	char debug_name[50] = "ti_sci_debug@";
+	char debug_name[50];
 
 	/* Debug region is optional */
 	res = platform_get_resource_byname(pdev, IORESOURCE_MEM,
@@ -201,10 +201,10 @@ static int ti_sci_debugfs_create(struct platform_device *pdev,
 	/* Setup NULL termination */
 	info->debug_buffer[info->debug_region_size] = 0;
 
-	info->d = debugfs_create_file(strncat(debug_name, dev_name(dev),
-					      sizeof(debug_name) -
-					      sizeof("ti_sci_debug@")),
-				      0444, NULL, info, &ti_sci_debug_fops);
+	snprintf(debug_name, sizeof(debug_name), "ti_sci_debug@%s",
+		 dev_name(dev));
+	info->d = debugfs_create_file(debug_name, 0444, NULL, info,
+				      &ti_sci_debug_fops);
 	if (IS_ERR(info->d))
 		return PTR_ERR(info->d);
 
diff --git drivers/gpio/gpio-74x164.c drivers/gpio/gpio-74x164.c
index 15a1f4b348c4..4043fe0c8247 100644
--- linux-4.14.336/drivers/gpio/gpio-74x164.c
+++ linux-4.14.336/drivers/gpio/gpio-74x164.c
@@ -133,8 +133,6 @@ static int gen_74x164_probe(struct spi_device *spi)
 	if (IS_ERR(chip->gpiod_oe))
 		return PTR_ERR(chip->gpiod_oe);
 
-	gpiod_set_value_cansleep(chip->gpiod_oe, 1);
-
 	spi_set_drvdata(spi, chip);
 
 	chip->gpio_chip.label = spi->modalias;
@@ -159,6 +157,8 @@ static int gen_74x164_probe(struct spi_device *spi)
 		goto exit_destroy;
 	}
 
+	gpiod_set_value_cansleep(chip->gpiod_oe, 1);
+
 	ret = gpiochip_add_data(&chip->gpio_chip, chip);
 	if (!ret)
 		return 0;
diff --git drivers/gpio/gpiolib-acpi.c drivers/gpio/gpiolib-acpi.c
index 713dc43024c9..a2d00b1ff117 100644
--- linux-4.14.336/drivers/gpio/gpiolib-acpi.c
+++ linux-4.14.336/drivers/gpio/gpiolib-acpi.c
@@ -1476,6 +1476,20 @@ static const struct dmi_system_id gpiolib_acpi_quirks[] = {
 			.ignore_wake = "INT33FF:01@0",
 		},
 	},
+	{
+		/*
+		 * Spurious wakeups from TP_ATTN# pin
+		 * Found in BIOS 0.35
+		 * https://gitlab.freedesktop.org/drm/amd/-/issues/3073
+		 */
+		.matches = {
+			DMI_MATCH(DMI_SYS_VENDOR, "GPD"),
+			DMI_MATCH(DMI_PRODUCT_NAME, "G1619-04"),
+		},
+		.driver_data = &(struct acpi_gpiolib_dmi_quirk) {
+			.ignore_wake = "PNP0C50:00@8",
+		},
+	},
 	{} /* Terminating entry */
 };
 
diff --git drivers/gpu/drm/amd/amdgpu/amdgpu_device.c drivers/gpu/drm/amd/amdgpu/amdgpu_device.c
index 076b22c44122..d7192b2a980c 100644
--- linux-4.14.336/drivers/gpu/drm/amd/amdgpu/amdgpu_device.c
+++ linux-4.14.336/drivers/gpu/drm/amd/amdgpu/amdgpu_device.c
@@ -701,6 +701,7 @@ static bool amdgpu_vpost_needed(struct amdgpu_device *adev)
 				return true;
 
 			fw_ver = *((uint32_t *)adev->pm.fw->data + 69);
+			release_firmware(adev->pm.fw);
 			if (fw_ver < 0x00160e00)
 				return true;
 		}
diff --git drivers/gpu/drm/amd/amdgpu/kv_dpm.c drivers/gpu/drm/amd/amdgpu/kv_dpm.c
index d99fb88341f4..a4c9a326e9f5 100644
--- linux-4.14.336/drivers/gpu/drm/amd/amdgpu/kv_dpm.c
+++ linux-4.14.336/drivers/gpu/drm/amd/amdgpu/kv_dpm.c
@@ -2718,10 +2718,8 @@ static int kv_parse_power_table(struct amdgpu_device *adev)
 		non_clock_info = (struct _ATOM_PPLIB_NONCLOCK_INFO *)
 			&non_clock_info_array->nonClockInfo[non_clock_array_index];
 		ps = kzalloc(sizeof(struct kv_ps), GFP_KERNEL);
-		if (ps == NULL) {
-			kfree(adev->pm.dpm.ps);
+		if (ps == NULL)
 			return -ENOMEM;
-		}
 		adev->pm.dpm.ps[i].ps_priv = ps;
 		k = 0;
 		idx = (u8 *)&power_state->v2.clockInfoIndex[0];
diff --git drivers/gpu/drm/amd/amdgpu/si_dpm.c drivers/gpu/drm/amd/amdgpu/si_dpm.c
index 288ac692f536..5f80f44f5f67 100644
--- linux-4.14.336/drivers/gpu/drm/amd/amdgpu/si_dpm.c
+++ linux-4.14.336/drivers/gpu/drm/amd/amdgpu/si_dpm.c
@@ -7336,10 +7336,9 @@ static int si_dpm_init(struct amdgpu_device *adev)
 
 	adev->pm.dpm.dyn_state.vddc_dependency_on_dispclk.entries =
 		kzalloc(4 * sizeof(struct amdgpu_clock_voltage_dependency_entry), GFP_KERNEL);
-	if (!adev->pm.dpm.dyn_state.vddc_dependency_on_dispclk.entries) {
-		amdgpu_free_extended_power_table(adev);
+	if (!adev->pm.dpm.dyn_state.vddc_dependency_on_dispclk.entries)
 		return -ENOMEM;
-	}
+
 	adev->pm.dpm.dyn_state.vddc_dependency_on_dispclk.count = 4;
 	adev->pm.dpm.dyn_state.vddc_dependency_on_dispclk.entries[0].clk = 0;
 	adev->pm.dpm.dyn_state.vddc_dependency_on_dispclk.entries[0].v = 0;
diff --git drivers/gpu/drm/bridge/nxp-ptn3460.c drivers/gpu/drm/bridge/nxp-ptn3460.c
index d64a3283822a..4ea809891f64 100644
--- linux-4.14.336/drivers/gpu/drm/bridge/nxp-ptn3460.c
+++ linux-4.14.336/drivers/gpu/drm/bridge/nxp-ptn3460.c
@@ -64,13 +64,13 @@ static int ptn3460_read_bytes(struct ptn3460_bridge *ptn_bridge, char addr,
 	int ret;
 
 	ret = i2c_master_send(ptn_bridge->client, &addr, 1);
-	if (ret <= 0) {
+	if (ret < 0) {
 		DRM_ERROR("Failed to send i2c command, ret=%d\n", ret);
 		return ret;
 	}
 
 	ret = i2c_master_recv(ptn_bridge->client, buf, len);
-	if (ret <= 0) {
+	if (ret < 0) {
 		DRM_ERROR("Failed to recv i2c data, ret=%d\n", ret);
 		return ret;
 	}
@@ -88,7 +88,7 @@ static int ptn3460_write_byte(struct ptn3460_bridge *ptn_bridge, char addr,
 	buf[1] = val;
 
 	ret = i2c_master_send(ptn_bridge->client, buf, ARRAY_SIZE(buf));
-	if (ret <= 0) {
+	if (ret < 0) {
 		DRM_ERROR("Failed to send i2c command, ret=%d\n", ret);
 		return ret;
 	}
diff --git drivers/gpu/drm/drm_crtc.c drivers/gpu/drm/drm_crtc.c
index 5af25ce5bf7c..7e37b439ecae 100644
--- linux-4.14.336/drivers/gpu/drm/drm_crtc.c
+++ linux-4.14.336/drivers/gpu/drm/drm_crtc.c
@@ -556,8 +556,7 @@ int drm_mode_setcrtc(struct drm_device *dev, void *data,
 	struct drm_mode_set set;
 	uint32_t __user *set_connectors_ptr;
 	struct drm_modeset_acquire_ctx ctx;
-	int ret;
-	int i;
+	int ret, i, num_connectors = 0;
 
 	if (!drm_core_check_feature(dev, DRIVER_MODESET))
 		return -EINVAL;
@@ -692,6 +691,7 @@ retry:
 					connector->name);
 
 			connector_set[i] = connector;
+			num_connectors++;
 		}
 	}
 
@@ -700,7 +700,7 @@ retry:
 	set.y = crtc_req->y;
 	set.mode = mode;
 	set.connectors = connector_set;
-	set.num_connectors = crtc_req->count_connectors;
+	set.num_connectors = num_connectors;
 	set.fb = fb;
 	ret = __drm_mode_set_config_internal(&set, &ctx);
 
@@ -709,7 +709,7 @@ out:
 		drm_framebuffer_put(fb);
 
 	if (connector_set) {
-		for (i = 0; i < crtc_req->count_connectors; i++) {
+		for (i = 0; i < num_connectors; i++) {
 			if (connector_set[i])
 				drm_connector_put(connector_set[i]);
 		}
diff --git drivers/gpu/drm/drm_drv.c drivers/gpu/drm/drm_drv.c
index 340440febf9a..384a060aa8a1 100644
--- linux-4.14.336/drivers/gpu/drm/drm_drv.c
+++ linux-4.14.336/drivers/gpu/drm/drm_drv.c
@@ -812,8 +812,11 @@ int drm_dev_register(struct drm_device *dev, unsigned long flags)
 			goto err_minors;
 	}
 
-	if (drm_core_check_feature(dev, DRIVER_MODESET))
-		drm_modeset_register_all(dev);
+	if (drm_core_check_feature(dev, DRIVER_MODESET)) {
+		ret = drm_modeset_register_all(dev);
+		if (ret)
+			goto err_unload;
+	}
 
 	ret = 0;
 
@@ -825,6 +828,9 @@ int drm_dev_register(struct drm_device *dev, unsigned long flags)
 
 	goto out_unlock;
 
+err_unload:
+	if (dev->driver->unload)
+		dev->driver->unload(dev);
 err_minors:
 	remove_compat_control_link(dev);
 	drm_minor_unregister(dev, DRM_MINOR_PRIMARY);
diff --git drivers/gpu/drm/drm_file.c drivers/gpu/drm/drm_file.c
index 3cf07f5063ff..8705060c72b4 100644
--- linux-4.14.336/drivers/gpu/drm/drm_file.c
+++ linux-4.14.336/drivers/gpu/drm/drm_file.c
@@ -138,7 +138,7 @@ int drm_open(struct inode *inode, struct file *filp)
 {
 	struct drm_device *dev;
 	struct drm_minor *minor;
-	int retcode;
+	int retcode = 0;
 	int need_setup = 0;
 
 	minor = drm_minor_acquire(iminor(inode));
diff --git drivers/gpu/drm/drm_framebuffer.c drivers/gpu/drm/drm_framebuffer.c
index af40189cdb60..d6476223a941 100644
--- linux-4.14.336/drivers/gpu/drm/drm_framebuffer.c
+++ linux-4.14.336/drivers/gpu/drm/drm_framebuffer.c
@@ -521,7 +521,7 @@ int drm_mode_dirtyfb_ioctl(struct drm_device *dev,
 	struct drm_framebuffer *fb;
 	unsigned flags;
 	int num_clips;
-	int ret;
+	int ret = 0;
 
 	if (!drm_core_check_feature(dev, DRIVER_MODESET))
 		return -EINVAL;
diff --git drivers/gpu/drm/drm_mipi_dsi.c drivers/gpu/drm/drm_mipi_dsi.c
index 6995bee5ad0f..488e8e35c722 100644
--- linux-4.14.336/drivers/gpu/drm/drm_mipi_dsi.c
+++ linux-4.14.336/drivers/gpu/drm/drm_mipi_dsi.c
@@ -305,7 +305,8 @@ static int mipi_dsi_remove_device_fn(struct device *dev, void *priv)
 {
 	struct mipi_dsi_device *dsi = to_mipi_dsi_device(dev);
 
-	mipi_dsi_detach(dsi);
+	if (dsi->attached)
+		mipi_dsi_detach(dsi);
 	mipi_dsi_device_unregister(dsi);
 
 	return 0;
@@ -328,11 +329,18 @@ EXPORT_SYMBOL(mipi_dsi_host_unregister);
 int mipi_dsi_attach(struct mipi_dsi_device *dsi)
 {
 	const struct mipi_dsi_host_ops *ops = dsi->host->ops;
+	int ret;
 
 	if (!ops || !ops->attach)
 		return -ENOSYS;
 
-	return ops->attach(dsi->host, dsi);
+	ret = ops->attach(dsi->host, dsi);
+	if (ret)
+		return ret;
+
+	dsi->attached = true;
+
+	return 0;
 }
 EXPORT_SYMBOL(mipi_dsi_attach);
 
@@ -344,9 +352,14 @@ int mipi_dsi_detach(struct mipi_dsi_device *dsi)
 {
 	const struct mipi_dsi_host_ops *ops = dsi->host->ops;
 
+	if (WARN_ON(!dsi->attached))
+		return -EINVAL;
+
 	if (!ops || !ops->detach)
 		return -ENOSYS;
 
+	dsi->attached = false;
+
 	return ops->detach(dsi->host, dsi);
 }
 EXPORT_SYMBOL(mipi_dsi_detach);
diff --git drivers/gpu/drm/drm_plane.c drivers/gpu/drm/drm_plane.c
index 71186bf90760..5354dedaa608 100644
--- linux-4.14.336/drivers/gpu/drm/drm_plane.c
+++ linux-4.14.336/drivers/gpu/drm/drm_plane.c
@@ -1072,6 +1072,7 @@ retry:
 out:
 	if (fb)
 		drm_framebuffer_put(fb);
+	fb = NULL;
 	if (crtc->primary->old_fb)
 		drm_framebuffer_put(crtc->primary->old_fb);
 	crtc->primary->old_fb = NULL;
diff --git drivers/gpu/drm/exynos/exynos_drm_drv.c drivers/gpu/drm/exynos/exynos_drm_drv.c
index 82b72425a42f..707b4fdd94a7 100644
--- linux-4.14.336/drivers/gpu/drm/exynos/exynos_drm_drv.c
+++ linux-4.14.336/drivers/gpu/drm/exynos/exynos_drm_drv.c
@@ -407,6 +407,7 @@ err_mode_config_cleanup:
 	drm_release_iommu_mapping(drm);
 err_free_private:
 	kfree(private);
+	dev_set_drvdata(dev, NULL);
 err_free_drm:
 	drm_dev_unref(drm);
 
@@ -423,6 +424,7 @@ static void exynos_drm_unbind(struct device *dev)
 
 	exynos_drm_fbdev_fini(drm);
 	drm_kms_helper_poll_fini(drm);
+	drm_atomic_helper_shutdown(drm);
 
 	component_unbind_all(drm->dev, drm);
 	drm_mode_config_cleanup(drm);
@@ -460,9 +462,18 @@ static int exynos_drm_platform_remove(struct platform_device *pdev)
 	return 0;
 }
 
+static void exynos_drm_platform_shutdown(struct platform_device *pdev)
+{
+	struct drm_device *drm = platform_get_drvdata(pdev);
+
+	if (drm)
+		drm_atomic_helper_shutdown(drm);
+}
+
 static struct platform_driver exynos_drm_platform_driver = {
 	.probe	= exynos_drm_platform_probe,
 	.remove	= exynos_drm_platform_remove,
+	.shutdown = exynos_drm_platform_shutdown,
 	.driver	= {
 		.name	= "exynos-drm",
 		.pm	= &exynos_drm_pm_ops,
diff --git drivers/gpu/drm/exynos/exynos_hdmi.c drivers/gpu/drm/exynos/exynos_hdmi.c
index 0109ff40b1db..3d79a7af8c86 100644
--- linux-4.14.336/drivers/gpu/drm/exynos/exynos_hdmi.c
+++ linux-4.14.336/drivers/gpu/drm/exynos/exynos_hdmi.c
@@ -1722,6 +1722,8 @@ static int hdmi_bind(struct device *dev, struct device *master, void *data)
 		return ret;
 
 	crtc = exynos_drm_crtc_get_by_type(drm_dev, EXYNOS_DISPLAY_TYPE_HDMI);
+	if (IS_ERR(crtc))
+		return PTR_ERR(crtc);
 	crtc->pipe_clk = &hdata->phy_clk;
 
 	ret = hdmi_create_connector(encoder);
diff --git drivers/gpu/drm/msm/mdp/mdp4/mdp4_crtc.c drivers/gpu/drm/msm/mdp/mdp4/mdp4_crtc.c
index 47fa2aba1983..de0dac7b5d85 100644
--- linux-4.14.336/drivers/gpu/drm/msm/mdp/mdp4/mdp4_crtc.c
+++ linux-4.14.336/drivers/gpu/drm/msm/mdp/mdp4/mdp4_crtc.c
@@ -284,6 +284,7 @@ static void mdp4_crtc_atomic_disable(struct drm_crtc *crtc,
 {
 	struct mdp4_crtc *mdp4_crtc = to_mdp4_crtc(crtc);
 	struct mdp4_kms *mdp4_kms = get_kms(crtc);
+	unsigned long flags;
 
 	DBG("%s", mdp4_crtc->name);
 
@@ -293,6 +294,14 @@ static void mdp4_crtc_atomic_disable(struct drm_crtc *crtc,
 	mdp_irq_unregister(&mdp4_kms->base, &mdp4_crtc->err);
 	mdp4_disable(mdp4_kms);
 
+	if (crtc->state->event && !crtc->state->active) {
+		WARN_ON(mdp4_crtc->event);
+		spin_lock_irqsave(&mdp4_kms->dev->event_lock, flags);
+		drm_crtc_send_vblank_event(crtc, crtc->state->event);
+		crtc->state->event = NULL;
+		spin_unlock_irqrestore(&mdp4_kms->dev->event_lock, flags);
+	}
+
 	mdp4_crtc->enabled = false;
 }
 
diff --git drivers/gpu/drm/nouveau/nvkm/subdev/bios/shadow.c drivers/gpu/drm/nouveau/nvkm/subdev/bios/shadow.c
index 4b571cc6bc70..6597def18627 100644
--- linux-4.14.336/drivers/gpu/drm/nouveau/nvkm/subdev/bios/shadow.c
+++ linux-4.14.336/drivers/gpu/drm/nouveau/nvkm/subdev/bios/shadow.c
@@ -154,11 +154,17 @@ shadow_fw_init(struct nvkm_bios *bios, const char *name)
 	return (void *)fw;
 }
 
+static void
+shadow_fw_release(void *fw)
+{
+	release_firmware(fw);
+}
+
 static const struct nvbios_source
 shadow_fw = {
 	.name = "firmware",
 	.init = shadow_fw_init,
-	.fini = (void(*)(void *))release_firmware,
+	.fini = shadow_fw_release,
 	.read = shadow_fw_read,
 	.rw = false,
 };
diff --git drivers/gpu/drm/radeon/r100.c drivers/gpu/drm/radeon/r100.c
index a4929372090d..56e13bdd4bd0 100644
--- linux-4.14.336/drivers/gpu/drm/radeon/r100.c
+++ linux-4.14.336/drivers/gpu/drm/radeon/r100.c
@@ -2307,7 +2307,7 @@ int r100_cs_track_check(struct radeon_device *rdev, struct r100_cs_track *track)
 	switch (prim_walk) {
 	case 1:
 		for (i = 0; i < track->num_arrays; i++) {
-			size = track->arrays[i].esize * track->max_indx * 4;
+			size = track->arrays[i].esize * track->max_indx * 4UL;
 			if (track->arrays[i].robj == NULL) {
 				DRM_ERROR("(PW %u) Vertex array %u no buffer "
 					  "bound\n", prim_walk, i);
@@ -2326,7 +2326,7 @@ int r100_cs_track_check(struct radeon_device *rdev, struct r100_cs_track *track)
 		break;
 	case 2:
 		for (i = 0; i < track->num_arrays; i++) {
-			size = track->arrays[i].esize * (nverts - 1) * 4;
+			size = track->arrays[i].esize * (nverts - 1) * 4UL;
 			if (track->arrays[i].robj == NULL) {
 				DRM_ERROR("(PW %u) Vertex array %u no buffer "
 					  "bound\n", prim_walk, i);
diff --git drivers/gpu/drm/radeon/r600_cs.c drivers/gpu/drm/radeon/r600_cs.c
index 97fd58e97043..f478d88aea8f 100644
--- linux-4.14.336/drivers/gpu/drm/radeon/r600_cs.c
+++ linux-4.14.336/drivers/gpu/drm/radeon/r600_cs.c
@@ -1278,7 +1278,7 @@ static int r600_cs_check_reg(struct radeon_cs_parser *p, u32 reg, u32 idx)
 			return -EINVAL;
 		}
 		tmp = (reg - CB_COLOR0_BASE) / 4;
-		track->cb_color_bo_offset[tmp] = radeon_get_ib_value(p, idx) << 8;
+		track->cb_color_bo_offset[tmp] = (u64)radeon_get_ib_value(p, idx) << 8;
 		ib[idx] += (u32)((reloc->gpu_offset >> 8) & 0xffffffff);
 		track->cb_color_base_last[tmp] = ib[idx];
 		track->cb_color_bo[tmp] = reloc->robj;
@@ -1305,7 +1305,7 @@ static int r600_cs_check_reg(struct radeon_cs_parser *p, u32 reg, u32 idx)
 					"0x%04X\n", reg);
 			return -EINVAL;
 		}
-		track->htile_offset = radeon_get_ib_value(p, idx) << 8;
+		track->htile_offset = (u64)radeon_get_ib_value(p, idx) << 8;
 		ib[idx] += (u32)((reloc->gpu_offset >> 8) & 0xffffffff);
 		track->htile_bo = reloc->robj;
 		track->db_dirty = true;
diff --git drivers/gpu/drm/radeon/radeon_display.c drivers/gpu/drm/radeon/radeon_display.c
index 173439a8c881..620f301737a4 100644
--- linux-4.14.336/drivers/gpu/drm/radeon/radeon_display.c
+++ linux-4.14.336/drivers/gpu/drm/radeon/radeon_display.c
@@ -678,11 +678,16 @@ static void radeon_crtc_init(struct drm_device *dev, int index)
 	if (radeon_crtc == NULL)
 		return;
 
+	radeon_crtc->flip_queue = alloc_workqueue("radeon-crtc", WQ_HIGHPRI, 0);
+	if (!radeon_crtc->flip_queue) {
+		kfree(radeon_crtc);
+		return;
+	}
+
 	drm_crtc_init(dev, &radeon_crtc->base, &radeon_crtc_funcs);
 
 	drm_mode_crtc_set_gamma_size(&radeon_crtc->base, 256);
 	radeon_crtc->crtc_id = index;
-	radeon_crtc->flip_queue = alloc_workqueue("radeon-crtc", WQ_HIGHPRI, 0);
 	rdev->mode_info.crtcs[index] = radeon_crtc;
 
 	if (rdev->family >= CHIP_BONAIRE) {
diff --git drivers/gpu/drm/radeon/radeon_vm.c drivers/gpu/drm/radeon/radeon_vm.c
index e5c0e635e371..6f2133ff7c2c 100644
--- linux-4.14.336/drivers/gpu/drm/radeon/radeon_vm.c
+++ linux-4.14.336/drivers/gpu/drm/radeon/radeon_vm.c
@@ -1205,13 +1205,17 @@ int radeon_vm_init(struct radeon_device *rdev, struct radeon_vm *vm)
 	r = radeon_bo_create(rdev, pd_size, align, true,
 			     RADEON_GEM_DOMAIN_VRAM, 0, NULL,
 			     NULL, &vm->page_directory);
-	if (r)
+	if (r) {
+		kfree(vm->page_tables);
+		vm->page_tables = NULL;
 		return r;
-
+	}
 	r = radeon_vm_clear_bo(rdev, vm->page_directory);
 	if (r) {
 		radeon_bo_unref(&vm->page_directory);
 		vm->page_directory = NULL;
+		kfree(vm->page_tables);
+		vm->page_tables = NULL;
 		return r;
 	}
 
diff --git drivers/gpu/drm/radeon/si.c drivers/gpu/drm/radeon/si.c
index 1144cafea9ac..6dc20e790556 100644
--- linux-4.14.336/drivers/gpu/drm/radeon/si.c
+++ linux-4.14.336/drivers/gpu/drm/radeon/si.c
@@ -3612,6 +3612,10 @@ static int si_cp_start(struct radeon_device *rdev)
 	for (i = RADEON_RING_TYPE_GFX_INDEX; i <= CAYMAN_RING_TYPE_CP2_INDEX; ++i) {
 		ring = &rdev->ring[i];
 		r = radeon_ring_lock(rdev, ring, 2);
+		if (r) {
+			DRM_ERROR("radeon: cp failed to lock ring (%d).\n", r);
+			return r;
+		}
 
 		/* clear the compute context state */
 		radeon_ring_write(ring, PACKET3_COMPUTE(PACKET3_CLEAR_STATE, 0));
diff --git drivers/gpu/drm/radeon/sumo_dpm.c drivers/gpu/drm/radeon/sumo_dpm.c
index fd4804829e46..258cca4ae59b 100644
--- linux-4.14.336/drivers/gpu/drm/radeon/sumo_dpm.c
+++ linux-4.14.336/drivers/gpu/drm/radeon/sumo_dpm.c
@@ -1493,8 +1493,10 @@ static int sumo_parse_power_table(struct radeon_device *rdev)
 		non_clock_array_index = power_state->v2.nonClockInfoIndex;
 		non_clock_info = (struct _ATOM_PPLIB_NONCLOCK_INFO *)
 			&non_clock_info_array->nonClockInfo[non_clock_array_index];
-		if (!rdev->pm.power_state[i].clock_info)
+		if (!rdev->pm.power_state[i].clock_info) {
+			kfree(rdev->pm.dpm.ps);
 			return -EINVAL;
+		}
 		ps = kzalloc(sizeof(struct sumo_ps), GFP_KERNEL);
 		if (ps == NULL) {
 			kfree(rdev->pm.dpm.ps);
diff --git drivers/gpu/drm/radeon/trinity_dpm.c drivers/gpu/drm/radeon/trinity_dpm.c
index 2ef7c4e5e495..8fcb7466bf8c 100644
--- linux-4.14.336/drivers/gpu/drm/radeon/trinity_dpm.c
+++ linux-4.14.336/drivers/gpu/drm/radeon/trinity_dpm.c
@@ -1768,8 +1768,10 @@ static int trinity_parse_power_table(struct radeon_device *rdev)
 		non_clock_array_index = power_state->v2.nonClockInfoIndex;
 		non_clock_info = (struct _ATOM_PPLIB_NONCLOCK_INFO *)
 			&non_clock_info_array->nonClockInfo[non_clock_array_index];
-		if (!rdev->pm.power_state[i].clock_info)
+		if (!rdev->pm.power_state[i].clock_info) {
+			kfree(rdev->pm.dpm.ps);
 			return -EINVAL;
+		}
 		ps = kzalloc(sizeof(struct sumo_ps), GFP_KERNEL);
 		if (ps == NULL) {
 			kfree(rdev->pm.dpm.ps);
diff --git drivers/hid/hid-apple.c drivers/hid/hid-apple.c
index 80ecbf14d3c8..8ba8f76c92c0 100644
--- linux-4.14.336/drivers/hid/hid-apple.c
+++ linux-4.14.336/drivers/hid/hid-apple.c
@@ -54,6 +54,12 @@ MODULE_PARM_DESC(swap_opt_cmd, "Swap the Option (\"Alt\") and Command (\"Flag\")
 		"(For people who want to keep Windows PC keyboard muscle memory. "
 		"[0] = as-is, Mac layout. 1 = swapped, Windows layout.)");
 
+static unsigned int swap_fn_leftctrl;
+module_param(swap_fn_leftctrl, uint, 0644);
+MODULE_PARM_DESC(swap_fn_leftctrl, "Swap the Fn and left Control keys. "
+		"(For people who want to keep PC keyboard muscle memory. "
+		"[0] = as-is, Mac layout, 1 = swapped, PC layout)");
+
 struct apple_sc {
 	unsigned long quirks;
 	unsigned int fn_on;
@@ -67,6 +73,28 @@ struct apple_key_translation {
 	u8 flags;
 };
 
+static const struct apple_key_translation apple2021_fn_keys[] = {
+	{ KEY_BACKSPACE, KEY_DELETE },
+	{ KEY_ENTER,	KEY_INSERT },
+	{ KEY_F1,	KEY_BRIGHTNESSDOWN, APPLE_FLAG_FKEY },
+	{ KEY_F2,	KEY_BRIGHTNESSUP,   APPLE_FLAG_FKEY },
+	{ KEY_F3,	KEY_SCALE,          APPLE_FLAG_FKEY },
+	{ KEY_F4,	KEY_SEARCH,         APPLE_FLAG_FKEY },
+	{ KEY_F5,	KEY_MICMUTE,        APPLE_FLAG_FKEY },
+	{ KEY_F6,	KEY_SLEEP,          APPLE_FLAG_FKEY },
+	{ KEY_F7,	KEY_PREVIOUSSONG,   APPLE_FLAG_FKEY },
+	{ KEY_F8,	KEY_PLAYPAUSE,      APPLE_FLAG_FKEY },
+	{ KEY_F9,	KEY_NEXTSONG,       APPLE_FLAG_FKEY },
+	{ KEY_F10,	KEY_MUTE,           APPLE_FLAG_FKEY },
+	{ KEY_F11,	KEY_VOLUMEDOWN,     APPLE_FLAG_FKEY },
+	{ KEY_F12,	KEY_VOLUMEUP,       APPLE_FLAG_FKEY },
+	{ KEY_UP,	KEY_PAGEUP },
+	{ KEY_DOWN,	KEY_PAGEDOWN },
+	{ KEY_LEFT,	KEY_HOME },
+	{ KEY_RIGHT,	KEY_END },
+	{ }
+};
+
 static const struct apple_key_translation macbookair_fn_keys[] = {
 	{ KEY_BACKSPACE, KEY_DELETE },
 	{ KEY_ENTER,	KEY_INSERT },
@@ -166,6 +194,11 @@ static const struct apple_key_translation swapped_option_cmd_keys[] = {
 	{ }
 };
 
+static const struct apple_key_translation swapped_fn_leftctrl_keys[] = {
+	{ KEY_FN, KEY_LEFTCTRL },
+	{ }
+};
+
 static const struct apple_key_translation *apple_find_translation(
 		const struct apple_key_translation *table, u16 from)
 {
@@ -187,14 +220,18 @@ static int hidinput_apple_event(struct hid_device *hid, struct input_dev *input,
 	bool do_translate;
 	u16 code = 0;
 
-	if (usage->code == KEY_FN) {
+	u16 fn_keycode = (swap_fn_leftctrl) ? (KEY_LEFTCTRL) : (KEY_FN);
+
+	if (usage->code == fn_keycode) {
 		asc->fn_on = !!value;
-		input_event(input, usage->type, usage->code, value);
+		input_event(input, usage->type, KEY_FN, value);
 		return 1;
 	}
 
 	if (fnmode) {
-		if (hid->product >= USB_DEVICE_ID_APPLE_WELLSPRING4_ANSI &&
+		if (hid->product == USB_DEVICE_ID_APPLE_MAGIC_KEYBOARD_2021)
+			table = apple2021_fn_keys;
+		else if (hid->product >= USB_DEVICE_ID_APPLE_WELLSPRING4_ANSI &&
 				hid->product <= USB_DEVICE_ID_APPLE_WELLSPRING4A_JIS)
 			table = macbookair_fn_keys;
 		else if (hid->product < 0x21d || hid->product >= 0x300)
@@ -274,6 +311,14 @@ static int hidinput_apple_event(struct hid_device *hid, struct input_dev *input,
 		}
 	}
 
+	if (swap_fn_leftctrl) {
+		trans = apple_find_translation(swapped_fn_leftctrl_keys, usage->code);
+		if (trans) {
+			input_event(input, usage->type, trans->to, value);
+			return 1;
+		}
+	}
+
 	return 0;
 }
 
@@ -344,6 +389,14 @@ static void apple_setup_input(struct input_dev *input)
 
 	for (trans = apple_iso_keyboard; trans->from; trans++)
 		set_bit(trans->to, input->keybit);
+
+	for (trans = apple2021_fn_keys; trans->from; trans++)
+		set_bit(trans->to, input->keybit);
+
+	if (swap_fn_leftctrl) {
+		for (trans = swapped_fn_leftctrl_keys; trans->from; trans++)
+			set_bit(trans->to, input->keybit);
+	}
 }
 
 static int apple_input_mapping(struct hid_device *hdev, struct hid_input *hi,
@@ -599,6 +652,10 @@ static const struct hid_device_id apple_devices[] = {
 		.driver_data = APPLE_NUMLOCK_EMULATION | APPLE_HAS_FN },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_APPLE, USB_DEVICE_ID_APPLE_GEYSER1_TP_ONLY),
 		.driver_data = APPLE_NUMLOCK_EMULATION | APPLE_HAS_FN },
+	{ HID_USB_DEVICE(USB_VENDOR_ID_APPLE, USB_DEVICE_ID_APPLE_MAGIC_KEYBOARD_2021),
+		.driver_data = APPLE_HAS_FN },
+	{ HID_BLUETOOTH_DEVICE(BT_VENDOR_ID_APPLE, USB_DEVICE_ID_APPLE_MAGIC_KEYBOARD_2021),
+		.driver_data = APPLE_HAS_FN },
 
 	{ }
 };
diff --git drivers/hid/hid-core.c drivers/hid/hid-core.c
index fe3824a6af5c..9bfae325a410 100644
--- linux-4.14.336/drivers/hid/hid-core.c
+++ linux-4.14.336/drivers/hid/hid-core.c
@@ -2063,6 +2063,7 @@ static const struct hid_device_id hid_have_special_driver[] = {
 	{ HID_BLUETOOTH_DEVICE(BT_VENDOR_ID_APPLE, USB_DEVICE_ID_APPLE_MAGIC_KEYBOARD_NUMPAD_ANSI) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_APPLE, USB_DEVICE_ID_APPLE_FOUNTAIN_TP_ONLY) },
 	{ HID_USB_DEVICE(USB_VENDOR_ID_APPLE, USB_DEVICE_ID_APPLE_GEYSER1_TP_ONLY) },
+	{ HID_USB_DEVICE(USB_VENDOR_ID_APPLE, USB_DEVICE_ID_APPLE_MAGIC_KEYBOARD_2021) },
 #endif
 #if IS_ENABLED(CONFIG_HID_APPLEIR)
 	{ HID_USB_DEVICE(USB_VENDOR_ID_APPLE, USB_DEVICE_ID_APPLE_IRCONTROL) },
diff --git drivers/hid/hid-ids.h drivers/hid/hid-ids.h
index 26db838be5a2..1b89c9185c14 100644
--- linux-4.14.336/drivers/hid/hid-ids.h
+++ linux-4.14.336/drivers/hid/hid-ids.h
@@ -172,6 +172,7 @@
 #define USB_DEVICE_ID_APPLE_IRCONTROL3	0x8241
 #define USB_DEVICE_ID_APPLE_IRCONTROL4	0x8242
 #define USB_DEVICE_ID_APPLE_IRCONTROL5	0x8243
+#define USB_DEVICE_ID_APPLE_MAGIC_KEYBOARD_2021   0x029c
 
 #define USB_VENDOR_ID_ASUS		0x0486
 #define USB_DEVICE_ID_ASUS_T91MT	0x0185
diff --git drivers/hid/wacom_sys.c drivers/hid/wacom_sys.c
index 3ca50505c78c..b4c25afb3a36 100644
--- linux-4.14.336/drivers/hid/wacom_sys.c
+++ linux-4.14.336/drivers/hid/wacom_sys.c
@@ -1920,7 +1920,7 @@ static int wacom_allocate_inputs(struct wacom *wacom)
 	return 0;
 }
 
-static int wacom_register_inputs(struct wacom *wacom)
+static int wacom_setup_inputs(struct wacom *wacom)
 {
 	struct input_dev *pen_input_dev, *touch_input_dev, *pad_input_dev;
 	struct wacom_wac *wacom_wac = &(wacom->wacom_wac);
@@ -1939,10 +1939,6 @@ static int wacom_register_inputs(struct wacom *wacom)
 		input_free_device(pen_input_dev);
 		wacom_wac->pen_input = NULL;
 		pen_input_dev = NULL;
-	} else {
-		error = input_register_device(pen_input_dev);
-		if (error)
-			goto fail;
 	}
 
 	error = wacom_setup_touch_input_capabilities(touch_input_dev, wacom_wac);
@@ -1951,10 +1947,6 @@ static int wacom_register_inputs(struct wacom *wacom)
 		input_free_device(touch_input_dev);
 		wacom_wac->touch_input = NULL;
 		touch_input_dev = NULL;
-	} else {
-		error = input_register_device(touch_input_dev);
-		if (error)
-			goto fail;
 	}
 
 	error = wacom_setup_pad_input_capabilities(pad_input_dev, wacom_wac);
@@ -1963,7 +1955,34 @@ static int wacom_register_inputs(struct wacom *wacom)
 		input_free_device(pad_input_dev);
 		wacom_wac->pad_input = NULL;
 		pad_input_dev = NULL;
-	} else {
+	}
+
+	return 0;
+}
+
+static int wacom_register_inputs(struct wacom *wacom)
+{
+	struct input_dev *pen_input_dev, *touch_input_dev, *pad_input_dev;
+	struct wacom_wac *wacom_wac = &(wacom->wacom_wac);
+	int error = 0;
+
+	pen_input_dev = wacom_wac->pen_input;
+	touch_input_dev = wacom_wac->touch_input;
+	pad_input_dev = wacom_wac->pad_input;
+
+	if (pen_input_dev) {
+		error = input_register_device(pen_input_dev);
+		if (error)
+			goto fail;
+	}
+
+	if (touch_input_dev) {
+		error = input_register_device(touch_input_dev);
+		if (error)
+			goto fail;
+	}
+
+	if (pad_input_dev) {
 		error = input_register_device(pad_input_dev);
 		if (error)
 			goto fail;
@@ -2213,6 +2232,20 @@ static int wacom_parse_and_register(struct wacom *wacom, bool wireless)
 			goto fail;
 	}
 
+	error = wacom_setup_inputs(wacom);
+	if (error)
+		goto fail;
+
+	if (features->type == HID_GENERIC)
+		connect_mask |= HID_CONNECT_DRIVER;
+
+	/* Regular HID work starts now */
+	error = hid_hw_start(hdev, connect_mask);
+	if (error) {
+		hid_err(hdev, "hw start failed\n");
+		goto fail;
+	}
+
 	error = wacom_register_inputs(wacom);
 	if (error)
 		goto fail;
@@ -2227,16 +2260,6 @@ static int wacom_parse_and_register(struct wacom *wacom, bool wireless)
 			goto fail;
 	}
 
-	if (features->type == HID_GENERIC)
-		connect_mask |= HID_CONNECT_DRIVER;
-
-	/* Regular HID work starts now */
-	error = hid_hw_start(hdev, connect_mask);
-	if (error) {
-		hid_err(hdev, "hw start failed\n");
-		goto fail;
-	}
-
 	if (!wireless) {
 		/* Note that if query fails it is not a hard failure */
 		wacom_query_tablet_data(wacom);
diff --git drivers/hid/wacom_wac.c drivers/hid/wacom_wac.c
index 19a798eb395c..eb39c88b5eac 100644
--- linux-4.14.336/drivers/hid/wacom_wac.c
+++ linux-4.14.336/drivers/hid/wacom_wac.c
@@ -2317,7 +2317,14 @@ static void wacom_wac_pen_report(struct hid_device *hdev,
 				wacom_wac->hid_data.tipswitch);
 		input_report_key(input, wacom_wac->tool[0], prox);
 		if (wacom_wac->serial[0]) {
-			input_event(input, EV_MSC, MSC_SERIAL, wacom_wac->serial[0]);
+			/*
+			 * xf86-input-wacom does not accept a serial number
+			 * of '0'. Report the low 32 bits if possible, but
+			 * if they are zero, report the upper ones instead.
+			 */
+			__u32 serial_lo = wacom_wac->serial[0] & 0xFFFFFFFFu;
+			__u32 serial_hi = wacom_wac->serial[0] >> 32;
+			input_event(input, EV_MSC, MSC_SERIAL, (int)(serial_lo ? serial_lo : serial_hi));
 			input_report_abs(input, ABS_MISC, prox ? id : 0);
 		}
 
@@ -2389,8 +2396,8 @@ static void wacom_wac_finger_slot(struct wacom_wac *wacom_wac,
 {
 	struct hid_data *hid_data = &wacom_wac->hid_data;
 	bool mt = wacom_wac->features.touch_max > 1;
-	bool prox = hid_data->tipswitch &&
-		    report_touch_events(wacom_wac);
+	bool touch_down = hid_data->tipswitch && hid_data->confidence;
+	bool prox = touch_down && report_touch_events(wacom_wac);
 
 	if (wacom_wac->shared->has_mute_touch_switch &&
 	    !wacom_wac->shared->is_touch_on) {
@@ -2429,24 +2436,6 @@ static void wacom_wac_finger_slot(struct wacom_wac *wacom_wac,
 	}
 }
 
-static bool wacom_wac_slot_is_active(struct input_dev *dev, int key)
-{
-	struct input_mt *mt = dev->mt;
-	struct input_mt_slot *s;
-
-	if (!mt)
-		return false;
-
-	for (s = mt->slots; s != mt->slots + mt->num_slots; s++) {
-		if (s->key == key &&
-			input_mt_get_value(s, ABS_MT_TRACKING_ID) >= 0) {
-			return true;
-		}
-	}
-
-	return false;
-}
-
 static void wacom_wac_finger_event(struct hid_device *hdev,
 		struct hid_field *field, struct hid_usage *usage, __s32 value)
 {
@@ -2489,14 +2478,8 @@ static void wacom_wac_finger_event(struct hid_device *hdev,
 
 
 	if (usage->usage_index + 1 == field->report_count) {
-		if (equivalent_usage == wacom_wac->hid_data.last_slot_field) {
-			bool touch_removed = wacom_wac_slot_is_active(wacom_wac->touch_input,
-				wacom_wac->hid_data.id) && !wacom_wac->hid_data.tipswitch;
-
-			if (wacom_wac->hid_data.confidence || touch_removed) {
-				wacom_wac_finger_slot(wacom_wac, wacom_wac->touch_input);
-			}
-		}
+		if (equivalent_usage == wacom_wac->hid_data.last_slot_field)
+			wacom_wac_finger_slot(wacom_wac, wacom_wac->touch_input);
 	}
 }
 
diff --git drivers/hwmon/aspeed-pwm-tacho.c drivers/hwmon/aspeed-pwm-tacho.c
index e4337e9dda44..922c5930373b 100644
--- linux-4.14.336/drivers/hwmon/aspeed-pwm-tacho.c
+++ linux-4.14.336/drivers/hwmon/aspeed-pwm-tacho.c
@@ -195,6 +195,8 @@ struct aspeed_pwm_tacho_data {
 	u8 fan_tach_ch_source[16];
 	struct aspeed_cooling_device *cdev[8];
 	const struct attribute_group *groups[3];
+	/* protects access to shared ASPEED_PTCR_RESULT */
+	struct mutex tach_lock;
 };
 
 enum type { TYPEM, TYPEN, TYPEO };
@@ -529,6 +531,8 @@ static int aspeed_get_fan_tach_ch_rpm(struct aspeed_pwm_tacho_data *priv,
 	u8 fan_tach_ch_source, type, mode, both;
 	int ret;
 
+	mutex_lock(&priv->tach_lock);
+
 	regmap_write(priv->regmap, ASPEED_PTCR_TRIGGER, 0);
 	regmap_write(priv->regmap, ASPEED_PTCR_TRIGGER, 0x1 << fan_tach_ch);
 
@@ -546,6 +550,8 @@ static int aspeed_get_fan_tach_ch_rpm(struct aspeed_pwm_tacho_data *priv,
 		ASPEED_RPM_STATUS_SLEEP_USEC,
 		usec);
 
+	mutex_unlock(&priv->tach_lock);
+
 	/* return -ETIMEDOUT if we didn't get an answer. */
 	if (ret)
 		return ret;
@@ -929,6 +935,7 @@ static int aspeed_pwm_tacho_probe(struct platform_device *pdev)
 	priv = devm_kzalloc(dev, sizeof(*priv), GFP_KERNEL);
 	if (!priv)
 		return -ENOMEM;
+	mutex_init(&priv->tach_lock);
 	priv->regmap = devm_regmap_init(dev, NULL, (__force void *)regs,
 			&aspeed_pwm_tacho_regmap_config);
 	if (IS_ERR(priv->regmap))
diff --git drivers/hwmon/coretemp.c drivers/hwmon/coretemp.c
index 770bf76a5348..532cc7286cf0 100644
--- linux-4.14.336/drivers/hwmon/coretemp.c
+++ linux-4.14.336/drivers/hwmon/coretemp.c
@@ -53,7 +53,7 @@ MODULE_PARM_DESC(tjmax, "TjMax value in degrees Celsius");
 
 #define PKG_SYSFS_ATTR_NO	1	/* Sysfs attribute for package temp */
 #define BASE_SYSFS_ATTR_NO	2	/* Sysfs Base attr no for coretemp */
-#define NUM_REAL_CORES		128	/* Number of Real cores per cpu */
+#define NUM_REAL_CORES		512	/* Number of Real cores per cpu */
 #define CORETEMP_NAME_LENGTH	19	/* String Length of attrs */
 #define MAX_CORE_ATTRS		4	/* Maximum no of basic attrs */
 #define TOTAL_ATTRS		(MAX_CORE_ATTRS + 1)
diff --git drivers/hwtracing/coresight/coresight-etm4x.h drivers/hwtracing/coresight/coresight-etm4x.h
index b3b5ea7b7fb3..d48c40d8fc28 100644
--- linux-4.14.336/drivers/hwtracing/coresight/coresight-etm4x.h
+++ linux-4.14.336/drivers/hwtracing/coresight/coresight-etm4x.h
@@ -373,7 +373,7 @@ struct etmv4_drvdata {
 	u8				ctxid_size;
 	u8				vmid_size;
 	u8				ccsize;
-	u8				ccitmin;
+	u16				ccitmin;
 	u8				s_ex_level;
 	u8				ns_ex_level;
 	u8				q_support;
diff --git drivers/i2c/busses/i2c-s3c2410.c drivers/i2c/busses/i2c-s3c2410.c
index 911f8628128e..299d8f388d62 100644
--- linux-4.14.336/drivers/i2c/busses/i2c-s3c2410.c
+++ linux-4.14.336/drivers/i2c/busses/i2c-s3c2410.c
@@ -235,8 +235,17 @@ static bool is_ack(struct s3c24xx_i2c *i2c)
 	int tries;
 
 	for (tries = 50; tries; --tries) {
-		if (readl(i2c->regs + S3C2410_IICCON)
-			& S3C2410_IICCON_IRQPEND) {
+		unsigned long tmp = readl(i2c->regs + S3C2410_IICCON);
+
+		if (!(tmp & S3C2410_IICCON_ACKEN)) {
+			/*
+			 * Wait a bit for the bus to stabilize,
+			 * delay estimated experimentally.
+			 */
+			usleep_range(100, 200);
+			return true;
+		}
+		if (tmp & S3C2410_IICCON_IRQPEND) {
 			if (!(readl(i2c->regs + S3C2410_IICSTAT)
 				& S3C2410_IICSTAT_LASTBIT))
 				return true;
@@ -289,16 +298,6 @@ static void s3c24xx_i2c_message_start(struct s3c24xx_i2c *i2c,
 
 	stat |= S3C2410_IICSTAT_START;
 	writel(stat, i2c->regs + S3C2410_IICSTAT);
-
-	if (i2c->quirks & QUIRK_POLL) {
-		while ((i2c->msg_num != 0) && is_ack(i2c)) {
-			i2c_s3c_irq_nextbyte(i2c, stat);
-			stat = readl(i2c->regs + S3C2410_IICSTAT);
-
-			if (stat & S3C2410_IICSTAT_ARBITR)
-				dev_err(i2c->dev, "deal with arbitration loss\n");
-		}
-	}
 }
 
 static inline void s3c24xx_i2c_stop(struct s3c24xx_i2c *i2c, int ret)
@@ -705,7 +704,7 @@ static void s3c24xx_i2c_wait_idle(struct s3c24xx_i2c *i2c)
 static int s3c24xx_i2c_doxfer(struct s3c24xx_i2c *i2c,
 			      struct i2c_msg *msgs, int num)
 {
-	unsigned long timeout;
+	unsigned long timeout = 0;
 	int ret;
 
 	if (i2c->suspended)
@@ -728,16 +727,19 @@ static int s3c24xx_i2c_doxfer(struct s3c24xx_i2c *i2c,
 	s3c24xx_i2c_message_start(i2c, msgs);
 
 	if (i2c->quirks & QUIRK_POLL) {
-		ret = i2c->msg_idx;
+		while ((i2c->msg_num != 0) && is_ack(i2c)) {
+			unsigned long stat = readl(i2c->regs + S3C2410_IICSTAT);
 
-		if (ret != num)
-			dev_dbg(i2c->dev, "incomplete xfer (%d)\n", ret);
+			i2c_s3c_irq_nextbyte(i2c, stat);
 
-		goto out;
+			stat = readl(i2c->regs + S3C2410_IICSTAT);
+			if (stat & S3C2410_IICSTAT_ARBITR)
+				dev_err(i2c->dev, "deal with arbitration loss\n");
+		}
+	} else {
+		timeout = wait_event_timeout(i2c->wait, i2c->msg_num == 0, HZ * 5);
 	}
 
-	timeout = wait_event_timeout(i2c->wait, i2c->msg_num == 0, HZ * 5);
-
 	ret = i2c->msg_idx;
 
 	/*
diff --git drivers/infiniband/hw/hfi1/pio.c drivers/infiniband/hw/hfi1/pio.c
index 07bf282fd8aa..162f4cb4851a 100644
--- linux-4.14.336/drivers/infiniband/hw/hfi1/pio.c
+++ linux-4.14.336/drivers/infiniband/hw/hfi1/pio.c
@@ -2133,7 +2133,7 @@ int init_credit_return(struct hfi1_devdata *dd)
 				   "Unable to allocate credit return DMA range for NUMA %d\n",
 				   i);
 			ret = -ENOMEM;
-			goto done;
+			goto free_cr_base;
 		}
 	}
 	set_dev_node(&dd->pcidev->dev, dd->node);
@@ -2141,6 +2141,10 @@ int init_credit_return(struct hfi1_devdata *dd)
 	ret = 0;
 done:
 	return ret;
+
+free_cr_base:
+	free_credit_return(dd);
+	goto done;
 }
 
 void free_credit_return(struct hfi1_devdata *dd)
diff --git drivers/infiniband/hw/mthca/mthca_cmd.c drivers/infiniband/hw/mthca/mthca_cmd.c
index 419a2a20c047..7df5155cdb48 100644
--- linux-4.14.336/drivers/infiniband/hw/mthca/mthca_cmd.c
+++ linux-4.14.336/drivers/infiniband/hw/mthca/mthca_cmd.c
@@ -641,7 +641,7 @@ void mthca_free_mailbox(struct mthca_dev *dev, struct mthca_mailbox *mailbox)
 
 int mthca_SYS_EN(struct mthca_dev *dev)
 {
-	u64 out;
+	u64 out = 0;
 	int ret;
 
 	ret = mthca_cmd_imm(dev, 0, &out, 0, 0, CMD_SYS_EN, CMD_TIME_CLASS_D);
@@ -1961,7 +1961,7 @@ int mthca_WRITE_MGM(struct mthca_dev *dev, int index,
 int mthca_MGID_HASH(struct mthca_dev *dev, struct mthca_mailbox *mailbox,
 		    u16 *hash)
 {
-	u64 imm;
+	u64 imm = 0;
 	int err;
 
 	err = mthca_cmd_imm(dev, mailbox->dma, &imm, 0, 0, CMD_MGID_HASH,
diff --git drivers/infiniband/hw/mthca/mthca_main.c drivers/infiniband/hw/mthca/mthca_main.c
index ccf50dafce9c..66a85f757a2f 100644
--- linux-4.14.336/drivers/infiniband/hw/mthca/mthca_main.c
+++ linux-4.14.336/drivers/infiniband/hw/mthca/mthca_main.c
@@ -382,7 +382,7 @@ static int mthca_init_icm(struct mthca_dev *mdev,
 			  struct mthca_init_hca_param *init_hca,
 			  u64 icm_size)
 {
-	u64 aux_pages;
+	u64 aux_pages = 0;
 	int err;
 
 	err = mthca_SET_ICM_SIZE(mdev, icm_size, &aux_pages);
diff --git drivers/infiniband/ulp/ipoib/ipoib_multicast.c drivers/infiniband/ulp/ipoib/ipoib_multicast.c
index 9b3f47ae2016..25d7d9219591 100644
--- linux-4.14.336/drivers/infiniband/ulp/ipoib/ipoib_multicast.c
+++ linux-4.14.336/drivers/infiniband/ulp/ipoib/ipoib_multicast.c
@@ -543,21 +543,18 @@ static int ipoib_mcast_join(struct net_device *dev, struct ipoib_mcast *mcast)
 			/* SM supports sendonly-fullmember, otherwise fallback to full-member */
 			rec.join_state = SENDONLY_FULLMEMBER_JOIN;
 	}
-	spin_unlock_irq(&priv->lock);
 
 	multicast = ib_sa_join_multicast(&ipoib_sa_client, priv->ca, priv->port,
-					 &rec, comp_mask, GFP_KERNEL,
+					 &rec, comp_mask, GFP_ATOMIC,
 					 ipoib_mcast_join_complete, mcast);
-	spin_lock_irq(&priv->lock);
 	if (IS_ERR(multicast)) {
 		ret = PTR_ERR(multicast);
 		ipoib_warn(priv, "ib_sa_join_multicast failed, status %d\n", ret);
 		/* Requeue this join task with a backoff delay */
 		__ipoib_mcast_schedule_join_thread(priv, mcast, 1);
 		clear_bit(IPOIB_MCAST_FLAG_BUSY, &mcast->flags);
-		spin_unlock_irq(&priv->lock);
 		complete(&mcast->done);
-		spin_lock_irq(&priv->lock);
+		return ret;
 	}
 	return 0;
 }
diff --git drivers/infiniband/ulp/srpt/ib_srpt.c drivers/infiniband/ulp/srpt/ib_srpt.c
index 1446e1cc69ae..08343e6116d2 100644
--- linux-4.14.336/drivers/infiniband/ulp/srpt/ib_srpt.c
+++ linux-4.14.336/drivers/infiniband/ulp/srpt/ib_srpt.c
@@ -80,12 +80,16 @@ module_param(srpt_srq_size, int, 0444);
 MODULE_PARM_DESC(srpt_srq_size,
 		 "Shared receive queue (SRQ) size.");
 
+static int srpt_set_u64_x(const char *buffer, struct kernel_param *kp)
+{
+	return kstrtou64(buffer, 16, (u64 *)kp->arg);
+}
 static int srpt_get_u64_x(char *buffer, struct kernel_param *kp)
 {
 	return sprintf(buffer, "0x%016llx", *(u64 *)kp->arg);
 }
-module_param_call(srpt_service_guid, NULL, srpt_get_u64_x, &srpt_service_guid,
-		  0444);
+module_param_call(srpt_service_guid, srpt_set_u64_x, srpt_get_u64_x,
+		  &srpt_service_guid, 0444);
 MODULE_PARM_DESC(srpt_service_guid,
 		 "Using this value for ioc_guid, id_ext, and cm_listen_id"
 		 " instead of using the node_guid of the first HCA.");
@@ -196,8 +200,10 @@ static const char *get_ch_state_name(enum rdma_ch_state s)
 /**
  * srpt_qp_event() - QP event callback function.
  */
-static void srpt_qp_event(struct ib_event *event, struct srpt_rdma_ch *ch)
+static void srpt_qp_event(struct ib_event *event, void *ptr)
 {
+	struct srpt_rdma_ch *ch = ptr;
+
 	pr_debug("QP event %d on cm_id=%p sess_name=%s state=%d\n",
 		 event->event, ch->cm_id, ch->sess_name, ch->state);
 
@@ -1663,8 +1669,7 @@ retry:
 	}
 
 	qp_init->qp_context = (void *)ch;
-	qp_init->event_handler
-		= (void(*)(struct ib_event *, void*))srpt_qp_event;
+	qp_init->event_handler = srpt_qp_event;
 	qp_init->send_cq = ch->cq;
 	qp_init->recv_cq = ch->cq;
 	qp_init->srq = sdev->srq;
diff --git drivers/input/joystick/xpad.c drivers/input/joystick/xpad.c
index 1dbe30335458..3fedc3688e8f 100644
--- linux-4.14.336/drivers/input/joystick/xpad.c
+++ linux-4.14.336/drivers/input/joystick/xpad.c
@@ -282,6 +282,7 @@ static const struct xpad_device {
 	{ 0x146b, 0x0604, "Bigben Interactive DAIJA Arcade Stick", MAP_TRIGGERS_TO_BUTTONS, XTYPE_XBOX360 },
 	{ 0x1532, 0x0a00, "Razer Atrox Arcade Stick", MAP_TRIGGERS_TO_BUTTONS, XTYPE_XBOXONE },
 	{ 0x1532, 0x0a03, "Razer Wildcat", 0, XTYPE_XBOXONE },
+	{ 0x1532, 0x0a29, "Razer Wolverine V2", 0, XTYPE_XBOXONE },
 	{ 0x15e4, 0x3f00, "Power A Mini Pro Elite", 0, XTYPE_XBOX360 },
 	{ 0x15e4, 0x3f0a, "Xbox Airflo wired controller", 0, XTYPE_XBOX360 },
 	{ 0x15e4, 0x3f10, "Batarang Xbox 360 controller", 0, XTYPE_XBOX360 },
diff --git drivers/input/keyboard/atkbd.c drivers/input/keyboard/atkbd.c
index 7e75835e220f..585bf7392539 100644
--- linux-4.14.336/drivers/input/keyboard/atkbd.c
+++ linux-4.14.336/drivers/input/keyboard/atkbd.c
@@ -717,6 +717,44 @@ static void atkbd_deactivate(struct atkbd *atkbd)
 			ps2dev->serio->phys);
 }
 
+#ifdef CONFIG_X86
+static bool atkbd_is_portable_device(void)
+{
+	static const char * const chassis_types[] = {
+		"8",	/* Portable */
+		"9",	/* Laptop */
+		"10",	/* Notebook */
+		"14",	/* Sub-Notebook */
+		"31",	/* Convertible */
+		"32",	/* Detachable */
+	};
+	int i;
+
+	for (i = 0; i < ARRAY_SIZE(chassis_types); i++)
+		if (dmi_match(DMI_CHASSIS_TYPE, chassis_types[i]))
+			return true;
+
+	return false;
+}
+
+/*
+ * On many modern laptops ATKBD_CMD_GETID may cause problems, on these laptops
+ * the controller is always in translated mode. In this mode mice/touchpads will
+ * not work. So in this case simply assume a keyboard is connected to avoid
+ * confusing some laptop keyboards.
+ *
+ * Skipping ATKBD_CMD_GETID ends up using a fake keyboard id. Using the standard
+ * 0xab83 id is ok in translated mode, only atkbd_select_set() checks atkbd->id
+ * and in translated mode that is a no-op.
+ */
+static bool atkbd_skip_getid(struct atkbd *atkbd)
+{
+	return atkbd->translated && atkbd_is_portable_device();
+}
+#else
+static inline bool atkbd_skip_getid(struct atkbd *atkbd) { return false; }
+#endif
+
 /*
  * atkbd_probe() probes for an AT keyboard on a serio port.
  */
@@ -738,6 +776,11 @@ static int atkbd_probe(struct atkbd *atkbd)
 				 "keyboard reset failed on %s\n",
 				 ps2dev->serio->phys);
 
+	if (atkbd_skip_getid(atkbd)) {
+		atkbd->id = 0xab83;
+		return 0;
+	}
+
 /*
  * Then we check the keyboard ID. We should get 0xab83 under normal conditions.
  * Some keyboards report different values, but the first byte is always 0xab or
@@ -749,9 +792,9 @@ static int atkbd_probe(struct atkbd *atkbd)
 	if (ps2_command(ps2dev, param, ATKBD_CMD_GETID)) {
 
 /*
- * If the get ID command failed, we check if we can at least set the LEDs on
- * the keyboard. This should work on every keyboard out there. It also turns
- * the LEDs off, which we want anyway.
+ * If the get ID command failed, we check if we can at least set
+ * the LEDs on the keyboard. This should work on every keyboard out there.
+ * It also turns the LEDs off, which we want anyway.
  */
 		param[0] = 0;
 		if (ps2_command(ps2dev, param, ATKBD_CMD_SETLEDS))
diff --git drivers/irqchip/irq-brcmstb-l2.c drivers/irqchip/irq-brcmstb-l2.c
index b009b916a292..da8a426e9def 100644
--- linux-4.14.336/drivers/irqchip/irq-brcmstb-l2.c
+++ linux-4.14.336/drivers/irqchip/irq-brcmstb-l2.c
@@ -76,6 +76,9 @@ static void brcmstb_l2_intc_irq_handle(struct irq_desc *desc)
 		generic_handle_irq(irq_find_mapping(b->domain, irq));
 	} while (status);
 out:
+	/* Don't ack parent before all device writes are done */
+	wmb();
+
 	chained_irq_exit(chip, desc);
 }
 
diff --git drivers/leds/trigger/ledtrig-panic.c drivers/leds/trigger/ledtrig-panic.c
index d735526b9db4..2fc04418a87e 100644
--- linux-4.14.336/drivers/leds/trigger/ledtrig-panic.c
+++ linux-4.14.336/drivers/leds/trigger/ledtrig-panic.c
@@ -67,10 +67,13 @@ static long led_panic_blink(int state)
 
 static int __init ledtrig_panic_init(void)
 {
+	led_trigger_register_simple("panic", &trigger);
+	if (!trigger)
+		return -ENOMEM;
+
 	atomic_notifier_chain_register(&panic_notifier_list,
 				       &led_trigger_panic_nb);
 
-	led_trigger_register_simple("panic", &trigger);
 	panic_blink = led_panic_blink;
 	return 0;
 }
diff --git drivers/md/dm-crypt.c drivers/md/dm-crypt.c
index 7cc4281d5a79..966fb898f4b8 100644
--- linux-4.14.336/drivers/md/dm-crypt.c
+++ linux-4.14.336/drivers/md/dm-crypt.c
@@ -1742,6 +1742,12 @@ static void kcryptd_crypt_write_convert(struct dm_crypt_io *io)
 	io->ctx.bio_out = clone;
 	io->ctx.iter_out = clone->bi_iter;
 
+	if (crypt_integrity_aead(cc)) {
+		bio_copy_data(clone, io->base_bio);
+		io->ctx.bio_in = clone;
+		io->ctx.iter_in = clone->bi_iter;
+	}
+
 	sector += bio_sectors(clone);
 
 	crypt_inc_pending(io);
diff --git drivers/md/md.c drivers/md/md.c
index 3c2364d0d88f..07da8d7569b5 100644
--- linux-4.14.336/drivers/md/md.c
+++ linux-4.14.336/drivers/md/md.c
@@ -1018,6 +1018,7 @@ struct super_type  {
 					  struct md_rdev *refdev,
 					  int minor_version);
 	int		    (*validate_super)(struct mddev *mddev,
+					      struct md_rdev *freshest,
 					      struct md_rdev *rdev);
 	void		    (*sync_super)(struct mddev *mddev,
 					  struct md_rdev *rdev);
@@ -1144,8 +1145,9 @@ static int super_90_load(struct md_rdev *rdev, struct md_rdev *refdev, int minor
 
 /*
  * validate_super for 0.90.0
+ * note: we are not using "freshest" for 0.9 superblock
  */
-static int super_90_validate(struct mddev *mddev, struct md_rdev *rdev)
+static int super_90_validate(struct mddev *mddev, struct md_rdev *freshest, struct md_rdev *rdev)
 {
 	mdp_disk_t *desc;
 	mdp_super_t *sb = page_address(rdev->sb_page);
@@ -1649,7 +1651,7 @@ static int super_1_load(struct md_rdev *rdev, struct md_rdev *refdev, int minor_
 	return ret;
 }
 
-static int super_1_validate(struct mddev *mddev, struct md_rdev *rdev)
+static int super_1_validate(struct mddev *mddev, struct md_rdev *freshest, struct md_rdev *rdev)
 {
 	struct mdp_superblock_1 *sb = page_address(rdev->sb_page);
 	__u64 ev1 = le64_to_cpu(sb->events);
@@ -1745,13 +1747,15 @@ static int super_1_validate(struct mddev *mddev, struct md_rdev *rdev)
 		}
 	} else if (mddev->pers == NULL) {
 		/* Insist of good event counter while assembling, except for
-		 * spares (which don't need an event count) */
-		++ev1;
+		 * spares (which don't need an event count).
+		 * Similar to mdadm, we allow event counter difference of 1
+		 * from the freshest device.
+		 */
 		if (rdev->desc_nr >= 0 &&
 		    rdev->desc_nr < le32_to_cpu(sb->max_dev) &&
 		    (le16_to_cpu(sb->dev_roles[rdev->desc_nr]) < MD_DISK_ROLE_MAX ||
 		     le16_to_cpu(sb->dev_roles[rdev->desc_nr]) == MD_DISK_ROLE_JOURNAL))
-			if (ev1 < mddev->events)
+			if (ev1 + 1 < mddev->events)
 				return -EINVAL;
 	} else if (mddev->bitmap) {
 		/* If adding to array with a bitmap, then we can accept an
@@ -1772,8 +1776,38 @@ static int super_1_validate(struct mddev *mddev, struct md_rdev *rdev)
 		    rdev->desc_nr >= le32_to_cpu(sb->max_dev)) {
 			role = MD_DISK_ROLE_SPARE;
 			rdev->desc_nr = -1;
-		} else
+		} else if (mddev->pers == NULL && freshest && ev1 < mddev->events) {
+			/*
+			 * If we are assembling, and our event counter is smaller than the
+			 * highest event counter, we cannot trust our superblock about the role.
+			 * It could happen that our rdev was marked as Faulty, and all other
+			 * superblocks were updated with +1 event counter.
+			 * Then, before the next superblock update, which typically happens when
+			 * remove_and_add_spares() removes the device from the array, there was
+			 * a crash or reboot.
+			 * If we allow current rdev without consulting the freshest superblock,
+			 * we could cause data corruption.
+			 * Note that in this case our event counter is smaller by 1 than the
+			 * highest, otherwise, this rdev would not be allowed into array;
+			 * both kernel and mdadm allow event counter difference of 1.
+			 */
+			struct mdp_superblock_1 *freshest_sb = page_address(freshest->sb_page);
+			u32 freshest_max_dev = le32_to_cpu(freshest_sb->max_dev);
+
+			if (rdev->desc_nr >= freshest_max_dev) {
+				/* this is unexpected, better not proceed */
+				pr_warn("md: %s: rdev[%pg]: desc_nr(%d) >= freshest(%pg)->sb->max_dev(%u)\n",
+						mdname(mddev), rdev->bdev, rdev->desc_nr,
+						freshest->bdev, freshest_max_dev);
+				return -EUCLEAN;
+			}
+
+			role = le16_to_cpu(freshest_sb->dev_roles[rdev->desc_nr]);
+			pr_debug("md: %s: rdev[%pg]: role=%d(0x%x) according to freshest %pg\n",
+				     mdname(mddev), rdev->bdev, role, role, freshest->bdev);
+		} else {
 			role = le16_to_cpu(sb->dev_roles[rdev->desc_nr]);
+		}
 		switch(role) {
 		case MD_DISK_ROLE_SPARE: /* spare */
 			break;
@@ -2667,7 +2701,7 @@ static int add_bound_rdev(struct md_rdev *rdev)
 		 * and should be added immediately.
 		 */
 		super_types[mddev->major_version].
-			validate_super(mddev, rdev);
+			validate_super(mddev, NULL/*freshest*/, rdev);
 		if (add_journal)
 			mddev_suspend(mddev);
 		err = mddev->pers->hot_add_disk(mddev, rdev);
@@ -3569,7 +3603,7 @@ static void analyze_sbs(struct mddev *mddev)
 		}
 
 	super_types[mddev->major_version].
-		validate_super(mddev, freshest);
+		validate_super(mddev, NULL/*freshest*/, freshest);
 
 	i = 0;
 	rdev_for_each_safe(rdev, tmp, mddev) {
@@ -3584,7 +3618,7 @@ static void analyze_sbs(struct mddev *mddev)
 		}
 		if (rdev != freshest) {
 			if (super_types[mddev->major_version].
-			    validate_super(mddev, rdev)) {
+			    validate_super(mddev, freshest, rdev)) {
 				pr_warn("md: kicking non-fresh %s from array!\n",
 					bdevname(rdev->bdev,b));
 				md_kick_rdev_from_array(rdev);
@@ -6424,7 +6458,7 @@ static int add_new_disk(struct mddev *mddev, mdu_disk_info_t *info)
 			rdev->saved_raid_disk = rdev->raid_disk;
 		} else
 			super_types[mddev->major_version].
-				validate_super(mddev, rdev);
+				validate_super(mddev, NULL/*freshest*/, rdev);
 		if ((info->state & (1<<MD_DISK_SYNC)) &&
 		     rdev->raid_disk != info->raid_disk) {
 			/* This was a hot-add request, but events doesn't
diff --git drivers/md/raid5.c drivers/md/raid5.c
index d2ac3d189410..6fca2df66550 100644
--- linux-4.14.336/drivers/md/raid5.c
+++ linux-4.14.336/drivers/md/raid5.c
@@ -44,7 +44,6 @@
  */
 
 #include <linux/blkdev.h>
-#include <linux/delay.h>
 #include <linux/kthread.h>
 #include <linux/raid/pq.h>
 #include <linux/async_tx.h>
@@ -6309,18 +6308,7 @@ static void raid5d(struct md_thread *thread)
 			spin_unlock_irq(&conf->device_lock);
 			md_check_recovery(mddev);
 			spin_lock_irq(&conf->device_lock);
-
-			/*
-			 * Waiting on MD_SB_CHANGE_PENDING below may deadlock
-			 * seeing md_check_recovery() is needed to clear
-			 * the flag when using mdmon.
-			 */
-			continue;
 		}
-
-		wait_event_lock_irq(mddev->sb_wait,
-			!test_bit(MD_SB_CHANGE_PENDING, &mddev->sb_flags),
-			conf->device_lock);
 	}
 	pr_debug("%d stripes handled\n", handled);
 
diff --git drivers/media/dvb-core/dvbdev.c drivers/media/dvb-core/dvbdev.c
index 1b3a54520d68..0506179a7c86 100644
--- linux-4.14.336/drivers/media/dvb-core/dvbdev.c
+++ linux-4.14.336/drivers/media/dvb-core/dvbdev.c
@@ -90,6 +90,8 @@ static int dvb_device_open(struct inode *inode, struct file *file)
 			err = file->f_op->open(inode, file);
 		up_read(&minor_rwsem);
 		mutex_unlock(&dvbdev_mutex);
+		if (err)
+			dvb_device_put(dvbdev);
 		return err;
 	}
 fail:
diff --git drivers/media/pci/ddbridge/ddbridge-main.c drivers/media/pci/ddbridge/ddbridge-main.c
index ccac7fe31336..13aab32f8048 100644
--- linux-4.14.336/drivers/media/pci/ddbridge/ddbridge-main.c
+++ linux-4.14.336/drivers/media/pci/ddbridge/ddbridge-main.c
@@ -265,7 +265,7 @@ fail:
 	ddb_unmap(dev);
 	pci_set_drvdata(pdev, NULL);
 	pci_disable_device(pdev);
-	return -1;
+	return stat;
 }
 
 /****************************************************************************/
diff --git drivers/media/usb/cx231xx/cx231xx-core.c drivers/media/usb/cx231xx/cx231xx-core.c
index f372ad3917a8..61fd934c0205 100644
--- linux-4.14.336/drivers/media/usb/cx231xx/cx231xx-core.c
+++ linux-4.14.336/drivers/media/usb/cx231xx/cx231xx-core.c
@@ -1038,6 +1038,7 @@ int cx231xx_init_isoc(struct cx231xx *dev, int max_packets,
 	if (!dev->video_mode.isoc_ctl.urb) {
 		dev_err(dev->dev,
 			"cannot alloc memory for usb buffers\n");
+		kfree(dma_q->p_left_data);
 		return -ENOMEM;
 	}
 
@@ -1047,6 +1048,7 @@ int cx231xx_init_isoc(struct cx231xx *dev, int max_packets,
 		dev_err(dev->dev,
 			"cannot allocate memory for usbtransfer\n");
 		kfree(dev->video_mode.isoc_ctl.urb);
+		kfree(dma_q->p_left_data);
 		return -ENOMEM;
 	}
 
diff --git drivers/media/usb/pvrusb2/pvrusb2-context.c drivers/media/usb/pvrusb2/pvrusb2-context.c
index d9e8481e9e28..9236463ba269 100644
--- linux-4.14.336/drivers/media/usb/pvrusb2/pvrusb2-context.c
+++ linux-4.14.336/drivers/media/usb/pvrusb2/pvrusb2-context.c
@@ -277,7 +277,8 @@ void pvr2_context_disconnect(struct pvr2_context *mp)
 {
 	pvr2_hdw_disconnect(mp->hdw);
 	mp->disconnect_flag = !0;
-	pvr2_context_notify(mp);
+	if (!pvr2_context_shutok())
+		pvr2_context_notify(mp);
 }
 
 
diff --git drivers/media/usb/stk1160/stk1160-video.c drivers/media/usb/stk1160/stk1160-video.c
index ce8ebbe395a6..8a6cdbc36a08 100644
--- linux-4.14.336/drivers/media/usb/stk1160/stk1160-video.c
+++ linux-4.14.336/drivers/media/usb/stk1160/stk1160-video.c
@@ -117,8 +117,7 @@ void stk1160_copy_video(struct stk1160 *dev, u8 *src, int len)
 
 	/*
 	 * TODO: These stk1160_dbg are very spammy!
-	 * We should 1) check why we are getting them
-	 * and 2) add ratelimit.
+	 * We should check why we are getting them.
 	 *
 	 * UPDATE: One of the reasons (the only one?) for getting these
 	 * is incorrect standard (mismatch between expected and configured).
@@ -161,7 +160,7 @@ void stk1160_copy_video(struct stk1160 *dev, u8 *src, int len)
 
 	/* Let the bug hunt begin! sanity checks! */
 	if (lencopy < 0) {
-		stk1160_dbg("copy skipped: negative lencopy\n");
+		printk_ratelimited(KERN_DEBUG "copy skipped: negative lencopy\n");
 		return;
 	}
 
diff --git drivers/mfd/Kconfig drivers/mfd/Kconfig
index fc5e4fef89d2..7e90ed8fdb1c 100644
--- linux-4.14.336/drivers/mfd/Kconfig
+++ linux-4.14.336/drivers/mfd/Kconfig
@@ -1199,6 +1199,7 @@ config MFD_DAVINCI_VOICECODEC
 
 config MFD_TI_AM335X_TSCADC
 	tristate "TI ADC / Touch Screen chip support"
+	depends on ARCH_OMAP2PLUS || ARCH_K3 || COMPILE_TEST
 	select MFD_CORE
 	select REGMAP
 	select REGMAP_MMIO
diff --git drivers/mmc/core/mmc.c drivers/mmc/core/mmc.c
index 32bf0b47e339..69f0cc3a28bc 100644
--- linux-4.14.336/drivers/mmc/core/mmc.c
+++ linux-4.14.336/drivers/mmc/core/mmc.c
@@ -990,10 +990,12 @@ static int mmc_select_bus_width(struct mmc_card *card)
 	static unsigned ext_csd_bits[] = {
 		EXT_CSD_BUS_WIDTH_8,
 		EXT_CSD_BUS_WIDTH_4,
+		EXT_CSD_BUS_WIDTH_1,
 	};
 	static unsigned bus_widths[] = {
 		MMC_BUS_WIDTH_8,
 		MMC_BUS_WIDTH_4,
+		MMC_BUS_WIDTH_1,
 	};
 	struct mmc_host *host = card->host;
 	unsigned idx, bus_width = 0;
diff --git drivers/mtd/mtd_blkdevs.c drivers/mtd/mtd_blkdevs.c
index 9ec8f033ac5f..5a76e7c549ef 100644
--- linux-4.14.336/drivers/mtd/mtd_blkdevs.c
+++ linux-4.14.336/drivers/mtd/mtd_blkdevs.c
@@ -513,7 +513,7 @@ static void blktrans_notify_add(struct mtd_info *mtd)
 {
 	struct mtd_blktrans_ops *tr;
 
-	if (mtd->type == MTD_ABSENT)
+	if (mtd->type == MTD_ABSENT || mtd->type == MTD_UBIVOLUME)
 		return;
 
 	list_for_each_entry(tr, &blktrans_majors, list)
@@ -556,7 +556,7 @@ int register_mtd_blktrans(struct mtd_blktrans_ops *tr)
 	list_add(&tr->list, &blktrans_majors);
 
 	mtd_for_each_device(mtd)
-		if (mtd->type != MTD_ABSENT)
+		if (mtd->type != MTD_ABSENT && mtd->type != MTD_UBIVOLUME)
 			tr->add_mtd(tr, mtd);
 
 	mutex_unlock(&mtd_table_mutex);
diff --git drivers/mtd/nand/fsl_ifc_nand.c drivers/mtd/nand/fsl_ifc_nand.c
index 0d4928161439..be7d9eb7359c 100644
--- linux-4.14.336/drivers/mtd/nand/fsl_ifc_nand.c
+++ linux-4.14.336/drivers/mtd/nand/fsl_ifc_nand.c
@@ -33,7 +33,7 @@
 
 #define ERR_BYTE		0xFF /* Value returned for read
 					bytes when read failed	*/
-#define IFC_TIMEOUT_MSECS	500  /* Maximum number of mSecs to wait
+#define IFC_TIMEOUT_MSECS	1000 /* Maximum timeout to wait
 					for IFC NAND Machine	*/
 
 struct fsl_ifc_ctrl;
diff --git drivers/net/bonding/bond_alb.c drivers/net/bonding/bond_alb.c
index 4926c3e06e4e..6cd4e024b41d 100644
--- linux-4.14.336/drivers/net/bonding/bond_alb.c
+++ linux-4.14.336/drivers/net/bonding/bond_alb.c
@@ -988,7 +988,8 @@ static int alb_upper_dev_walk(struct net_device *upper, void *_data)
 	if (netif_is_macvlan(upper) && !strict_match) {
 		tags = bond_verify_device_path(bond->dev, upper, 0);
 		if (IS_ERR_OR_NULL(tags))
-			BUG();
+			return -ENOMEM;
+
 		alb_send_lp_vid(slave, upper->dev_addr,
 				tags[0].vlan_proto, tags[0].vlan_id);
 		kfree(tags);
diff --git drivers/net/ethernet/aquantia/atlantic/aq_nic.c drivers/net/ethernet/aquantia/atlantic/aq_nic.c
index 7a900f76c9ac..396c335909af 100644
--- linux-4.14.336/drivers/net/ethernet/aquantia/atlantic/aq_nic.c
+++ linux-4.14.336/drivers/net/ethernet/aquantia/atlantic/aq_nic.c
@@ -884,7 +884,6 @@ int aq_nic_set_link_ksettings(struct aq_nic_s *self,
 		default:
 			err = -1;
 			goto err_exit;
-		break;
 		}
 		if (!(self->aq_hw_caps.link_speed_msk & rate)) {
 			err = -1;
diff --git drivers/net/ethernet/broadcom/bnxt/bnxt.c drivers/net/ethernet/broadcom/bnxt/bnxt.c
index ee438674d6cc..180a7ef588cf 100644
--- linux-4.14.336/drivers/net/ethernet/broadcom/bnxt/bnxt.c
+++ linux-4.14.336/drivers/net/ethernet/broadcom/bnxt/bnxt.c
@@ -7092,6 +7092,8 @@ static void bnxt_sp_task(struct work_struct *work)
 		bnxt_cfg_ntp_filters(bp);
 	if (test_and_clear_bit(BNXT_HWRM_EXEC_FWD_REQ_SP_EVENT, &bp->sp_event))
 		bnxt_hwrm_exec_fwd_req(bp);
+	if (test_and_clear_bit(BNXT_HWRM_PF_UNLOAD_SP_EVENT, &bp->sp_event))
+		netdev_info(bp->dev, "Receive PF driver unload event!\n");
 	if (test_and_clear_bit(BNXT_VXLAN_ADD_PORT_SP_EVENT, &bp->sp_event)) {
 		bnxt_hwrm_tunnel_dst_port_alloc(
 			bp, bp->vxlan_port,
@@ -7583,8 +7585,6 @@ static void bnxt_cfg_ntp_filters(struct bnxt *bp)
 			}
 		}
 	}
-	if (test_and_clear_bit(BNXT_HWRM_PF_UNLOAD_SP_EVENT, &bp->sp_event))
-		netdev_info(bp->dev, "Receive PF driver unload event!");
 }
 
 #else
diff --git drivers/net/ethernet/broadcom/tg3.c drivers/net/ethernet/broadcom/tg3.c
index dc27c81ad512..44556eea780b 100644
--- linux-4.14.336/drivers/net/ethernet/broadcom/tg3.c
+++ linux-4.14.336/drivers/net/ethernet/broadcom/tg3.c
@@ -6434,6 +6434,14 @@ static void tg3_dump_state(struct tg3 *tp)
 	int i;
 	u32 *regs;
 
+	/* If it is a PCI error, all registers will be 0xffff,
+	 * we don't dump them out, just report the error and return
+	 */
+	if (tp->pdev->error_state != pci_channel_io_normal) {
+		netdev_err(tp->dev, "PCI channel ERROR!\n");
+		return;
+	}
+
 	regs = kzalloc(TG3_REG_BLK_SIZE, GFP_ATOMIC);
 	if (!regs)
 		return;
@@ -11168,7 +11176,8 @@ static void tg3_reset_task(struct work_struct *work)
 	rtnl_lock();
 	tg3_full_lock(tp, 0);
 
-	if (tp->pcierr_recovery || !netif_running(tp->dev)) {
+	if (tp->pcierr_recovery || !netif_running(tp->dev) ||
+	    tp->pdev->error_state != pci_channel_io_normal) {
 		tg3_flag_clear(tp, RESET_TASK_PENDING);
 		tg3_full_unlock(tp);
 		rtnl_unlock();
diff --git drivers/net/ethernet/cisco/enic/enic_ethtool.c drivers/net/ethernet/cisco/enic/enic_ethtool.c
index fd3980cc1e34..3280fbad5d5a 100644
--- linux-4.14.336/drivers/net/ethernet/cisco/enic/enic_ethtool.c
+++ linux-4.14.336/drivers/net/ethernet/cisco/enic/enic_ethtool.c
@@ -378,7 +378,6 @@ static int enic_grxclsrule(struct enic *enic, struct ethtool_rxnfc *cmd)
 		break;
 	default:
 		return -EINVAL;
-		break;
 	}
 
 	fsp->h_u.tcp_ip4_spec.ip4src = flow_get_u32_src(&n->keys);
diff --git drivers/net/ethernet/freescale/fec_main.c drivers/net/ethernet/freescale/fec_main.c
index 1085f1d721b0..4b169890d301 100644
--- linux-4.14.336/drivers/net/ethernet/freescale/fec_main.c
+++ linux-4.14.336/drivers/net/ethernet/freescale/fec_main.c
@@ -1746,6 +1746,7 @@ static void fec_enet_adjust_link(struct net_device *ndev)
 
 		/* if any of the above changed restart the FEC */
 		if (status_change) {
+			netif_stop_queue(ndev);
 			napi_disable(&fep->napi);
 			netif_tx_lock_bh(ndev);
 			fec_restart(ndev);
@@ -1755,6 +1756,7 @@ static void fec_enet_adjust_link(struct net_device *ndev)
 		}
 	} else {
 		if (fep->link) {
+			netif_stop_queue(ndev);
 			napi_disable(&fep->napi);
 			netif_tx_lock_bh(ndev);
 			fec_stop(ndev);
diff --git drivers/net/ethernet/intel/i40e/i40e_main.c drivers/net/ethernet/intel/i40e/i40e_main.c
index a783ebb14db9..ec5da7cbf416 100644
--- linux-4.14.336/drivers/net/ethernet/intel/i40e/i40e_main.c
+++ linux-4.14.336/drivers/net/ethernet/intel/i40e/i40e_main.c
@@ -4708,7 +4708,7 @@ static int i40e_pf_wait_queues_disabled(struct i40e_pf *pf)
 {
 	int v, ret = 0;
 
-	for (v = 0; v < pf->hw.func_caps.num_vsis; v++) {
+	for (v = 0; v < pf->num_alloc_vsi; v++) {
 		if (pf->vsi[v]) {
 			ret = i40e_vsi_wait_queues_disabled(pf->vsi[v]);
 			if (ret)
diff --git drivers/net/ethernet/intel/ixgbe/ixgbe_common.c drivers/net/ethernet/intel/ixgbe/ixgbe_common.c
index 6b5662674c75..71583f8756c2 100644
--- linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_common.c
+++ linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_common.c
@@ -55,7 +55,7 @@ static s32 ixgbe_write_eeprom_buffer_bit_bang(struct ixgbe_hw *hw, u16 offset,
 					     u16 words, u16 *data);
 static s32 ixgbe_detect_eeprom_page_size_generic(struct ixgbe_hw *hw,
 						 u16 offset);
-static s32 ixgbe_disable_pcie_master(struct ixgbe_hw *hw);
+static s32 ixgbe_disable_pcie_primary(struct ixgbe_hw *hw);
 
 /* Base table for registers values that change by MAC */
 const u32 ixgbe_mvals_8259X[IXGBE_MVALS_IDX_LIMIT] = {
@@ -771,10 +771,10 @@ s32 ixgbe_stop_adapter_generic(struct ixgbe_hw *hw)
 	usleep_range(1000, 2000);
 
 	/*
-	 * Prevent the PCI-E bus from from hanging by disabling PCI-E master
+	 * Prevent the PCI-E bus from hanging by disabling PCI-E primary
 	 * access and verify no pending requests
 	 */
-	return ixgbe_disable_pcie_master(hw);
+	return ixgbe_disable_pcie_primary(hw);
 }
 
 /**
@@ -2530,15 +2530,15 @@ static u32 ixgbe_pcie_timeout_poll(struct ixgbe_hw *hw)
 }
 
 /**
- *  ixgbe_disable_pcie_master - Disable PCI-express master access
+ *  ixgbe_disable_pcie_primary - Disable PCI-express primary access
  *  @hw: pointer to hardware structure
  *
- *  Disables PCI-Express master access and verifies there are no pending
- *  requests. IXGBE_ERR_MASTER_REQUESTS_PENDING is returned if master disable
- *  bit hasn't caused the master requests to be disabled, else 0
- *  is returned signifying master requests disabled.
+ *  Disables PCI-Express primary access and verifies there are no pending
+ *  requests. IXGBE_ERR_PRIMARY_REQUESTS_PENDING is returned if primary disable
+ *  bit hasn't caused the primary requests to be disabled, else 0
+ *  is returned signifying primary requests disabled.
  **/
-static s32 ixgbe_disable_pcie_master(struct ixgbe_hw *hw)
+static s32 ixgbe_disable_pcie_primary(struct ixgbe_hw *hw)
 {
 	u32 i, poll;
 	u16 value;
@@ -2547,23 +2547,23 @@ static s32 ixgbe_disable_pcie_master(struct ixgbe_hw *hw)
 	IXGBE_WRITE_REG(hw, IXGBE_CTRL, IXGBE_CTRL_GIO_DIS);
 
 	/* Poll for bit to read as set */
-	for (i = 0; i < IXGBE_PCI_MASTER_DISABLE_TIMEOUT; i++) {
+	for (i = 0; i < IXGBE_PCI_PRIMARY_DISABLE_TIMEOUT; i++) {
 		if (IXGBE_READ_REG(hw, IXGBE_CTRL) & IXGBE_CTRL_GIO_DIS)
 			break;
 		usleep_range(100, 120);
 	}
-	if (i >= IXGBE_PCI_MASTER_DISABLE_TIMEOUT) {
+	if (i >= IXGBE_PCI_PRIMARY_DISABLE_TIMEOUT) {
 		hw_dbg(hw, "GIO disable did not set - requesting resets\n");
 		goto gio_disable_fail;
 	}
 
-	/* Exit if master requests are blocked */
+	/* Exit if primary requests are blocked */
 	if (!(IXGBE_READ_REG(hw, IXGBE_STATUS) & IXGBE_STATUS_GIO) ||
 	    ixgbe_removed(hw->hw_addr))
 		return 0;
 
-	/* Poll for master request bit to clear */
-	for (i = 0; i < IXGBE_PCI_MASTER_DISABLE_TIMEOUT; i++) {
+	/* Poll for primary request bit to clear */
+	for (i = 0; i < IXGBE_PCI_PRIMARY_DISABLE_TIMEOUT; i++) {
 		udelay(100);
 		if (!(IXGBE_READ_REG(hw, IXGBE_STATUS) & IXGBE_STATUS_GIO))
 			return 0;
@@ -2571,13 +2571,13 @@ static s32 ixgbe_disable_pcie_master(struct ixgbe_hw *hw)
 
 	/*
 	 * Two consecutive resets are required via CTRL.RST per datasheet
-	 * 5.2.5.3.2 Master Disable.  We set a flag to inform the reset routine
-	 * of this need.  The first reset prevents new master requests from
+	 * 5.2.5.3.2 Primary Disable.  We set a flag to inform the reset routine
+	 * of this need.  The first reset prevents new primary requests from
 	 * being issued by our device.  We then must wait 1usec or more for any
 	 * remaining completions from the PCIe bus to trickle in, and then reset
 	 * again to clear out any effects they may have had on our device.
 	 */
-	hw_dbg(hw, "GIO Master Disable bit didn't clear - requesting resets\n");
+	hw_dbg(hw, "GIO Primary Disable bit didn't clear - requesting resets\n");
 gio_disable_fail:
 	hw->mac.flags |= IXGBE_FLAGS_DOUBLE_RESET_REQUIRED;
 
@@ -2599,7 +2599,7 @@ gio_disable_fail:
 	}
 
 	hw_dbg(hw, "PCIe transaction pending bit also did not clear.\n");
-	return IXGBE_ERR_MASTER_REQUESTS_PENDING;
+	return IXGBE_ERR_PRIMARY_REQUESTS_PENDING;
 }
 
 /**
diff --git drivers/net/ethernet/intel/ixgbe/ixgbe_main.c drivers/net/ethernet/intel/ixgbe/ixgbe_main.c
index ac9835e61602..ca9bdaed31c5 100644
--- linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_main.c
+++ linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_main.c
@@ -2660,7 +2660,6 @@ static void ixgbe_check_overtemp_subtask(struct ixgbe_adapter *adapter)
 {
 	struct ixgbe_hw *hw = &adapter->hw;
 	u32 eicr = adapter->interrupt_event;
-	s32 rc;
 
 	if (test_bit(__IXGBE_DOWN, &adapter->state))
 		return;
@@ -2694,14 +2693,13 @@ static void ixgbe_check_overtemp_subtask(struct ixgbe_adapter *adapter)
 		}
 
 		/* Check if this is not due to overtemp */
-		if (hw->phy.ops.check_overtemp(hw) != IXGBE_ERR_OVERTEMP)
+		if (!hw->phy.ops.check_overtemp(hw))
 			return;
 
 		break;
 	case IXGBE_DEV_ID_X550EM_A_1G_T:
 	case IXGBE_DEV_ID_X550EM_A_1G_T_L:
-		rc = hw->phy.ops.check_overtemp(hw);
-		if (rc != IXGBE_ERR_OVERTEMP)
+		if (!hw->phy.ops.check_overtemp(hw))
 			return;
 		break;
 	default:
@@ -5690,8 +5688,8 @@ void ixgbe_reset(struct ixgbe_adapter *adapter)
 	case IXGBE_ERR_SFP_NOT_PRESENT:
 	case IXGBE_ERR_SFP_NOT_SUPPORTED:
 		break;
-	case IXGBE_ERR_MASTER_REQUESTS_PENDING:
-		e_dev_err("master disable timed out\n");
+	case IXGBE_ERR_PRIMARY_REQUESTS_PENDING:
+		e_dev_err("primary disable timed out\n");
 		break;
 	case IXGBE_ERR_EEPROM_VERSION:
 		/* We are running on a pre-production device, log a warning */
@@ -7636,7 +7634,7 @@ static void ixgbe_service_timer(unsigned long data)
 static void ixgbe_phy_interrupt_subtask(struct ixgbe_adapter *adapter)
 {
 	struct ixgbe_hw *hw = &adapter->hw;
-	u32 status;
+	bool overtemp;
 
 	if (!(adapter->flags2 & IXGBE_FLAG2_PHY_INTERRUPT))
 		return;
@@ -7646,11 +7644,9 @@ static void ixgbe_phy_interrupt_subtask(struct ixgbe_adapter *adapter)
 	if (!hw->phy.ops.handle_lasi)
 		return;
 
-	status = hw->phy.ops.handle_lasi(&adapter->hw);
-	if (status != IXGBE_ERR_OVERTEMP)
-		return;
-
-	e_crit(drv, "%s\n", ixgbe_overheat_msg);
+	hw->phy.ops.handle_lasi(&adapter->hw, &overtemp);
+	if (overtemp)
+		e_crit(drv, "%s\n", ixgbe_overheat_msg);
 }
 
 static void ixgbe_reset_subtask(struct ixgbe_adapter *adapter)
diff --git drivers/net/ethernet/intel/ixgbe/ixgbe_phy.c drivers/net/ethernet/intel/ixgbe/ixgbe_phy.c
index 654a402f0e9e..09a7c0f4aa2a 100644
--- linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_phy.c
+++ linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_phy.c
@@ -429,8 +429,7 @@ s32 ixgbe_reset_phy_generic(struct ixgbe_hw *hw)
 		return status;
 
 	/* Don't reset PHY if it's shut down due to overtemp. */
-	if (!hw->phy.reset_if_overtemp &&
-	    (IXGBE_ERR_OVERTEMP == hw->phy.ops.check_overtemp(hw)))
+	if (!hw->phy.reset_if_overtemp && hw->phy.ops.check_overtemp(hw))
 		return 0;
 
 	/* Blocked by MNG FW so bail */
@@ -2329,22 +2328,24 @@ static void ixgbe_i2c_bus_clear(struct ixgbe_hw *hw)
  *  @hw: pointer to hardware structure
  *
  *  Checks if the LASI temp alarm status was triggered due to overtemp
+ *
+ *  Return true when an overtemp event detected, otherwise false.
  **/
-s32 ixgbe_tn_check_overtemp(struct ixgbe_hw *hw)
+bool ixgbe_tn_check_overtemp(struct ixgbe_hw *hw)
 {
 	u16 phy_data = 0;
+	u32 status;
 
 	if (hw->device_id != IXGBE_DEV_ID_82599_T3_LOM)
-		return 0;
+		return false;
 
 	/* Check that the LASI temp alarm status was triggered */
-	hw->phy.ops.read_reg(hw, IXGBE_TN_LASI_STATUS_REG,
-			     MDIO_MMD_PMAPMD, &phy_data);
-
-	if (!(phy_data & IXGBE_TN_LASI_STATUS_TEMP_ALARM))
-		return 0;
+	status = hw->phy.ops.read_reg(hw, IXGBE_TN_LASI_STATUS_REG,
+				      MDIO_MMD_PMAPMD, &phy_data);
+	if (status)
+		return false;
 
-	return IXGBE_ERR_OVERTEMP;
+	return !!(phy_data & IXGBE_TN_LASI_STATUS_TEMP_ALARM);
 }
 
 /** ixgbe_set_copper_phy_power - Control power for copper phy
diff --git drivers/net/ethernet/intel/ixgbe/ixgbe_phy.h drivers/net/ethernet/intel/ixgbe/ixgbe_phy.h
index 94df1d99be95..7002f0a534c7 100644
--- linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_phy.h
+++ linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_phy.h
@@ -178,7 +178,7 @@ s32 ixgbe_identify_sfp_module_generic(struct ixgbe_hw *hw);
 s32 ixgbe_get_sfp_init_sequence_offsets(struct ixgbe_hw *hw,
 					u16 *list_offset,
 					u16 *data_offset);
-s32 ixgbe_tn_check_overtemp(struct ixgbe_hw *hw);
+bool ixgbe_tn_check_overtemp(struct ixgbe_hw *hw);
 s32 ixgbe_read_i2c_byte_generic(struct ixgbe_hw *hw, u8 byte_offset,
 				u8 dev_addr, u8 *data);
 s32 ixgbe_read_i2c_byte_generic_unlocked(struct ixgbe_hw *hw, u8 byte_offset,
diff --git drivers/net/ethernet/intel/ixgbe/ixgbe_type.h drivers/net/ethernet/intel/ixgbe/ixgbe_type.h
index ffa0ee5cd0f5..93d18050284d 100644
--- linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_type.h
+++ linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_type.h
@@ -1227,7 +1227,7 @@ struct ixgbe_thermal_sensor_data {
 #define IXGBE_PSRTYPE_RQPL_SHIFT    29
 
 /* CTRL Bit Masks */
-#define IXGBE_CTRL_GIO_DIS      0x00000004 /* Global IO Master Disable bit */
+#define IXGBE_CTRL_GIO_DIS      0x00000004 /* Global IO Primary Disable bit */
 #define IXGBE_CTRL_LNK_RST      0x00000008 /* Link Reset. Resets everything. */
 #define IXGBE_CTRL_RST          0x04000000 /* Reset (SW) */
 #define IXGBE_CTRL_RST_MASK     (IXGBE_CTRL_LNK_RST | IXGBE_CTRL_RST)
@@ -1790,7 +1790,7 @@ enum {
 /* STATUS Bit Masks */
 #define IXGBE_STATUS_LAN_ID         0x0000000C /* LAN ID */
 #define IXGBE_STATUS_LAN_ID_SHIFT   2          /* LAN ID Shift*/
-#define IXGBE_STATUS_GIO            0x00080000 /* GIO Master Enable Status */
+#define IXGBE_STATUS_GIO            0x00080000 /* GIO Primary Enable Status */
 
 #define IXGBE_STATUS_LAN_ID_0   0x00000000 /* LAN ID 0 */
 #define IXGBE_STATUS_LAN_ID_1   0x00000004 /* LAN ID 1 */
@@ -2172,8 +2172,8 @@ enum {
 #define IXGBE_PCIDEVCTRL2_4_8s		0xd
 #define IXGBE_PCIDEVCTRL2_17_34s	0xe
 
-/* Number of 100 microseconds we wait for PCI Express master disable */
-#define IXGBE_PCI_MASTER_DISABLE_TIMEOUT	800
+/* Number of 100 microseconds we wait for PCI Express primary disable */
+#define IXGBE_PCI_PRIMARY_DISABLE_TIMEOUT	800
 
 /* RAH */
 #define IXGBE_RAH_VIND_MASK     0x003C0000
@@ -3482,10 +3482,10 @@ struct ixgbe_phy_operations {
 	s32 (*read_i2c_sff8472)(struct ixgbe_hw *, u8 , u8 *);
 	s32 (*read_i2c_eeprom)(struct ixgbe_hw *, u8 , u8 *);
 	s32 (*write_i2c_eeprom)(struct ixgbe_hw *, u8, u8);
-	s32 (*check_overtemp)(struct ixgbe_hw *);
+	bool (*check_overtemp)(struct ixgbe_hw *);
 	s32 (*set_phy_power)(struct ixgbe_hw *, bool on);
 	s32 (*enter_lplu)(struct ixgbe_hw *);
-	s32 (*handle_lasi)(struct ixgbe_hw *hw);
+	s32 (*handle_lasi)(struct ixgbe_hw *hw, bool *);
 	s32 (*read_i2c_byte_unlocked)(struct ixgbe_hw *, u8 offset, u8 addr,
 				      u8 *value);
 	s32 (*write_i2c_byte_unlocked)(struct ixgbe_hw *, u8 offset, u8 addr,
@@ -3651,7 +3651,7 @@ struct ixgbe_info {
 #define IXGBE_ERR_ADAPTER_STOPPED               -9
 #define IXGBE_ERR_INVALID_MAC_ADDR              -10
 #define IXGBE_ERR_DEVICE_NOT_SUPPORTED          -11
-#define IXGBE_ERR_MASTER_REQUESTS_PENDING       -12
+#define IXGBE_ERR_PRIMARY_REQUESTS_PENDING      -12
 #define IXGBE_ERR_INVALID_LINK_SETTINGS         -13
 #define IXGBE_ERR_AUTONEG_NOT_COMPLETE          -14
 #define IXGBE_ERR_RESET_FAILED                  -15
diff --git drivers/net/ethernet/intel/ixgbe/ixgbe_x540.c drivers/net/ethernet/intel/ixgbe/ixgbe_x540.c
index 6ea0d6a5fb90..b5e4e78f86ee 100644
--- linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_x540.c
+++ linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_x540.c
@@ -375,7 +375,6 @@ static s32 ixgbe_calc_eeprom_checksum_X540(struct ixgbe_hw *hw)
 		if (ixgbe_read_eerd_generic(hw, pointer, &length)) {
 			hw_dbg(hw, "EEPROM read failed\n");
 			return IXGBE_ERR_EEPROM;
-			break;
 		}
 
 		/* Skip pointer section if length is invalid. */
diff --git drivers/net/ethernet/intel/ixgbe/ixgbe_x550.c drivers/net/ethernet/intel/ixgbe/ixgbe_x550.c
index 10fa0e095ec3..f99596cf3d7e 100644
--- linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_x550.c
+++ linux-4.14.336/drivers/net/ethernet/intel/ixgbe/ixgbe_x550.c
@@ -620,8 +620,10 @@ static s32 ixgbe_setup_fw_link(struct ixgbe_hw *hw)
 	rc = ixgbe_fw_phy_activity(hw, FW_PHY_ACT_SETUP_LINK, &setup);
 	if (rc)
 		return rc;
+
 	if (setup[0] == FW_PHY_ACT_SETUP_LINK_RSP_DOWN)
-		return IXGBE_ERR_OVERTEMP;
+		return -EIO;
+
 	return 0;
 }
 
@@ -735,7 +737,8 @@ static s32 ixgbe_read_iosf_sb_reg_x550(struct ixgbe_hw *hw, u32 reg_addr,
 		error = (command & IXGBE_SB_IOSF_CTRL_CMPL_ERR_MASK) >>
 			 IXGBE_SB_IOSF_CTRL_CMPL_ERR_SHIFT;
 		hw_dbg(hw, "Failed to read, error %x\n", error);
-		return IXGBE_ERR_PHY;
+		ret = IXGBE_ERR_PHY;
+		goto out;
 	}
 
 	if (!ret)
@@ -2314,18 +2317,18 @@ static s32 ixgbe_get_link_capabilities_X550em(struct ixgbe_hw *hw,
  * @hw: pointer to hardware structure
  * @lsc: pointer to boolean flag which indicates whether external Base T
  *	 PHY interrupt is lsc
+ * @is_overtemp: indicate whether an overtemp event encountered
  *
  * Determime if external Base T PHY interrupt cause is high temperature
  * failure alarm or link status change.
- *
- * Return IXGBE_ERR_OVERTEMP if interrupt is high temperature
- * failure alarm, else return PHY access status.
  **/
-static s32 ixgbe_get_lasi_ext_t_x550em(struct ixgbe_hw *hw, bool *lsc)
+static s32 ixgbe_get_lasi_ext_t_x550em(struct ixgbe_hw *hw, bool *lsc,
+				       bool *is_overtemp)
 {
 	u32 status;
 	u16 reg;
 
+	*is_overtemp = false;
 	*lsc = false;
 
 	/* Vendor alarm triggered */
@@ -2357,7 +2360,8 @@ static s32 ixgbe_get_lasi_ext_t_x550em(struct ixgbe_hw *hw, bool *lsc)
 	if (reg & IXGBE_MDIO_GLOBAL_ALM_1_HI_TMP_FAIL) {
 		/* power down the PHY in case the PHY FW didn't already */
 		ixgbe_set_copper_phy_power(hw, false);
-		return IXGBE_ERR_OVERTEMP;
+		*is_overtemp = true;
+		return -EIO;
 	}
 	if (reg & IXGBE_MDIO_GLOBAL_ALM_1_DEV_FAULT) {
 		/*  device fault alarm triggered */
@@ -2371,7 +2375,8 @@ static s32 ixgbe_get_lasi_ext_t_x550em(struct ixgbe_hw *hw, bool *lsc)
 		if (reg == IXGBE_MDIO_GLOBAL_FAULT_MSG_HI_TMP) {
 			/* power down the PHY in case the PHY FW didn't */
 			ixgbe_set_copper_phy_power(hw, false);
-			return IXGBE_ERR_OVERTEMP;
+			*is_overtemp = true;
+			return -EIO;
 		}
 	}
 
@@ -2407,12 +2412,12 @@ static s32 ixgbe_get_lasi_ext_t_x550em(struct ixgbe_hw *hw, bool *lsc)
  **/
 static s32 ixgbe_enable_lasi_ext_t_x550em(struct ixgbe_hw *hw)
 {
+	bool lsc, overtemp;
 	u32 status;
 	u16 reg;
-	bool lsc;
 
 	/* Clear interrupt flags */
-	status = ixgbe_get_lasi_ext_t_x550em(hw, &lsc);
+	status = ixgbe_get_lasi_ext_t_x550em(hw, &lsc, &overtemp);
 
 	/* Enable link status change alarm */
 
@@ -2491,21 +2496,20 @@ static s32 ixgbe_enable_lasi_ext_t_x550em(struct ixgbe_hw *hw)
 /**
  * ixgbe_handle_lasi_ext_t_x550em - Handle external Base T PHY interrupt
  * @hw: pointer to hardware structure
+ * @is_overtemp: indicate whether an overtemp event encountered
  *
  * Handle external Base T PHY interrupt. If high temperature
  * failure alarm then return error, else if link status change
  * then setup internal/external PHY link
- *
- * Return IXGBE_ERR_OVERTEMP if interrupt is high temperature
- * failure alarm, else return PHY access status.
  **/
-static s32 ixgbe_handle_lasi_ext_t_x550em(struct ixgbe_hw *hw)
+static s32 ixgbe_handle_lasi_ext_t_x550em(struct ixgbe_hw *hw,
+					  bool *is_overtemp)
 {
 	struct ixgbe_phy_info *phy = &hw->phy;
 	bool lsc;
 	u32 status;
 
-	status = ixgbe_get_lasi_ext_t_x550em(hw, &lsc);
+	status = ixgbe_get_lasi_ext_t_x550em(hw, &lsc, is_overtemp);
 	if (status)
 		return status;
 
@@ -3132,21 +3136,23 @@ static s32 ixgbe_reset_phy_fw(struct ixgbe_hw *hw)
 /**
  * ixgbe_check_overtemp_fw - Check firmware-controlled PHYs for overtemp
  * @hw: pointer to hardware structure
+ *
+ * Return true when an overtemp event detected, otherwise false.
  */
-static s32 ixgbe_check_overtemp_fw(struct ixgbe_hw *hw)
+static bool ixgbe_check_overtemp_fw(struct ixgbe_hw *hw)
 {
 	u32 store[FW_PHY_ACT_DATA_COUNT] = { 0 };
 	s32 rc;
 
 	rc = ixgbe_fw_phy_activity(hw, FW_PHY_ACT_GET_LINK_INFO, &store);
 	if (rc)
-		return rc;
+		return false;
 
 	if (store[0] & FW_PHY_ACT_GET_LINK_INFO_TEMP) {
 		ixgbe_shutdown_fw_phy(hw);
-		return IXGBE_ERR_OVERTEMP;
+		return true;
 	}
-	return 0;
+	return false;
 }
 
 /**
diff --git drivers/net/ethernet/mellanox/mlx5/core/en_arfs.c drivers/net/ethernet/mellanox/mlx5/core/en_arfs.c
index c567cff499d1..b8c7997ea52b 100644
--- linux-4.14.336/drivers/net/ethernet/mellanox/mlx5/core/en_arfs.c
+++ linux-4.14.336/drivers/net/ethernet/mellanox/mlx5/core/en_arfs.c
@@ -229,11 +229,13 @@ static int arfs_create_groups(struct mlx5e_flow_table *ft,
 
 	ft->g = kcalloc(MLX5E_ARFS_NUM_GROUPS,
 			sizeof(*ft->g), GFP_KERNEL);
-	in = kvzalloc(inlen, GFP_KERNEL);
-	if  (!in || !ft->g) {
-		kvfree(ft->g);
-		kvfree(in);
+	if (!ft->g)
 		return -ENOMEM;
+
+	in = kvzalloc(inlen, GFP_KERNEL);
+	if (!in) {
+		err = -ENOMEM;
+		goto err_free_g;
 	}
 
 	mc = MLX5_ADDR_OF(create_flow_group_in, in, match_criteria);
@@ -253,7 +255,7 @@ static int arfs_create_groups(struct mlx5e_flow_table *ft,
 		break;
 	default:
 		err = -EINVAL;
-		goto out;
+		goto err_free_in;
 	}
 
 	switch (type) {
@@ -275,7 +277,7 @@ static int arfs_create_groups(struct mlx5e_flow_table *ft,
 		break;
 	default:
 		err = -EINVAL;
-		goto out;
+		goto err_free_in;
 	}
 
 	MLX5_SET_CFG(in, match_criteria_enable, MLX5_MATCH_OUTER_HEADERS);
@@ -284,7 +286,7 @@ static int arfs_create_groups(struct mlx5e_flow_table *ft,
 	MLX5_SET_CFG(in, end_flow_index, ix - 1);
 	ft->g[ft->num_groups] = mlx5_create_flow_group(ft->t, in);
 	if (IS_ERR(ft->g[ft->num_groups]))
-		goto err;
+		goto err_clean_group;
 	ft->num_groups++;
 
 	memset(in, 0, inlen);
@@ -293,18 +295,20 @@ static int arfs_create_groups(struct mlx5e_flow_table *ft,
 	MLX5_SET_CFG(in, end_flow_index, ix - 1);
 	ft->g[ft->num_groups] = mlx5_create_flow_group(ft->t, in);
 	if (IS_ERR(ft->g[ft->num_groups]))
-		goto err;
+		goto err_clean_group;
 	ft->num_groups++;
 
 	kvfree(in);
 	return 0;
 
-err:
+err_clean_group:
 	err = PTR_ERR(ft->g[ft->num_groups]);
 	ft->g[ft->num_groups] = NULL;
-out:
+err_free_in:
 	kvfree(in);
-
+err_free_g:
+	kfree(ft->g);
+	ft->g = NULL;
 	return err;
 }
 
diff --git drivers/net/ethernet/netronome/nfp/nfpcore/nfp6000_pcie.c drivers/net/ethernet/netronome/nfp/nfpcore/nfp6000_pcie.c
index cd678323bacb..375c1c4ffc0c 100644
--- linux-4.14.336/drivers/net/ethernet/netronome/nfp/nfpcore/nfp6000_pcie.c
+++ linux-4.14.336/drivers/net/ethernet/netronome/nfp/nfpcore/nfp6000_pcie.c
@@ -571,11 +571,13 @@ static int enable_bars(struct nfp6000_pcie *nfp, u16 interface)
 	const u32 barcfg_msix_general =
 		NFP_PCIE_BAR_PCIE2CPP_MapType(
 			NFP_PCIE_BAR_PCIE2CPP_MapType_GENERAL) |
-		NFP_PCIE_BAR_PCIE2CPP_LengthSelect_32BIT;
+		NFP_PCIE_BAR_PCIE2CPP_LengthSelect(
+			NFP_PCIE_BAR_PCIE2CPP_LengthSelect_32BIT);
 	const u32 barcfg_msix_xpb =
 		NFP_PCIE_BAR_PCIE2CPP_MapType(
 			NFP_PCIE_BAR_PCIE2CPP_MapType_BULK) |
-		NFP_PCIE_BAR_PCIE2CPP_LengthSelect_32BIT |
+		NFP_PCIE_BAR_PCIE2CPP_LengthSelect(
+			NFP_PCIE_BAR_PCIE2CPP_LengthSelect_32BIT) |
 		NFP_PCIE_BAR_PCIE2CPP_Target_BaseAddress(
 			NFP_CPP_TARGET_ISLAND_XPB);
 	const u32 barcfg_explicit[4] = {
diff --git drivers/net/ethernet/qlogic/qla3xxx.c drivers/net/ethernet/qlogic/qla3xxx.c
index 6c8a591db713..bc3d268916b8 100644
--- linux-4.14.336/drivers/net/ethernet/qlogic/qla3xxx.c
+++ linux-4.14.336/drivers/net/ethernet/qlogic/qla3xxx.c
@@ -316,12 +316,11 @@ static void ql_release_to_lrg_buf_free_list(struct ql3_adapter *qdev,
 			 * buffer
 			 */
 			skb_reserve(lrg_buf_cb->skb, QL_HEADER_SPACE);
-			map = pci_map_single(qdev->pdev,
+			map = dma_map_single(&qdev->pdev->dev,
 					     lrg_buf_cb->skb->data,
-					     qdev->lrg_buffer_len -
-					     QL_HEADER_SPACE,
-					     PCI_DMA_FROMDEVICE);
-			err = pci_dma_mapping_error(qdev->pdev, map);
+					     qdev->lrg_buffer_len - QL_HEADER_SPACE,
+					     DMA_FROM_DEVICE);
+			err = dma_mapping_error(&qdev->pdev->dev, map);
 			if (err) {
 				netdev_err(qdev->ndev,
 					   "PCI mapping failed with error: %d\n",
@@ -1803,13 +1802,12 @@ static int ql_populate_free_queue(struct ql3_adapter *qdev)
 				 * first buffer
 				 */
 				skb_reserve(lrg_buf_cb->skb, QL_HEADER_SPACE);
-				map = pci_map_single(qdev->pdev,
+				map = dma_map_single(&qdev->pdev->dev,
 						     lrg_buf_cb->skb->data,
-						     qdev->lrg_buffer_len -
-						     QL_HEADER_SPACE,
-						     PCI_DMA_FROMDEVICE);
+						     qdev->lrg_buffer_len - QL_HEADER_SPACE,
+						     DMA_FROM_DEVICE);
 
-				err = pci_dma_mapping_error(qdev->pdev, map);
+				err = dma_mapping_error(&qdev->pdev->dev, map);
 				if (err) {
 					netdev_err(qdev->ndev,
 						   "PCI mapping failed with error: %d\n",
@@ -1944,18 +1942,16 @@ static void ql_process_mac_tx_intr(struct ql3_adapter *qdev,
 		goto invalid_seg_count;
 	}
 
-	pci_unmap_single(qdev->pdev,
+	dma_unmap_single(&qdev->pdev->dev,
 			 dma_unmap_addr(&tx_cb->map[0], mapaddr),
-			 dma_unmap_len(&tx_cb->map[0], maplen),
-			 PCI_DMA_TODEVICE);
+			 dma_unmap_len(&tx_cb->map[0], maplen), DMA_TO_DEVICE);
 	tx_cb->seg_count--;
 	if (tx_cb->seg_count) {
 		for (i = 1; i < tx_cb->seg_count; i++) {
-			pci_unmap_page(qdev->pdev,
-				       dma_unmap_addr(&tx_cb->map[i],
-						      mapaddr),
+			dma_unmap_page(&qdev->pdev->dev,
+				       dma_unmap_addr(&tx_cb->map[i], mapaddr),
 				       dma_unmap_len(&tx_cb->map[i], maplen),
-				       PCI_DMA_TODEVICE);
+				       DMA_TO_DEVICE);
 		}
 	}
 	qdev->ndev->stats.tx_packets++;
@@ -2022,10 +2018,9 @@ static void ql_process_mac_rx_intr(struct ql3_adapter *qdev,
 	qdev->ndev->stats.rx_bytes += length;
 
 	skb_put(skb, length);
-	pci_unmap_single(qdev->pdev,
+	dma_unmap_single(&qdev->pdev->dev,
 			 dma_unmap_addr(lrg_buf_cb2, mapaddr),
-			 dma_unmap_len(lrg_buf_cb2, maplen),
-			 PCI_DMA_FROMDEVICE);
+			 dma_unmap_len(lrg_buf_cb2, maplen), DMA_FROM_DEVICE);
 	prefetch(skb->data);
 	skb_checksum_none_assert(skb);
 	skb->protocol = eth_type_trans(skb, qdev->ndev);
@@ -2068,10 +2063,9 @@ static void ql_process_macip_rx_intr(struct ql3_adapter *qdev,
 	skb2 = lrg_buf_cb2->skb;
 
 	skb_put(skb2, length);	/* Just the second buffer length here. */
-	pci_unmap_single(qdev->pdev,
+	dma_unmap_single(&qdev->pdev->dev,
 			 dma_unmap_addr(lrg_buf_cb2, mapaddr),
-			 dma_unmap_len(lrg_buf_cb2, maplen),
-			 PCI_DMA_FROMDEVICE);
+			 dma_unmap_len(lrg_buf_cb2, maplen), DMA_FROM_DEVICE);
 	prefetch(skb2->data);
 
 	skb_checksum_none_assert(skb2);
@@ -2320,9 +2314,9 @@ static int ql_send_map(struct ql3_adapter *qdev,
 	/*
 	 * Map the skb buffer first.
 	 */
-	map = pci_map_single(qdev->pdev, skb->data, len, PCI_DMA_TODEVICE);
+	map = dma_map_single(&qdev->pdev->dev, skb->data, len, DMA_TO_DEVICE);
 
-	err = pci_dma_mapping_error(qdev->pdev, map);
+	err = dma_mapping_error(&qdev->pdev->dev, map);
 	if (err) {
 		netdev_err(qdev->ndev, "PCI mapping failed with error: %d\n",
 			   err);
@@ -2358,11 +2352,11 @@ static int ql_send_map(struct ql3_adapter *qdev,
 		    (seg == 7 && seg_cnt > 8) ||
 		    (seg == 12 && seg_cnt > 13) ||
 		    (seg == 17 && seg_cnt > 18)) {
-			map = pci_map_single(qdev->pdev, oal,
+			map = dma_map_single(&qdev->pdev->dev, oal,
 					     sizeof(struct oal),
-					     PCI_DMA_TODEVICE);
+					     DMA_TO_DEVICE);
 
-			err = pci_dma_mapping_error(qdev->pdev, map);
+			err = dma_mapping_error(&qdev->pdev->dev, map);
 			if (err) {
 				netdev_err(qdev->ndev,
 					   "PCI mapping outbound address list with error: %d\n",
@@ -2424,24 +2418,24 @@ map_error:
 		    (seg == 7 && seg_cnt > 8) ||
 		    (seg == 12 && seg_cnt > 13) ||
 		    (seg == 17 && seg_cnt > 18)) {
-			pci_unmap_single(qdev->pdev,
-				dma_unmap_addr(&tx_cb->map[seg], mapaddr),
-				dma_unmap_len(&tx_cb->map[seg], maplen),
-				 PCI_DMA_TODEVICE);
+			dma_unmap_single(&qdev->pdev->dev,
+					 dma_unmap_addr(&tx_cb->map[seg], mapaddr),
+					 dma_unmap_len(&tx_cb->map[seg], maplen),
+					 DMA_TO_DEVICE);
 			oal++;
 			seg++;
 		}
 
-		pci_unmap_page(qdev->pdev,
+		dma_unmap_page(&qdev->pdev->dev,
 			       dma_unmap_addr(&tx_cb->map[seg], mapaddr),
 			       dma_unmap_len(&tx_cb->map[seg], maplen),
-			       PCI_DMA_TODEVICE);
+			       DMA_TO_DEVICE);
 	}
 
-	pci_unmap_single(qdev->pdev,
+	dma_unmap_single(&qdev->pdev->dev,
 			 dma_unmap_addr(&tx_cb->map[0], mapaddr),
 			 dma_unmap_addr(&tx_cb->map[0], maplen),
-			 PCI_DMA_TODEVICE);
+			 DMA_TO_DEVICE);
 
 	return NETDEV_TX_BUSY;
 
@@ -2527,9 +2521,8 @@ static int ql_alloc_net_req_rsp_queues(struct ql3_adapter *qdev)
 	wmb();
 
 	qdev->req_q_virt_addr =
-	    pci_alloc_consistent(qdev->pdev,
-				 (size_t) qdev->req_q_size,
-				 &qdev->req_q_phy_addr);
+	    dma_alloc_coherent(&qdev->pdev->dev, (size_t)qdev->req_q_size,
+			       &qdev->req_q_phy_addr, GFP_KERNEL);
 
 	if ((qdev->req_q_virt_addr == NULL) ||
 	    LS_64BITS(qdev->req_q_phy_addr) & (qdev->req_q_size - 1)) {
@@ -2538,16 +2531,14 @@ static int ql_alloc_net_req_rsp_queues(struct ql3_adapter *qdev)
 	}
 
 	qdev->rsp_q_virt_addr =
-	    pci_alloc_consistent(qdev->pdev,
-				 (size_t) qdev->rsp_q_size,
-				 &qdev->rsp_q_phy_addr);
+	    dma_alloc_coherent(&qdev->pdev->dev, (size_t)qdev->rsp_q_size,
+			       &qdev->rsp_q_phy_addr, GFP_KERNEL);
 
 	if ((qdev->rsp_q_virt_addr == NULL) ||
 	    LS_64BITS(qdev->rsp_q_phy_addr) & (qdev->rsp_q_size - 1)) {
 		netdev_err(qdev->ndev, "rspQ allocation failed\n");
-		pci_free_consistent(qdev->pdev, (size_t) qdev->req_q_size,
-				    qdev->req_q_virt_addr,
-				    qdev->req_q_phy_addr);
+		dma_free_coherent(&qdev->pdev->dev, (size_t)qdev->req_q_size,
+				  qdev->req_q_virt_addr, qdev->req_q_phy_addr);
 		return -ENOMEM;
 	}
 
@@ -2563,15 +2554,13 @@ static void ql_free_net_req_rsp_queues(struct ql3_adapter *qdev)
 		return;
 	}
 
-	pci_free_consistent(qdev->pdev,
-			    qdev->req_q_size,
-			    qdev->req_q_virt_addr, qdev->req_q_phy_addr);
+	dma_free_coherent(&qdev->pdev->dev, qdev->req_q_size,
+			  qdev->req_q_virt_addr, qdev->req_q_phy_addr);
 
 	qdev->req_q_virt_addr = NULL;
 
-	pci_free_consistent(qdev->pdev,
-			    qdev->rsp_q_size,
-			    qdev->rsp_q_virt_addr, qdev->rsp_q_phy_addr);
+	dma_free_coherent(&qdev->pdev->dev, qdev->rsp_q_size,
+			  qdev->rsp_q_virt_addr, qdev->rsp_q_phy_addr);
 
 	qdev->rsp_q_virt_addr = NULL;
 
@@ -2595,12 +2584,13 @@ static int ql_alloc_buffer_queues(struct ql3_adapter *qdev)
 		return -ENOMEM;
 
 	qdev->lrg_buf_q_alloc_virt_addr =
-		pci_alloc_consistent(qdev->pdev,
-				     qdev->lrg_buf_q_alloc_size,
-				     &qdev->lrg_buf_q_alloc_phy_addr);
+		dma_alloc_coherent(&qdev->pdev->dev,
+				   qdev->lrg_buf_q_alloc_size,
+				   &qdev->lrg_buf_q_alloc_phy_addr, GFP_KERNEL);
 
 	if (qdev->lrg_buf_q_alloc_virt_addr == NULL) {
 		netdev_err(qdev->ndev, "lBufQ failed\n");
+		kfree(qdev->lrg_buf);
 		return -ENOMEM;
 	}
 	qdev->lrg_buf_q_virt_addr = qdev->lrg_buf_q_alloc_virt_addr;
@@ -2615,15 +2605,17 @@ static int ql_alloc_buffer_queues(struct ql3_adapter *qdev)
 		qdev->small_buf_q_alloc_size = qdev->small_buf_q_size * 2;
 
 	qdev->small_buf_q_alloc_virt_addr =
-		pci_alloc_consistent(qdev->pdev,
-				     qdev->small_buf_q_alloc_size,
-				     &qdev->small_buf_q_alloc_phy_addr);
+		dma_alloc_coherent(&qdev->pdev->dev,
+				   qdev->small_buf_q_alloc_size,
+				   &qdev->small_buf_q_alloc_phy_addr, GFP_KERNEL);
 
 	if (qdev->small_buf_q_alloc_virt_addr == NULL) {
 		netdev_err(qdev->ndev, "Small Buffer Queue allocation failed\n");
-		pci_free_consistent(qdev->pdev, qdev->lrg_buf_q_alloc_size,
-				    qdev->lrg_buf_q_alloc_virt_addr,
-				    qdev->lrg_buf_q_alloc_phy_addr);
+		dma_free_coherent(&qdev->pdev->dev,
+				  qdev->lrg_buf_q_alloc_size,
+				  qdev->lrg_buf_q_alloc_virt_addr,
+				  qdev->lrg_buf_q_alloc_phy_addr);
+		kfree(qdev->lrg_buf);
 		return -ENOMEM;
 	}
 
@@ -2640,17 +2632,15 @@ static void ql_free_buffer_queues(struct ql3_adapter *qdev)
 		return;
 	}
 	kfree(qdev->lrg_buf);
-	pci_free_consistent(qdev->pdev,
-			    qdev->lrg_buf_q_alloc_size,
-			    qdev->lrg_buf_q_alloc_virt_addr,
-			    qdev->lrg_buf_q_alloc_phy_addr);
+	dma_free_coherent(&qdev->pdev->dev, qdev->lrg_buf_q_alloc_size,
+			  qdev->lrg_buf_q_alloc_virt_addr,
+			  qdev->lrg_buf_q_alloc_phy_addr);
 
 	qdev->lrg_buf_q_virt_addr = NULL;
 
-	pci_free_consistent(qdev->pdev,
-			    qdev->small_buf_q_alloc_size,
-			    qdev->small_buf_q_alloc_virt_addr,
-			    qdev->small_buf_q_alloc_phy_addr);
+	dma_free_coherent(&qdev->pdev->dev, qdev->small_buf_q_alloc_size,
+			  qdev->small_buf_q_alloc_virt_addr,
+			  qdev->small_buf_q_alloc_phy_addr);
 
 	qdev->small_buf_q_virt_addr = NULL;
 
@@ -2668,9 +2658,9 @@ static int ql_alloc_small_buffers(struct ql3_adapter *qdev)
 		 QL_SMALL_BUFFER_SIZE);
 
 	qdev->small_buf_virt_addr =
-		pci_alloc_consistent(qdev->pdev,
-				     qdev->small_buf_total_size,
-				     &qdev->small_buf_phy_addr);
+		dma_alloc_coherent(&qdev->pdev->dev,
+				   qdev->small_buf_total_size,
+				   &qdev->small_buf_phy_addr, GFP_KERNEL);
 
 	if (qdev->small_buf_virt_addr == NULL) {
 		netdev_err(qdev->ndev, "Failed to get small buffer memory\n");
@@ -2703,10 +2693,10 @@ static void ql_free_small_buffers(struct ql3_adapter *qdev)
 		return;
 	}
 	if (qdev->small_buf_virt_addr != NULL) {
-		pci_free_consistent(qdev->pdev,
-				    qdev->small_buf_total_size,
-				    qdev->small_buf_virt_addr,
-				    qdev->small_buf_phy_addr);
+		dma_free_coherent(&qdev->pdev->dev,
+				  qdev->small_buf_total_size,
+				  qdev->small_buf_virt_addr,
+				  qdev->small_buf_phy_addr);
 
 		qdev->small_buf_virt_addr = NULL;
 	}
@@ -2721,10 +2711,10 @@ static void ql_free_large_buffers(struct ql3_adapter *qdev)
 		lrg_buf_cb = &qdev->lrg_buf[i];
 		if (lrg_buf_cb->skb) {
 			dev_kfree_skb(lrg_buf_cb->skb);
-			pci_unmap_single(qdev->pdev,
+			dma_unmap_single(&qdev->pdev->dev,
 					 dma_unmap_addr(lrg_buf_cb, mapaddr),
 					 dma_unmap_len(lrg_buf_cb, maplen),
-					 PCI_DMA_FROMDEVICE);
+					 DMA_FROM_DEVICE);
 			memset(lrg_buf_cb, 0, sizeof(struct ql_rcv_buf_cb));
 		} else {
 			break;
@@ -2776,13 +2766,11 @@ static int ql_alloc_large_buffers(struct ql3_adapter *qdev)
 			 * buffer
 			 */
 			skb_reserve(skb, QL_HEADER_SPACE);
-			map = pci_map_single(qdev->pdev,
-					     skb->data,
-					     qdev->lrg_buffer_len -
-					     QL_HEADER_SPACE,
-					     PCI_DMA_FROMDEVICE);
+			map = dma_map_single(&qdev->pdev->dev, skb->data,
+					     qdev->lrg_buffer_len - QL_HEADER_SPACE,
+					     DMA_FROM_DEVICE);
 
-			err = pci_dma_mapping_error(qdev->pdev, map);
+			err = dma_mapping_error(&qdev->pdev->dev, map);
 			if (err) {
 				netdev_err(qdev->ndev,
 					   "PCI mapping failed with error: %d\n",
@@ -2867,8 +2855,8 @@ static int ql_alloc_mem_resources(struct ql3_adapter *qdev)
 	 * Network Completion Queue Producer Index Register
 	 */
 	qdev->shadow_reg_virt_addr =
-		pci_alloc_consistent(qdev->pdev,
-				     PAGE_SIZE, &qdev->shadow_reg_phy_addr);
+		dma_alloc_coherent(&qdev->pdev->dev, PAGE_SIZE,
+				   &qdev->shadow_reg_phy_addr, GFP_KERNEL);
 
 	if (qdev->shadow_reg_virt_addr != NULL) {
 		qdev->preq_consumer_index = qdev->shadow_reg_virt_addr;
@@ -2923,10 +2911,9 @@ err_small_buffers:
 err_buffer_queues:
 	ql_free_net_req_rsp_queues(qdev);
 err_req_rsp:
-	pci_free_consistent(qdev->pdev,
-			    PAGE_SIZE,
-			    qdev->shadow_reg_virt_addr,
-			    qdev->shadow_reg_phy_addr);
+	dma_free_coherent(&qdev->pdev->dev, PAGE_SIZE,
+			  qdev->shadow_reg_virt_addr,
+			  qdev->shadow_reg_phy_addr);
 
 	return -ENOMEM;
 }
@@ -2939,10 +2926,9 @@ static void ql_free_mem_resources(struct ql3_adapter *qdev)
 	ql_free_buffer_queues(qdev);
 	ql_free_net_req_rsp_queues(qdev);
 	if (qdev->shadow_reg_virt_addr != NULL) {
-		pci_free_consistent(qdev->pdev,
-				    PAGE_SIZE,
-				    qdev->shadow_reg_virt_addr,
-				    qdev->shadow_reg_phy_addr);
+		dma_free_coherent(&qdev->pdev->dev, PAGE_SIZE,
+				  qdev->shadow_reg_virt_addr,
+				  qdev->shadow_reg_phy_addr);
 		qdev->shadow_reg_virt_addr = NULL;
 	}
 }
@@ -3643,18 +3629,15 @@ static void ql_reset_work(struct work_struct *work)
 			if (tx_cb->skb) {
 				netdev_printk(KERN_DEBUG, ndev,
 					      "Freeing lost SKB\n");
-				pci_unmap_single(qdev->pdev,
-					 dma_unmap_addr(&tx_cb->map[0],
-							mapaddr),
-					 dma_unmap_len(&tx_cb->map[0], maplen),
-					 PCI_DMA_TODEVICE);
+				dma_unmap_single(&qdev->pdev->dev,
+						 dma_unmap_addr(&tx_cb->map[0], mapaddr),
+						 dma_unmap_len(&tx_cb->map[0], maplen),
+						 DMA_TO_DEVICE);
 				for (j = 1; j < tx_cb->seg_count; j++) {
-					pci_unmap_page(qdev->pdev,
-					       dma_unmap_addr(&tx_cb->map[j],
-							      mapaddr),
-					       dma_unmap_len(&tx_cb->map[j],
-							     maplen),
-					       PCI_DMA_TODEVICE);
+					dma_unmap_page(&qdev->pdev->dev,
+						       dma_unmap_addr(&tx_cb->map[j], mapaddr),
+						       dma_unmap_len(&tx_cb->map[j], maplen),
+						       DMA_TO_DEVICE);
 				}
 				dev_kfree_skb(tx_cb->skb);
 				tx_cb->skb = NULL;
@@ -3786,13 +3769,10 @@ static int ql3xxx_probe(struct pci_dev *pdev,
 
 	pci_set_master(pdev);
 
-	if (!pci_set_dma_mask(pdev, DMA_BIT_MASK(64))) {
+	if (!dma_set_mask_and_coherent(&pdev->dev, DMA_BIT_MASK(64)))
 		pci_using_dac = 1;
-		err = pci_set_consistent_dma_mask(pdev, DMA_BIT_MASK(64));
-	} else if (!(err = pci_set_dma_mask(pdev, DMA_BIT_MASK(32)))) {
+	else if (!(err = dma_set_mask_and_coherent(&pdev->dev, DMA_BIT_MASK(32))))
 		pci_using_dac = 0;
-		err = pci_set_consistent_dma_mask(pdev, DMA_BIT_MASK(32));
-	}
 
 	if (err) {
 		pr_err("%s no usable DMA configuration\n", pci_name(pdev));
diff --git drivers/net/ethernet/renesas/ravb_main.c drivers/net/ethernet/renesas/ravb_main.c
index b97d450214df..2190ed6b0081 100644
--- linux-4.14.336/drivers/net/ethernet/renesas/ravb_main.c
+++ linux-4.14.336/drivers/net/ethernet/renesas/ravb_main.c
@@ -1545,7 +1545,7 @@ static netdev_tx_t ravb_start_xmit(struct sk_buff *skb, struct net_device *ndev)
 	struct ravb_tstamp_skb *ts_skb;
 	struct ravb_tx_desc *desc;
 	unsigned long flags;
-	u32 dma_addr;
+	dma_addr_t dma_addr;
 	void *buffer;
 	u32 entry;
 	u32 len;
diff --git drivers/net/fjes/fjes_hw.c drivers/net/fjes/fjes_hw.c
index 9c652c04375b..c3fa8db69b9e 100644
--- linux-4.14.336/drivers/net/fjes/fjes_hw.c
+++ linux-4.14.336/drivers/net/fjes/fjes_hw.c
@@ -235,21 +235,25 @@ static int fjes_hw_setup(struct fjes_hw *hw)
 
 	mem_size = FJES_DEV_REQ_BUF_SIZE(hw->max_epid);
 	hw->hw_info.req_buf = kzalloc(mem_size, GFP_KERNEL);
-	if (!(hw->hw_info.req_buf))
-		return -ENOMEM;
+	if (!(hw->hw_info.req_buf)) {
+		result = -ENOMEM;
+		goto free_ep_info;
+	}
 
 	hw->hw_info.req_buf_size = mem_size;
 
 	mem_size = FJES_DEV_RES_BUF_SIZE(hw->max_epid);
 	hw->hw_info.res_buf = kzalloc(mem_size, GFP_KERNEL);
-	if (!(hw->hw_info.res_buf))
-		return -ENOMEM;
+	if (!(hw->hw_info.res_buf)) {
+		result = -ENOMEM;
+		goto free_req_buf;
+	}
 
 	hw->hw_info.res_buf_size = mem_size;
 
 	result = fjes_hw_alloc_shared_status_region(hw);
 	if (result)
-		return result;
+		goto free_res_buf;
 
 	hw->hw_info.buffer_share_bit = 0;
 	hw->hw_info.buffer_unshare_reserve_bit = 0;
@@ -260,11 +264,11 @@ static int fjes_hw_setup(struct fjes_hw *hw)
 
 			result = fjes_hw_alloc_epbuf(&buf_pair->tx);
 			if (result)
-				return result;
+				goto free_epbuf;
 
 			result = fjes_hw_alloc_epbuf(&buf_pair->rx);
 			if (result)
-				return result;
+				goto free_epbuf;
 
 			spin_lock_irqsave(&hw->rx_status_lock, flags);
 			fjes_hw_setup_epbuf(&buf_pair->tx, mac,
@@ -287,6 +291,25 @@ static int fjes_hw_setup(struct fjes_hw *hw)
 	fjes_hw_init_command_registers(hw, &param);
 
 	return 0;
+
+free_epbuf:
+	for (epidx = 0; epidx < hw->max_epid ; epidx++) {
+		if (epidx == hw->my_epid)
+			continue;
+		fjes_hw_free_epbuf(&hw->ep_shm_info[epidx].tx);
+		fjes_hw_free_epbuf(&hw->ep_shm_info[epidx].rx);
+	}
+	fjes_hw_free_shared_status_region(hw);
+free_res_buf:
+	kfree(hw->hw_info.res_buf);
+	hw->hw_info.res_buf = NULL;
+free_req_buf:
+	kfree(hw->hw_info.req_buf);
+	hw->hw_info.req_buf = NULL;
+free_ep_info:
+	kfree(hw->ep_shm_info);
+	hw->ep_shm_info = NULL;
+	return result;
 }
 
 static void fjes_hw_cleanup(struct fjes_hw *hw)
diff --git drivers/net/gtp.c drivers/net/gtp.c
index d7bf8212ff04..a222736c3117 100644
--- linux-4.14.336/drivers/net/gtp.c
+++ linux-4.14.336/drivers/net/gtp.c
@@ -1380,26 +1380,26 @@ static int __init gtp_init(void)
 
 	get_random_bytes(&gtp_h_initval, sizeof(gtp_h_initval));
 
-	err = rtnl_link_register(&gtp_link_ops);
+	err = register_pernet_subsys(&gtp_net_ops);
 	if (err < 0)
 		goto error_out;
 
-	err = genl_register_family(&gtp_genl_family);
+	err = rtnl_link_register(&gtp_link_ops);
 	if (err < 0)
-		goto unreg_rtnl_link;
+		goto unreg_pernet_subsys;
 
-	err = register_pernet_subsys(&gtp_net_ops);
+	err = genl_register_family(&gtp_genl_family);
 	if (err < 0)
-		goto unreg_genl_family;
+		goto unreg_rtnl_link;
 
 	pr_info("GTP module loaded (pdp ctx size %zd bytes)\n",
 		sizeof(struct pdp_ctx));
 	return 0;
 
-unreg_genl_family:
-	genl_unregister_family(&gtp_genl_family);
 unreg_rtnl_link:
 	rtnl_link_unregister(&gtp_link_ops);
+unreg_pernet_subsys:
+	unregister_pernet_subsys(&gtp_net_ops);
 error_out:
 	pr_err("error loading GTP module loaded\n");
 	return err;
diff --git drivers/net/ppp/ppp_async.c drivers/net/ppp/ppp_async.c
index 297a986e6653..4d981d9e0e38 100644
--- linux-4.14.336/drivers/net/ppp/ppp_async.c
+++ linux-4.14.336/drivers/net/ppp/ppp_async.c
@@ -474,6 +474,10 @@ ppp_async_ioctl(struct ppp_channel *chan, unsigned int cmd, unsigned long arg)
 	case PPPIOCSMRU:
 		if (get_user(val, p))
 			break;
+		if (val > U16_MAX) {
+			err = -EINVAL;
+			break;
+		}
 		if (val < PPP_MRU)
 			val = PPP_MRU;
 		ap->mru = val;
diff --git drivers/net/usb/ax88172a.c drivers/net/usb/ax88172a.c
index 909755ef71ac..5881620e4436 100644
--- linux-4.14.336/drivers/net/usb/ax88172a.c
+++ linux-4.14.336/drivers/net/usb/ax88172a.c
@@ -198,7 +198,9 @@ static int ax88172a_bind(struct usbnet *dev, struct usb_interface *intf)
 	u8 buf[ETH_ALEN];
 	struct ax88172a_private *priv;
 
-	usbnet_get_endpoints(dev, intf);
+	ret = usbnet_get_endpoints(dev, intf);
+	if (ret)
+		return ret;
 
 	priv = kzalloc(sizeof(*priv), GFP_KERNEL);
 	if (!priv)
diff --git drivers/net/usb/dm9601.c drivers/net/usb/dm9601.c
index 5aad26600b03..9b7db5fd9e08 100644
--- linux-4.14.336/drivers/net/usb/dm9601.c
+++ linux-4.14.336/drivers/net/usb/dm9601.c
@@ -231,7 +231,7 @@ static int dm9601_mdio_read(struct net_device *netdev, int phy_id, int loc)
 	err = dm_read_shared_word(dev, 1, loc, &res);
 	if (err < 0) {
 		netdev_err(dev->net, "MDIO read error: %d\n", err);
-		return err;
+		return 0;
 	}
 
 	netdev_dbg(dev->net,
diff --git drivers/net/usb/lan78xx.c drivers/net/usb/lan78xx.c
index d6a71c051ec1..171accb5ebbf 100644
--- linux-4.14.336/drivers/net/usb/lan78xx.c
+++ linux-4.14.336/drivers/net/usb/lan78xx.c
@@ -2450,7 +2450,8 @@ static int lan78xx_reset(struct lan78xx_net *dev)
 	if (dev->chipid == ID_REV_CHIP_ID_7801_)
 		buf &= ~MAC_CR_GMII_EN_;
 
-	if (dev->chipid == ID_REV_CHIP_ID_7800_) {
+	if (dev->chipid == ID_REV_CHIP_ID_7800_ ||
+	    dev->chipid == ID_REV_CHIP_ID_7850_) {
 		ret = lan78xx_read_raw_eeprom(dev, 0, 1, &sig);
 		if (!ret && sig != EEPROM_INDICATOR) {
 			/* Implies there is no external eeprom. Set mac speed */
diff --git drivers/net/virtio_net.c drivers/net/virtio_net.c
index 067ebdd0d589..8e1a3c523b09 100644
--- linux-4.14.336/drivers/net/virtio_net.c
+++ linux-4.14.336/drivers/net/virtio_net.c
@@ -2277,10 +2277,11 @@ static int virtnet_find_vqs(struct virtnet_info *vi)
 {
 	vq_callback_t **callbacks;
 	struct virtqueue **vqs;
-	int ret = -ENOMEM;
-	int i, total_vqs;
 	const char **names;
+	int ret = -ENOMEM;
+	int total_vqs;
 	bool *ctx;
+	u16 i;
 
 	/* We expect 1 RX virtqueue followed by 1 TX virtqueue, followed by
 	 * possible N-1 RX/TX queue pairs used in multiqueue mode, followed by
@@ -2317,8 +2318,8 @@ static int virtnet_find_vqs(struct virtnet_info *vi)
 	for (i = 0; i < vi->max_queue_pairs; i++) {
 		callbacks[rxq2vq(i)] = skb_recv_done;
 		callbacks[txq2vq(i)] = skb_xmit_done;
-		sprintf(vi->rq[i].name, "input.%d", i);
-		sprintf(vi->sq[i].name, "output.%d", i);
+		sprintf(vi->rq[i].name, "input.%u", i);
+		sprintf(vi->sq[i].name, "output.%u", i);
 		names[rxq2vq(i)] = vi->rq[i].name;
 		names[txq2vq(i)] = vi->sq[i].name;
 		if (ctx)
diff --git drivers/net/wan/lmc/lmc_proto.c drivers/net/wan/lmc/lmc_proto.c
index f600075e84a2..7ae39a2b6340 100644
--- linux-4.14.336/drivers/net/wan/lmc/lmc_proto.c
+++ linux-4.14.336/drivers/net/wan/lmc/lmc_proto.c
@@ -103,17 +103,13 @@ __be16 lmc_proto_type(lmc_softc_t *sc, struct sk_buff *skb) /*FOLD00*/
     switch(sc->if_type){
     case LMC_PPP:
 	    return hdlc_type_trans(skb, sc->lmc_device);
-	    break;
     case LMC_NET:
         return htons(ETH_P_802_2);
-        break;
     case LMC_RAW: /* Packet type for skbuff kind of useless */
         return htons(ETH_P_802_2);
-        break;
     default:
         printk(KERN_WARNING "%s: No protocol set for this interface, assuming 802.2 (which is wrong!!)\n", sc->name);
         return htons(ETH_P_802_2);
-        break;
     }
     lmc_trace(sc->lmc_device, "lmc_proto_tye out");
 
diff --git drivers/net/wireless/ath/ath9k/htc_drv_txrx.c drivers/net/wireless/ath/ath9k/htc_drv_txrx.c
index e62ed7f42281..763521fca11d 100644
--- linux-4.14.336/drivers/net/wireless/ath/ath9k/htc_drv_txrx.c
+++ linux-4.14.336/drivers/net/wireless/ath/ath9k/htc_drv_txrx.c
@@ -647,9 +647,10 @@ void ath9k_htc_txstatus(struct ath9k_htc_priv *priv, void *wmi_event)
 	struct ath9k_htc_tx_event *tx_pend;
 	int i;
 
-	for (i = 0; i < txs->cnt; i++) {
-		WARN_ON(txs->cnt > HTC_MAX_TX_STATUS);
+	if (WARN_ON_ONCE(txs->cnt > HTC_MAX_TX_STATUS))
+		return;
 
+	for (i = 0; i < txs->cnt; i++) {
 		__txs = &txs->txstatus[i];
 
 		skb = ath9k_htc_tx_get_packet(priv, __txs);
diff --git drivers/net/wireless/marvell/libertas/Kconfig drivers/net/wireless/marvell/libertas/Kconfig
index e6268ceacbf1..28985cdac541 100644
--- linux-4.14.336/drivers/net/wireless/marvell/libertas/Kconfig
+++ linux-4.14.336/drivers/net/wireless/marvell/libertas/Kconfig
@@ -1,8 +1,6 @@
 config LIBERTAS
 	tristate "Marvell 8xxx Libertas WLAN driver support"
 	depends on CFG80211
-	select WIRELESS_EXT
-	select WEXT_SPY
 	select LIB80211
 	select FW_LOADER
 	---help---
diff --git drivers/net/wireless/marvell/mwifiex/cfg80211.c drivers/net/wireless/marvell/mwifiex/cfg80211.c
index a88bddc38389..76205d6b2f9c 100644
--- linux-4.14.336/drivers/net/wireless/marvell/mwifiex/cfg80211.c
+++ linux-4.14.336/drivers/net/wireless/marvell/mwifiex/cfg80211.c
@@ -1940,6 +1940,8 @@ static int mwifiex_cfg80211_start_ap(struct wiphy *wiphy,
 
 	mwifiex_set_sys_config_invalid_data(bss_cfg);
 
+	memcpy(bss_cfg->mac_addr, priv->curr_addr, ETH_ALEN);
+
 	if (params->beacon_interval)
 		bss_cfg->beacon_period = params->beacon_interval;
 	if (params->dtim_period)
diff --git drivers/net/wireless/marvell/mwifiex/fw.h drivers/net/wireless/marvell/mwifiex/fw.h
index c802b73a15c5..99b40bc6e7a6 100644
--- linux-4.14.336/drivers/net/wireless/marvell/mwifiex/fw.h
+++ linux-4.14.336/drivers/net/wireless/marvell/mwifiex/fw.h
@@ -168,6 +168,7 @@ enum MWIFIEX_802_11_PRIVACY_FILTER {
 #define TLV_TYPE_STA_MAC_ADDR       (PROPRIETARY_TLV_BASE_ID + 32)
 #define TLV_TYPE_BSSID              (PROPRIETARY_TLV_BASE_ID + 35)
 #define TLV_TYPE_CHANNELBANDLIST    (PROPRIETARY_TLV_BASE_ID + 42)
+#define TLV_TYPE_UAP_MAC_ADDRESS    (PROPRIETARY_TLV_BASE_ID + 43)
 #define TLV_TYPE_UAP_BEACON_PERIOD  (PROPRIETARY_TLV_BASE_ID + 44)
 #define TLV_TYPE_UAP_DTIM_PERIOD    (PROPRIETARY_TLV_BASE_ID + 45)
 #define TLV_TYPE_UAP_BCAST_SSID     (PROPRIETARY_TLV_BASE_ID + 48)
diff --git drivers/net/wireless/marvell/mwifiex/ioctl.h drivers/net/wireless/marvell/mwifiex/ioctl.h
index 0dd592ea6e83..96ff91655a77 100644
--- linux-4.14.336/drivers/net/wireless/marvell/mwifiex/ioctl.h
+++ linux-4.14.336/drivers/net/wireless/marvell/mwifiex/ioctl.h
@@ -119,6 +119,7 @@ struct mwifiex_uap_bss_param {
 	u8 qos_info;
 	u8 power_constraint;
 	struct mwifiex_types_wmm_info wmm_info;
+	u8 mac_addr[ETH_ALEN];
 };
 
 enum {
diff --git drivers/net/wireless/marvell/mwifiex/uap_cmd.c drivers/net/wireless/marvell/mwifiex/uap_cmd.c
index 0939a8c8f3ab..1ab253c97c14 100644
--- linux-4.14.336/drivers/net/wireless/marvell/mwifiex/uap_cmd.c
+++ linux-4.14.336/drivers/net/wireless/marvell/mwifiex/uap_cmd.c
@@ -479,6 +479,7 @@ void mwifiex_config_uap_11d(struct mwifiex_private *priv,
 static int
 mwifiex_uap_bss_param_prepare(u8 *tlv, void *cmd_buf, u16 *param_size)
 {
+	struct host_cmd_tlv_mac_addr *mac_tlv;
 	struct host_cmd_tlv_dtim_period *dtim_period;
 	struct host_cmd_tlv_beacon_period *beacon_period;
 	struct host_cmd_tlv_ssid *ssid;
@@ -498,6 +499,13 @@ mwifiex_uap_bss_param_prepare(u8 *tlv, void *cmd_buf, u16 *param_size)
 	int i;
 	u16 cmd_size = *param_size;
 
+	mac_tlv = (struct host_cmd_tlv_mac_addr *)tlv;
+	mac_tlv->header.type = cpu_to_le16(TLV_TYPE_UAP_MAC_ADDRESS);
+	mac_tlv->header.len = cpu_to_le16(ETH_ALEN);
+	memcpy(mac_tlv->mac_addr, bss_cfg->mac_addr, ETH_ALEN);
+	cmd_size += sizeof(struct host_cmd_tlv_mac_addr);
+	tlv += sizeof(struct host_cmd_tlv_mac_addr);
+
 	if (bss_cfg->ssid.ssid_len) {
 		ssid = (struct host_cmd_tlv_ssid *)tlv;
 		ssid->header.type = cpu_to_le16(TLV_TYPE_UAP_SSID);
diff --git drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_core.c drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_core.c
index bfd704b17a44..9263a6a64788 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_core.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtl8xxxu/rtl8xxxu_core.c
@@ -6366,6 +6366,18 @@ static const struct usb_device_id dev_table[] = {
 	.driver_info = (unsigned long)&rtl8192eu_fops},
 {USB_DEVICE_AND_INTERFACE_INFO(USB_VENDOR_ID_REALTEK, 0x818c, 0xff, 0xff, 0xff),
 	.driver_info = (unsigned long)&rtl8192eu_fops},
+/* D-Link DWA-131 rev C1 */
+{USB_DEVICE_AND_INTERFACE_INFO(0x2001, 0x3312, 0xff, 0xff, 0xff),
+	.driver_info = (unsigned long)&rtl8192eu_fops},
+/* TP-Link TL-WN8200ND V2 */
+{USB_DEVICE_AND_INTERFACE_INFO(0x2357, 0x0126, 0xff, 0xff, 0xff),
+	.driver_info = (unsigned long)&rtl8192eu_fops},
+/* Mercusys MW300UM */
+{USB_DEVICE_AND_INTERFACE_INFO(0x2c4e, 0x0100, 0xff, 0xff, 0xff),
+	.driver_info = (unsigned long)&rtl8192eu_fops},
+/* Mercusys MW300UH */
+{USB_DEVICE_AND_INTERFACE_INFO(0x2c4e, 0x0104, 0xff, 0xff, 0xff),
+	.driver_info = (unsigned long)&rtl8192eu_fops},
 #endif
 { }
 };
diff --git drivers/net/wireless/realtek/rtlwifi/pci.c drivers/net/wireless/realtek/rtlwifi/pci.c
index ab74f3155854..b6c3a6d422ea 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/pci.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/pci.c
@@ -194,21 +194,29 @@ static bool _rtl_pci_platform_switch_device_pci_aspm(
 	struct rtl_pci *rtlpci = rtl_pcidev(rtl_pcipriv(hw));
 	struct rtl_hal *rtlhal = rtl_hal(rtl_priv(hw));
 
+	value &= PCI_EXP_LNKCTL_ASPMC;
+
 	if (rtlhal->hw_type != HARDWARE_TYPE_RTL8192SE)
-		value |= 0x40;
+		value |= PCI_EXP_LNKCTL_CCC;
 
-	pci_write_config_byte(rtlpci->pdev, 0x80, value);
+	pcie_capability_clear_and_set_word(rtlpci->pdev, PCI_EXP_LNKCTL,
+					   PCI_EXP_LNKCTL_ASPMC | value,
+					   value);
 
 	return false;
 }
 
-/*When we set 0x01 to enable clk request. Set 0x0 to disable clk req.*/
-static void _rtl_pci_switch_clk_req(struct ieee80211_hw *hw, u8 value)
+/* @value is PCI_EXP_LNKCTL_CLKREQ_EN or 0 to enable/disable clk request. */
+static void _rtl_pci_switch_clk_req(struct ieee80211_hw *hw, u16 value)
 {
 	struct rtl_pci *rtlpci = rtl_pcidev(rtl_pcipriv(hw));
 	struct rtl_hal *rtlhal = rtl_hal(rtl_priv(hw));
 
-	pci_write_config_byte(rtlpci->pdev, 0x81, value);
+	value &= PCI_EXP_LNKCTL_CLKREQ_EN;
+
+	pcie_capability_clear_and_set_word(rtlpci->pdev, PCI_EXP_LNKCTL,
+					   PCI_EXP_LNKCTL_CLKREQ_EN,
+					   value);
 
 	if (rtlhal->hw_type == HARDWARE_TYPE_RTL8192SE)
 		udelay(100);
@@ -222,11 +230,8 @@ static void rtl_pci_disable_aspm(struct ieee80211_hw *hw)
 	struct rtl_ps_ctl *ppsc = rtl_psc(rtl_priv(hw));
 	struct rtl_pci *rtlpci = rtl_pcidev(rtl_pcipriv(hw));
 	u8 pcibridge_vendor = pcipriv->ndis_adapter.pcibridge_vendor;
-	u8 num4bytes = pcipriv->ndis_adapter.num4bytes;
 	/*Retrieve original configuration settings. */
 	u8 linkctrl_reg = pcipriv->ndis_adapter.linkctrl_reg;
-	u16 pcibridge_linkctrlreg = pcipriv->ndis_adapter.
-				pcibridge_linkctrlreg;
 	u16 aspmlevel = 0;
 	u8 tmp_u1b = 0;
 
@@ -251,16 +256,8 @@ static void rtl_pci_disable_aspm(struct ieee80211_hw *hw)
 	/*Set corresponding value. */
 	aspmlevel |= BIT(0) | BIT(1);
 	linkctrl_reg &= ~aspmlevel;
-	pcibridge_linkctrlreg &= ~(BIT(0) | BIT(1));
 
 	_rtl_pci_platform_switch_device_pci_aspm(hw, linkctrl_reg);
-	udelay(50);
-
-	/*4 Disable Pci Bridge ASPM */
-	pci_write_config_byte(rtlpci->pdev, (num4bytes << 2),
-			      pcibridge_linkctrlreg);
-
-	udelay(50);
 }
 
 /*
@@ -276,9 +273,7 @@ static void rtl_pci_enable_aspm(struct ieee80211_hw *hw)
 	struct rtl_ps_ctl *ppsc = rtl_psc(rtl_priv(hw));
 	struct rtl_pci *rtlpci = rtl_pcidev(rtl_pcipriv(hw));
 	u8 pcibridge_vendor = pcipriv->ndis_adapter.pcibridge_vendor;
-	u8 num4bytes = pcipriv->ndis_adapter.num4bytes;
 	u16 aspmlevel;
-	u8 u_pcibridge_aspmsetting;
 	u8 u_device_aspmsetting;
 
 	if (!ppsc->support_aspm)
@@ -290,25 +285,6 @@ static void rtl_pci_enable_aspm(struct ieee80211_hw *hw)
 		return;
 	}
 
-	/*4 Enable Pci Bridge ASPM */
-
-	u_pcibridge_aspmsetting =
-	    pcipriv->ndis_adapter.pcibridge_linkctrlreg |
-	    rtlpci->const_hostpci_aspm_setting;
-
-	if (pcibridge_vendor == PCI_BRIDGE_VENDOR_INTEL)
-		u_pcibridge_aspmsetting &= ~BIT(0);
-
-	pci_write_config_byte(rtlpci->pdev, (num4bytes << 2),
-			      u_pcibridge_aspmsetting);
-
-	RT_TRACE(rtlpriv, COMP_INIT, DBG_LOUD,
-		 "PlatformEnableASPM(): Write reg[%x] = %x\n",
-		 (pcipriv->ndis_adapter.pcibridge_pciehdr_offset + 0x10),
-		 u_pcibridge_aspmsetting);
-
-	udelay(50);
-
 	/*Get ASPM level (with/without Clock Req) */
 	aspmlevel = rtlpci->const_devicepci_aspm_setting;
 	u_device_aspmsetting = pcipriv->ndis_adapter.linkctrl_reg;
@@ -322,7 +298,8 @@ static void rtl_pci_enable_aspm(struct ieee80211_hw *hw)
 
 	if (ppsc->reg_rfps_level & RT_RF_OFF_LEVL_CLK_REQ) {
 		_rtl_pci_switch_clk_req(hw, (ppsc->reg_rfps_level &
-					     RT_RF_OFF_LEVL_CLK_REQ) ? 1 : 0);
+					     RT_RF_OFF_LEVL_CLK_REQ) ?
+					     PCI_EXP_LNKCTL_CLKREQ_EN : 0);
 		RT_SET_PS_LEVEL(ppsc, RT_RF_OFF_LEVL_CLK_REQ);
 	}
 	udelay(100);
@@ -390,22 +367,6 @@ static bool rtl_pci_check_buddy_priv(struct ieee80211_hw *hw,
 	return find_buddy_priv;
 }
 
-static void rtl_pci_get_linkcontrol_field(struct ieee80211_hw *hw)
-{
-	struct rtl_pci_priv *pcipriv = rtl_pcipriv(hw);
-	struct rtl_pci *rtlpci = rtl_pcidev(pcipriv);
-	u8 capabilityoffset = pcipriv->ndis_adapter.pcibridge_pciehdr_offset;
-	u8 linkctrl_reg;
-	u8 num4bbytes;
-
-	num4bbytes = (capabilityoffset + 0x10) / 4;
-
-	/*Read  Link Control Register */
-	pci_read_config_byte(rtlpci->pdev, (num4bbytes << 2), &linkctrl_reg);
-
-	pcipriv->ndis_adapter.pcibridge_linkctrlreg = linkctrl_reg;
-}
-
 static void rtl_pci_parse_configuration(struct pci_dev *pdev,
 		struct ieee80211_hw *hw)
 {
@@ -2076,12 +2037,6 @@ static bool _rtl_pci_find_adapter(struct pci_dev *pdev,
 		    PCI_SLOT(bridge_pdev->devfn);
 		pcipriv->ndis_adapter.pcibridge_funcnum =
 		    PCI_FUNC(bridge_pdev->devfn);
-		pcipriv->ndis_adapter.pcibridge_pciehdr_offset =
-		    pci_pcie_cap(bridge_pdev);
-		pcipriv->ndis_adapter.num4bytes =
-		    (pcipriv->ndis_adapter.pcibridge_pciehdr_offset + 0x10) / 4;
-
-		rtl_pci_get_linkcontrol_field(hw);
 
 		if (pcipriv->ndis_adapter.pcibridge_vendor ==
 		    PCI_BRIDGE_VENDOR_AMD) {
@@ -2098,13 +2053,11 @@ static bool _rtl_pci_find_adapter(struct pci_dev *pdev,
 		 pdev->vendor, pcipriv->ndis_adapter.linkctrl_reg);
 
 	RT_TRACE(rtlpriv, COMP_INIT, DBG_DMESG,
-		 "pci_bridge busnumber:devnumber:funcnumber:vendor:pcie_cap:link_ctl_reg:amd %d:%d:%d:%x:%x:%x:%x\n",
+		 "pci_bridge busnumber:devnumber:funcnumber:vendor:amd %d:%d:%d:%x:%x\n",
 		 pcipriv->ndis_adapter.pcibridge_busnum,
 		 pcipriv->ndis_adapter.pcibridge_devnum,
 		 pcipriv->ndis_adapter.pcibridge_funcnum,
 		 pcibridge_vendors[pcipriv->ndis_adapter.pcibridge_vendor],
-		 pcipriv->ndis_adapter.pcibridge_pciehdr_offset,
-		 pcipriv->ndis_adapter.pcibridge_linkctrlreg,
 		 pcipriv->ndis_adapter.amd_l1_patch);
 
 	rtl_pci_parse_configuration(pdev, hw);
diff --git drivers/net/wireless/realtek/rtlwifi/pci.h drivers/net/wireless/realtek/rtlwifi/pci.h
index d9039ea10ba4..19b7a57313da 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/pci.h
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/pci.h
@@ -262,11 +262,6 @@ struct mp_adapter {
 	u16 pcibridge_vendorid;
 	u16 pcibridge_deviceid;
 
-	u8 num4bytes;
-
-	u8 pcibridge_pciehdr_offset;
-	u8 pcibridge_linkctrlreg;
-
 	bool amd_l1_patch;
 };
 
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8188ee/phy.c drivers/net/wireless/realtek/rtlwifi/rtl8188ee/phy.c
index 14a256062614..44cabfa1ca27 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8188ee/phy.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8188ee/phy.c
@@ -38,7 +38,6 @@ static u32 _rtl88e_phy_rf_serial_read(struct ieee80211_hw *hw,
 static void _rtl88e_phy_rf_serial_write(struct ieee80211_hw *hw,
 					enum radio_path rfpath, u32 offset,
 					u32 data);
-static u32 _rtl88e_phy_calculate_bit_shift(u32 bitmask);
 static bool _rtl88e_phy_bb8188e_config_parafile(struct ieee80211_hw *hw);
 static bool _rtl88e_phy_config_mac_with_headerfile(struct ieee80211_hw *hw);
 static bool phy_config_bb_with_headerfile(struct ieee80211_hw *hw,
@@ -68,7 +67,7 @@ u32 rtl88e_phy_query_bb_reg(struct ieee80211_hw *hw, u32 regaddr, u32 bitmask)
 	RT_TRACE(rtlpriv, COMP_RF, DBG_TRACE,
 		 "regaddr(%#x), bitmask(%#x)\n", regaddr, bitmask);
 	originalvalue = rtl_read_dword(rtlpriv, regaddr);
-	bitshift = _rtl88e_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	returnvalue = (originalvalue & bitmask) >> bitshift;
 
 	RT_TRACE(rtlpriv, COMP_RF, DBG_TRACE,
@@ -91,7 +90,7 @@ void rtl88e_phy_set_bb_reg(struct ieee80211_hw *hw,
 
 	if (bitmask != MASKDWORD) {
 		originalvalue = rtl_read_dword(rtlpriv, regaddr);
-		bitshift = _rtl88e_phy_calculate_bit_shift(bitmask);
+		bitshift = calculate_bit_shift(bitmask);
 		data = ((originalvalue & (~bitmask)) | (data << bitshift));
 	}
 
@@ -117,7 +116,7 @@ u32 rtl88e_phy_query_rf_reg(struct ieee80211_hw *hw,
 
 
 	original_value = _rtl88e_phy_rf_serial_read(hw, rfpath, regaddr);
-	bitshift = _rtl88e_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	readback_value = (original_value & bitmask) >> bitshift;
 
 	spin_unlock_irqrestore(&rtlpriv->locks.rf_lock, flags);
@@ -146,7 +145,7 @@ void rtl88e_phy_set_rf_reg(struct ieee80211_hw *hw,
 			original_value = _rtl88e_phy_rf_serial_read(hw,
 								    rfpath,
 								    regaddr);
-			bitshift = _rtl88e_phy_calculate_bit_shift(bitmask);
+			bitshift = calculate_bit_shift(bitmask);
 			data =
 			    ((original_value & (~bitmask)) |
 			     (data << bitshift));
@@ -232,17 +231,6 @@ static void _rtl88e_phy_rf_serial_write(struct ieee80211_hw *hw,
 		 rfpath, pphyreg->rf3wire_offset, data_and_addr);
 }
 
-static u32 _rtl88e_phy_calculate_bit_shift(u32 bitmask)
-{
-	u32 i;
-
-	for (i = 0; i <= 31; i++) {
-		if (((bitmask >> i) & 0x1) == 1)
-			break;
-	}
-	return i;
-}
-
 bool rtl88e_phy_mac_config(struct ieee80211_hw *hw)
 {
 	struct rtl_priv *rtlpriv = rtl_priv(hw);
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8192c/phy_common.c drivers/net/wireless/realtek/rtlwifi/rtl8192c/phy_common.c
index 7c6e5d91439d..bc2b3849828d 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192c/phy_common.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192c/phy_common.c
@@ -39,7 +39,7 @@ u32 rtl92c_phy_query_bb_reg(struct ieee80211_hw *hw, u32 regaddr, u32 bitmask)
 	RT_TRACE(rtlpriv, COMP_RF, DBG_TRACE, "regaddr(%#x), bitmask(%#x)\n",
 		 regaddr, bitmask);
 	originalvalue = rtl_read_dword(rtlpriv, regaddr);
-	bitshift = _rtl92c_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	returnvalue = (originalvalue & bitmask) >> bitshift;
 
 	RT_TRACE(rtlpriv, COMP_RF, DBG_TRACE,
@@ -62,7 +62,7 @@ void rtl92c_phy_set_bb_reg(struct ieee80211_hw *hw,
 
 	if (bitmask != MASKDWORD) {
 		originalvalue = rtl_read_dword(rtlpriv, regaddr);
-		bitshift = _rtl92c_phy_calculate_bit_shift(bitmask);
+		bitshift = calculate_bit_shift(bitmask);
 		data = ((originalvalue & (~bitmask)) | (data << bitshift));
 	}
 
@@ -165,18 +165,6 @@ void _rtl92c_phy_rf_serial_write(struct ieee80211_hw *hw,
 }
 EXPORT_SYMBOL(_rtl92c_phy_rf_serial_write);
 
-u32 _rtl92c_phy_calculate_bit_shift(u32 bitmask)
-{
-	u32 i;
-
-	for (i = 0; i <= 31; i++) {
-		if (((bitmask >> i) & 0x1) == 1)
-			break;
-	}
-	return i;
-}
-EXPORT_SYMBOL(_rtl92c_phy_calculate_bit_shift);
-
 static void _rtl92c_phy_bb_config_1t(struct ieee80211_hw *hw)
 {
 	rtl_set_bbreg(hw, RFPGA0_TXINFO, 0x3, 0x2);
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8192c/phy_common.h drivers/net/wireless/realtek/rtlwifi/rtl8192c/phy_common.h
index d11261e05a2e..76f574047c62 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192c/phy_common.h
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192c/phy_common.h
@@ -218,7 +218,6 @@ bool rtl92c_phy_set_rf_power_state(struct ieee80211_hw *hw,
 void rtl92ce_phy_set_rf_on(struct ieee80211_hw *hw);
 void rtl92c_phy_set_io(struct ieee80211_hw *hw);
 void rtl92c_bb_block_on(struct ieee80211_hw *hw);
-u32 _rtl92c_phy_calculate_bit_shift(u32 bitmask);
 long _rtl92c_phy_txpwr_idx_to_dbm(struct ieee80211_hw *hw,
 				  enum wireless_mode wirelessmode,
 				  u8 txpwridx);
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8192ce/phy.c drivers/net/wireless/realtek/rtlwifi/rtl8192ce/phy.c
index 7c6d7fc1ef9a..9f478d8af804 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192ce/phy.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192ce/phy.c
@@ -61,7 +61,7 @@ u32 rtl92c_phy_query_rf_reg(struct ieee80211_hw *hw,
 							       rfpath, regaddr);
 	}
 
-	bitshift = _rtl92c_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	readback_value = (original_value & bitmask) >> bitshift;
 
 	spin_unlock(&rtlpriv->locks.rf_lock);
@@ -132,7 +132,7 @@ void rtl92ce_phy_set_rf_reg(struct ieee80211_hw *hw,
 			original_value = _rtl92c_phy_rf_serial_read(hw,
 								    rfpath,
 								    regaddr);
-			bitshift = _rtl92c_phy_calculate_bit_shift(bitmask);
+			bitshift = calculate_bit_shift(bitmask);
 			data =
 			    ((original_value & (~bitmask)) |
 			     (data << bitshift));
@@ -144,7 +144,7 @@ void rtl92ce_phy_set_rf_reg(struct ieee80211_hw *hw,
 			original_value = _rtl92c_phy_fw_rf_serial_read(hw,
 								       rfpath,
 								       regaddr);
-			bitshift = _rtl92c_phy_calculate_bit_shift(bitmask);
+			bitshift = calculate_bit_shift(bitmask);
 			data =
 			    ((original_value & (~bitmask)) |
 			     (data << bitshift));
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8192ce/phy.h drivers/net/wireless/realtek/rtlwifi/rtl8192ce/phy.h
index 93f3bc0197b4..e084a91e26d9 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192ce/phy.h
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192ce/phy.h
@@ -116,7 +116,6 @@ u32 _rtl92c_phy_rf_serial_read(struct ieee80211_hw *hw, enum radio_path rfpath,
 			       u32 offset);
 u32 _rtl92c_phy_fw_rf_serial_read(struct ieee80211_hw *hw,
 				  enum radio_path rfpath, u32 offset);
-u32 _rtl92c_phy_calculate_bit_shift(u32 bitmask);
 void _rtl92c_phy_rf_serial_write(struct ieee80211_hw *hw,
 				 enum radio_path rfpath, u32 offset, u32 data);
 void _rtl92c_phy_fw_rf_serial_write(struct ieee80211_hw *hw,
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8192cu/phy.c drivers/net/wireless/realtek/rtlwifi/rtl8192cu/phy.c
index f068dd5317a7..5a5476a2dc2f 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192cu/phy.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192cu/phy.c
@@ -54,7 +54,7 @@ u32 rtl92cu_phy_query_rf_reg(struct ieee80211_hw *hw,
 		original_value = _rtl92c_phy_fw_rf_serial_read(hw,
 							       rfpath, regaddr);
 	}
-	bitshift = _rtl92c_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	readback_value = (original_value & bitmask) >> bitshift;
 	RT_TRACE(rtlpriv, COMP_RF, DBG_TRACE,
 		 "regaddr(%#x), rfpath(%#x), bitmask(%#x), original_value(%#x)\n",
@@ -78,7 +78,7 @@ void rtl92cu_phy_set_rf_reg(struct ieee80211_hw *hw,
 			original_value = _rtl92c_phy_rf_serial_read(hw,
 								    rfpath,
 								    regaddr);
-			bitshift = _rtl92c_phy_calculate_bit_shift(bitmask);
+			bitshift = calculate_bit_shift(bitmask);
 			data =
 			    ((original_value & (~bitmask)) |
 			     (data << bitshift));
@@ -89,7 +89,7 @@ void rtl92cu_phy_set_rf_reg(struct ieee80211_hw *hw,
 			original_value = _rtl92c_phy_fw_rf_serial_read(hw,
 								       rfpath,
 								       regaddr);
-			bitshift = _rtl92c_phy_calculate_bit_shift(bitmask);
+			bitshift = calculate_bit_shift(bitmask);
 			data =
 			    ((original_value & (~bitmask)) |
 			     (data << bitshift));
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8192de/phy.c drivers/net/wireless/realtek/rtlwifi/rtl8192de/phy.c
index 53734250479c..2ee779614269 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192de/phy.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192de/phy.c
@@ -182,17 +182,14 @@ static u32 targetchnl_2g[TARGET_CHNL_NUM_2G] = {
 	25711, 25658, 25606, 25554, 25502, 25451, 25328
 };
 
-static u32 _rtl92d_phy_calculate_bit_shift(u32 bitmask)
-{
-	u32 i;
-
-	for (i = 0; i <= 31; i++) {
-		if (((bitmask >> i) & 0x1) == 1)
-			break;
-	}
-
-	return i;
-}
+static const u8 channel_all[59] = {
+	1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14,
+	36, 38, 40, 42, 44, 46, 48, 50, 52, 54, 56, 58,
+	60, 62, 64, 100, 102, 104, 106, 108, 110, 112,
+	114, 116, 118, 120, 122, 124, 126, 128,	130,
+	132, 134, 136, 138, 140, 149, 151, 153, 155,
+	157, 159, 161, 163, 165
+};
 
 u32 rtl92d_phy_query_bb_reg(struct ieee80211_hw *hw, u32 regaddr, u32 bitmask)
 {
@@ -216,7 +213,7 @@ u32 rtl92d_phy_query_bb_reg(struct ieee80211_hw *hw, u32 regaddr, u32 bitmask)
 	} else {
 		originalvalue = rtl_read_dword(rtlpriv, regaddr);
 	}
-	bitshift = _rtl92d_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	returnvalue = (originalvalue & bitmask) >> bitshift;
 	RT_TRACE(rtlpriv, COMP_RF, DBG_TRACE,
 		 "BBR MASK=0x%x Addr[0x%x]=0x%x\n",
@@ -248,7 +245,7 @@ void rtl92d_phy_set_bb_reg(struct ieee80211_hw *hw,
 					dbi_direct);
 		else
 			originalvalue = rtl_read_dword(rtlpriv, regaddr);
-		bitshift = _rtl92d_phy_calculate_bit_shift(bitmask);
+		bitshift = calculate_bit_shift(bitmask);
 		data = ((originalvalue & (~bitmask)) | (data << bitshift));
 	}
 	if (rtlhal->during_mac1init_radioa || rtlhal->during_mac0init_radiob)
@@ -336,7 +333,7 @@ u32 rtl92d_phy_query_rf_reg(struct ieee80211_hw *hw,
 		 regaddr, rfpath, bitmask);
 	spin_lock_irqsave(&rtlpriv->locks.rf_lock, flags);
 	original_value = _rtl92d_phy_rf_serial_read(hw, rfpath, regaddr);
-	bitshift = _rtl92d_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	readback_value = (original_value & bitmask) >> bitshift;
 	spin_unlock_irqrestore(&rtlpriv->locks.rf_lock, flags);
 	RT_TRACE(rtlpriv, COMP_RF, DBG_TRACE,
@@ -363,7 +360,7 @@ void rtl92d_phy_set_rf_reg(struct ieee80211_hw *hw, enum radio_path rfpath,
 		if (bitmask != RFREG_OFFSET_MASK) {
 			original_value = _rtl92d_phy_rf_serial_read(hw,
 				rfpath, regaddr);
-			bitshift = _rtl92d_phy_calculate_bit_shift(bitmask);
+			bitshift = calculate_bit_shift(bitmask);
 			data = ((original_value & (~bitmask)) |
 				(data << bitshift));
 		}
@@ -1383,14 +1380,6 @@ static void _rtl92d_phy_switch_rf_setting(struct ieee80211_hw *hw, u8 channel)
 
 u8 rtl92d_get_rightchnlplace_for_iqk(u8 chnl)
 {
-	u8 channel_all[59] = {
-		1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14,
-		36, 38, 40, 42, 44, 46, 48, 50, 52, 54, 56, 58,
-		60, 62, 64, 100, 102, 104, 106, 108, 110, 112,
-		114, 116, 118, 120, 122, 124, 126, 128,	130,
-		132, 134, 136, 138, 140, 149, 151, 153, 155,
-		157, 159, 161, 163, 165
-	};
 	u8 place = chnl;
 
 	if (chnl > 14) {
@@ -3245,37 +3234,28 @@ void rtl92d_phy_config_macphymode_info(struct ieee80211_hw *hw)
 u8 rtl92d_get_chnlgroup_fromarray(u8 chnl)
 {
 	u8 group;
-	u8 channel_info[59] = {
-		1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14,
-		36, 38, 40, 42, 44, 46, 48, 50, 52, 54, 56,
-		58, 60, 62, 64, 100, 102, 104, 106, 108,
-		110, 112, 114, 116, 118, 120, 122, 124,
-		126, 128, 130, 132, 134, 136, 138, 140,
-		149, 151, 153, 155, 157, 159, 161, 163,
-		165
-	};
 
-	if (channel_info[chnl] <= 3)
+	if (channel_all[chnl] <= 3)
 		group = 0;
-	else if (channel_info[chnl] <= 9)
+	else if (channel_all[chnl] <= 9)
 		group = 1;
-	else if (channel_info[chnl] <= 14)
+	else if (channel_all[chnl] <= 14)
 		group = 2;
-	else if (channel_info[chnl] <= 44)
+	else if (channel_all[chnl] <= 44)
 		group = 3;
-	else if (channel_info[chnl] <= 54)
+	else if (channel_all[chnl] <= 54)
 		group = 4;
-	else if (channel_info[chnl] <= 64)
+	else if (channel_all[chnl] <= 64)
 		group = 5;
-	else if (channel_info[chnl] <= 112)
+	else if (channel_all[chnl] <= 112)
 		group = 6;
-	else if (channel_info[chnl] <= 126)
+	else if (channel_all[chnl] <= 126)
 		group = 7;
-	else if (channel_info[chnl] <= 140)
+	else if (channel_all[chnl] <= 140)
 		group = 8;
-	else if (channel_info[chnl] <= 153)
+	else if (channel_all[chnl] <= 153)
 		group = 9;
-	else if (channel_info[chnl] <= 159)
+	else if (channel_all[chnl] <= 159)
 		group = 10;
 	else
 		group = 11;
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8192ee/phy.c drivers/net/wireless/realtek/rtlwifi/rtl8192ee/phy.c
index 8b072ee8e0d5..9a3e88d6a570 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192ee/phy.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192ee/phy.c
@@ -38,7 +38,6 @@ static u32 _rtl92ee_phy_rf_serial_read(struct ieee80211_hw *hw,
 static void _rtl92ee_phy_rf_serial_write(struct ieee80211_hw *hw,
 					 enum radio_path rfpath, u32 offset,
 					 u32 data);
-static u32 _rtl92ee_phy_calculate_bit_shift(u32 bitmask);
 static bool _rtl92ee_phy_bb8192ee_config_parafile(struct ieee80211_hw *hw);
 static bool _rtl92ee_phy_config_mac_with_headerfile(struct ieee80211_hw *hw);
 static bool phy_config_bb_with_hdr_file(struct ieee80211_hw *hw,
@@ -68,7 +67,7 @@ u32 rtl92ee_phy_query_bb_reg(struct ieee80211_hw *hw, u32 regaddr, u32 bitmask)
 	RT_TRACE(rtlpriv, COMP_RF, DBG_TRACE,
 		 "regaddr(%#x), bitmask(%#x)\n", regaddr, bitmask);
 	originalvalue = rtl_read_dword(rtlpriv, regaddr);
-	bitshift = _rtl92ee_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	returnvalue = (originalvalue & bitmask) >> bitshift;
 
 	RT_TRACE(rtlpriv, COMP_RF, DBG_TRACE,
@@ -90,7 +89,7 @@ void rtl92ee_phy_set_bb_reg(struct ieee80211_hw *hw, u32 regaddr,
 
 	if (bitmask != MASKDWORD) {
 		originalvalue = rtl_read_dword(rtlpriv, regaddr);
-		bitshift = _rtl92ee_phy_calculate_bit_shift(bitmask);
+		bitshift = calculate_bit_shift(bitmask);
 		data = ((originalvalue & (~bitmask)) | (data << bitshift));
 	}
 
@@ -115,7 +114,7 @@ u32 rtl92ee_phy_query_rf_reg(struct ieee80211_hw *hw,
 	spin_lock_irqsave(&rtlpriv->locks.rf_lock, flags);
 
 	original_value = _rtl92ee_phy_rf_serial_read(hw , rfpath, regaddr);
-	bitshift = _rtl92ee_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	readback_value = (original_value & bitmask) >> bitshift;
 
 	spin_unlock_irqrestore(&rtlpriv->locks.rf_lock, flags);
@@ -143,7 +142,7 @@ void rtl92ee_phy_set_rf_reg(struct ieee80211_hw *hw,
 
 	if (bitmask != RFREG_OFFSET_MASK) {
 		original_value = _rtl92ee_phy_rf_serial_read(hw, rfpath, addr);
-		bitshift = _rtl92ee_phy_calculate_bit_shift(bitmask);
+		bitshift = calculate_bit_shift(bitmask);
 		data = (original_value & (~bitmask)) | (data << bitshift);
 	}
 
@@ -226,17 +225,6 @@ static void _rtl92ee_phy_rf_serial_write(struct ieee80211_hw *hw,
 		 pphyreg->rf3wire_offset, data_and_addr);
 }
 
-static u32 _rtl92ee_phy_calculate_bit_shift(u32 bitmask)
-{
-	u32 i;
-
-	for (i = 0; i <= 31; i++) {
-		if (((bitmask >> i) & 0x1) == 1)
-			break;
-	}
-	return i;
-}
-
 bool rtl92ee_phy_mac_config(struct ieee80211_hw *hw)
 {
 	return _rtl92ee_phy_config_mac_with_headerfile(hw);
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8192se/phy.c drivers/net/wireless/realtek/rtlwifi/rtl8192se/phy.c
index 86cb853f7169..0430a3b823d6 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192se/phy.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8192se/phy.c
@@ -36,18 +36,6 @@
 #include "hw.h"
 #include "table.h"
 
-static u32 _rtl92s_phy_calculate_bit_shift(u32 bitmask)
-{
-	u32 i;
-
-	for (i = 0; i <= 31; i++) {
-		if (((bitmask >> i) & 0x1) == 1)
-			break;
-	}
-
-	return i;
-}
-
 u32 rtl92s_phy_query_bb_reg(struct ieee80211_hw *hw, u32 regaddr, u32 bitmask)
 {
 	struct rtl_priv *rtlpriv = rtl_priv(hw);
@@ -57,7 +45,7 @@ u32 rtl92s_phy_query_bb_reg(struct ieee80211_hw *hw, u32 regaddr, u32 bitmask)
 		 regaddr, bitmask);
 
 	originalvalue = rtl_read_dword(rtlpriv, regaddr);
-	bitshift = _rtl92s_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	returnvalue = (originalvalue & bitmask) >> bitshift;
 
 	RT_TRACE(rtlpriv, COMP_RF, DBG_TRACE, "BBR MASK=0x%x Addr[0x%x]=0x%x\n",
@@ -79,7 +67,7 @@ void rtl92s_phy_set_bb_reg(struct ieee80211_hw *hw, u32 regaddr, u32 bitmask,
 
 	if (bitmask != MASKDWORD) {
 		originalvalue = rtl_read_dword(rtlpriv, regaddr);
-		bitshift = _rtl92s_phy_calculate_bit_shift(bitmask);
+		bitshift = calculate_bit_shift(bitmask);
 		data = ((originalvalue & (~bitmask)) | (data << bitshift));
 	}
 
@@ -187,7 +175,7 @@ u32 rtl92s_phy_query_rf_reg(struct ieee80211_hw *hw, enum radio_path rfpath,
 
 	original_value = _rtl92s_phy_rf_serial_read(hw, rfpath, regaddr);
 
-	bitshift = _rtl92s_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	readback_value = (original_value & bitmask) >> bitshift;
 
 	spin_unlock(&rtlpriv->locks.rf_lock);
@@ -218,7 +206,7 @@ void rtl92s_phy_set_rf_reg(struct ieee80211_hw *hw, enum radio_path rfpath,
 	if (bitmask != RFREG_OFFSET_MASK) {
 		original_value = _rtl92s_phy_rf_serial_read(hw, rfpath,
 							    regaddr);
-		bitshift = _rtl92s_phy_calculate_bit_shift(bitmask);
+		bitshift = calculate_bit_shift(bitmask);
 		data = ((original_value & (~bitmask)) | (data << bitshift));
 	}
 
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8723ae/phy.c drivers/net/wireless/realtek/rtlwifi/rtl8723ae/phy.c
index 5cf29f5a4b54..e6ac496e898e 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8723ae/phy.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8723ae/phy.c
@@ -72,7 +72,7 @@ u32 rtl8723e_phy_query_rf_reg(struct ieee80211_hw *hw,
 							    rfpath, regaddr);
 	}
 
-	bitshift = rtl8723_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	readback_value = (original_value & bitmask) >> bitshift;
 
 	spin_unlock_irqrestore(&rtlpriv->locks.rf_lock, flags);
@@ -104,7 +104,7 @@ void rtl8723e_phy_set_rf_reg(struct ieee80211_hw *hw,
 			original_value = rtl8723_phy_rf_serial_read(hw,
 								    rfpath,
 								    regaddr);
-			bitshift = rtl8723_phy_calculate_bit_shift(bitmask);
+			bitshift = calculate_bit_shift(bitmask);
 			data =
 			    ((original_value & (~bitmask)) |
 			     (data << bitshift));
@@ -113,7 +113,7 @@ void rtl8723e_phy_set_rf_reg(struct ieee80211_hw *hw,
 		rtl8723_phy_rf_serial_write(hw, rfpath, regaddr, data);
 	} else {
 		if (bitmask != RFREG_OFFSET_MASK) {
-			bitshift = rtl8723_phy_calculate_bit_shift(bitmask);
+			bitshift = calculate_bit_shift(bitmask);
 			data =
 			    ((original_value & (~bitmask)) |
 			     (data << bitshift));
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8723be/phy.c drivers/net/wireless/realtek/rtlwifi/rtl8723be/phy.c
index 9606641519e7..f1b42f9d6cd1 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8723be/phy.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8723be/phy.c
@@ -63,7 +63,7 @@ u32 rtl8723be_phy_query_rf_reg(struct ieee80211_hw *hw, enum radio_path rfpath,
 	spin_lock_irqsave(&rtlpriv->locks.rf_lock, flags);
 
 	original_value = rtl8723_phy_rf_serial_read(hw, rfpath, regaddr);
-	bitshift = rtl8723_phy_calculate_bit_shift(bitmask);
+	bitshift = calculate_bit_shift(bitmask);
 	readback_value = (original_value & bitmask) >> bitshift;
 
 	spin_unlock_irqrestore(&rtlpriv->locks.rf_lock, flags);
@@ -91,7 +91,7 @@ void rtl8723be_phy_set_rf_reg(struct ieee80211_hw *hw, enum radio_path path,
 	if (bitmask != RFREG_OFFSET_MASK) {
 			original_value = rtl8723_phy_rf_serial_read(hw, path,
 								    regaddr);
-			bitshift = rtl8723_phy_calculate_bit_shift(bitmask);
+			bitshift = calculate_bit_shift(bitmask);
 			data = ((original_value & (~bitmask)) |
 				(data << bitshift));
 		}
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8723com/phy_common.c drivers/net/wireless/realtek/rtlwifi/rtl8723com/phy_common.c
index 43d24e1ee5e6..af9cd74e09d4 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8723com/phy_common.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8723com/phy_common.c
@@ -75,13 +75,9 @@ EXPORT_SYMBOL_GPL(rtl8723_phy_set_bb_reg);
 
 u32 rtl8723_phy_calculate_bit_shift(u32 bitmask)
 {
-	u32 i;
+	u32 i = ffs(bitmask);
 
-	for (i = 0; i <= 31; i++) {
-		if (((bitmask >> i) & 0x1) == 1)
-			break;
-	}
-	return i;
+	return i ? i - 1 : 32;
 }
 EXPORT_SYMBOL_GPL(rtl8723_phy_calculate_bit_shift);
 
diff --git drivers/net/wireless/realtek/rtlwifi/rtl8821ae/phy.c drivers/net/wireless/realtek/rtlwifi/rtl8821ae/phy.c
index 176deb2b5386..f96d823e7f14 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8821ae/phy.c
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/rtl8821ae/phy.c
@@ -49,7 +49,13 @@ static u32 _rtl8821ae_phy_rf_serial_read(struct ieee80211_hw *hw,
 static void _rtl8821ae_phy_rf_serial_write(struct ieee80211_hw *hw,
 					   enum radio_path rfpath, u32 offset,
 					   u32 data);
-static u32 _rtl8821ae_phy_calculate_bit_shift(u32 bitmask);
+static u32 _rtl8821ae_phy_calculate_bit_shift(u32 bitmask)
+{
+	if (WARN_ON_ONCE(!bitmask))
+		return 0;
+
+	return __ffs(bitmask);
+}
 static bool _rtl8821ae_phy_bb8821a_config_parafile(struct ieee80211_hw *hw);
 /*static bool _rtl8812ae_phy_config_mac_with_headerfile(struct ieee80211_hw *hw);*/
 static bool _rtl8821ae_phy_config_mac_with_headerfile(struct ieee80211_hw *hw);
@@ -296,17 +302,6 @@ static void _rtl8821ae_phy_rf_serial_write(struct ieee80211_hw *hw,
 		 rfpath, pphyreg->rf3wire_offset, data_and_addr);
 }
 
-static u32 _rtl8821ae_phy_calculate_bit_shift(u32 bitmask)
-{
-	u32 i;
-
-	for (i = 0; i <= 31; i++) {
-		if (((bitmask >> i) & 0x1) == 1)
-			break;
-	}
-	return i;
-}
-
 bool rtl8821ae_phy_mac_config(struct ieee80211_hw *hw)
 {
 	bool rtstatus = 0;
diff --git drivers/net/wireless/realtek/rtlwifi/wifi.h drivers/net/wireless/realtek/rtlwifi/wifi.h
index c73ce334ce6c..61f5b6fc1754 100644
--- linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/wifi.h
+++ linux-4.14.336/drivers/net/wireless/realtek/rtlwifi/wifi.h
@@ -3095,4 +3095,11 @@ static inline struct ieee80211_sta *rtl_find_sta(struct ieee80211_hw *hw,
 	return ieee80211_find_sta(mac->vif, mac_addr);
 }
 
+static inline u32 calculate_bit_shift(u32 bitmask)
+{
+	if (WARN_ON_ONCE(!bitmask))
+		return 0;
+
+	return __ffs(bitmask);
+}
 #endif
diff --git drivers/net/xen-netback/netback.c drivers/net/xen-netback/netback.c
index 47e7e9aab9cf..901ddea37da6 100644
--- linux-4.14.336/drivers/net/xen-netback/netback.c
+++ linux-4.14.336/drivers/net/xen-netback/netback.c
@@ -97,13 +97,12 @@ module_param_named(hash_cache_size, xenvif_hash_cache_size, uint, 0644);
 MODULE_PARM_DESC(hash_cache_size, "Number of flows in the hash cache");
 
 static void xenvif_idx_release(struct xenvif_queue *queue, u16 pending_idx,
-			       u8 status);
+			       s8 status);
 
 static void make_tx_response(struct xenvif_queue *queue,
-			     struct xen_netif_tx_request *txp,
+			     const struct xen_netif_tx_request *txp,
 			     unsigned int extra_count,
-			     s8       st);
-static void push_tx_responses(struct xenvif_queue *queue);
+			     s8 status);
 
 static void xenvif_idx_unmap(struct xenvif_queue *queue, u16 pending_idx);
 
@@ -201,13 +200,9 @@ static void xenvif_tx_err(struct xenvif_queue *queue,
 			  unsigned int extra_count, RING_IDX end)
 {
 	RING_IDX cons = queue->tx.req_cons;
-	unsigned long flags;
 
 	do {
-		spin_lock_irqsave(&queue->response_lock, flags);
 		make_tx_response(queue, txp, extra_count, XEN_NETIF_RSP_ERROR);
-		push_tx_responses(queue);
-		spin_unlock_irqrestore(&queue->response_lock, flags);
 		if (cons == end)
 			break;
 		RING_COPY_REQUEST(&queue->tx, cons++, txp);
@@ -456,12 +451,20 @@ static void xenvif_get_requests(struct xenvif_queue *queue,
 	}
 
 	for (shinfo->nr_frags = 0; nr_slots > 0 && shinfo->nr_frags < MAX_SKB_FRAGS;
-	     shinfo->nr_frags++, gop++, nr_slots--) {
+	     nr_slots--) {
+		if (unlikely(!txp->size)) {
+			make_tx_response(queue, txp, 0, XEN_NETIF_RSP_OKAY);
+			++txp;
+			continue;
+		}
+
 		index = pending_index(queue->pending_cons++);
 		pending_idx = queue->pending_ring[index];
 		xenvif_tx_create_map_op(queue, pending_idx, txp,
 				        txp == first ? extra_count : 0, gop);
 		frag_set_pending_idx(&frags[shinfo->nr_frags], pending_idx);
+		++shinfo->nr_frags;
+		++gop;
 
 		if (txp == first)
 			txp = txfrags;
@@ -474,20 +477,33 @@ static void xenvif_get_requests(struct xenvif_queue *queue,
 		shinfo = skb_shinfo(nskb);
 		frags = shinfo->frags;
 
-		for (shinfo->nr_frags = 0; shinfo->nr_frags < nr_slots;
-		     shinfo->nr_frags++, txp++, gop++) {
+		for (shinfo->nr_frags = 0; shinfo->nr_frags < nr_slots; ++txp) {
+			if (unlikely(!txp->size)) {
+				make_tx_response(queue, txp, 0,
+						 XEN_NETIF_RSP_OKAY);
+				continue;
+			}
+
 			index = pending_index(queue->pending_cons++);
 			pending_idx = queue->pending_ring[index];
 			xenvif_tx_create_map_op(queue, pending_idx, txp, 0,
 						gop);
 			frag_set_pending_idx(&frags[shinfo->nr_frags],
 					     pending_idx);
+			++shinfo->nr_frags;
+			++gop;
+		}
+
+		if (shinfo->nr_frags) {
+			skb_shinfo(skb)->frag_list = nskb;
+			nskb = NULL;
 		}
+	}
 
-		skb_shinfo(skb)->frag_list = nskb;
-	} else if (nskb) {
+	if (nskb) {
 		/* A frag_list skb was allocated but it is no longer needed
-		 * because enough slots were converted to copy ops above.
+		 * because enough slots were converted to copy ops above or some
+		 * were empty.
 		 */
 		kfree_skb(nskb);
 	}
@@ -960,7 +976,6 @@ static void xenvif_tx_build_gops(struct xenvif_queue *queue,
 					 (ret == 0) ?
 					 XEN_NETIF_RSP_OKAY :
 					 XEN_NETIF_RSP_ERROR);
-			push_tx_responses(queue);
 			continue;
 		}
 
@@ -972,7 +987,6 @@ static void xenvif_tx_build_gops(struct xenvif_queue *queue,
 
 			make_tx_response(queue, &txreq, extra_count,
 					 XEN_NETIF_RSP_OKAY);
-			push_tx_responses(queue);
 			continue;
 		}
 
@@ -1398,8 +1412,35 @@ int xenvif_tx_action(struct xenvif_queue *queue, int budget)
 	return work_done;
 }
 
+static void _make_tx_response(struct xenvif_queue *queue,
+			     const struct xen_netif_tx_request *txp,
+			     unsigned int extra_count,
+			     s8 status)
+{
+	RING_IDX i = queue->tx.rsp_prod_pvt;
+	struct xen_netif_tx_response *resp;
+
+	resp = RING_GET_RESPONSE(&queue->tx, i);
+	resp->id     = txp->id;
+	resp->status = status;
+
+	while (extra_count-- != 0)
+		RING_GET_RESPONSE(&queue->tx, ++i)->status = XEN_NETIF_RSP_NULL;
+
+	queue->tx.rsp_prod_pvt = ++i;
+}
+
+static void push_tx_responses(struct xenvif_queue *queue)
+{
+	int notify;
+
+	RING_PUSH_RESPONSES_AND_CHECK_NOTIFY(&queue->tx, notify);
+	if (notify)
+		notify_remote_via_irq(queue->tx_irq);
+}
+
 static void xenvif_idx_release(struct xenvif_queue *queue, u16 pending_idx,
-			       u8 status)
+			       s8 status)
 {
 	struct pending_tx_info *pending_tx_info;
 	pending_ring_idx_t index;
@@ -1409,8 +1450,8 @@ static void xenvif_idx_release(struct xenvif_queue *queue, u16 pending_idx,
 
 	spin_lock_irqsave(&queue->response_lock, flags);
 
-	make_tx_response(queue, &pending_tx_info->req,
-			 pending_tx_info->extra_count, status);
+	_make_tx_response(queue, &pending_tx_info->req,
+			  pending_tx_info->extra_count, status);
 
 	/* Release the pending index before pusing the Tx response so
 	 * its available before a new Tx request is pushed by the
@@ -1424,32 +1465,19 @@ static void xenvif_idx_release(struct xenvif_queue *queue, u16 pending_idx,
 	spin_unlock_irqrestore(&queue->response_lock, flags);
 }
 
-
 static void make_tx_response(struct xenvif_queue *queue,
-			     struct xen_netif_tx_request *txp,
+			     const struct xen_netif_tx_request *txp,
 			     unsigned int extra_count,
-			     s8       st)
+			     s8 status)
 {
-	RING_IDX i = queue->tx.rsp_prod_pvt;
-	struct xen_netif_tx_response *resp;
-
-	resp = RING_GET_RESPONSE(&queue->tx, i);
-	resp->id     = txp->id;
-	resp->status = st;
-
-	while (extra_count-- != 0)
-		RING_GET_RESPONSE(&queue->tx, ++i)->status = XEN_NETIF_RSP_NULL;
+	unsigned long flags;
 
-	queue->tx.rsp_prod_pvt = ++i;
-}
+	spin_lock_irqsave(&queue->response_lock, flags);
 
-static void push_tx_responses(struct xenvif_queue *queue)
-{
-	int notify;
+	_make_tx_response(queue, txp, extra_count, status);
+	push_tx_responses(queue);
 
-	RING_PUSH_RESPONSES_AND_CHECK_NOTIFY(&queue->tx, notify);
-	if (notify)
-		notify_remote_via_irq(queue->tx_irq);
+	spin_unlock_irqrestore(&queue->response_lock, flags);
 }
 
 static void xenvif_idx_unmap(struct xenvif_queue *queue, u16 pending_idx)
diff --git drivers/pci/host/pcie-mediatek.c drivers/pci/host/pcie-mediatek.c
index 60c3110b5151..6a47a6681f8d 100644
--- linux-4.14.336/drivers/pci/host/pcie-mediatek.c
+++ linux-4.14.336/drivers/pci/host/pcie-mediatek.c
@@ -628,6 +628,14 @@ static irqreturn_t mtk_pcie_intr_handler(int irq, void *data)
 		while ((status = readl(port->base + PCIE_INT_STATUS)) & MSI_STATUS) {
 			unsigned long imsi_status;
 
+			/*
+			 * The interrupt status can be cleared even if the
+			 * MSI status remains pending. As such, given the
+			 * edge-triggered interrupt type, its status should
+			 * be cleared before being dispatched to the
+			 * handler of the underlying device.
+			 */
+			writel(MSI_STATUS, port->base + PCIE_INT_STATUS);
 			while ((imsi_status = readl(port->base + PCIE_IMSI_STATUS))) {
 				for_each_set_bit(bit, &imsi_status, MTK_MSI_IRQS_NUM) {
 					/* Clear the MSI */
@@ -636,8 +644,6 @@ static irqreturn_t mtk_pcie_intr_handler(int irq, void *data)
 					generic_handle_irq(virq);
 				}
 			}
-			/* Clear MSI interrupt status */
-			writel(MSI_STATUS, port->base + PCIE_INT_STATUS);
 		}
 	}
 
diff --git drivers/pci/msi.c drivers/pci/msi.c
index bbddf492da9f..548045dda97c 100644
--- linux-4.14.336/drivers/pci/msi.c
+++ linux-4.14.336/drivers/pci/msi.c
@@ -1380,7 +1380,7 @@ irq_hw_number_t pci_msi_domain_calc_hwirq(struct pci_dev *dev,
 {
 	return (irq_hw_number_t)desc->msi_attrib.entry_nr |
 		PCI_DEVID(dev->bus->number, dev->devfn) << 11 |
-		(pci_domain_nr(dev->bus) & 0xFFFFFFFF) << 27;
+		((irq_hw_number_t)(pci_domain_nr(dev->bus) & 0xFFFFFFFF)) << 27;
 }
 
 static inline bool pci_msi_desc_is_multi_msi(struct msi_desc *desc)
diff --git drivers/pci/quirks.c drivers/pci/quirks.c
index e32147929cf3..ef9303547484 100644
--- linux-4.14.336/drivers/pci/quirks.c
+++ linux-4.14.336/drivers/pci/quirks.c
@@ -441,10 +441,13 @@ static void quirk_amd_dwc_class(struct pci_dev *pdev)
 {
 	u32 class = pdev->class;
 
-	/* Use "USB Device (not host controller)" class */
-	pdev->class = PCI_CLASS_SERIAL_USB_DEVICE;
-	dev_info(&pdev->dev, "PCI class overridden (%#08x -> %#08x) so dwc3 driver can claim this instead of xhci\n",
-		 class, pdev->class);
+	if (class != PCI_CLASS_SERIAL_USB_DEVICE) {
+		/* Use "USB Device (not host controller)" class */
+		pdev->class = PCI_CLASS_SERIAL_USB_DEVICE;
+		dev_info(&pdev->dev,
+			"PCI class overridden (%#08x -> %#08x) so dwc3 driver can claim this instead of xhci\n",
+			class, pdev->class);
+	}
 }
 DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_AMD, PCI_DEVICE_ID_AMD_NL_USB,
 		quirk_amd_dwc_class);
@@ -3450,6 +3453,19 @@ static void quirk_no_pm_reset(struct pci_dev *dev)
 DECLARE_PCI_FIXUP_CLASS_HEADER(PCI_VENDOR_ID_ATI, PCI_ANY_ID,
 			       PCI_CLASS_DISPLAY_VGA, 8, quirk_no_pm_reset);
 
+/*
+ * Spectrum-{1,2,3,4} devices report that a D3hot->D0 transition causes a reset
+ * (i.e., they advertise NoSoftRst-). However, this transition does not have
+ * any effect on the device: It continues to be operational and network ports
+ * remain up. Advertising this support makes it seem as if a PM reset is viable
+ * for these devices. Mark it as unavailable to skip it when testing reset
+ * methods.
+ */
+DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_MELLANOX, 0xcb84, quirk_no_pm_reset);
+DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_MELLANOX, 0xcf6c, quirk_no_pm_reset);
+DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_MELLANOX, 0xcf70, quirk_no_pm_reset);
+DECLARE_PCI_FIXUP_HEADER(PCI_VENDOR_ID_MELLANOX, 0xcf80, quirk_no_pm_reset);
+
 /*
  * Thunderbolt controllers with broken MSI hotplug signaling:
  * Entire 1st generation (Light Ridge, Eagle Ridge, Light Peak) and part
diff --git drivers/phy/ti/phy-omap-usb2.c drivers/phy/ti/phy-omap-usb2.c
index fe909fd8144f..ae94e1e66bcc 100644
--- linux-4.14.336/drivers/phy/ti/phy-omap-usb2.c
+++ linux-4.14.336/drivers/phy/ti/phy-omap-usb2.c
@@ -64,7 +64,7 @@ static int omap_usb_set_vbus(struct usb_otg *otg, bool enabled)
 {
 	struct omap_usb *phy = phy_to_omapusb(otg->usb_phy);
 
-	if (!phy->comparator)
+	if (!phy->comparator || !phy->comparator->set_vbus)
 		return -ENODEV;
 
 	return phy->comparator->set_vbus(phy->comparator, enabled);
@@ -74,7 +74,7 @@ static int omap_usb_start_srp(struct usb_otg *otg)
 {
 	struct omap_usb *phy = phy_to_omapusb(otg->usb_phy);
 
-	if (!phy->comparator)
+	if (!phy->comparator || !phy->comparator->start_srp)
 		return -ENODEV;
 
 	return phy->comparator->start_srp(phy->comparator);
diff --git drivers/pnp/pnpacpi/rsparser.c drivers/pnp/pnpacpi/rsparser.c
index 43d8ed577e70..d8cee80e8df8 100644
--- linux-4.14.336/drivers/pnp/pnpacpi/rsparser.c
+++ linux-4.14.336/drivers/pnp/pnpacpi/rsparser.c
@@ -160,13 +160,13 @@ static int vendor_resource_matches(struct pnp_dev *dev,
 static void pnpacpi_parse_allocated_vendor(struct pnp_dev *dev,
 				    struct acpi_resource_vendor_typed *vendor)
 {
-	if (vendor_resource_matches(dev, vendor, &hp_ccsr_uuid, 16)) {
-		u64 start, length;
+	struct { u64 start, length; } range;
 
-		memcpy(&start, vendor->byte_data, sizeof(start));
-		memcpy(&length, vendor->byte_data + 8, sizeof(length));
-
-		pnp_add_mem_resource(dev, start, start + length - 1, 0);
+	if (vendor_resource_matches(dev, vendor, &hp_ccsr_uuid,
+				    sizeof(range))) {
+		memcpy(&range, vendor->byte_data, sizeof(range));
+		pnp_add_mem_resource(dev, range.start, range.start +
+				     range.length - 1, 0);
 	}
 }
 
diff --git drivers/power/supply/bq27xxx_battery_i2c.c drivers/power/supply/bq27xxx_battery_i2c.c
index 426ce81333a5..3eb839405d3f 100644
--- linux-4.14.336/drivers/power/supply/bq27xxx_battery_i2c.c
+++ linux-4.14.336/drivers/power/supply/bq27xxx_battery_i2c.c
@@ -217,7 +217,9 @@ static int bq27xxx_battery_i2c_remove(struct i2c_client *client)
 {
 	struct bq27xxx_device_info *di = i2c_get_clientdata(client);
 
-	free_irq(client->irq, di);
+	if (client->irq)
+		free_irq(client->irq, di);
+
 	bq27xxx_battery_teardown(di);
 
 	mutex_lock(&battery_mutex);
diff --git drivers/regulator/pwm-regulator.c drivers/regulator/pwm-regulator.c
index a2fd140eff81..5faa5906ad69 100644
--- linux-4.14.336/drivers/regulator/pwm-regulator.c
+++ linux-4.14.336/drivers/regulator/pwm-regulator.c
@@ -164,6 +164,9 @@ static int pwm_regulator_get_voltage(struct regulator_dev *rdev)
 	pwm_get_state(drvdata->pwm, &pstate);
 
 	voltage = pwm_get_relative_duty_cycle(&pstate, duty_unit);
+	if (voltage < min(max_uV_duty, min_uV_duty) ||
+	    voltage > max(max_uV_duty, min_uV_duty))
+		return -ENOTRECOVERABLE;
 
 	/*
 	 * The dutycycle for min_uV might be greater than the one for max_uV.
diff --git drivers/reset/hisilicon/hi6220_reset.c drivers/reset/hisilicon/hi6220_reset.c
index d5e5229308f2..d77a7ad7e57a 100644
--- linux-4.14.336/drivers/reset/hisilicon/hi6220_reset.c
+++ linux-4.14.336/drivers/reset/hisilicon/hi6220_reset.c
@@ -107,7 +107,7 @@ static int hi6220_reset_probe(struct platform_device *pdev)
 	if (!data)
 		return -ENOMEM;
 
-	type = (enum hi6220_reset_ctrl_type)of_device_get_match_data(dev);
+	type = (uintptr_t)of_device_get_match_data(dev);
 
 	regmap = syscon_node_to_regmap(np);
 	if (IS_ERR(regmap)) {
diff --git drivers/rpmsg/virtio_rpmsg_bus.c drivers/rpmsg/virtio_rpmsg_bus.c
index 82b83002fcba..5aeb976fb4ee 100644
--- linux-4.14.336/drivers/rpmsg/virtio_rpmsg_bus.c
+++ linux-4.14.336/drivers/rpmsg/virtio_rpmsg_bus.c
@@ -389,6 +389,7 @@ static void virtio_rpmsg_release_device(struct device *dev)
 	struct rpmsg_device *rpdev = to_rpmsg_device(dev);
 	struct virtio_rpmsg_channel *vch = to_virtio_rpmsg_channel(rpdev);
 
+	kfree(rpdev->driver_override);
 	kfree(vch);
 }
 
diff --git drivers/s390/block/scm_blk.c drivers/s390/block/scm_blk.c
index 5c944ee76ec1..a37fd27258bd 100644
--- linux-4.14.336/drivers/s390/block/scm_blk.c
+++ linux-4.14.336/drivers/s390/block/scm_blk.c
@@ -17,6 +17,7 @@
 #include <linux/genhd.h>
 #include <linux/slab.h>
 #include <linux/list.h>
+#include <linux/io.h>
 #include <asm/eadm.h>
 #include "scm_blk.h"
 
@@ -130,7 +131,7 @@ static void scm_request_done(struct scm_request *scmrq)
 
 	for (i = 0; i < nr_requests_per_io && scmrq->request[i]; i++) {
 		msb = &scmrq->aob->msb[i];
-		aidaw = msb->data_addr;
+		aidaw = (u64)phys_to_virt(msb->data_addr);
 
 		if ((msb->flags & MSB_FLAG_IDA) && aidaw &&
 		    IS_ALIGNED(aidaw, PAGE_SIZE))
@@ -195,12 +196,12 @@ static int scm_request_prepare(struct scm_request *scmrq)
 	msb->scm_addr = scmdev->address + ((u64) blk_rq_pos(req) << 9);
 	msb->oc = (rq_data_dir(req) == READ) ? MSB_OC_READ : MSB_OC_WRITE;
 	msb->flags |= MSB_FLAG_IDA;
-	msb->data_addr = (u64) aidaw;
+	msb->data_addr = (u64)virt_to_phys(aidaw);
 
 	rq_for_each_segment(bv, req, iter) {
 		WARN_ON(bv.bv_offset);
 		msb->blk_count += bv.bv_len >> 12;
-		aidaw->data_addr = (u64) page_address(bv.bv_page);
+		aidaw->data_addr = virt_to_phys(page_address(bv.bv_page));
 		aidaw++;
 	}
 
diff --git drivers/s390/net/qeth_l3_main.c drivers/s390/net/qeth_l3_main.c
index 8bccfd686b73..7d9a64e2691a 100644
--- linux-4.14.336/drivers/s390/net/qeth_l3_main.c
+++ linux-4.14.336/drivers/s390/net/qeth_l3_main.c
@@ -364,9 +364,10 @@ static void qeth_l3_clear_ip_htable(struct qeth_card *card, int recover)
 		if (!recover) {
 			hash_del(&addr->hnode);
 			kfree(addr);
-			continue;
+		} else {
+			/* prepare for recovery */
+			addr->disp_flag = QETH_DISP_ADDR_ADD;
 		}
-		addr->disp_flag = QETH_DISP_ADDR_ADD;
 	}
 
 	spin_unlock_bh(&card->ip_lock);
@@ -404,11 +405,13 @@ static void qeth_l3_recover_ip(struct qeth_card *card)
 			} else
 				rc = qeth_l3_register_addr_entry(card, addr);
 
-			if (!rc) {
+			if (!rc || rc == -EADDRINUSE || rc == -ENETDOWN) {
+				/* keep it in the records */
 				addr->disp_flag = QETH_DISP_ADDR_DO_NOTHING;
 				if (addr->ref_counter < 1)
 					qeth_l3_delete_ip(card, addr);
 			} else {
+				/* bad address */
 				hash_del(&addr->hnode);
 				kfree(addr);
 			}
diff --git drivers/scsi/Kconfig drivers/scsi/Kconfig
index ba1bfb30a272..aeb73c170b3a 100644
--- linux-4.14.336/drivers/scsi/Kconfig
+++ linux-4.14.336/drivers/scsi/Kconfig
@@ -1394,7 +1394,7 @@ source "drivers/scsi/arm/Kconfig"
 
 config JAZZ_ESP
 	bool "MIPS JAZZ FAS216 SCSI support"
-	depends on MACH_JAZZ && SCSI
+	depends on MACH_JAZZ && SCSI=y
 	select SCSI_SPI_ATTRS
 	help
 	  This is the driver for the onboard SCSI host adapter of MIPS Magnum
diff --git drivers/scsi/fcoe/fcoe_ctlr.c drivers/scsi/fcoe/fcoe_ctlr.c
index 57826f7bb9f2..1c8fa41aa3ab 100644
--- linux-4.14.336/drivers/scsi/fcoe/fcoe_ctlr.c
+++ linux-4.14.336/drivers/scsi/fcoe/fcoe_ctlr.c
@@ -330,17 +330,16 @@ static void fcoe_ctlr_announce(struct fcoe_ctlr *fip)
 {
 	struct fcoe_fcf *sel;
 	struct fcoe_fcf *fcf;
-	unsigned long flags;
 
 	mutex_lock(&fip->ctlr_mutex);
-	spin_lock_irqsave(&fip->ctlr_lock, flags);
+	spin_lock_bh(&fip->ctlr_lock);
 
 	kfree_skb(fip->flogi_req);
 	fip->flogi_req = NULL;
 	list_for_each_entry(fcf, &fip->fcfs, list)
 		fcf->flogi_sent = 0;
 
-	spin_unlock_irqrestore(&fip->ctlr_lock, flags);
+	spin_unlock_bh(&fip->ctlr_lock);
 	sel = fip->sel_fcf;
 
 	if (sel && ether_addr_equal(sel->fcf_mac, fip->dest_addr))
@@ -710,7 +709,6 @@ int fcoe_ctlr_els_send(struct fcoe_ctlr *fip, struct fc_lport *lport,
 {
 	struct fc_frame *fp;
 	struct fc_frame_header *fh;
-	unsigned long flags;
 	u16 old_xid;
 	u8 op;
 	u8 mac[ETH_ALEN];
@@ -744,11 +742,11 @@ int fcoe_ctlr_els_send(struct fcoe_ctlr *fip, struct fc_lport *lport,
 		op = FIP_DT_FLOGI;
 		if (fip->mode == FIP_MODE_VN2VN)
 			break;
-		spin_lock_irqsave(&fip->ctlr_lock, flags);
+		spin_lock_bh(&fip->ctlr_lock);
 		kfree_skb(fip->flogi_req);
 		fip->flogi_req = skb;
 		fip->flogi_req_send = 1;
-		spin_unlock_irqrestore(&fip->ctlr_lock, flags);
+		spin_unlock_bh(&fip->ctlr_lock);
 		schedule_work(&fip->timer_work);
 		return -EINPROGRESS;
 	case ELS_FDISC:
@@ -1725,11 +1723,10 @@ static int fcoe_ctlr_flogi_send_locked(struct fcoe_ctlr *fip)
 static int fcoe_ctlr_flogi_retry(struct fcoe_ctlr *fip)
 {
 	struct fcoe_fcf *fcf;
-	unsigned long flags;
 	int error;
 
 	mutex_lock(&fip->ctlr_mutex);
-	spin_lock_irqsave(&fip->ctlr_lock, flags);
+	spin_lock_bh(&fip->ctlr_lock);
 	LIBFCOE_FIP_DBG(fip, "re-sending FLOGI - reselect\n");
 	fcf = fcoe_ctlr_select(fip);
 	if (!fcf || fcf->flogi_sent) {
@@ -1740,7 +1737,7 @@ static int fcoe_ctlr_flogi_retry(struct fcoe_ctlr *fip)
 		fcoe_ctlr_solicit(fip, NULL);
 		error = fcoe_ctlr_flogi_send_locked(fip);
 	}
-	spin_unlock_irqrestore(&fip->ctlr_lock, flags);
+	spin_unlock_bh(&fip->ctlr_lock);
 	mutex_unlock(&fip->ctlr_mutex);
 	return error;
 }
@@ -1757,9 +1754,8 @@ static int fcoe_ctlr_flogi_retry(struct fcoe_ctlr *fip)
 static void fcoe_ctlr_flogi_send(struct fcoe_ctlr *fip)
 {
 	struct fcoe_fcf *fcf;
-	unsigned long flags;
 
-	spin_lock_irqsave(&fip->ctlr_lock, flags);
+	spin_lock_bh(&fip->ctlr_lock);
 	fcf = fip->sel_fcf;
 	if (!fcf || !fip->flogi_req_send)
 		goto unlock;
@@ -1786,7 +1782,7 @@ static void fcoe_ctlr_flogi_send(struct fcoe_ctlr *fip)
 	} else /* XXX */
 		LIBFCOE_FIP_DBG(fip, "No FCF selected - defer send\n");
 unlock:
-	spin_unlock_irqrestore(&fip->ctlr_lock, flags);
+	spin_unlock_bh(&fip->ctlr_lock);
 }
 
 /**
diff --git drivers/scsi/isci/request.c drivers/scsi/isci/request.c
index 2f151708b59a..13ecf554762e 100644
--- linux-4.14.336/drivers/scsi/isci/request.c
+++ linux-4.14.336/drivers/scsi/isci/request.c
@@ -3398,7 +3398,7 @@ static enum sci_status isci_io_request_build(struct isci_host *ihost,
 		return SCI_FAILURE;
 	}
 
-	return SCI_SUCCESS;
+	return status;
 }
 
 static struct isci_request *isci_request_from_tag(struct isci_host *ihost, u16 tag)
diff --git drivers/scsi/libfc/fc_fcp.c drivers/scsi/libfc/fc_fcp.c
index 772c35a5c49e..72ceffc58112 100644
--- linux-4.14.336/drivers/scsi/libfc/fc_fcp.c
+++ linux-4.14.336/drivers/scsi/libfc/fc_fcp.c
@@ -283,6 +283,11 @@ static int fc_fcp_send_abort(struct fc_fcp_pkt *fsp)
 	if (!fsp->seq_ptr)
 		return -EINVAL;
 
+	if (fsp->state & FC_SRB_ABORT_PENDING) {
+		FC_FCP_DBG(fsp, "abort already pending\n");
+		return -EBUSY;
+	}
+
 	per_cpu_ptr(fsp->lp->stats, get_cpu())->FcpPktAborts++;
 	put_cpu();
 
@@ -1693,7 +1698,7 @@ static void fc_fcp_rec_error(struct fc_fcp_pkt *fsp, struct fc_frame *fp)
 		if (fsp->recov_retry++ < FC_MAX_RECOV_RETRY)
 			fc_fcp_rec(fsp);
 		else
-			fc_fcp_recovery(fsp, FC_ERROR);
+			fc_fcp_recovery(fsp, FC_TIMED_OUT);
 		break;
 	}
 	fc_fcp_unlock_pkt(fsp);
@@ -1711,11 +1716,12 @@ static void fc_fcp_recovery(struct fc_fcp_pkt *fsp, u8 code)
 	fsp->status_code = code;
 	fsp->cdb_status = 0;
 	fsp->io_status = 0;
-	/*
-	 * if this fails then we let the scsi command timer fire and
-	 * scsi-ml escalate.
-	 */
-	fc_fcp_send_abort(fsp);
+	if (!fsp->cmd)
+		/*
+		 * Only abort non-scsi commands; otherwise let the
+		 * scsi command timer fire and scsi-ml escalate.
+		 */
+		fc_fcp_send_abort(fsp);
 }
 
 /**
diff --git drivers/scsi/lpfc/lpfc.h drivers/scsi/lpfc/lpfc.h
index 5fc41aa53ceb..97a2f6c6337c 100644
--- linux-4.14.336/drivers/scsi/lpfc/lpfc.h
+++ linux-4.14.336/drivers/scsi/lpfc/lpfc.h
@@ -31,6 +31,7 @@
 struct lpfc_sli2_slim;
 
 #define ELX_MODEL_NAME_SIZE	80
+#define ELX_FW_NAME_SIZE	84
 
 #define LPFC_PCI_DEV_LP		0x1
 #define LPFC_PCI_DEV_OC		0x2
diff --git drivers/scsi/lpfc/lpfc_init.c drivers/scsi/lpfc/lpfc_init.c
index 3e9574eede20..0f954853ccad 100644
--- linux-4.14.336/drivers/scsi/lpfc/lpfc_init.c
+++ linux-4.14.336/drivers/scsi/lpfc/lpfc_init.c
@@ -11086,7 +11086,7 @@ out:
 int
 lpfc_sli4_request_firmware_update(struct lpfc_hba *phba, uint8_t fw_upgrade)
 {
-	uint8_t file_name[ELX_MODEL_NAME_SIZE];
+	char file_name[ELX_FW_NAME_SIZE] = {0};
 	int ret;
 	const struct firmware *fw;
 
@@ -11095,7 +11095,7 @@ lpfc_sli4_request_firmware_update(struct lpfc_hba *phba, uint8_t fw_upgrade)
 	    LPFC_SLI_INTF_IF_TYPE_2)
 		return -EPERM;
 
-	snprintf(file_name, ELX_MODEL_NAME_SIZE, "%s.grp", phba->ModelName);
+	scnprintf(file_name, sizeof(file_name), "%s.grp", phba->ModelName);
 
 	if (fw_upgrade == INT_FW_UPGRADE) {
 		ret = request_firmware_nowait(THIS_MODULE, FW_ACTION_HOTPLUG,
diff --git drivers/spi/spi-ppc4xx.c drivers/spi/spi-ppc4xx.c
index 967d94844b30..58765a62fc15 100644
--- linux-4.14.336/drivers/spi/spi-ppc4xx.c
+++ linux-4.14.336/drivers/spi/spi-ppc4xx.c
@@ -173,10 +173,8 @@ static int spi_ppc4xx_setupxfer(struct spi_device *spi, struct spi_transfer *t)
 	int scr;
 	u8 cdm = 0;
 	u32 speed;
-	u8 bits_per_word;
 
 	/* Start with the generic configuration for this device. */
-	bits_per_word = spi->bits_per_word;
 	speed = spi->max_speed_hz;
 
 	/*
@@ -184,9 +182,6 @@ static int spi_ppc4xx_setupxfer(struct spi_device *spi, struct spi_transfer *t)
 	 * the transfer to overwrite the generic configuration with zeros.
 	 */
 	if (t) {
-		if (t->bits_per_word)
-			bits_per_word = t->bits_per_word;
-
 		if (t->speed_hz)
 			speed = min(t->speed_hz, spi->max_speed_hz);
 	}
diff --git drivers/staging/iio/impedance-analyzer/ad5933.c drivers/staging/iio/impedance-analyzer/ad5933.c
index 6d31001d1825..344053df0383 100644
--- linux-4.14.336/drivers/staging/iio/impedance-analyzer/ad5933.c
+++ linux-4.14.336/drivers/staging/iio/impedance-analyzer/ad5933.c
@@ -658,7 +658,7 @@ static void ad5933_work(struct work_struct *work)
 		struct ad5933_state, work.work);
 	struct iio_dev *indio_dev = i2c_get_clientdata(st->client);
 	__be16 buf[2];
-	int val[2];
+	u16 val[2];
 	unsigned char status;
 	int ret;
 
diff --git drivers/target/target_core_device.c drivers/target/target_core_device.c
index 907b06056f02..ccefa4eb9f1f 100644
--- linux-4.14.336/drivers/target/target_core_device.c
+++ linux-4.14.336/drivers/target/target_core_device.c
@@ -164,7 +164,6 @@ int transport_lookup_tmr_lun(struct se_cmd *se_cmd, u64 unpacked_lun)
 	struct se_session *se_sess = se_cmd->se_sess;
 	struct se_node_acl *nacl = se_sess->se_node_acl;
 	struct se_tmr_req *se_tmr = se_cmd->se_tmr_req;
-	unsigned long flags;
 
 	rcu_read_lock();
 	deve = target_nacl_find_deve(nacl, unpacked_lun);
@@ -195,10 +194,6 @@ out_unlock:
 	se_cmd->se_dev = rcu_dereference_raw(se_lun->lun_se_dev);
 	se_tmr->tmr_dev = rcu_dereference_raw(se_lun->lun_se_dev);
 
-	spin_lock_irqsave(&se_tmr->tmr_dev->se_tmr_lock, flags);
-	list_add_tail(&se_tmr->tmr_list, &se_tmr->tmr_dev->dev_tmr_list);
-	spin_unlock_irqrestore(&se_tmr->tmr_dev->se_tmr_lock, flags);
-
 	return 0;
 }
 EXPORT_SYMBOL(transport_lookup_tmr_lun);
diff --git drivers/target/target_core_transport.c drivers/target/target_core_transport.c
index c20997bf314e..41ebdd629b9d 100644
--- linux-4.14.336/drivers/target/target_core_transport.c
+++ linux-4.14.336/drivers/target/target_core_transport.c
@@ -3424,6 +3424,10 @@ int transport_generic_handle_tmr(
 	unsigned long flags;
 	bool aborted = false;
 
+	spin_lock_irqsave(&cmd->se_dev->se_tmr_lock, flags);
+	list_add_tail(&cmd->se_tmr_req->tmr_list, &cmd->se_dev->dev_tmr_list);
+	spin_unlock_irqrestore(&cmd->se_dev->se_tmr_lock, flags);
+
 	spin_lock_irqsave(&cmd->t_state_lock, flags);
 	if (cmd->transport_state & CMD_T_ABORTED) {
 		aborted = true;
diff --git drivers/tty/serial/imx.c drivers/tty/serial/imx.c
index 7fccf69931c5..6cfa6a908336 100644
--- linux-4.14.336/drivers/tty/serial/imx.c
+++ linux-4.14.336/drivers/tty/serial/imx.c
@@ -2215,7 +2215,7 @@ static int serial_imx_probe(struct platform_device *pdev)
 	/* For register access, we only need to enable the ipg clock. */
 	ret = clk_prepare_enable(sport->clk_ipg);
 	if (ret) {
-		dev_err(&pdev->dev, "failed to enable per clk: %d\n", ret);
+		dev_err(&pdev->dev, "failed to enable ipg clk: %d\n", ret);
 		return ret;
 	}
 
diff --git drivers/tty/serial/sc16is7xx.c drivers/tty/serial/sc16is7xx.c
index 73280d400eb2..3afaab69f0e2 100644
--- linux-4.14.336/drivers/tty/serial/sc16is7xx.c
+++ linux-4.14.336/drivers/tty/serial/sc16is7xx.c
@@ -29,6 +29,7 @@
 #include <linux/tty_flip.h>
 #include <linux/spi/spi.h>
 #include <linux/uaccess.h>
+#include <linux/units.h>
 #include <uapi/linux/sched/types.h>
 
 #define SC16IS7XX_NAME			"sc16is7xx"
@@ -1401,9 +1402,12 @@ static int sc16is7xx_spi_probe(struct spi_device *spi)
 
 	/* Setup SPI bus */
 	spi->bits_per_word	= 8;
-	/* only supports mode 0 on SC16IS762 */
+	/* For all variants, only mode 0 is supported */
+	if ((spi->mode & SPI_MODE_X_MASK) != SPI_MODE_0)
+		return dev_err_probe(&spi->dev, -EINVAL, "Unsupported SPI mode\n");
+
 	spi->mode		= spi->mode ? : SPI_MODE_0;
-	spi->max_speed_hz	= spi->max_speed_hz ? : 15000000;
+	spi->max_speed_hz	= spi->max_speed_hz ? : 4 * HZ_PER_MHZ;
 	ret = spi_setup(spi);
 	if (ret)
 		return ret;
diff --git drivers/uio/uio.c drivers/uio/uio.c
index be33a5ce3d8e..3ebea6388220 100644
--- linux-4.14.336/drivers/uio/uio.c
+++ linux-4.14.336/drivers/uio/uio.c
@@ -465,13 +465,13 @@ static int uio_open(struct inode *inode, struct file *filep)
 
 	mutex_lock(&minor_lock);
 	idev = idr_find(&uio_idr, iminor(inode));
-	mutex_unlock(&minor_lock);
 	if (!idev) {
 		ret = -ENODEV;
+		mutex_unlock(&minor_lock);
 		goto out;
 	}
-
 	get_device(&idev->dev);
+	mutex_unlock(&minor_lock);
 
 	if (!try_module_get(idev->owner)) {
 		ret = -ENODEV;
@@ -1020,9 +1020,8 @@ void uio_unregister_device(struct uio_info *info)
 	idev->info = NULL;
 	mutex_unlock(&idev->info_lock);
 
-	device_unregister(&idev->dev);
-
 	uio_free_minor(minor);
+	device_unregister(&idev->dev);
 
 	return;
 }
diff --git drivers/usb/chipidea/core.c drivers/usb/chipidea/core.c
index 4cacb91c4729..a4880b137f1b 100644
--- linux-4.14.336/drivers/usb/chipidea/core.c
+++ linux-4.14.336/drivers/usb/chipidea/core.c
@@ -542,6 +542,13 @@ static irqreturn_t ci_irq_handler(int irq, void *data)
 	u32 otgsc = 0;
 
 	if (ci->in_lpm) {
+		/*
+		 * If we already have a wakeup irq pending there,
+		 * let's just return to wait resume finished firstly.
+		 */
+		if (ci->wakeup_int)
+			return IRQ_HANDLED;
+
 		disable_irq_nosync(irq);
 		ci->wakeup_int = true;
 		pm_runtime_get(ci->dev);
diff --git drivers/usb/core/hub.c drivers/usb/core/hub.c
index 4a0765bca8e7..afe3a46a0d2d 100644
--- linux-4.14.336/drivers/usb/core/hub.c
+++ linux-4.14.336/drivers/usb/core/hub.c
@@ -43,8 +43,8 @@
 #define USB_VENDOR_TEXAS_INSTRUMENTS		0x0451
 #define USB_PRODUCT_TUSB8041_USB3		0x8140
 #define USB_PRODUCT_TUSB8041_USB2		0x8142
-#define HUB_QUIRK_CHECK_PORT_AUTOSUSPEND	0x01
-#define HUB_QUIRK_DISABLE_AUTOSUSPEND		0x02
+#define HUB_QUIRK_CHECK_PORT_AUTOSUSPEND	BIT(0)
+#define HUB_QUIRK_DISABLE_AUTOSUSPEND		BIT(1)
 
 /* Protect struct usb_device->state and ->children members
  * Note: Both are also protected by ->dev.sem, except that ->state can
@@ -2308,17 +2308,25 @@ static int usb_enumerate_device_otg(struct usb_device *udev)
 			}
 		} else if (desc->bLength == sizeof
 				(struct usb_otg_descriptor)) {
-			/* Set a_alt_hnp_support for legacy otg device */
-			err = usb_control_msg(udev,
-				usb_sndctrlpipe(udev, 0),
-				USB_REQ_SET_FEATURE, 0,
-				USB_DEVICE_A_ALT_HNP_SUPPORT,
-				0, NULL, 0,
-				USB_CTRL_SET_TIMEOUT);
-			if (err < 0)
-				dev_err(&udev->dev,
-					"set a_alt_hnp_support failed: %d\n",
-					err);
+			/*
+			 * We are operating on a legacy OTP device
+			 * These should be told that they are operating
+			 * on the wrong port if we have another port that does
+			 * support HNP
+			 */
+			if (bus->otg_port != 0) {
+				/* Set a_alt_hnp_support for legacy otg device */
+				err = usb_control_msg(udev,
+					usb_sndctrlpipe(udev, 0),
+					USB_REQ_SET_FEATURE, 0,
+					USB_DEVICE_A_ALT_HNP_SUPPORT,
+					0, NULL, 0,
+					USB_CTRL_SET_TIMEOUT);
+				if (err < 0)
+					dev_err(&udev->dev,
+						"set a_alt_hnp_support failed: %d\n",
+						err);
+			}
 		}
 	}
 #endif
diff --git drivers/usb/dwc3/ep0.c drivers/usb/dwc3/ep0.c
index 17bc5b958ea0..f3f9fca246b8 100644
--- linux-4.14.336/drivers/usb/dwc3/ep0.c
+++ linux-4.14.336/drivers/usb/dwc3/ep0.c
@@ -246,7 +246,10 @@ static void dwc3_ep0_stall_and_restart(struct dwc3 *dwc)
 		struct dwc3_request	*req;
 
 		req = next_request(&dep->pending_list);
-		dwc3_gadget_giveback(dep, req, -ECONNRESET);
+		if (!dwc->connected)
+			dwc3_gadget_giveback(dep, req, -ESHUTDOWN);
+		else
+			dwc3_gadget_giveback(dep, req, -ECONNRESET);
 	}
 
 	dwc->ep0state = EP0_SETUP_PHASE;
diff --git drivers/usb/gadget/function/f_mass_storage.c drivers/usb/gadget/function/f_mass_storage.c
index 6aee3cf50c74..43bceee1d6c7 100644
--- linux-4.14.336/drivers/usb/gadget/function/f_mass_storage.c
+++ linux-4.14.336/drivers/usb/gadget/function/f_mass_storage.c
@@ -576,21 +576,37 @@ static int start_transfer(struct fsg_dev *fsg, struct usb_ep *ep,
 
 static bool start_in_transfer(struct fsg_common *common, struct fsg_buffhd *bh)
 {
+	int rc;
+
 	if (!fsg_is_set(common))
 		return false;
 	bh->state = BUF_STATE_SENDING;
-	if (start_transfer(common->fsg, common->fsg->bulk_in, bh->inreq))
+	rc = start_transfer(common->fsg, common->fsg->bulk_in, bh->inreq);
+	if (rc) {
 		bh->state = BUF_STATE_EMPTY;
+		if (rc == -ESHUTDOWN) {
+			common->running = 0;
+			return false;
+		}
+	}
 	return true;
 }
 
 static bool start_out_transfer(struct fsg_common *common, struct fsg_buffhd *bh)
 {
+	int rc;
+
 	if (!fsg_is_set(common))
 		return false;
 	bh->state = BUF_STATE_RECEIVING;
-	if (start_transfer(common->fsg, common->fsg->bulk_out, bh->outreq))
+	rc = start_transfer(common->fsg, common->fsg->bulk_out, bh->outreq);
+	if (rc) {
 		bh->state = BUF_STATE_FULL;
+		if (rc == -ESHUTDOWN) {
+			common->running = 0;
+			return false;
+		}
+	}
 	return true;
 }
 
diff --git drivers/usb/gadget/function/f_ncm.c drivers/usb/gadget/function/f_ncm.c
index 47d1f4e960cb..9a75e4c49976 100644
--- linux-4.14.336/drivers/usb/gadget/function/f_ncm.c
+++ linux-4.14.336/drivers/usb/gadget/function/f_ncm.c
@@ -1370,7 +1370,15 @@ parse_ntb:
 	     "Parsed NTB with %d frames\n", dgram_counter);
 
 	to_process -= block_len;
-	if (to_process != 0) {
+
+	/*
+	 * Windows NCM driver avoids USB ZLPs by adding a 1-byte
+	 * zero pad as needed.
+	 */
+	if (to_process == 1 &&
+	    (*(unsigned char *)(ntb_ptr + block_len) == 0x00)) {
+		to_process--;
+	} else if (to_process > 0) {
 		ntb_ptr = (unsigned char *)(ntb_ptr + block_len);
 		goto parse_ntb;
 	}
diff --git drivers/usb/mon/mon_bin.c drivers/usb/mon/mon_bin.c
index a6da9b72f46b..21b184d2170a 100644
--- linux-4.14.336/drivers/usb/mon/mon_bin.c
+++ linux-4.14.336/drivers/usb/mon/mon_bin.c
@@ -1246,14 +1246,19 @@ static int mon_bin_vma_fault(struct vm_fault *vmf)
 	struct mon_reader_bin *rp = vmf->vma->vm_private_data;
 	unsigned long offset, chunk_idx;
 	struct page *pageptr;
+	unsigned long flags;
 
+	spin_lock_irqsave(&rp->b_lock, flags);
 	offset = vmf->pgoff << PAGE_SHIFT;
-	if (offset >= rp->b_size)
+	if (offset >= rp->b_size) {
+		spin_unlock_irqrestore(&rp->b_lock, flags);
 		return VM_FAULT_SIGBUS;
+	}
 	chunk_idx = offset / CHUNK_SIZE;
 	pageptr = rp->b_vec[chunk_idx].pg;
 	get_page(pageptr);
 	vmf->page = pageptr;
+	spin_unlock_irqrestore(&rp->b_lock, flags);
 	return 0;
 }
 
diff --git drivers/usb/phy/phy-mxs-usb.c drivers/usb/phy/phy-mxs-usb.c
index 6e462a8d8309..bbfdd926bc70 100644
--- linux-4.14.336/drivers/usb/phy/phy-mxs-usb.c
+++ linux-4.14.336/drivers/usb/phy/phy-mxs-usb.c
@@ -303,8 +303,7 @@ static void __mxs_phy_disconnect_line(struct mxs_phy *mxs_phy, bool disconnect)
 
 static bool mxs_phy_is_otg_host(struct mxs_phy *mxs_phy)
 {
-	return IS_ENABLED(CONFIG_USB_OTG) &&
-		mxs_phy->phy.last_event == USB_EVENT_ID;
+	return mxs_phy->phy.last_event == USB_EVENT_ID;
 }
 
 static void mxs_phy_disconnect_line(struct mxs_phy *mxs_phy, bool on)
diff --git drivers/usb/serial/cp210x.c drivers/usb/serial/cp210x.c
index df524ce8c050..4158432fc16f 100644
--- linux-4.14.336/drivers/usb/serial/cp210x.c
+++ linux-4.14.336/drivers/usb/serial/cp210x.c
@@ -150,6 +150,7 @@ static const struct usb_device_id id_table[] = {
 	{ USB_DEVICE(0x10C4, 0x85F8) }, /* Virtenio Preon32 */
 	{ USB_DEVICE(0x10C4, 0x8664) }, /* AC-Services CAN-IF */
 	{ USB_DEVICE(0x10C4, 0x8665) }, /* AC-Services OBD-IF */
+	{ USB_DEVICE(0x10C4, 0x87ED) }, /* IMST USB-Stick for Smart Meter */
 	{ USB_DEVICE(0x10C4, 0x8856) },	/* CEL EM357 ZigBee USB Stick - LR */
 	{ USB_DEVICE(0x10C4, 0x8857) },	/* CEL EM357 ZigBee USB Stick */
 	{ USB_DEVICE(0x10C4, 0x88A4) }, /* MMB Networks ZigBee USB Device */
diff --git drivers/usb/serial/option.c drivers/usb/serial/option.c
index 902bbe52a1d6..8744d91de155 100644
--- linux-4.14.336/drivers/usb/serial/option.c
+++ linux-4.14.336/drivers/usb/serial/option.c
@@ -2271,6 +2271,7 @@ static const struct usb_device_id option_ids[] = {
 	{ USB_DEVICE_INTERFACE_CLASS(0x2cb7, 0x0111, 0xff) },			/* Fibocom FM160 (MBIM mode) */
 	{ USB_DEVICE_INTERFACE_CLASS(0x2cb7, 0x01a0, 0xff) },			/* Fibocom NL668-AM/NL652-EU (laptop MBIM) */
 	{ USB_DEVICE_INTERFACE_CLASS(0x2cb7, 0x01a2, 0xff) },			/* Fibocom FM101-GL (laptop MBIM) */
+	{ USB_DEVICE_INTERFACE_CLASS(0x2cb7, 0x01a3, 0xff) },			/* Fibocom FM101-GL (laptop MBIM) */
 	{ USB_DEVICE_INTERFACE_CLASS(0x2cb7, 0x01a4, 0xff),			/* Fibocom FM101-GL (laptop MBIM) */
 	  .driver_info = RSVD(4) },
 	{ USB_DEVICE_INTERFACE_CLASS(0x2df3, 0x9d03, 0xff) },			/* LongSung M5710 */
diff --git drivers/usb/serial/qcserial.c drivers/usb/serial/qcserial.c
index 6ea6cbbebfba..03dc86977e6d 100644
--- linux-4.14.336/drivers/usb/serial/qcserial.c
+++ linux-4.14.336/drivers/usb/serial/qcserial.c
@@ -188,6 +188,8 @@ static const struct usb_device_id id_table[] = {
 	{DEVICE_SWI(0x413c, 0x81d0)},   /* Dell Wireless 5819 */
 	{DEVICE_SWI(0x413c, 0x81d1)},   /* Dell Wireless 5818 */
 	{DEVICE_SWI(0x413c, 0x81d2)},   /* Dell Wireless 5818 */
+	{DEVICE_SWI(0x413c, 0x8217)},	/* Dell Wireless DW5826e */
+	{DEVICE_SWI(0x413c, 0x8218)},	/* Dell Wireless DW5826e QDL */
 
 	/* Huawei devices */
 	{DEVICE_HWI(0x03f0, 0x581d)},	/* HP lt4112 LTE/HSPA+ Gobi 4G Modem (Huawei me906e) */
diff --git drivers/vhost/vhost.c drivers/vhost/vhost.c
index 93cdeb516594..03eb2941ff6c 100644
--- linux-4.14.336/drivers/vhost/vhost.c
+++ linux-4.14.336/drivers/vhost/vhost.c
@@ -2483,12 +2483,11 @@ EXPORT_SYMBOL_GPL(vhost_disable_notify);
 /* Create a new message. */
 struct vhost_msg_node *vhost_new_msg(struct vhost_virtqueue *vq, int type)
 {
-	struct vhost_msg_node *node = kmalloc(sizeof *node, GFP_KERNEL);
+	/* Make sure all padding within the structure is initialized. */
+	struct vhost_msg_node *node = kzalloc(sizeof(*node), GFP_KERNEL);
 	if (!node)
 		return NULL;
 
-	/* Make sure all padding within the structure is initialized. */
-	memset(&node->msg, 0, sizeof node->msg);
 	node->vq = vq;
 	node->msg.type = type;
 	return node;
diff --git drivers/video/fbdev/core/fb_defio.c drivers/video/fbdev/core/fb_defio.c
index 487d5e336e1b..36972138340d 100644
--- linux-4.14.336/drivers/video/fbdev/core/fb_defio.c
+++ linux-4.14.336/drivers/video/fbdev/core/fb_defio.c
@@ -78,11 +78,7 @@ int fb_deferred_io_fsync(struct file *file, loff_t start, loff_t end, int datasy
 		return 0;
 
 	inode_lock(inode);
-	/* Kill off the delayed work */
-	cancel_delayed_work_sync(&info->deferred_work);
-
-	/* Run it immediately */
-	schedule_delayed_work(&info->deferred_work, 0);
+	flush_delayed_work(&info->deferred_work);
 	inode_unlock(inode);
 
 	return 0;
diff --git drivers/video/fbdev/savage/savagefb_driver.c drivers/video/fbdev/savage/savagefb_driver.c
index c20468362f11..a4f15b9de2b6 100644
--- linux-4.14.336/drivers/video/fbdev/savage/savagefb_driver.c
+++ linux-4.14.336/drivers/video/fbdev/savage/savagefb_driver.c
@@ -869,6 +869,9 @@ static int savagefb_check_var(struct fb_var_screeninfo   *var,
 
 	DBG("savagefb_check_var");
 
+	if (!var->pixclock)
+		return -EINVAL;
+
 	var->transp.offset = 0;
 	var->transp.length = 0;
 	switch (var->bits_per_pixel) {
diff --git drivers/video/fbdev/sis/sis_main.c drivers/video/fbdev/sis/sis_main.c
index e92303823a4b..9575a481eeaf 100644
--- linux-4.14.336/drivers/video/fbdev/sis/sis_main.c
+++ linux-4.14.336/drivers/video/fbdev/sis/sis_main.c
@@ -1437,6 +1437,8 @@ sisfb_check_var(struct fb_var_screeninfo *var, struct fb_info *info)
 
 	vtotal = var->upper_margin + var->lower_margin + var->vsync_len;
 
+	if (!var->pixclock)
+		return -EINVAL;
 	pixclock = var->pixclock;
 
 	if((var->vmode & FB_VMODE_MASK) == FB_VMODE_NONINTERLACED) {
diff --git drivers/watchdog/bcm2835_wdt.c drivers/watchdog/bcm2835_wdt.c
index adb699145a07..4e653e71e232 100644
--- linux-4.14.336/drivers/watchdog/bcm2835_wdt.c
+++ linux-4.14.336/drivers/watchdog/bcm2835_wdt.c
@@ -44,6 +44,7 @@
 
 #define SECS_TO_WDOG_TICKS(x) ((x) << 16)
 #define WDOG_TICKS_TO_SECS(x) ((x) >> 16)
+#define WDOG_TICKS_TO_MSECS(x) ((x) * 1000 >> 16)
 
 struct bcm2835_wdt {
 	void __iomem		*base;
@@ -140,7 +141,7 @@ static struct watchdog_device bcm2835_wdt_wdd = {
 	.info =		&bcm2835_wdt_info,
 	.ops =		&bcm2835_wdt_ops,
 	.min_timeout =	1,
-	.max_timeout =	WDOG_TICKS_TO_SECS(PM_WDOG_TIME_SET),
+	.max_hw_heartbeat_ms =	WDOG_TICKS_TO_MSECS(PM_WDOG_TIME_SET),
 	.timeout =	WDOG_TICKS_TO_SECS(PM_WDOG_TIME_SET),
 };
 
diff --git drivers/watchdog/watchdog_dev.c drivers/watchdog/watchdog_dev.c
index 337ca3690d62..d26fb9016a9f 100644
--- linux-4.14.336/drivers/watchdog/watchdog_dev.c
+++ linux-4.14.336/drivers/watchdog/watchdog_dev.c
@@ -956,6 +956,7 @@ static int watchdog_cdev_register(struct watchdog_device *wdd)
 
 	/* Fill in the data structures */
 	cdev_init(&wd_data->cdev, &watchdog_fops);
+	wd_data->cdev.owner = wdd->ops->owner;
 
 	/* Add the device */
 	err = cdev_device_add(&wd_data->cdev, &wd_data->dev);
@@ -970,8 +971,6 @@ static int watchdog_cdev_register(struct watchdog_device *wdd)
 		return err;
 	}
 
-	wd_data->cdev.owner = wdd->ops->owner;
-
 	/* Record time of most recent heartbeat as 'just before now'. */
 	wd_data->last_hw_keepalive = jiffies - 1;
 
diff --git fs/aio.c fs/aio.c
index 2eb3dba5ed16..816f1443626b 100644
--- linux-4.14.336/fs/aio.c
+++ linux-4.14.336/fs/aio.c
@@ -562,6 +562,13 @@ void kiocb_set_cancel_fn(struct kiocb *iocb, kiocb_cancel_fn *cancel)
 	struct kioctx *ctx = req->ki_ctx;
 	unsigned long flags;
 
+	/*
+	 * kiocb didn't come from aio or is neither a read nor a write, hence
+	 * ignore it.
+	 */
+	if (!(iocb->ki_flags & IOCB_AIO_RW))
+		return;
+
 	spin_lock_irqsave(&ctx->ctx_lock, flags);
 
 	if (!req->ki_list.next)
@@ -1601,7 +1608,7 @@ static int io_submit_one(struct kioctx *ctx, struct iocb __user *user_iocb,
 	}
 	req->common.ki_pos = iocb->aio_offset;
 	req->common.ki_complete = aio_complete;
-	req->common.ki_flags = iocb_flags(req->common.ki_filp);
+	req->common.ki_flags = iocb_flags(req->common.ki_filp) | IOCB_AIO_RW;
 	req->common.ki_hint = file_write_hint(file);
 
 	if (iocb->aio_flags & IOCB_FLAG_RESFD) {
diff --git fs/btrfs/dev-replace.c fs/btrfs/dev-replace.c
index f1e9dd246ab0..3238bd9c0d39 100644
--- linux-4.14.336/fs/btrfs/dev-replace.c
+++ linux-4.14.336/fs/btrfs/dev-replace.c
@@ -426,6 +426,23 @@ leave:
 	return ret;
 }
 
+static int btrfs_check_replace_dev_names(struct btrfs_ioctl_dev_replace_args *args)
+{
+	if (args->start.srcdevid == 0) {
+		if (memchr(args->start.srcdev_name, 0,
+			   sizeof(args->start.srcdev_name)) == NULL)
+			return -ENAMETOOLONG;
+	} else {
+		args->start.srcdev_name[0] = 0;
+	}
+
+	if (memchr(args->start.tgtdev_name, 0,
+		   sizeof(args->start.tgtdev_name)) == NULL)
+	    return -ENAMETOOLONG;
+
+	return 0;
+}
+
 int btrfs_dev_replace_by_ioctl(struct btrfs_fs_info *fs_info,
 			    struct btrfs_ioctl_dev_replace_args *args)
 {
@@ -438,10 +455,9 @@ int btrfs_dev_replace_by_ioctl(struct btrfs_fs_info *fs_info,
 	default:
 		return -EINVAL;
 	}
-
-	if ((args->start.srcdevid == 0 && args->start.srcdev_name[0] == '\0') ||
-	    args->start.tgtdev_name[0] == '\0')
-		return -EINVAL;
+	ret = btrfs_check_replace_dev_names(args);
+	if (ret < 0)
+		return ret;
 
 	ret = btrfs_dev_replace_start(fs_info, args->start.tgtdev_name,
 					args->start.srcdevid,
diff --git fs/btrfs/extent-tree.c fs/btrfs/extent-tree.c
index deb01e59da02..6741710a149e 100644
--- linux-4.14.336/fs/btrfs/extent-tree.c
+++ linux-4.14.336/fs/btrfs/extent-tree.c
@@ -2070,7 +2070,8 @@ static int btrfs_issue_discard(struct block_device *bdev, u64 start, u64 len,
 	u64 bytes_left, end;
 	u64 aligned_start = ALIGN(start, 1 << 9);
 
-	if (WARN_ON(start != aligned_start)) {
+	/* Adjust the range to be aligned to 512B sectors if necessary. */
+	if (start != aligned_start) {
 		len -= aligned_start - start;
 		len = round_down(len, 1 << 9);
 		start = aligned_start;
diff --git fs/btrfs/ioctl.c fs/btrfs/ioctl.c
index 93b83dc298ac..c8bc8cf5a41f 100644
--- linux-4.14.336/fs/btrfs/ioctl.c
+++ linux-4.14.336/fs/btrfs/ioctl.c
@@ -2668,6 +2668,10 @@ static int btrfs_ioctl_defrag(struct file *file, void __user *argp)
 				kfree(range);
 				goto out;
 			}
+			if (range->flags & ~BTRFS_DEFRAG_RANGE_FLAGS_SUPP) {
+				ret = -EOPNOTSUPP;
+				goto out;
+			}
 			/* compression requires us to start the IO */
 			if ((range->flags & BTRFS_DEFRAG_RANGE_COMPRESS)) {
 				range->flags |= BTRFS_DEFRAG_RANGE_START_IO;
diff --git fs/btrfs/send.c fs/btrfs/send.c
index f2cb7fec7547..fa9797f8501e 100644
--- linux-4.14.336/fs/btrfs/send.c
+++ linux-4.14.336/fs/btrfs/send.c
@@ -6662,7 +6662,7 @@ long btrfs_ioctl_send(struct file *mnt_file, void __user *arg_)
 	}
 
 	if (arg->flags & ~BTRFS_SEND_FLAG_MASK) {
-		ret = -EINVAL;
+		ret = -EOPNOTSUPP;
 		goto out;
 	}
 
diff --git fs/cachefiles/bind.c fs/cachefiles/bind.c
index d9f001078e08..5aa9f4578f3e 100644
--- linux-4.14.336/fs/cachefiles/bind.c
+++ linux-4.14.336/fs/cachefiles/bind.c
@@ -248,6 +248,8 @@ error_open_root:
 	kmem_cache_free(cachefiles_object_jar, fsdef);
 error_root_object:
 	cachefiles_end_secure(cache, saved_cred);
+	put_cred(cache->cache_cred);
+	cache->cache_cred = NULL;
 	pr_err("Failed to register: %d\n", ret);
 	return ret;
 }
@@ -268,6 +270,7 @@ void cachefiles_daemon_unbind(struct cachefiles_cache *cache)
 
 	dput(cache->graveyard);
 	mntput(cache->mnt);
+	put_cred(cache->cache_cred);
 
 	kfree(cache->rootdirname);
 	kfree(cache->secctx);
diff --git fs/ceph/caps.c fs/ceph/caps.c
index e36786f574b8..b84ce90953c6 100644
--- linux-4.14.336/fs/ceph/caps.c
+++ linux-4.14.336/fs/ceph/caps.c
@@ -4026,12 +4026,14 @@ int ceph_encode_dentry_release(void **p, struct dentry *dentry,
 			       struct inode *dir,
 			       int mds, int drop, int unless)
 {
-	struct dentry *parent = NULL;
 	struct ceph_mds_request_release *rel = *p;
 	struct ceph_dentry_info *di = ceph_dentry(dentry);
 	int force = 0;
 	int ret;
 
+	/* This shouldn't happen */
+	BUG_ON(!dir);
+
 	/*
 	 * force an record for the directory caps if we have a dentry lease.
 	 * this is racy (can't take i_ceph_lock and d_lock together), but it
@@ -4041,14 +4043,9 @@ int ceph_encode_dentry_release(void **p, struct dentry *dentry,
 	spin_lock(&dentry->d_lock);
 	if (di->lease_session && di->lease_session->s_mds == mds)
 		force = 1;
-	if (!dir) {
-		parent = dget(dentry->d_parent);
-		dir = d_inode(parent);
-	}
 	spin_unlock(&dentry->d_lock);
 
 	ret = ceph_encode_inode_release(p, dir, mds, drop, unless, force);
-	dput(parent);
 
 	spin_lock(&dentry->d_lock);
 	if (ret && di->lease_session && di->lease_session->s_mds == mds) {
diff --git fs/compat_ioctl.c fs/compat_ioctl.c
index f445bc9cdc94..74e8507419d7 100644
--- linux-4.14.336/fs/compat_ioctl.c
+++ linux-4.14.336/fs/compat_ioctl.c
@@ -1546,8 +1546,7 @@ COMPAT_SYSCALL_DEFINE3(ioctl, unsigned int, fd, unsigned int, cmd,
 	if (!f.file)
 		goto out;
 
-	/* RED-PEN how should LSM module know it's handling 32bit? */
-	error = security_file_ioctl(f.file, cmd, arg);
+	error = security_file_ioctl_compat(f.file, cmd, arg);
 	if (error)
 		goto out_fput;
 
diff --git fs/dcache.c fs/dcache.c
index 9ac1290ae44f..5a9a773ece54 100644
--- linux-4.14.336/fs/dcache.c
+++ linux-4.14.336/fs/dcache.c
@@ -709,12 +709,12 @@ static inline bool fast_dput(struct dentry *dentry)
 	 */
 	if (unlikely(ret < 0)) {
 		spin_lock(&dentry->d_lock);
-		if (dentry->d_lockref.count > 1) {
-			dentry->d_lockref.count--;
+		if (WARN_ON_ONCE(dentry->d_lockref.count <= 0)) {
 			spin_unlock(&dentry->d_lock);
 			return 1;
 		}
-		return 0;
+		dentry->d_lockref.count--;
+		goto locked;
 	}
 
 	/*
@@ -765,6 +765,7 @@ static inline bool fast_dput(struct dentry *dentry)
 	 * else could have killed it and marked it dead. Either way, we
 	 * don't need to do anything else.
 	 */
+locked:
 	if (dentry->d_lockref.count) {
 		spin_unlock(&dentry->d_lock);
 		return 1;
diff --git fs/ext4/mballoc.c fs/ext4/mballoc.c
index 91d1de198fed..64ce26ec9c68 100644
--- linux-4.14.336/fs/ext4/mballoc.c
+++ linux-4.14.336/fs/ext4/mballoc.c
@@ -1817,6 +1817,9 @@ int ext4_mb_try_best_found(struct ext4_allocation_context *ac,
 		return err;
 
 	ext4_lock_group(ac->ac_sb, group);
+	if (unlikely(EXT4_MB_GRP_BBITMAP_CORRUPT(e4b->bd_info)))
+		goto out;
+
 	max = mb_find_extent(e4b, ex.fe_start, ex.fe_len, &ex);
 
 	if (max > 0) {
@@ -1824,6 +1827,7 @@ int ext4_mb_try_best_found(struct ext4_allocation_context *ac,
 		ext4_mb_use_best_found(ac, e4b);
 	}
 
+out:
 	ext4_unlock_group(ac->ac_sb, group);
 	ext4_mb_unload_buddy(e4b);
 
@@ -1850,12 +1854,10 @@ int ext4_mb_find_by_goal(struct ext4_allocation_context *ac,
 	if (err)
 		return err;
 
-	if (unlikely(EXT4_MB_GRP_BBITMAP_CORRUPT(e4b->bd_info))) {
-		ext4_mb_unload_buddy(e4b);
-		return 0;
-	}
-
 	ext4_lock_group(ac->ac_sb, group);
+	if (unlikely(EXT4_MB_GRP_BBITMAP_CORRUPT(e4b->bd_info)))
+		goto out;
+
 	max = mb_find_extent(e4b, ac->ac_g_ex.fe_start,
 			     ac->ac_g_ex.fe_len, &ex);
 	ex.fe_logical = 0xDEADFA11; /* debug value */
@@ -1888,6 +1890,7 @@ int ext4_mb_find_by_goal(struct ext4_allocation_context *ac,
 		ac->ac_b_ex = ex;
 		ext4_mb_use_best_found(ac, e4b);
 	}
+out:
 	ext4_unlock_group(ac->ac_sb, group);
 	ext4_mb_unload_buddy(e4b);
 
diff --git fs/ext4/move_extent.c fs/ext4/move_extent.c
index ef60f2e92da6..a10c560405b2 100644
--- linux-4.14.336/fs/ext4/move_extent.c
+++ linux-4.14.336/fs/ext4/move_extent.c
@@ -628,6 +628,7 @@ ext4_move_extents(struct file *o_filp, struct file *d_filp, __u64 orig_blk,
 		goto out;
 	o_end = o_start + len;
 
+	*moved_len = 0;
 	while (o_start < o_end) {
 		struct ext4_extent *ex;
 		ext4_lblk_t cur_blk, next_blk;
@@ -683,7 +684,7 @@ ext4_move_extents(struct file *o_filp, struct file *d_filp, __u64 orig_blk,
 		 */
 		ext4_double_up_write_data_sem(orig_inode, donor_inode);
 		/* Swap original branches with new branches */
-		move_extent_per_page(o_filp, donor_inode,
+		*moved_len += move_extent_per_page(o_filp, donor_inode,
 				     orig_page_index, donor_page_index,
 				     offset_in_page, cur_len,
 				     unwritten, &ret);
@@ -693,9 +694,6 @@ ext4_move_extents(struct file *o_filp, struct file *d_filp, __u64 orig_blk,
 		o_start += cur_len;
 		d_start += cur_len;
 	}
-	*moved_len = o_start - orig_blk;
-	if (*moved_len > len)
-		*moved_len = len;
 
 out:
 	if (*moved_len) {
diff --git fs/ext4/resize.c fs/ext4/resize.c
index f0b27be5892a..47ecf0826899 100644
--- linux-4.14.336/fs/ext4/resize.c
+++ linux-4.14.336/fs/ext4/resize.c
@@ -237,7 +237,7 @@ struct ext4_new_flex_group_data {
  *
  * Returns NULL on failure otherwise address of the allocated structure.
  */
-static struct ext4_new_flex_group_data *alloc_flex_gd(unsigned long flexbg_size)
+static struct ext4_new_flex_group_data *alloc_flex_gd(unsigned int flexbg_size)
 {
 	struct ext4_new_flex_group_data *flex_gd;
 
@@ -290,7 +290,7 @@ static void free_flex_gd(struct ext4_new_flex_group_data *flex_gd)
  */
 static int ext4_alloc_group_tables(struct super_block *sb,
 				struct ext4_new_flex_group_data *flex_gd,
-				int flexbg_size)
+				unsigned int flexbg_size)
 {
 	struct ext4_new_group_data *group_data = flex_gd->groups;
 	ext4_fsblk_t start_blk;
@@ -383,12 +383,12 @@ next_group:
 		group = group_data[0].group;
 
 		printk(KERN_DEBUG "EXT4-fs: adding a flex group with "
-		       "%d groups, flexbg size is %d:\n", flex_gd->count,
+		       "%u groups, flexbg size is %u:\n", flex_gd->count,
 		       flexbg_size);
 
 		for (i = 0; i < flex_gd->count; i++) {
 			printk(KERN_DEBUG "adding %s group %u: %u "
-			       "blocks (%d free)\n",
+			       "blocks (%u free)\n",
 			       ext4_bg_has_super(sb, group + i) ? "normal" :
 			       "no-super", group + i,
 			       group_data[i].blocks_count,
@@ -1558,7 +1558,7 @@ exit:
 static int ext4_setup_next_flex_gd(struct super_block *sb,
 				    struct ext4_new_flex_group_data *flex_gd,
 				    ext4_fsblk_t n_blocks_count,
-				    unsigned long flexbg_size)
+				    unsigned int flexbg_size)
 {
 	struct ext4_super_block *es = EXT4_SB(sb)->s_es;
 	struct ext4_new_group_data *group_data = flex_gd->groups;
@@ -1935,8 +1935,9 @@ int ext4_resize_fs(struct super_block *sb, ext4_fsblk_t n_blocks_count)
 	ext4_fsblk_t o_blocks_count;
 	ext4_fsblk_t n_blocks_count_retry = 0;
 	unsigned long last_update_time = 0;
-	int err = 0, flexbg_size = 1 << sbi->s_log_groups_per_flex;
+	int err = 0;
 	int meta_bg;
+	unsigned int flexbg_size = ext4_flex_bg_size(sbi);
 
 	/* See if the device is actually as big as what was requested */
 	bh = sb_bread(sb, n_blocks_count - 1);
diff --git fs/f2fs/namei.c fs/f2fs/namei.c
index 9fb98fce7096..eb9db586c01d 100644
--- linux-4.14.336/fs/f2fs/namei.c
+++ linux-4.14.336/fs/f2fs/namei.c
@@ -882,7 +882,7 @@ static int f2fs_rename(struct inode *old_dir, struct dentry *old_dentry,
 	}
 
 	if (old_dir_entry) {
-		if (old_dir != new_dir && !whiteout) {
+		if (old_dir != new_dir) {
 			f2fs_set_link(old_inode, old_dir_entry,
 						old_dir_page, new_dir);
 		} else {
diff --git fs/f2fs/xattr.c fs/f2fs/xattr.c
index b3c64ab0d5a5..f52c01804f81 100644
--- linux-4.14.336/fs/f2fs/xattr.c
+++ linux-4.14.336/fs/f2fs/xattr.c
@@ -695,6 +695,12 @@ static int __f2fs_setxattr(struct inode *inode, int index,
 		memcpy(pval, value, size);
 		last->e_value_size = cpu_to_le16(size);
 		new_hsize += newsize;
+		/*
+		 * Explicitly add the null terminator.  The unused xattr space
+		 * is supposed to always be zeroed, which would make this
+		 * unnecessary, but don't depend on that.
+		 */
+		*(u32 *)((u8 *)last + newsize) = 0;
 	}
 
 	error = write_all_xattrs(inode, new_hsize, base_addr, ipage);
diff --git fs/fuse/dir.c fs/fuse/dir.c
index 8e5125904762..bd602b7e8e46 100644
--- linux-4.14.336/fs/fuse/dir.c
+++ linux-4.14.336/fs/fuse/dir.c
@@ -1299,8 +1299,16 @@ retry:
 			dput(dentry);
 			dentry = alias;
 		}
-		if (IS_ERR(dentry))
+		if (IS_ERR(dentry)) {
+			if (!IS_ERR(inode)) {
+				struct fuse_inode *fi = get_fuse_inode(inode);
+
+				spin_lock(&fc->lock);
+				fi->nlookup--;
+				spin_unlock(&fc->lock);
+			}
 			return PTR_ERR(dentry);
+		}
 	}
 	if (fc->readdirplus_auto)
 		set_bit(FUSE_I_INIT_RDPLUS, &get_fuse_inode(inode)->state);
diff --git fs/jbd2/journal.c fs/jbd2/journal.c
index 93a466cf58ba..ee114f0b625a 100644
--- linux-4.14.336/fs/jbd2/journal.c
+++ linux-4.14.336/fs/jbd2/journal.c
@@ -1361,9 +1361,11 @@ static int jbd2_write_superblock(journal_t *journal, int write_flags)
 		return -EIO;
 	}
 
-	trace_jbd2_write_superblock(journal, write_flags);
 	if (!(journal->j_flags & JBD2_BARRIER))
 		write_flags &= ~(REQ_FUA | REQ_PREFLUSH);
+
+	trace_jbd2_write_superblock(journal, write_flags);
+
 	if (buffer_write_io_error(bh)) {
 		/*
 		 * Oh, dear.  A previous attempt to write the journal
diff --git fs/jfs/jfs_dmap.c fs/jfs/jfs_dmap.c
index ed7989d7b2ba..6c6efb5a168b 100644
--- linux-4.14.336/fs/jfs/jfs_dmap.c
+++ linux-4.14.336/fs/jfs/jfs_dmap.c
@@ -76,10 +76,10 @@
  */
 static void dbAllocBits(struct bmap * bmp, struct dmap * dp, s64 blkno,
 			int nblocks);
-static void dbSplit(dmtree_t * tp, int leafno, int splitsz, int newval);
-static int dbBackSplit(dmtree_t * tp, int leafno);
-static int dbJoin(dmtree_t * tp, int leafno, int newval);
-static void dbAdjTree(dmtree_t * tp, int leafno, int newval);
+static void dbSplit(dmtree_t *tp, int leafno, int splitsz, int newval, bool is_ctl);
+static int dbBackSplit(dmtree_t *tp, int leafno, bool is_ctl);
+static int dbJoin(dmtree_t *tp, int leafno, int newval, bool is_ctl);
+static void dbAdjTree(dmtree_t *tp, int leafno, int newval, bool is_ctl);
 static int dbAdjCtl(struct bmap * bmp, s64 blkno, int newval, int alloc,
 		    int level);
 static int dbAllocAny(struct bmap * bmp, s64 nblocks, int l2nb, s64 * results);
@@ -2184,7 +2184,7 @@ static int dbFreeDmap(struct bmap * bmp, struct dmap * dp, s64 blkno,
 		 * system.
 		 */
 		if (dp->tree.stree[word] == NOFREE)
-			dbBackSplit((dmtree_t *) & dp->tree, word);
+			dbBackSplit((dmtree_t *)&dp->tree, word, false);
 
 		dbAllocBits(bmp, dp, blkno, nblocks);
 	}
@@ -2270,7 +2270,7 @@ static void dbAllocBits(struct bmap * bmp, struct dmap * dp, s64 blkno,
 			 * the binary system of the leaves if need be.
 			 */
 			dbSplit(tp, word, BUDMIN,
-				dbMaxBud((u8 *) & dp->wmap[word]));
+				dbMaxBud((u8 *)&dp->wmap[word]), false);
 
 			word += 1;
 		} else {
@@ -2310,7 +2310,7 @@ static void dbAllocBits(struct bmap * bmp, struct dmap * dp, s64 blkno,
 				 * system of the leaves to reflect the current
 				 * allocation (size).
 				 */
-				dbSplit(tp, word, size, NOFREE);
+				dbSplit(tp, word, size, NOFREE, false);
 
 				/* get the number of dmap words handled */
 				nw = BUDSIZE(size, BUDMIN);
@@ -2417,7 +2417,7 @@ static int dbFreeBits(struct bmap * bmp, struct dmap * dp, s64 blkno,
 			/* update the leaf for this dmap word.
 			 */
 			rc = dbJoin(tp, word,
-				    dbMaxBud((u8 *) & dp->wmap[word]));
+				    dbMaxBud((u8 *)&dp->wmap[word]), false);
 			if (rc)
 				return rc;
 
@@ -2450,7 +2450,7 @@ static int dbFreeBits(struct bmap * bmp, struct dmap * dp, s64 blkno,
 
 				/* update the leaf.
 				 */
-				rc = dbJoin(tp, word, size);
+				rc = dbJoin(tp, word, size, false);
 				if (rc)
 					return rc;
 
@@ -2602,14 +2602,14 @@ dbAdjCtl(struct bmap * bmp, s64 blkno, int newval, int alloc, int level)
 		 * that it is at the front of a binary buddy system.
 		 */
 		if (oldval == NOFREE) {
-			rc = dbBackSplit((dmtree_t *) dcp, leafno);
+			rc = dbBackSplit((dmtree_t *)dcp, leafno, true);
 			if (rc)
 				return rc;
 			oldval = dcp->stree[ti];
 		}
-		dbSplit((dmtree_t *) dcp, leafno, dcp->budmin, newval);
+		dbSplit((dmtree_t *) dcp, leafno, dcp->budmin, newval, true);
 	} else {
-		rc = dbJoin((dmtree_t *) dcp, leafno, newval);
+		rc = dbJoin((dmtree_t *) dcp, leafno, newval, true);
 		if (rc)
 			return rc;
 	}
@@ -2638,7 +2638,7 @@ dbAdjCtl(struct bmap * bmp, s64 blkno, int newval, int alloc, int level)
 				 */
 				if (alloc) {
 					dbJoin((dmtree_t *) dcp, leafno,
-					       oldval);
+					       oldval, true);
 				} else {
 					/* the dbJoin() above might have
 					 * caused a larger binary buddy system
@@ -2648,9 +2648,9 @@ dbAdjCtl(struct bmap * bmp, s64 blkno, int newval, int alloc, int level)
 					 */
 					if (dcp->stree[ti] == NOFREE)
 						dbBackSplit((dmtree_t *)
-							    dcp, leafno);
+							    dcp, leafno, true);
 					dbSplit((dmtree_t *) dcp, leafno,
-						dcp->budmin, oldval);
+						dcp->budmin, oldval, true);
 				}
 
 				/* release the buffer and return the error.
@@ -2698,7 +2698,7 @@ dbAdjCtl(struct bmap * bmp, s64 blkno, int newval, int alloc, int level)
  *
  * serialization: IREAD_LOCK(ipbmap) or IWRITE_LOCK(ipbmap) held on entry/exit;
  */
-static void dbSplit(dmtree_t * tp, int leafno, int splitsz, int newval)
+static void dbSplit(dmtree_t *tp, int leafno, int splitsz, int newval, bool is_ctl)
 {
 	int budsz;
 	int cursz;
@@ -2720,7 +2720,7 @@ static void dbSplit(dmtree_t * tp, int leafno, int splitsz, int newval)
 		while (cursz >= splitsz) {
 			/* update the buddy's leaf with its new value.
 			 */
-			dbAdjTree(tp, leafno ^ budsz, cursz);
+			dbAdjTree(tp, leafno ^ budsz, cursz, is_ctl);
 
 			/* on to the next size and buddy.
 			 */
@@ -2732,7 +2732,7 @@ static void dbSplit(dmtree_t * tp, int leafno, int splitsz, int newval)
 	/* adjust the dmap tree to reflect the specified leaf's new
 	 * value.
 	 */
-	dbAdjTree(tp, leafno, newval);
+	dbAdjTree(tp, leafno, newval, is_ctl);
 }
 
 
@@ -2763,7 +2763,7 @@ static void dbSplit(dmtree_t * tp, int leafno, int splitsz, int newval)
  *
  * serialization: IREAD_LOCK(ipbmap) or IWRITE_LOCK(ipbmap) held on entry/exit;
  */
-static int dbBackSplit(dmtree_t * tp, int leafno)
+static int dbBackSplit(dmtree_t *tp, int leafno, bool is_ctl)
 {
 	int budsz, bud, w, bsz, size;
 	int cursz;
@@ -2814,7 +2814,7 @@ static int dbBackSplit(dmtree_t * tp, int leafno)
 				 * system in two.
 				 */
 				cursz = leaf[bud] - 1;
-				dbSplit(tp, bud, cursz, cursz);
+				dbSplit(tp, bud, cursz, cursz, is_ctl);
 				break;
 			}
 		}
@@ -2842,7 +2842,7 @@ static int dbBackSplit(dmtree_t * tp, int leafno)
  *
  * RETURN VALUES: none
  */
-static int dbJoin(dmtree_t * tp, int leafno, int newval)
+static int dbJoin(dmtree_t *tp, int leafno, int newval, bool is_ctl)
 {
 	int budsz, buddy;
 	s8 *leaf;
@@ -2897,12 +2897,12 @@ static int dbJoin(dmtree_t * tp, int leafno, int newval)
 			if (leafno < buddy) {
 				/* leafno is the left buddy.
 				 */
-				dbAdjTree(tp, buddy, NOFREE);
+				dbAdjTree(tp, buddy, NOFREE, is_ctl);
 			} else {
 				/* buddy is the left buddy and becomes
 				 * leafno.
 				 */
-				dbAdjTree(tp, leafno, NOFREE);
+				dbAdjTree(tp, leafno, NOFREE, is_ctl);
 				leafno = buddy;
 			}
 
@@ -2915,7 +2915,7 @@ static int dbJoin(dmtree_t * tp, int leafno, int newval)
 
 	/* update the leaf value.
 	 */
-	dbAdjTree(tp, leafno, newval);
+	dbAdjTree(tp, leafno, newval, is_ctl);
 
 	return 0;
 }
@@ -2936,15 +2936,20 @@ static int dbJoin(dmtree_t * tp, int leafno, int newval)
  *
  * RETURN VALUES: none
  */
-static void dbAdjTree(dmtree_t * tp, int leafno, int newval)
+static void dbAdjTree(dmtree_t *tp, int leafno, int newval, bool is_ctl)
 {
 	int lp, pp, k;
-	int max;
+	int max, size;
+
+	size = is_ctl ? CTLTREESIZE : TREESIZE;
 
 	/* pick up the index of the leaf for this leafno.
 	 */
 	lp = leafno + le32_to_cpu(tp->dmt_leafidx);
 
+	if (WARN_ON_ONCE(lp >= size || lp < 0))
+		return;
+
 	/* is the current value the same as the old value ?  if so,
 	 * there is nothing to do.
 	 */
diff --git fs/jfs/jfs_dtree.c fs/jfs/jfs_dtree.c
index de2bcb36e079..14a16bb906e8 100644
--- linux-4.14.336/fs/jfs/jfs_dtree.c
+++ linux-4.14.336/fs/jfs/jfs_dtree.c
@@ -645,6 +645,11 @@ int dtSearch(struct inode *ip, struct component_name * key, ino_t * data,
 		for (base = 0, lim = p->header.nextindex; lim; lim >>= 1) {
 			index = base + (lim >> 1);
 
+			if (stbl[index] < 0) {
+				rc = -EIO;
+				goto out;
+			}
+
 			if (p->header.flag & BT_LEAF) {
 				/* uppercase leaf name to compare */
 				cmp =
@@ -1982,7 +1987,7 @@ static int dtSplitRoot(tid_t tid,
 		do {
 			f = &rp->slot[fsi];
 			fsi = f->next;
-		} while (fsi != -1);
+		} while (fsi >= 0);
 
 		f->next = n;
 	}
diff --git fs/jfs/jfs_imap.c fs/jfs/jfs_imap.c
index 131dce5316ac..5cdcf68a4803 100644
--- linux-4.14.336/fs/jfs/jfs_imap.c
+++ linux-4.14.336/fs/jfs/jfs_imap.c
@@ -2200,6 +2200,9 @@ static int diNewExt(struct inomap * imap, struct iag * iagp, int extno)
 	/* get the ag and iag numbers for this iag.
 	 */
 	agno = BLKTOAG(le64_to_cpu(iagp->agstart), sbi);
+	if (agno >= MAXAG || agno < 0)
+		return -EIO;
+
 	iagno = le32_to_cpu(iagp->iagnum);
 
 	/* check if this is the last free extent within the
diff --git fs/jfs/jfs_mount.c fs/jfs/jfs_mount.c
index f1a705d15904..97d91c1686b8 100644
--- linux-4.14.336/fs/jfs/jfs_mount.c
+++ linux-4.14.336/fs/jfs/jfs_mount.c
@@ -184,15 +184,15 @@ int jfs_mount(struct super_block *sb)
 	}
 	jfs_info("jfs_mount: ipimap:0x%p", ipimap);
 
-	/* map further access of per fileset inodes by the fileset inode */
-	sbi->ipimap = ipimap;
-
 	/* initialize fileset inode allocation map */
 	if ((rc = diMount(ipimap))) {
 		jfs_err("jfs_mount: diMount failed w/rc = %d", rc);
 		goto err_ipimap;
 	}
 
+	/* map further access of per fileset inodes by the fileset inode */
+	sbi->ipimap = ipimap;
+
 	return rc;
 
 	/*
diff --git fs/nfs/nfs4proc.c fs/nfs/nfs4proc.c
index ff41d726f758..77c207a0fb81 100644
--- linux-4.14.336/fs/nfs/nfs4proc.c
+++ linux-4.14.336/fs/nfs/nfs4proc.c
@@ -161,6 +161,7 @@ static int nfs4_map_errors(int err)
 	case -NFS4ERR_RESOURCE:
 	case -NFS4ERR_LAYOUTTRYLATER:
 	case -NFS4ERR_RECALLCONFLICT:
+	case -NFS4ERR_RETURNCONFLICT:
 		return -EREMOTEIO;
 	case -NFS4ERR_WRONGSEC:
 	case -NFS4ERR_WRONG_CRED:
@@ -472,6 +473,7 @@ static int nfs4_do_handle_exception(struct nfs_server *server,
 		case -NFS4ERR_GRACE:
 		case -NFS4ERR_LAYOUTTRYLATER:
 		case -NFS4ERR_RECALLCONFLICT:
+		case -NFS4ERR_RETURNCONFLICT:
 			exception->delay = 1;
 			return 0;
 
@@ -8540,6 +8542,7 @@ nfs4_layoutget_handle_exception(struct rpc_task *task,
 		status = -EBUSY;
 		break;
 	case -NFS4ERR_RECALLCONFLICT:
+	case -NFS4ERR_RETURNCONFLICT:
 		status = -ERECALLCONFLICT;
 		break;
 	case -NFS4ERR_DELEG_REVOKED:
diff --git fs/nfsd/nfs4state.c fs/nfsd/nfs4state.c
index 2adbf471d107..6720c82ac351 100644
--- linux-4.14.336/fs/nfsd/nfs4state.c
+++ linux-4.14.336/fs/nfsd/nfs4state.c
@@ -6351,12 +6351,16 @@ nfsd4_release_lockowner(struct svc_rqst *rqstp,
 		if (sop->so_is_open_owner || !same_owner_str(sop, owner))
 			continue;
 
-		if (atomic_read(&sop->so_count) != 1) {
-			spin_unlock(&clp->cl_lock);
-			return nfserr_locks_held;
+		/* see if there are still any locks associated with it */
+		lo = lockowner(sop);
+		list_for_each_entry(stp, &sop->so_stateids, st_perstateowner) {
+			if (check_for_locks(stp->st_stid.sc_file, lo)) {
+				status = nfserr_locks_held;
+				spin_unlock(&clp->cl_lock);
+				return status;
+			}
 		}
 
-		lo = lockowner(sop);
 		nfs4_get_stateowner(sop);
 		break;
 	}
diff --git fs/nilfs2/dat.c fs/nilfs2/dat.c
index 185db3c3033b..63bd20032fa7 100644
--- linux-4.14.336/fs/nilfs2/dat.c
+++ linux-4.14.336/fs/nilfs2/dat.c
@@ -49,8 +49,21 @@ static inline struct nilfs_dat_info *NILFS_DAT_I(struct inode *dat)
 static int nilfs_dat_prepare_entry(struct inode *dat,
 				   struct nilfs_palloc_req *req, int create)
 {
-	return nilfs_palloc_get_entry_block(dat, req->pr_entry_nr,
-					    create, &req->pr_entry_bh);
+	int ret;
+
+	ret = nilfs_palloc_get_entry_block(dat, req->pr_entry_nr,
+					   create, &req->pr_entry_bh);
+	if (unlikely(ret == -ENOENT)) {
+		nilfs_msg(dat->i_sb, KERN_ERR,
+			  "DAT doesn't have a block to manage vblocknr = %llu",
+			  (unsigned long long)req->pr_entry_nr);
+		/*
+		 * Return internal code -EINVAL to notify bmap layer of
+		 * metadata corruption.
+		 */
+		ret = -EINVAL;
+	}
+	return ret;
 }
 
 static void nilfs_dat_commit_entry(struct inode *dat,
@@ -132,11 +145,7 @@ static void nilfs_dat_commit_free(struct inode *dat,
 
 int nilfs_dat_prepare_start(struct inode *dat, struct nilfs_palloc_req *req)
 {
-	int ret;
-
-	ret = nilfs_dat_prepare_entry(dat, req, 0);
-	WARN_ON(ret == -ENOENT);
-	return ret;
+	return nilfs_dat_prepare_entry(dat, req, 0);
 }
 
 void nilfs_dat_commit_start(struct inode *dat, struct nilfs_palloc_req *req,
@@ -163,10 +172,8 @@ int nilfs_dat_prepare_end(struct inode *dat, struct nilfs_palloc_req *req)
 	int ret;
 
 	ret = nilfs_dat_prepare_entry(dat, req, 0);
-	if (ret < 0) {
-		WARN_ON(ret == -ENOENT);
+	if (ret < 0)
 		return ret;
-	}
 
 	kaddr = kmap_atomic(req->pr_entry_bh->b_page);
 	entry = nilfs_palloc_block_get_entry(dat, req->pr_entry_nr,
diff --git fs/nilfs2/file.c fs/nilfs2/file.c
index c5fa3dee72fc..43501da7ef66 100644
--- linux-4.14.336/fs/nilfs2/file.c
+++ linux-4.14.336/fs/nilfs2/file.c
@@ -114,7 +114,13 @@ static int nilfs_page_mkwrite(struct vm_fault *vmf)
 	nilfs_transaction_commit(inode->i_sb);
 
  mapped:
-	wait_for_stable_page(page);
+	/*
+	 * Since checksumming including data blocks is performed to determine
+	 * the validity of the log to be written and used for recovery, it is
+	 * necessary to wait for writeback to finish here, regardless of the
+	 * stable write requirement of the backing device.
+	 */
+	wait_on_page_writeback(page);
  out:
 	sb_end_pagefault(inode->i_sb);
 	return block_page_mkwrite_return(ret);
diff --git fs/nilfs2/recovery.c fs/nilfs2/recovery.c
index 5139efed1888..cff597333afe 100644
--- linux-4.14.336/fs/nilfs2/recovery.c
+++ linux-4.14.336/fs/nilfs2/recovery.c
@@ -481,9 +481,10 @@ static int nilfs_prepare_segment_for_recovery(struct the_nilfs *nilfs,
 
 static int nilfs_recovery_copy_block(struct the_nilfs *nilfs,
 				     struct nilfs_recovery_block *rb,
-				     struct page *page)
+				     loff_t pos, struct page *page)
 {
 	struct buffer_head *bh_org;
+	size_t from = pos & ~PAGE_MASK;
 	void *kaddr;
 
 	bh_org = __bread(nilfs->ns_bdev, rb->blocknr, nilfs->ns_blocksize);
@@ -491,7 +492,7 @@ static int nilfs_recovery_copy_block(struct the_nilfs *nilfs,
 		return -EIO;
 
 	kaddr = kmap_atomic(page);
-	memcpy(kaddr + bh_offset(bh_org), bh_org->b_data, bh_org->b_size);
+	memcpy(kaddr + from, bh_org->b_data, bh_org->b_size);
 	kunmap_atomic(kaddr);
 	brelse(bh_org);
 	return 0;
@@ -530,7 +531,7 @@ static int nilfs_recover_dsync_blocks(struct the_nilfs *nilfs,
 			goto failed_inode;
 		}
 
-		err = nilfs_recovery_copy_block(nilfs, rb, page);
+		err = nilfs_recovery_copy_block(nilfs, rb, pos, page);
 		if (unlikely(err))
 			goto failed_page;
 
diff --git fs/nilfs2/segment.c fs/nilfs2/segment.c
index ca4b1675c147..b9fd60e07701 100644
--- linux-4.14.336/fs/nilfs2/segment.c
+++ linux-4.14.336/fs/nilfs2/segment.c
@@ -1715,7 +1715,6 @@ static void nilfs_segctor_prepare_write(struct nilfs_sc_info *sci)
 
 		list_for_each_entry(bh, &segbuf->sb_payload_buffers,
 				    b_assoc_buffers) {
-			set_buffer_async_write(bh);
 			if (bh == segbuf->sb_super_root) {
 				if (bh->b_page != bd_page) {
 					lock_page(bd_page);
@@ -1726,6 +1725,7 @@ static void nilfs_segctor_prepare_write(struct nilfs_sc_info *sci)
 				}
 				break;
 			}
+			set_buffer_async_write(bh);
 			if (bh->b_page != fs_page) {
 				nilfs_begin_page_io(fs_page);
 				fs_page = bh->b_page;
@@ -1811,7 +1811,6 @@ static void nilfs_abort_logs(struct list_head *logs, int err)
 
 		list_for_each_entry(bh, &segbuf->sb_payload_buffers,
 				    b_assoc_buffers) {
-			clear_buffer_async_write(bh);
 			if (bh == segbuf->sb_super_root) {
 				clear_buffer_uptodate(bh);
 				if (bh->b_page != bd_page) {
@@ -1820,6 +1819,7 @@ static void nilfs_abort_logs(struct list_head *logs, int err)
 				}
 				break;
 			}
+			clear_buffer_async_write(bh);
 			if (bh->b_page != fs_page) {
 				nilfs_end_page_io(fs_page, err);
 				fs_page = bh->b_page;
@@ -1907,8 +1907,9 @@ static void nilfs_segctor_complete_write(struct nilfs_sc_info *sci)
 				 BIT(BH_Delay) | BIT(BH_NILFS_Volatile) |
 				 BIT(BH_NILFS_Redirected));
 
-			set_mask_bits(&bh->b_state, clear_bits, set_bits);
 			if (bh == segbuf->sb_super_root) {
+				set_buffer_uptodate(bh);
+				clear_buffer_dirty(bh);
 				if (bh->b_page != bd_page) {
 					end_page_writeback(bd_page);
 					bd_page = bh->b_page;
@@ -1916,6 +1917,7 @@ static void nilfs_segctor_complete_write(struct nilfs_sc_info *sci)
 				update_sr = true;
 				break;
 			}
+			set_mask_bits(&bh->b_state, clear_bits, set_bits);
 			if (bh->b_page != fs_page) {
 				nilfs_end_page_io(fs_page, 0);
 				fs_page = bh->b_page;
diff --git fs/pstore/ram.c fs/pstore/ram.c
index dc5a40058c2f..bbd90fef7fcd 100644
--- linux-4.14.336/fs/pstore/ram.c
+++ linux-4.14.336/fs/pstore/ram.c
@@ -586,6 +586,7 @@ static int ramoops_init_przs(const char *name,
 	}
 
 	zone_sz = mem_sz / *cnt;
+	zone_sz = ALIGN_DOWN(zone_sz, 2);
 	if (!zone_sz) {
 		dev_err(dev, "%s zone size == 0\n", name);
 		goto fail;
diff --git fs/pstore/ram_core.c fs/pstore/ram_core.c
index 58ac4e1a61a3..a323ed939aa8 100644
--- linux-4.14.336/fs/pstore/ram_core.c
+++ linux-4.14.336/fs/pstore/ram_core.c
@@ -190,7 +190,7 @@ static int persistent_ram_init_ecc(struct persistent_ram_zone *prz,
 {
 	int numerr;
 	struct persistent_ram_buffer *buffer = prz->buffer;
-	int ecc_blocks;
+	size_t ecc_blocks;
 	size_t ecc_total;
 
 	if (!ecc_info || !ecc_info->ecc_size)
diff --git include/crypto/if_alg.h include/crypto/if_alg.h
index 2ea6a95ca825..f803dc8c45ad 100644
--- linux-4.14.336/include/crypto/if_alg.h
+++ linux-4.14.336/include/crypto/if_alg.h
@@ -146,6 +146,7 @@ struct af_alg_async_req {
  * @enc:		Cryptographic operation to be performed when
  *			recvmsg is invoked.
  * @len:		Length of memory allocated for this data structure.
+ * @inflight:		Non-zero when AIO requests are in flight.
  */
 struct af_alg_ctx {
 	struct list_head tsgl_list;
@@ -163,6 +164,8 @@ struct af_alg_ctx {
 	bool enc;
 
 	unsigned int len;
+
+	unsigned int inflight;
 };
 
 int af_alg_register_type(const struct af_alg_type *type);
diff --git include/drm/drm_bridge.h include/drm/drm_bridge.h
index 6522d4cbc9d9..bfbd38c0b609 100644
--- linux-4.14.336/include/drm/drm_bridge.h
+++ linux-4.14.336/include/drm/drm_bridge.h
@@ -161,7 +161,7 @@ struct drm_bridge_funcs {
 	 * or &drm_encoder_helper_funcs.dpms hook.
 	 *
 	 * The bridge must assume that the display pipe (i.e. clocks and timing
-	 * singals) feeding it is no longer running when this callback is
+	 * signals) feeding it is no longer running when this callback is
 	 * called.
 	 *
 	 * The post_disable callback is optional.
diff --git include/drm/drm_mipi_dsi.h include/drm/drm_mipi_dsi.h
index 689f615471ab..a059f1d968b7 100644
--- linux-4.14.336/include/drm/drm_mipi_dsi.h
+++ linux-4.14.336/include/drm/drm_mipi_dsi.h
@@ -163,6 +163,7 @@ struct mipi_dsi_device_info {
  * struct mipi_dsi_device - DSI peripheral device
  * @host: DSI host for this peripheral
  * @dev: driver model device node for this peripheral
+ * @attached: the DSI device has been successfully attached
  * @name: DSI peripheral chip type
  * @channel: virtual channel assigned to the peripheral
  * @format: pixel format for video mode
@@ -172,6 +173,7 @@ struct mipi_dsi_device_info {
 struct mipi_dsi_device {
 	struct mipi_dsi_host *host;
 	struct device dev;
+	bool attached;
 
 	char name[DSI_DEV_NAME_SIZE];
 	unsigned int channel;
diff --git include/linux/bpf.h include/linux/bpf.h
index 3aa05ea79ba1..0d7a61df056b 100644
--- linux-4.14.336/include/linux/bpf.h
+++ linux-4.14.336/include/linux/bpf.h
@@ -38,7 +38,11 @@ struct bpf_map_ops {
 	/* funcs called by prog_array and perf_event_array map */
 	void *(*map_fd_get_ptr)(struct bpf_map *map, struct file *map_file,
 				int fd);
-	void (*map_fd_put_ptr)(void *ptr);
+	/* If need_defer is true, the implementation should guarantee that
+	 * the to-be-put element is still alive before the bpf program, which
+	 * may manipulate it, exists.
+	 */
+	void (*map_fd_put_ptr)(struct bpf_map *map, void *ptr, bool need_defer);
 	u32 (*map_gen_lookup)(struct bpf_map *map, struct bpf_insn *insn_buf);
 	u32 (*map_fd_sys_lookup_elem)(void *ptr);
 };
diff --git include/linux/device.h include/linux/device.h
index 65e06a066b67..27b70b810463 100644
--- linux-4.14.336/include/linux/device.h
+++ linux-4.14.336/include/linux/device.h
@@ -1474,6 +1474,9 @@ do {									\
 	WARN_ONCE(condition, "%s %s: " format, \
 			dev_driver_string(dev), dev_name(dev), ## arg)
 
+extern __printf(3, 4)
+int dev_err_probe(const struct device *dev, int err, const char *fmt, ...);
+
 /* Create alias, so I can be autoloaded. */
 #define MODULE_ALIAS_CHARDEV(major,minor) \
 	MODULE_ALIAS("char-major-" __stringify(major) "-" __stringify(minor))
diff --git include/linux/dmaengine.h include/linux/dmaengine.h
index 8089e28539f1..d5a7d320e05c 100644
--- linux-4.14.336/include/linux/dmaengine.h
+++ linux-4.14.336/include/linux/dmaengine.h
@@ -816,7 +816,8 @@ static inline int dmaengine_slave_config(struct dma_chan *chan,
 
 static inline bool is_slave_direction(enum dma_transfer_direction direction)
 {
-	return (direction == DMA_MEM_TO_DEV) || (direction == DMA_DEV_TO_MEM);
+	return (direction == DMA_MEM_TO_DEV) || (direction == DMA_DEV_TO_MEM) ||
+	       (direction == DMA_DEV_TO_DEV);
 }
 
 static inline struct dma_async_tx_descriptor *dmaengine_prep_slave_single(
diff --git include/linux/fs.h include/linux/fs.h
index ff0a992846a3..bd6072556269 100644
--- linux-4.14.336/include/linux/fs.h
+++ linux-4.14.336/include/linux/fs.h
@@ -296,6 +296,8 @@ enum rw_hint {
 #define IOCB_SYNC		(1 << 5)
 #define IOCB_WRITE		(1 << 6)
 #define IOCB_NOWAIT		(1 << 7)
+/* kiocb is a read or write operation submitted by fs/aio.c. */
+#define IOCB_AIO_RW		(1 << 23)
 
 struct kiocb {
 	struct file		*ki_filp;
diff --git include/linux/lsm_hooks.h include/linux/lsm_hooks.h
index 569debc49f3d..28ff40daccff 100644
--- linux-4.14.336/include/linux/lsm_hooks.h
+++ linux-4.14.336/include/linux/lsm_hooks.h
@@ -466,6 +466,12 @@
  *	simple integer value.  When @arg represents a user space pointer, it
  *	should never be used by the security module.
  *	Return 0 if permission is granted.
+ * @file_ioctl_compat:
+ *	@file contains the file structure.
+ *	@cmd contains the operation to perform.
+ *	@arg contains the operational arguments.
+ *	Check permission for a compat ioctl operation on @file.
+ *	Return 0 if permission is granted.
  * @mmap_addr :
  *	Check permissions for a mmap operation at @addr.
  *	@addr contains virtual address that will be used for the operation.
@@ -1486,6 +1492,8 @@ union security_list_options {
 	void (*file_free_security)(struct file *file);
 	int (*file_ioctl)(struct file *file, unsigned int cmd,
 				unsigned long arg);
+	int (*file_ioctl_compat)(struct file *file, unsigned int cmd,
+				unsigned long arg);
 	int (*mmap_addr)(unsigned long addr);
 	int (*mmap_file)(struct file *file, unsigned long reqprot,
 				unsigned long prot, unsigned long flags);
@@ -1764,6 +1772,7 @@ struct security_hook_heads {
 	struct list_head file_alloc_security;
 	struct list_head file_free_security;
 	struct list_head file_ioctl;
+	struct list_head file_ioctl_compat;
 	struct list_head mmap_addr;
 	struct list_head mmap_file;
 	struct list_head file_mprotect;
diff --git include/linux/pci_ids.h include/linux/pci_ids.h
index 83f576d45d78..c977e636a1dd 100644
--- linux-4.14.336/include/linux/pci_ids.h
+++ linux-4.14.336/include/linux/pci_ids.h
@@ -2953,6 +2953,7 @@
 #define PCI_DEVICE_ID_INTEL_82443GX_0	0x71a0
 #define PCI_DEVICE_ID_INTEL_82443GX_2	0x71a2
 #define PCI_DEVICE_ID_INTEL_82372FB_1	0x7601
+#define PCI_DEVICE_ID_INTEL_HDA_ARL	0x7728
 #define PCI_DEVICE_ID_INTEL_SCH_LPC	0x8119
 #define PCI_DEVICE_ID_INTEL_SCH_IDE	0x811a
 #define PCI_DEVICE_ID_INTEL_E6XX_CU	0x8183
diff --git include/linux/security.h include/linux/security.h
index 1c8968a267c2..cf77cd971795 100644
--- linux-4.14.336/include/linux/security.h
+++ linux-4.14.336/include/linux/security.h
@@ -306,6 +306,8 @@ int security_file_permission(struct file *file, int mask);
 int security_file_alloc(struct file *file);
 void security_file_free(struct file *file);
 int security_file_ioctl(struct file *file, unsigned int cmd, unsigned long arg);
+int security_file_ioctl_compat(struct file *file, unsigned int cmd,
+			       unsigned long arg);
 int security_mmap_file(struct file *file, unsigned long prot,
 			unsigned long flags);
 int security_mmap_addr(unsigned long addr);
@@ -827,6 +829,13 @@ static inline int security_file_ioctl(struct file *file, unsigned int cmd,
 	return 0;
 }
 
+static inline int security_file_ioctl_compat(struct file *file,
+					     unsigned int cmd,
+					     unsigned long arg)
+{
+	return 0;
+}
+
 static inline int security_mmap_file(struct file *file, unsigned long prot,
 				     unsigned long flags)
 {
diff --git include/linux/spi/spi.h include/linux/spi/spi.h
index a8f6606dd498..5c7741ca3b99 100644
--- linux-4.14.336/include/linux/spi/spi.h
+++ linux-4.14.336/include/linux/spi/spi.h
@@ -153,6 +153,7 @@ struct spi_device {
 #define	SPI_MODE_1	(0|SPI_CPHA)
 #define	SPI_MODE_2	(SPI_CPOL|0)
 #define	SPI_MODE_3	(SPI_CPOL|SPI_CPHA)
+#define	SPI_MODE_X_MASK	(SPI_CPOL|SPI_CPHA)
 #define	SPI_CS_HIGH	0x04			/* chipselect active high? */
 #define	SPI_LSB_FIRST	0x08			/* per-word bits-on-wire */
 #define	SPI_3WIRE	0x10			/* SI/SO signals shared */
diff --git include/linux/units.h include/linux/units.h
new file mode 100644
index 000000000000..a0af6d2ef4e5
--- linux-4.14.336//dev/null
+++ linux-4.14.336/include/linux/units.h
@@ -0,0 +1,92 @@
+/* SPDX-License-Identifier: GPL-2.0 */
+#ifndef _LINUX_UNITS_H
+#define _LINUX_UNITS_H
+
+#include <linux/kernel.h>
+
+#define HZ_PER_KHZ		1000UL
+#define KHZ_PER_MHZ		1000UL
+#define HZ_PER_MHZ		1000000UL
+
+#define MILLIWATT_PER_WATT	1000UL
+#define MICROWATT_PER_MILLIWATT	1000UL
+#define MICROWATT_PER_WATT	1000000UL
+
+#define ABSOLUTE_ZERO_MILLICELSIUS -273150
+
+static inline long milli_kelvin_to_millicelsius(long t)
+{
+	return t + ABSOLUTE_ZERO_MILLICELSIUS;
+}
+
+static inline long millicelsius_to_milli_kelvin(long t)
+{
+	return t - ABSOLUTE_ZERO_MILLICELSIUS;
+}
+
+#define MILLIDEGREE_PER_DEGREE 1000
+#define MILLIDEGREE_PER_DECIDEGREE 100
+
+static inline long kelvin_to_millicelsius(long t)
+{
+	return milli_kelvin_to_millicelsius(t * MILLIDEGREE_PER_DEGREE);
+}
+
+static inline long millicelsius_to_kelvin(long t)
+{
+	t = millicelsius_to_milli_kelvin(t);
+
+	return DIV_ROUND_CLOSEST(t, MILLIDEGREE_PER_DEGREE);
+}
+
+static inline long deci_kelvin_to_celsius(long t)
+{
+	t = milli_kelvin_to_millicelsius(t * MILLIDEGREE_PER_DECIDEGREE);
+
+	return DIV_ROUND_CLOSEST(t, MILLIDEGREE_PER_DEGREE);
+}
+
+static inline long celsius_to_deci_kelvin(long t)
+{
+	t = millicelsius_to_milli_kelvin(t * MILLIDEGREE_PER_DEGREE);
+
+	return DIV_ROUND_CLOSEST(t, MILLIDEGREE_PER_DECIDEGREE);
+}
+
+/**
+ * deci_kelvin_to_millicelsius_with_offset - convert Kelvin to Celsius
+ * @t: temperature value in decidegrees Kelvin
+ * @offset: difference between Kelvin and Celsius in millidegrees
+ *
+ * Return: temperature value in millidegrees Celsius
+ */
+static inline long deci_kelvin_to_millicelsius_with_offset(long t, long offset)
+{
+	return t * MILLIDEGREE_PER_DECIDEGREE - offset;
+}
+
+static inline long deci_kelvin_to_millicelsius(long t)
+{
+	return milli_kelvin_to_millicelsius(t * MILLIDEGREE_PER_DECIDEGREE);
+}
+
+static inline long millicelsius_to_deci_kelvin(long t)
+{
+	t = millicelsius_to_milli_kelvin(t);
+
+	return DIV_ROUND_CLOSEST(t, MILLIDEGREE_PER_DECIDEGREE);
+}
+
+static inline long kelvin_to_celsius(long t)
+{
+	return t + DIV_ROUND_CLOSEST(ABSOLUTE_ZERO_MILLICELSIUS,
+				     MILLIDEGREE_PER_DEGREE);
+}
+
+static inline long celsius_to_kelvin(long t)
+{
+	return t - DIV_ROUND_CLOSEST(ABSOLUTE_ZERO_MILLICELSIUS,
+				     MILLIDEGREE_PER_DEGREE);
+}
+
+#endif /* _LINUX_UNITS_H */
diff --git include/net/af_unix.h include/net/af_unix.h
index 7ec1cdb66be8..e514508bdc92 100644
--- linux-4.14.336/include/net/af_unix.h
+++ linux-4.14.336/include/net/af_unix.h
@@ -43,12 +43,6 @@ struct unix_skb_parms {
 
 #define UNIXCB(skb) 	(*(struct unix_skb_parms *)&((skb)->cb))
 
-#define unix_state_lock(s)	spin_lock(&unix_sk(s)->lock)
-#define unix_state_unlock(s)	spin_unlock(&unix_sk(s)->lock)
-#define unix_state_lock_nested(s) \
-				spin_lock_nested(&unix_sk(s)->lock, \
-				SINGLE_DEPTH_NESTING)
-
 /* The AF_UNIX socket */
 struct unix_sock {
 	/* WARNING: sk has to be the first member */
@@ -72,6 +66,20 @@ static inline struct unix_sock *unix_sk(const struct sock *sk)
 	return (struct unix_sock *)sk;
 }
 
+#define unix_state_lock(s)	spin_lock(&unix_sk(s)->lock)
+#define unix_state_unlock(s)	spin_unlock(&unix_sk(s)->lock)
+enum unix_socket_lock_class {
+	U_LOCK_NORMAL,
+	U_LOCK_SECOND,	/* for double locking, see unix_state_double_lock(). */
+	U_LOCK_DIAG, /* used while dumping icons, see sk_diag_dump_icons(). */
+};
+
+static inline void unix_state_lock_nested(struct sock *sk,
+				   enum unix_socket_lock_class subclass)
+{
+	spin_lock_nested(&unix_sk(sk)->lock, subclass);
+}
+
 #define peer_wait peer_wq.wait
 
 long unix_inq_len(struct sock *sk);
diff --git include/net/bluetooth/hci_core.h include/net/bluetooth/hci_core.h
index 8f899ad4a754..bac3d79139b2 100644
--- linux-4.14.336/include/net/bluetooth/hci_core.h
+++ linux-4.14.336/include/net/bluetooth/hci_core.h
@@ -647,7 +647,6 @@ void hci_inquiry_cache_flush(struct hci_dev *hdev);
 /* ----- HCI Connections ----- */
 enum {
 	HCI_CONN_AUTH_PEND,
-	HCI_CONN_REAUTH_PEND,
 	HCI_CONN_ENCRYPT_PEND,
 	HCI_CONN_RSWITCH_PEND,
 	HCI_CONN_MODE_CHANGE_PEND,
diff --git include/net/dst_ops.h include/net/dst_ops.h
index 443863c7b8da..632086b2f644 100644
--- linux-4.14.336/include/net/dst_ops.h
+++ linux-4.14.336/include/net/dst_ops.h
@@ -16,7 +16,7 @@ struct dst_ops {
 	unsigned short		family;
 	unsigned int		gc_thresh;
 
-	int			(*gc)(struct dst_ops *ops);
+	void			(*gc)(struct dst_ops *ops);
 	struct dst_entry *	(*check)(struct dst_entry *, __u32 cookie);
 	unsigned int		(*default_advmss)(const struct dst_entry *);
 	unsigned int		(*mtu)(const struct dst_entry *);
@@ -53,9 +53,11 @@ static inline int dst_entries_get_slow(struct dst_ops *dst)
 	return percpu_counter_sum_positive(&dst->pcpuc_entries);
 }
 
+#define DST_PERCPU_COUNTER_BATCH 32
 static inline void dst_entries_add(struct dst_ops *dst, int val)
 {
-	percpu_counter_add(&dst->pcpuc_entries, val);
+	percpu_counter_add_batch(&dst->pcpuc_entries, val,
+				 DST_PERCPU_COUNTER_BATCH);
 }
 
 static inline int dst_entries_init(struct dst_ops *dst)
diff --git include/net/llc_pdu.h include/net/llc_pdu.h
index 49aa79c7b278..581cd37aa98b 100644
--- linux-4.14.336/include/net/llc_pdu.h
+++ linux-4.14.336/include/net/llc_pdu.h
@@ -262,8 +262,7 @@ static inline void llc_pdu_header_init(struct sk_buff *skb, u8 type,
  */
 static inline void llc_pdu_decode_sa(struct sk_buff *skb, u8 *sa)
 {
-	if (skb->protocol == htons(ETH_P_802_2))
-		memcpy(sa, eth_hdr(skb)->h_source, ETH_ALEN);
+	memcpy(sa, eth_hdr(skb)->h_source, ETH_ALEN);
 }
 
 /**
@@ -275,8 +274,7 @@ static inline void llc_pdu_decode_sa(struct sk_buff *skb, u8 *sa)
  */
 static inline void llc_pdu_decode_da(struct sk_buff *skb, u8 *da)
 {
-	if (skb->protocol == htons(ETH_P_802_2))
-		memcpy(da, eth_hdr(skb)->h_dest, ETH_ALEN);
+	memcpy(da, eth_hdr(skb)->h_dest, ETH_ALEN);
 }
 
 /**
diff --git include/net/netns/ipv6.h include/net/netns/ipv6.h
index c004d051c2d3..290ca18589ee 100644
--- linux-4.14.336/include/net/netns/ipv6.h
+++ linux-4.14.336/include/net/netns/ipv6.h
@@ -64,8 +64,8 @@ struct netns_ipv6 {
 	struct dst_ops		ip6_dst_ops;
 	rwlock_t		fib6_walker_lock;
 	spinlock_t		fib6_gc_lock;
-	unsigned int		 ip6_rt_gc_expire;
-	unsigned long		 ip6_rt_last_gc;
+	atomic_t		ip6_rt_gc_expire;
+	unsigned long		ip6_rt_last_gc;
 #ifdef CONFIG_IPV6_MULTIPLE_TABLES
 	bool			 fib6_has_custom_rules;
 	struct rt6_info         *ip6_prohibit_entry;
diff --git include/uapi/linux/btrfs.h include/uapi/linux/btrfs.h
index 86d2a52b4665..ee7a34c237a5 100644
--- linux-4.14.336/include/uapi/linux/btrfs.h
+++ linux-4.14.336/include/uapi/linux/btrfs.h
@@ -522,6 +522,9 @@ struct btrfs_ioctl_clone_range_args {
  */
 #define BTRFS_DEFRAG_RANGE_COMPRESS 1
 #define BTRFS_DEFRAG_RANGE_START_IO 2
+#define BTRFS_DEFRAG_RANGE_FLAGS_SUPP	(BTRFS_DEFRAG_RANGE_COMPRESS |		\
+					 BTRFS_DEFRAG_RANGE_START_IO)
+
 struct btrfs_ioctl_defrag_range_args {
 	/* start of the defrag operation */
 	__u64 start;
diff --git include/uapi/linux/netfilter/nf_tables.h include/uapi/linux/netfilter/nf_tables.h
index c7bb18ea4962..835e9f345f35 100644
--- linux-4.14.336/include/uapi/linux/netfilter/nf_tables.h
+++ linux-4.14.336/include/uapi/linux/netfilter/nf_tables.h
@@ -229,9 +229,11 @@ enum nft_rule_attributes {
 /**
  * enum nft_rule_compat_flags - nf_tables rule compat flags
  *
+ * @NFT_RULE_COMPAT_F_UNUSED: unused
  * @NFT_RULE_COMPAT_F_INV: invert the check result
  */
 enum nft_rule_compat_flags {
+	NFT_RULE_COMPAT_F_UNUSED = (1 << 0),
 	NFT_RULE_COMPAT_F_INV	= (1 << 1),
 	NFT_RULE_COMPAT_F_MASK	= NFT_RULE_COMPAT_F_INV,
 };
diff --git kernel/audit.c kernel/audit.c
index b694a265533f..819bdf0b6e5f 100644
--- linux-4.14.336/kernel/audit.c
+++ linux-4.14.336/kernel/audit.c
@@ -458,15 +458,19 @@ static int audit_set_failure(u32 state)
  * @pid: auditd PID
  * @portid: auditd netlink portid
  * @net: auditd network namespace pointer
+ * @skb: the netlink command from the audit daemon
+ * @ack: netlink ack flag, cleared if ack'd here
  *
  * Description:
  * This function will obtain and drop network namespace references as
  * necessary.  Returns zero on success, negative values on failure.
  */
-static int auditd_set(struct pid *pid, u32 portid, struct net *net)
+static int auditd_set(struct pid *pid, u32 portid, struct net *net,
+		      struct sk_buff *skb, bool *ack)
 {
 	unsigned long flags;
 	struct auditd_connection *ac_old, *ac_new;
+	struct nlmsghdr *nlh;
 
 	if (!pid || !net)
 		return -EINVAL;
@@ -478,6 +482,13 @@ static int auditd_set(struct pid *pid, u32 portid, struct net *net)
 	ac_new->portid = portid;
 	ac_new->net = get_net(net);
 
+	/* send the ack now to avoid a race with the queue backlog */
+	if (*ack) {
+		nlh = nlmsg_hdr(skb);
+		netlink_ack(skb, nlh, 0, NULL);
+		*ack = false;
+	}
+
 	spin_lock_irqsave(&auditd_conn_lock, flags);
 	ac_old = rcu_dereference_protected(auditd_conn,
 					   lockdep_is_held(&auditd_conn_lock));
@@ -1165,7 +1176,8 @@ static int audit_replace(struct pid *pid)
 	return auditd_send_unicast_skb(skb);
 }
 
-static int audit_receive_msg(struct sk_buff *skb, struct nlmsghdr *nlh)
+static int audit_receive_msg(struct sk_buff *skb, struct nlmsghdr *nlh,
+			     bool *ack)
 {
 	u32			seq;
 	void			*data;
@@ -1257,7 +1269,8 @@ static int audit_receive_msg(struct sk_buff *skb, struct nlmsghdr *nlh)
 				/* register a new auditd connection */
 				err = auditd_set(req_pid,
 						 NETLINK_CB(skb).portid,
-						 sock_net(NETLINK_CB(skb).sk));
+						 sock_net(NETLINK_CB(skb).sk),
+						 skb, ack);
 				if (audit_enabled != AUDIT_OFF)
 					audit_log_config_change("audit_pid",
 								new_pid,
@@ -1490,9 +1503,10 @@ static int audit_receive_msg(struct sk_buff *skb, struct nlmsghdr *nlh)
  * Parse the provided skb and deal with any messages that may be present,
  * malformed skbs are discarded.
  */
-static void audit_receive(struct sk_buff  *skb)
+static void audit_receive(struct sk_buff *skb)
 {
 	struct nlmsghdr *nlh;
+	bool ack;
 	/*
 	 * len MUST be signed for nlmsg_next to be able to dec it below 0
 	 * if the nlmsg_len was not aligned
@@ -1505,9 +1519,12 @@ static void audit_receive(struct sk_buff  *skb)
 
 	mutex_lock(&audit_cmd_mutex);
 	while (nlmsg_ok(nlh, len)) {
-		err = audit_receive_msg(skb, nlh);
-		/* if err or if this message says it wants a response */
-		if (err || (nlh->nlmsg_flags & NLM_F_ACK))
+		ack = nlh->nlmsg_flags & NLM_F_ACK;
+		err = audit_receive_msg(skb, nlh, &ack);
+
+		/* send an ack if the user asked for one and audit_receive_msg
+		 * didn't already do it, or if there was an error. */
+		if (ack || err)
 			netlink_ack(skb, nlh, err, NULL);
 
 		nlh = nlmsg_next(nlh, &len);
diff --git kernel/bpf/arraymap.c kernel/bpf/arraymap.c
index a8f55ea4146b..3291c856cea9 100644
--- linux-4.14.336/kernel/bpf/arraymap.c
+++ linux-4.14.336/kernel/bpf/arraymap.c
@@ -416,7 +416,7 @@ int bpf_fd_array_map_update_elem(struct bpf_map *map, struct file *map_file,
 
 	old_ptr = xchg(array->ptrs + index, new_ptr);
 	if (old_ptr)
-		map->ops->map_fd_put_ptr(old_ptr);
+		map->ops->map_fd_put_ptr(map, old_ptr, true);
 
 	return 0;
 }
@@ -432,7 +432,7 @@ static int fd_array_map_delete_elem(struct bpf_map *map, void *key)
 
 	old_ptr = xchg(array->ptrs + index, NULL);
 	if (old_ptr) {
-		map->ops->map_fd_put_ptr(old_ptr);
+		map->ops->map_fd_put_ptr(map, old_ptr, true);
 		return 0;
 	} else {
 		return -ENOENT;
@@ -456,8 +456,9 @@ static void *prog_fd_array_get_ptr(struct bpf_map *map,
 	return prog;
 }
 
-static void prog_fd_array_put_ptr(void *ptr)
+static void prog_fd_array_put_ptr(struct bpf_map *map, void *ptr, bool need_defer)
 {
+	/* bpf_prog is freed after one RCU or tasks trace grace period */
 	bpf_prog_put(ptr);
 }
 
@@ -543,8 +544,9 @@ err_out:
 	return ee;
 }
 
-static void perf_event_fd_array_put_ptr(void *ptr)
+static void perf_event_fd_array_put_ptr(struct bpf_map *map, void *ptr, bool need_defer)
 {
+	/* bpf_perf_event is freed after one RCU grace period */
 	bpf_event_entry_free_rcu(ptr);
 }
 
@@ -583,7 +585,7 @@ static void *cgroup_fd_array_get_ptr(struct bpf_map *map,
 	return cgroup_get_from_fd(fd);
 }
 
-static void cgroup_fd_array_put_ptr(void *ptr)
+static void cgroup_fd_array_put_ptr(struct bpf_map *map, void *ptr, bool need_defer)
 {
 	/* cgroup_put free cgrp after a rcu grace period */
 	cgroup_put(ptr);
diff --git kernel/bpf/hashtab.c kernel/bpf/hashtab.c
index ecc58137525b..db2c3e019daf 100644
--- linux-4.14.336/kernel/bpf/hashtab.c
+++ linux-4.14.336/kernel/bpf/hashtab.c
@@ -655,7 +655,7 @@ static void htab_put_fd_value(struct bpf_htab *htab, struct htab_elem *l)
 
 	if (map->ops->map_fd_put_ptr) {
 		ptr = fd_htab_map_get_ptr(map, l);
-		map->ops->map_fd_put_ptr(ptr);
+		map->ops->map_fd_put_ptr(map, ptr, true);
 	}
 }
 
@@ -1288,7 +1288,7 @@ static void fd_htab_map_free(struct bpf_map *map)
 		hlist_nulls_for_each_entry_safe(l, n, head, hash_node) {
 			void *ptr = fd_htab_map_get_ptr(map, l);
 
-			map->ops->map_fd_put_ptr(ptr);
+			map->ops->map_fd_put_ptr(map, ptr, false);
 		}
 	}
 
@@ -1329,7 +1329,7 @@ int bpf_fd_htab_map_update_elem(struct bpf_map *map, struct file *map_file,
 
 	ret = htab_map_update_elem(map, key, &ptr, map_flags);
 	if (ret)
-		map->ops->map_fd_put_ptr(ptr);
+		map->ops->map_fd_put_ptr(map, ptr, false);
 
 	return ret;
 }
diff --git kernel/bpf/lpm_trie.c kernel/bpf/lpm_trie.c
index c28c584b734e..ef324c9c1eca 100644
--- linux-4.14.336/kernel/bpf/lpm_trie.c
+++ linux-4.14.336/kernel/bpf/lpm_trie.c
@@ -192,6 +192,9 @@ static void *trie_lookup_elem(struct bpf_map *map, void *_key)
 	struct lpm_trie_node *node, *found = NULL;
 	struct bpf_lpm_trie_key *key = _key;
 
+	if (key->prefixlen > trie->max_prefixlen)
+		return NULL;
+
 	/* Start walking the trie from the root node ... */
 
 	for (node = rcu_dereference(trie->root); node;) {
diff --git kernel/bpf/map_in_map.c kernel/bpf/map_in_map.c
index c0c494b7647b..1878aace6a5c 100644
--- linux-4.14.336/kernel/bpf/map_in_map.c
+++ linux-4.14.336/kernel/bpf/map_in_map.c
@@ -101,7 +101,7 @@ void *bpf_map_fd_get_ptr(struct bpf_map *map,
 	return inner_map;
 }
 
-void bpf_map_fd_put_ptr(void *ptr)
+void bpf_map_fd_put_ptr(struct bpf_map *map, void *ptr, bool need_defer)
 {
 	/* ptr->ops->map_free() has to go through one
 	 * rcu grace period by itself.
diff --git kernel/bpf/map_in_map.h kernel/bpf/map_in_map.h
index 6183db9ec08c..1e652a7bf60e 100644
--- linux-4.14.336/kernel/bpf/map_in_map.h
+++ linux-4.14.336/kernel/bpf/map_in_map.h
@@ -18,7 +18,7 @@ bool bpf_map_meta_equal(const struct bpf_map *meta0,
 			const struct bpf_map *meta1);
 void *bpf_map_fd_get_ptr(struct bpf_map *map, struct file *map_file,
 			 int ufd);
-void bpf_map_fd_put_ptr(void *ptr);
+void bpf_map_fd_put_ptr(struct bpf_map *map, void *ptr, bool need_defer);
 u32 bpf_map_fd_sys_lookup_elem(void *ptr);
 
 #endif
diff --git kernel/debug/kdb/kdb_main.c kernel/debug/kdb/kdb_main.c
index 15d902daeef6..01a4312ede49 100644
--- linux-4.14.336/kernel/debug/kdb/kdb_main.c
+++ linux-4.14.336/kernel/debug/kdb/kdb_main.c
@@ -399,6 +399,13 @@ int kdb_set(int argc, const char **argv)
 	if (argc != 2)
 		return KDB_ARGCOUNT;
 
+	/*
+	 * Censor sensitive variables
+	 */
+	if (strcmp(argv[1], "PROMPT") == 0 &&
+	    !kdb_check_flags(KDB_ENABLE_MEM_READ, kdb_cmd_enabled, false))
+		return KDB_NOPERM;
+
 	/*
 	 * Check for internal variables
 	 */
@@ -1289,14 +1296,9 @@ static int kdb_local(kdb_reason_t reason, int error, struct pt_regs *regs,
 		*(cmd_hist[cmd_head]) = '\0';
 
 do_full_getstr:
-#if defined(CONFIG_SMP)
+		/* PROMPT can only be set if we have MEM_READ permission. */
 		snprintf(kdb_prompt_str, CMD_BUFLEN, kdbgetenv("PROMPT"),
 			 raw_smp_processor_id());
-#else
-		snprintf(kdb_prompt_str, CMD_BUFLEN, kdbgetenv("PROMPT"));
-#endif
-		if (defcmd_in_progress)
-			strncat(kdb_prompt_str, "[defcmd]", CMD_BUFLEN);
 
 		/*
 		 * Fetch command from keyboard
diff --git kernel/power/swap.c kernel/power/swap.c
index 8b37085a6690..b62a56de91d6 100644
--- linux-4.14.336/kernel/power/swap.c
+++ linux-4.14.336/kernel/power/swap.c
@@ -595,11 +595,11 @@ static int crc32_threadfn(void *data)
 	unsigned i;
 
 	while (1) {
-		wait_event(d->go, atomic_read(&d->ready) ||
+		wait_event(d->go, atomic_read_acquire(&d->ready) ||
 		                  kthread_should_stop());
 		if (kthread_should_stop()) {
 			d->thr = NULL;
-			atomic_set(&d->stop, 1);
+			atomic_set_release(&d->stop, 1);
 			wake_up(&d->done);
 			break;
 		}
@@ -608,7 +608,7 @@ static int crc32_threadfn(void *data)
 		for (i = 0; i < d->run_threads; i++)
 			*d->crc32 = crc32_le(*d->crc32,
 			                     d->unc[i], *d->unc_len[i]);
-		atomic_set(&d->stop, 1);
+		atomic_set_release(&d->stop, 1);
 		wake_up(&d->done);
 	}
 	return 0;
@@ -638,12 +638,12 @@ static int lzo_compress_threadfn(void *data)
 	struct cmp_data *d = data;
 
 	while (1) {
-		wait_event(d->go, atomic_read(&d->ready) ||
+		wait_event(d->go, atomic_read_acquire(&d->ready) ||
 		                  kthread_should_stop());
 		if (kthread_should_stop()) {
 			d->thr = NULL;
 			d->ret = -1;
-			atomic_set(&d->stop, 1);
+			atomic_set_release(&d->stop, 1);
 			wake_up(&d->done);
 			break;
 		}
@@ -652,7 +652,7 @@ static int lzo_compress_threadfn(void *data)
 		d->ret = lzo1x_1_compress(d->unc, d->unc_len,
 		                          d->cmp + LZO_HEADER, &d->cmp_len,
 		                          d->wrk);
-		atomic_set(&d->stop, 1);
+		atomic_set_release(&d->stop, 1);
 		wake_up(&d->done);
 	}
 	return 0;
@@ -794,7 +794,7 @@ static int save_image_lzo(struct swap_map_handle *handle,
 
 			data[thr].unc_len = off;
 
-			atomic_set(&data[thr].ready, 1);
+			atomic_set_release(&data[thr].ready, 1);
 			wake_up(&data[thr].go);
 		}
 
@@ -802,12 +802,12 @@ static int save_image_lzo(struct swap_map_handle *handle,
 			break;
 
 		crc->run_threads = thr;
-		atomic_set(&crc->ready, 1);
+		atomic_set_release(&crc->ready, 1);
 		wake_up(&crc->go);
 
 		for (run_threads = thr, thr = 0; thr < run_threads; thr++) {
 			wait_event(data[thr].done,
-			           atomic_read(&data[thr].stop));
+				atomic_read_acquire(&data[thr].stop));
 			atomic_set(&data[thr].stop, 0);
 
 			ret = data[thr].ret;
@@ -847,7 +847,7 @@ static int save_image_lzo(struct swap_map_handle *handle,
 			}
 		}
 
-		wait_event(crc->done, atomic_read(&crc->stop));
+		wait_event(crc->done, atomic_read_acquire(&crc->stop));
 		atomic_set(&crc->stop, 0);
 	}
 
@@ -1129,12 +1129,12 @@ static int lzo_decompress_threadfn(void *data)
 	struct dec_data *d = data;
 
 	while (1) {
-		wait_event(d->go, atomic_read(&d->ready) ||
+		wait_event(d->go, atomic_read_acquire(&d->ready) ||
 		                  kthread_should_stop());
 		if (kthread_should_stop()) {
 			d->thr = NULL;
 			d->ret = -1;
-			atomic_set(&d->stop, 1);
+			atomic_set_release(&d->stop, 1);
 			wake_up(&d->done);
 			break;
 		}
@@ -1147,7 +1147,7 @@ static int lzo_decompress_threadfn(void *data)
 			flush_icache_range((unsigned long)d->unc,
 					   (unsigned long)d->unc + d->unc_len);
 
-		atomic_set(&d->stop, 1);
+		atomic_set_release(&d->stop, 1);
 		wake_up(&d->done);
 	}
 	return 0;
@@ -1338,7 +1338,7 @@ static int load_image_lzo(struct swap_map_handle *handle,
 		}
 
 		if (crc->run_threads) {
-			wait_event(crc->done, atomic_read(&crc->stop));
+			wait_event(crc->done, atomic_read_acquire(&crc->stop));
 			atomic_set(&crc->stop, 0);
 			crc->run_threads = 0;
 		}
@@ -1375,7 +1375,7 @@ static int load_image_lzo(struct swap_map_handle *handle,
 					pg = 0;
 			}
 
-			atomic_set(&data[thr].ready, 1);
+			atomic_set_release(&data[thr].ready, 1);
 			wake_up(&data[thr].go);
 		}
 
@@ -1394,7 +1394,7 @@ static int load_image_lzo(struct swap_map_handle *handle,
 
 		for (run_threads = thr, thr = 0; thr < run_threads; thr++) {
 			wait_event(data[thr].done,
-			           atomic_read(&data[thr].stop));
+				atomic_read_acquire(&data[thr].stop));
 			atomic_set(&data[thr].stop, 0);
 
 			ret = data[thr].ret;
@@ -1429,7 +1429,7 @@ static int load_image_lzo(struct swap_map_handle *handle,
 				ret = snapshot_write_next(snapshot);
 				if (ret <= 0) {
 					crc->run_threads = thr + 1;
-					atomic_set(&crc->ready, 1);
+					atomic_set_release(&crc->ready, 1);
 					wake_up(&crc->go);
 					goto out_finish;
 				}
@@ -1437,13 +1437,13 @@ static int load_image_lzo(struct swap_map_handle *handle,
 		}
 
 		crc->run_threads = thr;
-		atomic_set(&crc->ready, 1);
+		atomic_set_release(&crc->ready, 1);
 		wake_up(&crc->go);
 	}
 
 out_finish:
 	if (crc->run_threads) {
-		wait_event(crc->done, atomic_read(&crc->stop));
+		wait_event(crc->done, atomic_read_acquire(&crc->stop));
 		atomic_set(&crc->stop, 0);
 	}
 	stop = ktime_get();
diff --git kernel/sched/membarrier.c kernel/sched/membarrier.c
index 9bcbacba82a8..d936a130814e 100644
--- linux-4.14.336/kernel/sched/membarrier.c
+++ linux-4.14.336/kernel/sched/membarrier.c
@@ -30,6 +30,8 @@
 	(MEMBARRIER_CMD_SHARED | MEMBARRIER_CMD_PRIVATE_EXPEDITED	\
 	| MEMBARRIER_CMD_REGISTER_PRIVATE_EXPEDITED)
 
+static DEFINE_MUTEX(membarrier_ipi_mutex);
+
 static void ipi_mb(void *info)
 {
 	smp_mb();	/* IPIs should be serializing but paranoid. */
@@ -64,6 +66,7 @@ static int membarrier_private_expedited(void)
 		fallback = true;
 	}
 
+	mutex_lock(&membarrier_ipi_mutex);
 	cpus_read_lock();
 	for_each_online_cpu(cpu) {
 		struct task_struct *p;
@@ -102,6 +105,7 @@ static int membarrier_private_expedited(void)
 	 * rq->curr modification in scheduler.
 	 */
 	smp_mb();	/* exit from system call is not a mb */
+	mutex_unlock(&membarrier_ipi_mutex);
 	return 0;
 }
 
diff --git kernel/sched/rt.c kernel/sched/rt.c
index c093bb0f52eb..85cc7ab4f38d 100644
--- linux-4.14.336/kernel/sched/rt.c
+++ linux-4.14.336/kernel/sched/rt.c
@@ -10,7 +10,7 @@
 #include <linux/irq_work.h>
 
 int sched_rr_timeslice = RR_TIMESLICE;
-int sysctl_sched_rr_timeslice = (MSEC_PER_SEC / HZ) * RR_TIMESLICE;
+int sysctl_sched_rr_timeslice = (MSEC_PER_SEC * RR_TIMESLICE) / HZ;
 
 static int do_sched_rt_period_timer(struct rt_bandwidth *rt_b, int overrun);
 
@@ -2626,9 +2626,6 @@ static int sched_rt_global_constraints(void)
 
 static int sched_rt_global_validate(void)
 {
-	if (sysctl_sched_rt_period <= 0)
-		return -EINVAL;
-
 	if ((sysctl_sched_rt_runtime != RUNTIME_INF) &&
 		(sysctl_sched_rt_runtime > sysctl_sched_rt_period))
 		return -EINVAL;
@@ -2658,7 +2655,7 @@ int sched_rt_handler(struct ctl_table *table, int write,
 	old_period = sysctl_sched_rt_period;
 	old_runtime = sysctl_sched_rt_runtime;
 
-	ret = proc_dointvec(table, write, buffer, lenp, ppos);
+	ret = proc_dointvec_minmax(table, write, buffer, lenp, ppos);
 
 	if (!ret && write) {
 		ret = sched_rt_global_validate();
@@ -2703,6 +2700,9 @@ int sched_rr_handler(struct ctl_table *table, int write,
 		sched_rr_timeslice =
 			sysctl_sched_rr_timeslice <= 0 ? RR_TIMESLICE :
 			msecs_to_jiffies(sysctl_sched_rr_timeslice);
+
+		if (sysctl_sched_rr_timeslice <= 0)
+			sysctl_sched_rr_timeslice = jiffies_to_msecs(RR_TIMESLICE);
 	}
 	mutex_unlock(&mutex);
 	return ret;
diff --git kernel/sysctl.c kernel/sysctl.c
index de4a197570b1..5bee2eb28ff6 100644
--- linux-4.14.336/kernel/sysctl.c
+++ linux-4.14.336/kernel/sysctl.c
@@ -124,6 +124,7 @@ static int zero;
 static int __maybe_unused one = 1;
 static int __maybe_unused two = 2;
 static int __maybe_unused four = 4;
+static int int_max = INT_MAX;
 static unsigned long zero_ul;
 static unsigned long one_ul = 1;
 static unsigned long long_max = LONG_MAX;
@@ -460,6 +461,8 @@ static struct ctl_table kern_table[] = {
 		.maxlen		= sizeof(unsigned int),
 		.mode		= 0644,
 		.proc_handler	= sched_rt_handler,
+		.extra1		= &one,
+		.extra2		= &int_max,
 	},
 	{
 		.procname	= "sched_rt_runtime_us",
@@ -467,6 +470,8 @@ static struct ctl_table kern_table[] = {
 		.maxlen		= sizeof(int),
 		.mode		= 0644,
 		.proc_handler	= sched_rt_handler,
+		.extra1		= &neg_one,
+		.extra2		= &int_max,
 	},
 	{
 		.procname	= "sched_rr_timeslice_ms",
diff --git kernel/time/tick-sched.c kernel/time/tick-sched.c
index 3c7b400512eb..387de1b6dd93 100644
--- linux-4.14.336/kernel/time/tick-sched.c
+++ linux-4.14.336/kernel/time/tick-sched.c
@@ -1278,13 +1278,23 @@ void tick_setup_sched_timer(void)
 void tick_cancel_sched_timer(int cpu)
 {
 	struct tick_sched *ts = &per_cpu(tick_cpu_sched, cpu);
+	ktime_t idle_sleeptime, iowait_sleeptime;
+	unsigned long idle_calls, idle_sleeps;
 
 # ifdef CONFIG_HIGH_RES_TIMERS
 	if (ts->sched_timer.base)
 		hrtimer_cancel(&ts->sched_timer);
 # endif
 
+	idle_sleeptime = ts->idle_sleeptime;
+	iowait_sleeptime = ts->iowait_sleeptime;
+	idle_calls = ts->idle_calls;
+	idle_sleeps = ts->idle_sleeps;
 	memset(ts, 0, sizeof(*ts));
+	ts->idle_sleeptime = idle_sleeptime;
+	ts->iowait_sleeptime = iowait_sleeptime;
+	ts->idle_calls = idle_calls;
+	ts->idle_sleeps = idle_sleeps;
 }
 #endif
 
diff --git kernel/trace/ring_buffer.c kernel/trace/ring_buffer.c
index 3fc09d765f2a..8c09e8ca1561 100644
--- linux-4.14.336/kernel/trace/ring_buffer.c
+++ linux-4.14.336/kernel/trace/ring_buffer.c
@@ -2776,6 +2776,12 @@ rb_reserve_next_event(struct ring_buffer *buffer,
 	int nr_loops = 0;
 	u64 diff;
 
+	/* ring buffer does cmpxchg, make sure it is safe in NMI context */
+	if (!IS_ENABLED(CONFIG_ARCH_HAVE_NMI_SAFE_CMPXCHG) &&
+	    (unlikely(in_nmi()))) {
+		return NULL;
+	}
+
 	rb_start_commit(cpu_buffer);
 
 #ifdef CONFIG_RING_BUFFER_ALLOW_SWAP
diff --git kernel/trace/trace.c kernel/trace/trace.c
index c5fe020336be..755d6146c738 100644
--- linux-4.14.336/kernel/trace/trace.c
+++ linux-4.14.336/kernel/trace/trace.c
@@ -3826,7 +3826,11 @@ static int s_show(struct seq_file *m, void *v)
 		iter->leftover = ret;
 
 	} else {
-		print_trace_line(iter);
+		ret = print_trace_line(iter);
+		if (ret == TRACE_TYPE_PARTIAL_LINE) {
+			iter->seq.full = 0;
+			trace_seq_puts(&iter->seq, "[LINE TOO BIG]\n");
+		}
 		ret = trace_print_seq(m, &iter->seq);
 		/*
 		 * If we overflow the seq_file buffer, then it will
diff --git kernel/trace/trace_events_trigger.c kernel/trace/trace_events_trigger.c
index 40c1a2dd48f0..871ea0fa78bb 100644
--- linux-4.14.336/kernel/trace/trace_events_trigger.c
+++ linux-4.14.336/kernel/trace/trace_events_trigger.c
@@ -1127,8 +1127,10 @@ register_snapshot_trigger(char *glob, struct event_trigger_ops *ops,
 			  struct event_trigger_data *data,
 			  struct trace_event_file *file)
 {
-	if (tracing_alloc_snapshot_instance(file->tr) != 0)
-		return 0;
+	int ret = tracing_alloc_snapshot_instance(file->tr);
+
+	if (ret < 0)
+		return ret;
 
 	return register_trigger(glob, ops, data, file);
 }
diff --git kernel/trace/trace_output.c kernel/trace/trace_output.c
index e3ab66e6fd85..3ca9ddfef2b8 100644
--- linux-4.14.336/kernel/trace/trace_output.c
+++ linux-4.14.336/kernel/trace/trace_output.c
@@ -1319,11 +1319,12 @@ static enum print_line_t trace_print_print(struct trace_iterator *iter,
 {
 	struct print_entry *field;
 	struct trace_seq *s = &iter->seq;
+	int max = iter->ent_size - offsetof(struct print_entry, buf);
 
 	trace_assign_type(field, iter->ent);
 
 	seq_print_ip_sym(s, field->ip, flags);
-	trace_seq_printf(s, ": %s", field->buf);
+	trace_seq_printf(s, ": %.*s", max, field->buf);
 
 	return trace_handle_return(s);
 }
@@ -1332,10 +1333,11 @@ static enum print_line_t trace_print_raw(struct trace_iterator *iter, int flags,
 					 struct trace_event *event)
 {
 	struct print_entry *field;
+	int max = iter->ent_size - offsetof(struct print_entry, buf);
 
 	trace_assign_type(field, iter->ent);
 
-	trace_seq_printf(&iter->seq, "# %lx %s", field->ip, field->buf);
+	trace_seq_printf(&iter->seq, "# %lx %.*s", field->ip, max, field->buf);
 
 	return trace_handle_return(&iter->seq);
 }
diff --git mm/memcontrol.c mm/memcontrol.c
index 22d13c98e274..e6a351e69ac3 100644
--- linux-4.14.336/mm/memcontrol.c
+++ linux-4.14.336/mm/memcontrol.c
@@ -1747,6 +1747,9 @@ static void drain_stock(struct memcg_stock_pcp *stock)
 {
 	struct mem_cgroup *old = stock->cached;
 
+	if (!old)
+		return;
+
 	if (stock->nr_pages) {
 		page_counter_uncharge(&old->memory, stock->nr_pages);
 		if (do_memsw_account())
@@ -1754,6 +1757,8 @@ static void drain_stock(struct memcg_stock_pcp *stock)
 		css_put_many(&old->css, stock->nr_pages);
 		stock->nr_pages = 0;
 	}
+
+	css_put(&old->css);
 	stock->cached = NULL;
 }
 
@@ -1789,6 +1794,7 @@ static void refill_stock(struct mem_cgroup *memcg, unsigned int nr_pages)
 	stock = this_cpu_ptr(&memcg_stock);
 	if (stock->cached != memcg) { /* reset if necessary */
 		drain_stock(stock);
+		css_get(&memcg->css);
 		stock->cached = memcg;
 	}
 	stock->nr_pages += nr_pages;
@@ -1820,21 +1826,22 @@ static void drain_all_stock(struct mem_cgroup *root_memcg)
 	for_each_online_cpu(cpu) {
 		struct memcg_stock_pcp *stock = &per_cpu(memcg_stock, cpu);
 		struct mem_cgroup *memcg;
+		bool flush = false;
 
+		rcu_read_lock();
 		memcg = stock->cached;
-		if (!memcg || !stock->nr_pages || !css_tryget(&memcg->css))
-			continue;
-		if (!mem_cgroup_is_descendant(memcg, root_memcg)) {
-			css_put(&memcg->css);
-			continue;
-		}
-		if (!test_and_set_bit(FLUSHING_CACHED_CHARGE, &stock->flags)) {
+		if (memcg && stock->nr_pages &&
+		    mem_cgroup_is_descendant(memcg, root_memcg))
+			flush = true;
+		rcu_read_unlock();
+
+		if (flush &&
+		    !test_and_set_bit(FLUSHING_CACHED_CHARGE, &stock->flags)) {
 			if (cpu == curcpu)
 				drain_local_stock(&stock->work);
 			else
 				schedule_work_on(cpu, &stock->work);
 		}
-		css_put(&memcg->css);
 	}
 	put_cpu();
 	mutex_unlock(&percpu_charge_mutex);
diff --git mm/memory-failure.c mm/memory-failure.c
index e7827b9e6397..e179ffa15026 100644
--- linux-4.14.336/mm/memory-failure.c
+++ linux-4.14.336/mm/memory-failure.c
@@ -952,7 +952,7 @@ static bool hwpoison_user_mappings(struct page *p, unsigned long pfn,
 	 * This check implies we don't kill processes if their pages
 	 * are in the swap cache early. Those are always late kills.
 	 */
-	if (!page_mapped(hpage))
+	if (!page_mapped(p))
 		return true;
 
 	if (PageKsm(p)) {
@@ -996,10 +996,10 @@ static bool hwpoison_user_mappings(struct page *p, unsigned long pfn,
 	if (kill)
 		collect_procs(hpage, &tokill, flags & MF_ACTION_REQUIRED);
 
-	unmap_success = try_to_unmap(hpage, ttu);
+	unmap_success = try_to_unmap(p, ttu);
 	if (!unmap_success)
 		pr_err("Memory failure: %#lx: failed to unmap page (mapcount=%d)\n",
-		       pfn, page_mapcount(hpage));
+		       pfn, page_mapcount(p));
 
 	/*
 	 * try_to_unmap() might put mlocked page in lru cache, so call
diff --git mm/memory.c mm/memory.c
index 0136af15ba18..aa0c46997ce8 100644
--- linux-4.14.336/mm/memory.c
+++ linux-4.14.336/mm/memory.c
@@ -2958,8 +2958,8 @@ void unmap_mapping_range(struct address_space *mapping,
 		loff_t const holebegin, loff_t const holelen, int even_cows)
 {
 	struct zap_details details = { };
-	pgoff_t hba = holebegin >> PAGE_SHIFT;
-	pgoff_t hlen = (holelen + PAGE_SIZE - 1) >> PAGE_SHIFT;
+	pgoff_t hba = (pgoff_t)(holebegin) >> PAGE_SHIFT;
+	pgoff_t hlen = ((pgoff_t)(holelen) + PAGE_SIZE - 1) >> PAGE_SHIFT;
 
 	/* Check for overflow. */
 	if (sizeof(holelen) > sizeof(hlen)) {
diff --git mm/page-writeback.c mm/page-writeback.c
index 29f9980c13ac..2193086847b3 100644
--- linux-4.14.336/mm/page-writeback.c
+++ linux-4.14.336/mm/page-writeback.c
@@ -1531,7 +1531,7 @@ static inline void wb_dirty_limits(struct dirty_throttle_control *dtc)
 	 */
 	dtc->wb_thresh = __wb_calc_thresh(dtc);
 	dtc->wb_bg_thresh = dtc->thresh ?
-		div_u64((u64)dtc->wb_thresh * dtc->bg_thresh, dtc->thresh) : 0;
+		div64_u64(dtc->wb_thresh * dtc->bg_thresh, dtc->thresh) : 0;
 
 	/*
 	 * In order to avoid the stacked BDI deadlock we need
diff --git net/8021q/vlan_netlink.c net/8021q/vlan_netlink.c
index fdf39dd5e755..aad09715ac49 100644
--- linux-4.14.336/net/8021q/vlan_netlink.c
+++ linux-4.14.336/net/8021q/vlan_netlink.c
@@ -105,12 +105,16 @@ static int vlan_changelink(struct net_device *dev, struct nlattr *tb[],
 	}
 	if (data[IFLA_VLAN_INGRESS_QOS]) {
 		nla_for_each_nested(attr, data[IFLA_VLAN_INGRESS_QOS], rem) {
+			if (nla_type(attr) != IFLA_VLAN_QOS_MAPPING)
+				continue;
 			m = nla_data(attr);
 			vlan_dev_set_ingress_priority(dev, m->to, m->from);
 		}
 	}
 	if (data[IFLA_VLAN_EGRESS_QOS]) {
 		nla_for_each_nested(attr, data[IFLA_VLAN_EGRESS_QOS], rem) {
+			if (nla_type(attr) != IFLA_VLAN_QOS_MAPPING)
+				continue;
 			m = nla_data(attr);
 			err = vlan_dev_set_egress_priority(dev, m->from, m->to);
 			if (err)
diff --git net/bluetooth/hci_conn.c net/bluetooth/hci_conn.c
index ce4bbc426946..017abffccc15 100644
--- linux-4.14.336/net/bluetooth/hci_conn.c
+++ linux-4.14.336/net/bluetooth/hci_conn.c
@@ -1221,12 +1221,10 @@ static int hci_conn_auth(struct hci_conn *conn, __u8 sec_level, __u8 auth_type)
 		hci_send_cmd(conn->hdev, HCI_OP_AUTH_REQUESTED,
 			     sizeof(cp), &cp);
 
-		/* If we're already encrypted set the REAUTH_PEND flag,
-		 * otherwise set the ENCRYPT_PEND.
+		/* Set the ENCRYPT_PEND to trigger encryption after
+		 * authentication.
 		 */
-		if (test_bit(HCI_CONN_ENCRYPT, &conn->flags))
-			set_bit(HCI_CONN_REAUTH_PEND, &conn->flags);
-		else
+		if (!test_bit(HCI_CONN_ENCRYPT, &conn->flags))
 			set_bit(HCI_CONN_ENCRYPT_PEND, &conn->flags);
 	}
 
diff --git net/bluetooth/hci_core.c net/bluetooth/hci_core.c
index 2bf0bdee7186..8faecd94bf5a 100644
--- linux-4.14.336/net/bluetooth/hci_core.c
+++ linux-4.14.336/net/bluetooth/hci_core.c
@@ -2167,6 +2167,7 @@ static void hci_error_reset(struct work_struct *work)
 {
 	struct hci_dev *hdev = container_of(work, struct hci_dev, error_reset);
 
+	hci_dev_hold(hdev);
 	BT_DBG("%s", hdev->name);
 
 	if (hdev->hw_error)
@@ -2175,10 +2176,10 @@ static void hci_error_reset(struct work_struct *work)
 		BT_ERR("%s hardware error 0x%2.2x", hdev->name,
 		       hdev->hw_error_code);
 
-	if (hci_dev_do_close(hdev))
-		return;
+	if (!hci_dev_do_close(hdev))
+		hci_dev_do_open(hdev);
 
-	hci_dev_do_open(hdev);
+	hci_dev_put(hdev);
 }
 
 void hci_uuids_clear(struct hci_dev *hdev)
diff --git net/bluetooth/hci_event.c net/bluetooth/hci_event.c
index 07605fcc9091..987ba33375c9 100644
--- linux-4.14.336/net/bluetooth/hci_event.c
+++ linux-4.14.336/net/bluetooth/hci_event.c
@@ -2459,14 +2459,8 @@ static void hci_auth_complete_evt(struct hci_dev *hdev, struct sk_buff *skb)
 
 	if (!ev->status) {
 		clear_bit(HCI_CONN_AUTH_FAILURE, &conn->flags);
-
-		if (!hci_conn_ssp_enabled(conn) &&
-		    test_bit(HCI_CONN_REAUTH_PEND, &conn->flags)) {
-			BT_INFO("re-auth of legacy device is not possible.");
-		} else {
-			set_bit(HCI_CONN_AUTH, &conn->flags);
-			conn->sec_level = conn->pending_sec_level;
-		}
+		set_bit(HCI_CONN_AUTH, &conn->flags);
+		conn->sec_level = conn->pending_sec_level;
 	} else {
 		if (ev->status == HCI_ERROR_PIN_OR_KEY_MISSING)
 			set_bit(HCI_CONN_AUTH_FAILURE, &conn->flags);
@@ -2475,7 +2469,6 @@ static void hci_auth_complete_evt(struct hci_dev *hdev, struct sk_buff *skb)
 	}
 
 	clear_bit(HCI_CONN_AUTH_PEND, &conn->flags);
-	clear_bit(HCI_CONN_REAUTH_PEND, &conn->flags);
 
 	if (conn->state == BT_CONFIG) {
 		if (!ev->status && hci_conn_ssp_enabled(conn)) {
@@ -4022,9 +4015,12 @@ static void hci_io_capa_request_evt(struct hci_dev *hdev, struct sk_buff *skb)
 	hci_dev_lock(hdev);
 
 	conn = hci_conn_hash_lookup_ba(hdev, ACL_LINK, &ev->bdaddr);
-	if (!conn || !hci_conn_ssp_enabled(conn))
+	if (!conn || !hci_dev_test_flag(hdev, HCI_SSP_ENABLED))
 		goto unlock;
 
+	/* Assume remote supports SSP since it has triggered this event */
+	set_bit(HCI_CONN_SSP_ENABLED, &conn->flags);
+
 	hci_conn_hold(conn);
 
 	if (!hci_dev_test_flag(hdev, HCI_MGMT))
@@ -5148,6 +5144,10 @@ static void hci_le_remote_conn_param_req_evt(struct hci_dev *hdev,
 		return send_conn_param_neg_reply(hdev, handle,
 						 HCI_ERROR_UNKNOWN_CONN_ID);
 
+	if (max > hcon->le_conn_max_interval)
+		return send_conn_param_neg_reply(hdev, handle,
+						 HCI_ERROR_INVALID_LL_PARAMS);
+
 	if (hci_check_conn_params(min, max, latency, timeout))
 		return send_conn_param_neg_reply(hdev, handle,
 						 HCI_ERROR_INVALID_LL_PARAMS);
diff --git net/bluetooth/l2cap_core.c net/bluetooth/l2cap_core.c
index 6bae68b5d439..e52657f05f78 100644
--- linux-4.14.336/net/bluetooth/l2cap_core.c
+++ linux-4.14.336/net/bluetooth/l2cap_core.c
@@ -5313,7 +5313,13 @@ static inline int l2cap_conn_param_update_req(struct l2cap_conn *conn,
 
 	memset(&rsp, 0, sizeof(rsp));
 
-	err = hci_check_conn_params(min, max, latency, to_multiplier);
+	if (max > hcon->le_conn_max_interval) {
+		BT_DBG("requested connection interval exceeds current bounds.");
+		err = -EINVAL;
+	} else {
+		err = hci_check_conn_params(min, max, latency, to_multiplier);
+	}
+
 	if (err)
 		rsp.result = cpu_to_le16(L2CAP_CONN_PARAM_REJECTED);
 	else
diff --git net/core/dst.c net/core/dst.c
index a6c47da7d0f8..2d121958d5b0 100644
--- linux-4.14.336/net/core/dst.c
+++ linux-4.14.336/net/core/dst.c
@@ -99,10 +99,10 @@ void *dst_alloc(struct dst_ops *ops, struct net_device *dev,
 {
 	struct dst_entry *dst;
 
-	if (ops->gc && dst_entries_get_fast(ops) > ops->gc_thresh) {
-		if (ops->gc(ops))
-			return NULL;
-	}
+	if (ops->gc &&
+	    !(flags & DST_NOCOUNT) &&
+	    dst_entries_get_fast(ops) > ops->gc_thresh)
+		ops->gc(ops);
 
 	dst = kmem_cache_alloc(ops->kmem_cachep, GFP_ATOMIC);
 	if (!dst)
diff --git net/ipv4/af_inet.c net/ipv4/af_inet.c
index 1eee002b12d2..5feb84c43564 100644
--- linux-4.14.336/net/ipv4/af_inet.c
+++ linux-4.14.336/net/ipv4/af_inet.c
@@ -1480,10 +1480,12 @@ EXPORT_SYMBOL(inet_current_timestamp);
 
 int inet_recv_error(struct sock *sk, struct msghdr *msg, int len, int *addr_len)
 {
-	if (sk->sk_family == AF_INET)
+	unsigned int family = READ_ONCE(sk->sk_family);
+
+	if (family == AF_INET)
 		return ip_recv_error(sk, msg, len, addr_len);
 #if IS_ENABLED(CONFIG_IPV6)
-	if (sk->sk_family == AF_INET6)
+	if (family == AF_INET6)
 		return pingv6_ops.ipv6_recv_error(sk, msg, len, addr_len);
 #endif
 	return -EINVAL;
diff --git net/ipv4/ip_output.c net/ipv4/ip_output.c
index c242c412dabc..947655e4ab5c 100644
--- linux-4.14.336/net/ipv4/ip_output.c
+++ linux-4.14.336/net/ipv4/ip_output.c
@@ -1114,6 +1114,16 @@ static int ip_setup_cork(struct sock *sk, struct inet_cork *cork,
 	struct ip_options_rcu *opt;
 	struct rtable *rt;
 
+	rt = *rtp;
+	if (unlikely(!rt))
+		return -EFAULT;
+
+	cork->fragsize = ip_sk_use_pmtu(sk) ?
+			 dst_mtu(&rt->dst) : READ_ONCE(rt->dst.dev->mtu);
+
+	if (!inetdev_valid_mtu(cork->fragsize))
+		return -ENETUNREACH;
+
 	/*
 	 * setup for corking.
 	 */
@@ -1129,15 +1139,6 @@ static int ip_setup_cork(struct sock *sk, struct inet_cork *cork,
 		cork->flags |= IPCORK_OPT;
 		cork->addr = ipc->addr;
 	}
-	rt = *rtp;
-	if (unlikely(!rt))
-		return -EFAULT;
-
-	cork->fragsize = ip_sk_use_pmtu(sk) ?
-			 dst_mtu(&rt->dst) : READ_ONCE(rt->dst.dev->mtu);
-
-	if (!inetdev_valid_mtu(cork->fragsize))
-		return -ENETUNREACH;
 
 	cork->dst = &rt->dst;
 	/* We stole this route, caller should not release it. */
diff --git net/ipv4/tcp.c net/ipv4/tcp.c
index 0859f968c9b2..eb5458cbdc1c 100644
--- linux-4.14.336/net/ipv4/tcp.c
+++ linux-4.14.336/net/ipv4/tcp.c
@@ -701,6 +701,7 @@ static void tcp_push(struct sock *sk, int flags, int mss_now,
 		if (!test_bit(TSQ_THROTTLED, &sk->sk_tsq_flags)) {
 			NET_INC_STATS(sock_net(sk), LINUX_MIB_TCPAUTOCORKING);
 			set_bit(TSQ_THROTTLED, &sk->sk_tsq_flags);
+			smp_mb__after_atomic();
 		}
 		/* It is possible TX completion already happened
 		 * before we set TSQ_THROTTLED.
diff --git net/ipv6/addrconf_core.c net/ipv6/addrconf_core.c
index e6c5a4b5921d..f5a267972c57 100644
--- linux-4.14.336/net/ipv6/addrconf_core.c
+++ linux-4.14.336/net/ipv6/addrconf_core.c
@@ -140,19 +140,26 @@ const struct ipv6_stub *ipv6_stub __read_mostly = &(struct ipv6_stub) {
 EXPORT_SYMBOL_GPL(ipv6_stub);
 
 /* IPv6 Wildcard Address and Loopback Address defined by RFC2553 */
-const struct in6_addr in6addr_loopback = IN6ADDR_LOOPBACK_INIT;
+const struct in6_addr in6addr_loopback __aligned(BITS_PER_LONG/8)
+	= IN6ADDR_LOOPBACK_INIT;
 EXPORT_SYMBOL(in6addr_loopback);
-const struct in6_addr in6addr_any = IN6ADDR_ANY_INIT;
+const struct in6_addr in6addr_any __aligned(BITS_PER_LONG/8)
+	= IN6ADDR_ANY_INIT;
 EXPORT_SYMBOL(in6addr_any);
-const struct in6_addr in6addr_linklocal_allnodes = IN6ADDR_LINKLOCAL_ALLNODES_INIT;
+const struct in6_addr in6addr_linklocal_allnodes __aligned(BITS_PER_LONG/8)
+	= IN6ADDR_LINKLOCAL_ALLNODES_INIT;
 EXPORT_SYMBOL(in6addr_linklocal_allnodes);
-const struct in6_addr in6addr_linklocal_allrouters = IN6ADDR_LINKLOCAL_ALLROUTERS_INIT;
+const struct in6_addr in6addr_linklocal_allrouters __aligned(BITS_PER_LONG/8)
+	= IN6ADDR_LINKLOCAL_ALLROUTERS_INIT;
 EXPORT_SYMBOL(in6addr_linklocal_allrouters);
-const struct in6_addr in6addr_interfacelocal_allnodes = IN6ADDR_INTERFACELOCAL_ALLNODES_INIT;
+const struct in6_addr in6addr_interfacelocal_allnodes __aligned(BITS_PER_LONG/8)
+	= IN6ADDR_INTERFACELOCAL_ALLNODES_INIT;
 EXPORT_SYMBOL(in6addr_interfacelocal_allnodes);
-const struct in6_addr in6addr_interfacelocal_allrouters = IN6ADDR_INTERFACELOCAL_ALLROUTERS_INIT;
+const struct in6_addr in6addr_interfacelocal_allrouters __aligned(BITS_PER_LONG/8)
+	= IN6ADDR_INTERFACELOCAL_ALLROUTERS_INIT;
 EXPORT_SYMBOL(in6addr_interfacelocal_allrouters);
-const struct in6_addr in6addr_sitelocal_allrouters = IN6ADDR_SITELOCAL_ALLROUTERS_INIT;
+const struct in6_addr in6addr_sitelocal_allrouters __aligned(BITS_PER_LONG/8)
+	= IN6ADDR_SITELOCAL_ALLROUTERS_INIT;
 EXPORT_SYMBOL(in6addr_sitelocal_allrouters);
 
 static void snmp6_free_dev(struct inet6_dev *idev)
diff --git net/ipv6/ip6_tunnel.c net/ipv6/ip6_tunnel.c
index d59bf0da2912..cfe3a72a1159 100644
--- linux-4.14.336/net/ipv6/ip6_tunnel.c
+++ linux-4.14.336/net/ipv6/ip6_tunnel.c
@@ -404,7 +404,7 @@ __u16 ip6_tnl_parse_tlv_enc_lim(struct sk_buff *skb, __u8 *raw)
 	const struct ipv6hdr *ipv6h = (const struct ipv6hdr *)raw;
 	unsigned int nhoff = raw - skb->data;
 	unsigned int off = nhoff + sizeof(*ipv6h);
-	u8 next, nexthdr = ipv6h->nexthdr;
+	u8 nexthdr = ipv6h->nexthdr;
 
 	while (ipv6_ext_hdr(nexthdr) && nexthdr != NEXTHDR_NONE) {
 		struct ipv6_opt_hdr *hdr;
@@ -415,25 +415,25 @@ __u16 ip6_tnl_parse_tlv_enc_lim(struct sk_buff *skb, __u8 *raw)
 
 		hdr = (struct ipv6_opt_hdr *)(skb->data + off);
 		if (nexthdr == NEXTHDR_FRAGMENT) {
-			struct frag_hdr *frag_hdr = (struct frag_hdr *) hdr;
-			if (frag_hdr->frag_off)
-				break;
 			optlen = 8;
 		} else if (nexthdr == NEXTHDR_AUTH) {
 			optlen = (hdr->hdrlen + 2) << 2;
 		} else {
 			optlen = ipv6_optlen(hdr);
 		}
-		/* cache hdr->nexthdr, since pskb_may_pull() might
-		 * invalidate hdr
-		 */
-		next = hdr->nexthdr;
-		if (nexthdr == NEXTHDR_DEST) {
-			u16 i = 2;
 
-			/* Remember : hdr is no longer valid at this point. */
-			if (!pskb_may_pull(skb, off + optlen))
+		if (!pskb_may_pull(skb, off + optlen))
+			break;
+
+		hdr = (struct ipv6_opt_hdr *)(skb->data + off);
+		if (nexthdr == NEXTHDR_FRAGMENT) {
+			struct frag_hdr *frag_hdr = (struct frag_hdr *)hdr;
+
+			if (frag_hdr->frag_off)
 				break;
+		}
+		if (nexthdr == NEXTHDR_DEST) {
+			u16 i = 2;
 
 			while (1) {
 				struct ipv6_tlv_tnl_enc_lim *tel;
@@ -454,7 +454,7 @@ __u16 ip6_tnl_parse_tlv_enc_lim(struct sk_buff *skb, __u8 *raw)
 					i++;
 			}
 		}
-		nexthdr = next;
+		nexthdr = hdr->nexthdr;
 		off += optlen;
 	}
 	return 0;
diff --git net/ipv6/route.c net/ipv6/route.c
index 79b67f8048b5..6e4d31524268 100644
--- linux-4.14.336/net/ipv6/route.c
+++ linux-4.14.336/net/ipv6/route.c
@@ -85,7 +85,7 @@ static struct dst_entry *ip6_negative_advice(struct dst_entry *);
 static void		ip6_dst_destroy(struct dst_entry *);
 static void		ip6_dst_ifdown(struct dst_entry *,
 				       struct net_device *dev, int how);
-static int		 ip6_dst_gc(struct dst_ops *ops);
+static void		 ip6_dst_gc(struct dst_ops *ops);
 
 static int		ip6_pkt_discard(struct sk_buff *skb);
 static int		ip6_pkt_discard_out(struct net *net, struct sock *sk, struct sk_buff *skb);
@@ -1792,29 +1792,30 @@ out:
 	return dst;
 }
 
-static int ip6_dst_gc(struct dst_ops *ops)
+static void ip6_dst_gc(struct dst_ops *ops)
 {
 	struct net *net = container_of(ops, struct net, ipv6.ip6_dst_ops);
 	int rt_min_interval = net->ipv6.sysctl.ip6_rt_gc_min_interval;
-	int rt_max_size = net->ipv6.sysctl.ip6_rt_max_size;
 	int rt_elasticity = net->ipv6.sysctl.ip6_rt_gc_elasticity;
 	int rt_gc_timeout = net->ipv6.sysctl.ip6_rt_gc_timeout;
 	unsigned long rt_last_gc = net->ipv6.ip6_rt_last_gc;
+	unsigned int val;
 	int entries;
 
 	entries = dst_entries_get_fast(ops);
-	if (time_after(rt_last_gc + rt_min_interval, jiffies) &&
-	    entries <= rt_max_size)
+	if (entries > ops->gc_thresh)
+		entries = dst_entries_get_slow(ops);
+
+	if (time_after(rt_last_gc + rt_min_interval, jiffies))
 		goto out;
 
-	net->ipv6.ip6_rt_gc_expire++;
-	fib6_run_gc(net->ipv6.ip6_rt_gc_expire, net, true);
+	fib6_run_gc(atomic_inc_return(&net->ipv6.ip6_rt_gc_expire), net, true);
 	entries = dst_entries_get_slow(ops);
 	if (entries < ops->gc_thresh)
-		net->ipv6.ip6_rt_gc_expire = rt_gc_timeout>>1;
+		atomic_set(&net->ipv6.ip6_rt_gc_expire, rt_gc_timeout >> 1);
 out:
-	net->ipv6.ip6_rt_gc_expire -= net->ipv6.ip6_rt_gc_expire>>rt_elasticity;
-	return entries > rt_max_size;
+	val = atomic_read(&net->ipv6.ip6_rt_gc_expire);
+	atomic_set(&net->ipv6.ip6_rt_gc_expire, val - (val >> rt_elasticity));
 }
 
 static int ip6_convert_metrics(struct mx6_config *mxc,
@@ -4091,7 +4092,7 @@ static int __net_init ip6_route_net_init(struct net *net)
 #endif
 
 	net->ipv6.sysctl.flush_delay = 0;
-	net->ipv6.sysctl.ip6_rt_max_size = 4096;
+	net->ipv6.sysctl.ip6_rt_max_size = INT_MAX;
 	net->ipv6.sysctl.ip6_rt_gc_min_interval = HZ / 2;
 	net->ipv6.sysctl.ip6_rt_gc_timeout = 60*HZ;
 	net->ipv6.sysctl.ip6_rt_gc_interval = 30*HZ;
@@ -4099,7 +4100,7 @@ static int __net_init ip6_route_net_init(struct net *net)
 	net->ipv6.sysctl.ip6_rt_mtu_expires = 10*60*HZ;
 	net->ipv6.sysctl.ip6_rt_min_advmss = IPV6_MIN_MTU - 20 - 40;
 
-	net->ipv6.ip6_rt_gc_expire = 30*HZ;
+	atomic_set(&net->ipv6.ip6_rt_gc_expire, 30*HZ);
 
 	ret = 0;
 out:
diff --git net/ipv6/seg6.c net/ipv6/seg6.c
index 9c45165fe79b..b785bf569049 100644
--- linux-4.14.336/net/ipv6/seg6.c
+++ linux-4.14.336/net/ipv6/seg6.c
@@ -447,22 +447,24 @@ int __init seg6_init(void)
 {
 	int err = -ENOMEM;
 
-	err = genl_register_family(&seg6_genl_family);
+	err = register_pernet_subsys(&ip6_segments_ops);
 	if (err)
 		goto out;
 
-	err = register_pernet_subsys(&ip6_segments_ops);
+	err = genl_register_family(&seg6_genl_family);
 	if (err)
-		goto out_unregister_genl;
+		goto out_unregister_pernet;
 
 #ifdef CONFIG_IPV6_SEG6_LWTUNNEL
 	err = seg6_iptunnel_init();
 	if (err)
-		goto out_unregister_pernet;
+		goto out_unregister_genl;
 
 	err = seg6_local_init();
-	if (err)
-		goto out_unregister_pernet;
+	if (err) {
+		seg6_iptunnel_exit();
+		goto out_unregister_genl;
+	}
 #endif
 
 #ifdef CONFIG_IPV6_SEG6_HMAC
@@ -483,11 +485,11 @@ out_unregister_iptun:
 #endif
 #endif
 #ifdef CONFIG_IPV6_SEG6_LWTUNNEL
-out_unregister_pernet:
-	unregister_pernet_subsys(&ip6_segments_ops);
-#endif
 out_unregister_genl:
 	genl_unregister_family(&seg6_genl_family);
+#endif
+out_unregister_pernet:
+	unregister_pernet_subsys(&ip6_segments_ops);
 	goto out;
 }
 
diff --git net/iucv/af_iucv.c net/iucv/af_iucv.c
index 07e397a5edc6..d7dd92274957 100644
--- linux-4.14.336/net/iucv/af_iucv.c
+++ linux-4.14.336/net/iucv/af_iucv.c
@@ -2458,7 +2458,7 @@ static int __init afiucv_init(void)
 {
 	int err;
 
-	if (MACHINE_IS_VM) {
+	if (MACHINE_IS_VM && IS_ENABLED(CONFIG_IUCV)) {
 		cpcmd("QUERY USERID", iucv_userid, sizeof(iucv_userid), &err);
 		if (unlikely(err)) {
 			WARN_ON(err);
@@ -2466,11 +2466,7 @@ static int __init afiucv_init(void)
 			goto out;
 		}
 
-		pr_iucv = try_then_request_module(symbol_get(iucv_if), "iucv");
-		if (!pr_iucv) {
-			printk(KERN_WARNING "iucv_if lookup failed\n");
-			memset(&iucv_userid, 0, sizeof(iucv_userid));
-		}
+		pr_iucv = &iucv_if;
 	} else {
 		memset(&iucv_userid, 0, sizeof(iucv_userid));
 		pr_iucv = NULL;
@@ -2504,17 +2500,13 @@ out_sock:
 out_proto:
 	proto_unregister(&iucv_proto);
 out:
-	if (pr_iucv)
-		symbol_put(iucv_if);
 	return err;
 }
 
 static void __exit afiucv_exit(void)
 {
-	if (pr_iucv) {
+	if (pr_iucv)
 		afiucv_iucv_exit();
-		symbol_put(iucv_if);
-	}
 
 	unregister_netdevice_notifier(&afiucv_netdev_notifier);
 	dev_remove_pack(&iucv_packet_type);
diff --git net/l2tp/l2tp_ip6.c net/l2tp/l2tp_ip6.c
index d797708a1a5e..4a5f6ca12342 100644
--- linux-4.14.336/net/l2tp/l2tp_ip6.c
+++ linux-4.14.336/net/l2tp/l2tp_ip6.c
@@ -658,7 +658,7 @@ static int l2tp_ip6_sendmsg(struct sock *sk, struct msghdr *msg, size_t len)
 
 back_from_confirm:
 	lock_sock(sk);
-	ulen = len + skb_queue_empty(&sk->sk_write_queue) ? transhdrlen : 0;
+	ulen = len + (skb_queue_empty(&sk->sk_write_queue) ? transhdrlen : 0);
 	err = ip6_append_data(sk, ip_generic_getfrag, msg,
 			      ulen, transhdrlen, &ipc6,
 			      &fl6, (struct rt6_info *)dst,
diff --git net/llc/af_llc.c net/llc/af_llc.c
index 1e20b719fb3c..727af511297c 100644
--- linux-4.14.336/net/llc/af_llc.c
+++ linux-4.14.336/net/llc/af_llc.c
@@ -227,6 +227,8 @@ static int llc_ui_release(struct socket *sock)
 	if (llc->dev)
 		dev_put(llc->dev);
 	sock_put(sk);
+	sock_orphan(sk);
+	sock->sk = NULL;
 	llc_sk_free(sk);
 out:
 	return 0;
@@ -926,14 +928,15 @@ copy_uaddr:
  */
 static int llc_ui_sendmsg(struct socket *sock, struct msghdr *msg, size_t len)
 {
+	DECLARE_SOCKADDR(struct sockaddr_llc *, addr, msg->msg_name);
 	struct sock *sk = sock->sk;
 	struct llc_sock *llc = llc_sk(sk);
-	DECLARE_SOCKADDR(struct sockaddr_llc *, addr, msg->msg_name);
 	int flags = msg->msg_flags;
 	int noblock = flags & MSG_DONTWAIT;
+	int rc = -EINVAL, copied = 0, hdrlen, hh_len;
 	struct sk_buff *skb = NULL;
+	struct net_device *dev;
 	size_t size = 0;
-	int rc = -EINVAL, copied = 0, hdrlen;
 
 	dprintk("%s: sending from %02X to %02X\n", __func__,
 		llc->laddr.lsap, llc->daddr.lsap);
@@ -953,22 +956,29 @@ static int llc_ui_sendmsg(struct socket *sock, struct msghdr *msg, size_t len)
 		if (rc)
 			goto out;
 	}
-	hdrlen = llc->dev->hard_header_len + llc_ui_header_len(sk, addr);
+	dev = llc->dev;
+	hh_len = LL_RESERVED_SPACE(dev);
+	hdrlen = llc_ui_header_len(sk, addr);
 	size = hdrlen + len;
-	if (size > llc->dev->mtu)
-		size = llc->dev->mtu;
+	size = min_t(size_t, size, READ_ONCE(dev->mtu));
 	copied = size - hdrlen;
 	rc = -EINVAL;
 	if (copied < 0)
 		goto out;
 	release_sock(sk);
-	skb = sock_alloc_send_skb(sk, size, noblock, &rc);
+	skb = sock_alloc_send_skb(sk, hh_len + size, noblock, &rc);
 	lock_sock(sk);
 	if (!skb)
 		goto out;
-	skb->dev      = llc->dev;
+	if (sock_flag(sk, SOCK_ZAPPED) ||
+	    llc->dev != dev ||
+	    hdrlen != llc_ui_header_len(sk, addr) ||
+	    hh_len != LL_RESERVED_SPACE(dev) ||
+	    size > READ_ONCE(dev->mtu))
+		goto out;
+	skb->dev      = dev;
 	skb->protocol = llc_proto_type(addr->sllc_arphrd);
-	skb_reserve(skb, hdrlen);
+	skb_reserve(skb, hh_len + hdrlen);
 	rc = memcpy_from_msg(skb_put(skb, copied), msg, copied);
 	if (rc)
 		goto out;
diff --git net/llc/llc_core.c net/llc/llc_core.c
index 64d4bef04e73..4900a27b5176 100644
--- linux-4.14.336/net/llc/llc_core.c
+++ linux-4.14.336/net/llc/llc_core.c
@@ -135,22 +135,15 @@ static struct packet_type llc_packet_type __read_mostly = {
 	.func = llc_rcv,
 };
 
-static struct packet_type llc_tr_packet_type __read_mostly = {
-	.type = cpu_to_be16(ETH_P_TR_802_2),
-	.func = llc_rcv,
-};
-
 static int __init llc_init(void)
 {
 	dev_add_pack(&llc_packet_type);
-	dev_add_pack(&llc_tr_packet_type);
 	return 0;
 }
 
 static void __exit llc_exit(void)
 {
 	dev_remove_pack(&llc_packet_type);
-	dev_remove_pack(&llc_tr_packet_type);
 }
 
 module_init(llc_init);
diff --git net/mac80211/sta_info.c net/mac80211/sta_info.c
index 4e406cd11573..f2663c0a1e6f 100644
--- linux-4.14.336/net/mac80211/sta_info.c
+++ linux-4.14.336/net/mac80211/sta_info.c
@@ -602,6 +602,8 @@ static int sta_info_insert_finish(struct sta_info *sta) __acquires(RCU)
 	if (ieee80211_vif_is_mesh(&sdata->vif))
 		mesh_accept_plinks_update(sdata);
 
+	ieee80211_check_fast_xmit(sta);
+
 	return 0;
  out_remove:
 	sta_info_hash_del(local, sta);
diff --git net/mac80211/tx.c net/mac80211/tx.c
index 3914214dee05..995b0f444351 100644
--- linux-4.14.336/net/mac80211/tx.c
+++ linux-4.14.336/net/mac80211/tx.c
@@ -2808,7 +2808,7 @@ void ieee80211_check_fast_xmit(struct sta_info *sta)
 	    sdata->vif.type == NL80211_IFTYPE_STATION)
 		goto out;
 
-	if (!test_sta_flag(sta, WLAN_STA_AUTHORIZED))
+	if (!test_sta_flag(sta, WLAN_STA_AUTHORIZED) || !sta->uploaded)
 		goto out;
 
 	if (test_sta_flag(sta, WLAN_STA_PS_STA) ||
diff --git net/ncsi/internal.h net/ncsi/internal.h
index 8055e3965cef..2477caf9c967 100644
--- linux-4.14.336/net/ncsi/internal.h
+++ linux-4.14.336/net/ncsi/internal.h
@@ -69,9 +69,12 @@ enum {
 };
 
 struct ncsi_channel_version {
-	u32 version;		/* Supported BCD encoded NCSI version */
-	u32 alpha2;		/* Supported BCD encoded NCSI version */
-	u8  fw_name[12];	/* Firware name string                */
+	u8   major;		/* NCSI version major */
+	u8   minor;		/* NCSI version minor */
+	u8   update;		/* NCSI version update */
+	char alpha1;		/* NCSI version alpha1 */
+	char alpha2;		/* NCSI version alpha2 */
+	u8  fw_name[12];	/* Firmware name string                */
 	u32 fw_version;		/* Firmware version                   */
 	u16 pci_ids[4];		/* PCI identification                 */
 	u32 mf_id;		/* Manufacture ID                     */
diff --git net/ncsi/ncsi-netlink.c net/ncsi/ncsi-netlink.c
index 9073911ac97b..5c88201ec9d8 100644
--- linux-4.14.336/net/ncsi/ncsi-netlink.c
+++ linux-4.14.336/net/ncsi/ncsi-netlink.c
@@ -71,8 +71,8 @@ static int ncsi_write_channel_info(struct sk_buff *skb,
 	if (ndp->force_channel == nc)
 		nla_put_flag(skb, NCSI_CHANNEL_ATTR_FORCED);
 
-	nla_put_u32(skb, NCSI_CHANNEL_ATTR_VERSION_MAJOR, nc->version.version);
-	nla_put_u32(skb, NCSI_CHANNEL_ATTR_VERSION_MINOR, nc->version.alpha2);
+	nla_put_u32(skb, NCSI_CHANNEL_ATTR_VERSION_MAJOR, nc->version.major);
+	nla_put_u32(skb, NCSI_CHANNEL_ATTR_VERSION_MINOR, nc->version.minor);
 	nla_put_string(skb, NCSI_CHANNEL_ATTR_VERSION_STR, nc->version.fw_name);
 
 	vid_nest = nla_nest_start(skb, NCSI_CHANNEL_ATTR_VLAN_LIST);
diff --git net/ncsi/ncsi-pkt.h net/ncsi/ncsi-pkt.h
index 91b4b66438df..0bf62b4883d4 100644
--- linux-4.14.336/net/ncsi/ncsi-pkt.h
+++ linux-4.14.336/net/ncsi/ncsi-pkt.h
@@ -164,9 +164,12 @@ struct ncsi_rsp_gls_pkt {
 /* Get Version ID */
 struct ncsi_rsp_gvi_pkt {
 	struct ncsi_rsp_pkt_hdr rsp;          /* Response header */
-	__be32                  ncsi_version; /* NCSI version    */
+	unsigned char           major;        /* NCSI version major */
+	unsigned char           minor;        /* NCSI version minor */
+	unsigned char           update;       /* NCSI version update */
+	unsigned char           alpha1;       /* NCSI version alpha1 */
 	unsigned char           reserved[3];  /* Reserved        */
-	unsigned char           alpha2;       /* NCSI version    */
+	unsigned char           alpha2;       /* NCSI version alpha2 */
 	unsigned char           fw_name[12];  /* f/w name string */
 	__be32                  fw_version;   /* f/w version     */
 	__be16                  pci_ids[4];   /* PCI IDs         */
diff --git net/ncsi/ncsi-rsp.c net/ncsi/ncsi-rsp.c
index 42878d843c3c..1ae1de24b202 100644
--- linux-4.14.336/net/ncsi/ncsi-rsp.c
+++ linux-4.14.336/net/ncsi/ncsi-rsp.c
@@ -20,6 +20,19 @@
 #include "internal.h"
 #include "ncsi-pkt.h"
 
+/* Nibbles within [0xA, 0xF] add zero "0" to the returned value.
+ * Optional fields (encoded as 0xFF) will default to zero.
+ */
+static u8 decode_bcd_u8(u8 x)
+{
+	int lo = x & 0xF;
+	int hi = x >> 4;
+
+	lo = lo < 0xA ? lo : 0;
+	hi = hi < 0xA ? hi : 0;
+	return lo + hi * 10;
+}
+
 static int ncsi_validate_rsp_pkt(struct ncsi_request *nr,
 				 unsigned short payload)
 {
@@ -610,9 +623,18 @@ static int ncsi_rsp_handler_gvi(struct ncsi_request *nr)
 	if (!nc)
 		return -ENODEV;
 
-	/* Update to channel's version info */
+	/* Update channel's version info
+	 *
+	 * Major, minor, and update fields are supposed to be
+	 * unsigned integers encoded as packed BCD.
+	 *
+	 * Alpha1 and alpha2 are ISO/IEC 8859-1 characters.
+	 */
 	ncv = &nc->version;
-	ncv->version = ntohl(rsp->ncsi_version);
+	ncv->major = decode_bcd_u8(rsp->major);
+	ncv->minor = decode_bcd_u8(rsp->minor);
+	ncv->update = decode_bcd_u8(rsp->update);
+	ncv->alpha1 = rsp->alpha1;
 	ncv->alpha2 = rsp->alpha2;
 	memcpy(ncv->fw_name, rsp->fw_name, 12);
 	ncv->fw_version = ntohl(rsp->fw_version);
diff --git net/netfilter/ipvs/ip_vs_xmit.c net/netfilter/ipvs/ip_vs_xmit.c
index 97d411033f8a..8792cad28e29 100644
--- linux-4.14.336/net/netfilter/ipvs/ip_vs_xmit.c
+++ linux-4.14.336/net/netfilter/ipvs/ip_vs_xmit.c
@@ -270,8 +270,8 @@ static inline bool decrement_ttl(struct netns_ipvs *ipvs,
 			skb->dev = dst->dev;
 			icmpv6_send(skb, ICMPV6_TIME_EXCEED,
 				    ICMPV6_EXC_HOPLIMIT, 0);
-			__IP6_INC_STATS(net, ip6_dst_idev(dst),
-					IPSTATS_MIB_INHDRERRORS);
+			IP6_INC_STATS(net, ip6_dst_idev(dst),
+				      IPSTATS_MIB_INHDRERRORS);
 
 			return false;
 		}
@@ -286,7 +286,7 @@ static inline bool decrement_ttl(struct netns_ipvs *ipvs,
 	{
 		if (ip_hdr(skb)->ttl <= 1) {
 			/* Tell the sender its packet died... */
-			__IP_INC_STATS(net, IPSTATS_MIB_INHDRERRORS);
+			IP_INC_STATS(net, IPSTATS_MIB_INHDRERRORS);
 			icmp_send(skb, ICMP_TIME_EXCEEDED, ICMP_EXC_TTL, 0);
 			return false;
 		}
diff --git net/netfilter/nf_log.c net/netfilter/nf_log.c
index cdc744aa5889..a16156598905 100644
--- linux-4.14.336/net/netfilter/nf_log.c
+++ linux-4.14.336/net/netfilter/nf_log.c
@@ -202,11 +202,12 @@ void nf_logger_put(int pf, enum nf_log_type type)
 		return;
 	}
 
-	BUG_ON(loggers[pf][type] == NULL);
-
 	rcu_read_lock();
 	logger = rcu_dereference(loggers[pf][type]);
-	module_put(logger->me);
+	if (!logger)
+		WARN_ON_ONCE(1);
+	else
+		module_put(logger->me);
 	rcu_read_unlock();
 }
 EXPORT_SYMBOL_GPL(nf_logger_put);
diff --git net/netfilter/nf_tables_api.c net/netfilter/nf_tables_api.c
index 27c24c99d23b..407346ba89d4 100644
--- linux-4.14.336/net/netfilter/nf_tables_api.c
+++ linux-4.14.336/net/netfilter/nf_tables_api.c
@@ -22,6 +22,8 @@
 #include <net/net_namespace.h>
 #include <net/sock.h>
 
+#define NFT_SET_MAX_ANONLEN 16
+
 static LIST_HEAD(nf_tables_expressions);
 static LIST_HEAD(nf_tables_objects);
 
@@ -744,6 +746,30 @@ err:
 	return ret;
 }
 
+static bool nft_supported_family(u8 family)
+{
+	return false
+#ifdef CONFIG_NF_TABLES_INET
+		|| family == NFPROTO_INET
+#endif
+#ifdef CONFIG_NF_TABLES_IPV4
+		|| family == NFPROTO_IPV4
+#endif
+#ifdef CONFIG_NF_TABLES_ARP
+		|| family == NFPROTO_ARP
+#endif
+#ifdef CONFIG_NF_TABLES_NETDEV
+		|| family == NFPROTO_NETDEV
+#endif
+#if IS_ENABLED(CONFIG_NF_TABLES_BRIDGE)
+		|| family == NFPROTO_BRIDGE
+#endif
+#ifdef CONFIG_NF_TABLES_IPV6
+		|| family == NFPROTO_IPV6
+#endif
+		;
+}
+
 static int nf_tables_newtable(struct net *net, struct sock *nlsk,
 			      struct sk_buff *skb, const struct nlmsghdr *nlh,
 			      const struct nlattr * const nla[],
@@ -759,6 +785,9 @@ static int nf_tables_newtable(struct net *net, struct sock *nlsk,
 	struct nft_ctx ctx;
 	int err;
 
+	if (!nft_supported_family(family))
+		return -EOPNOTSUPP;
+
 	afi = nf_tables_afinfo_lookup(net, family, true);
 	if (IS_ERR(afi))
 		return PTR_ERR(afi);
@@ -2817,6 +2846,9 @@ static int nf_tables_set_alloc_name(struct nft_ctx *ctx, struct nft_set *set,
 		if (p[1] != 'd' || strchr(p + 2, '%'))
 			return -EINVAL;
 
+		if (strnlen(name, NFT_SET_MAX_ANONLEN) >= NFT_SET_MAX_ANONLEN)
+			return -EINVAL;
+
 		inuse = (unsigned long *)get_zeroed_page(GFP_KERNEL);
 		if (inuse == NULL)
 			return -ENOMEM;
@@ -5889,16 +5921,10 @@ static int nft_verdict_init(const struct nft_ctx *ctx, struct nft_data *data,
 	data->verdict.code = ntohl(nla_get_be32(tb[NFTA_VERDICT_CODE]));
 
 	switch (data->verdict.code) {
-	default:
-		switch (data->verdict.code & NF_VERDICT_MASK) {
-		case NF_ACCEPT:
-		case NF_DROP:
-		case NF_QUEUE:
-			break;
-		default:
-			return -EINVAL;
-		}
-		/* fall through */
+	case NF_ACCEPT:
+	case NF_DROP:
+	case NF_QUEUE:
+		break;
 	case NFT_CONTINUE:
 	case NFT_BREAK:
 	case NFT_RETURN:
@@ -5918,6 +5944,8 @@ static int nft_verdict_init(const struct nft_ctx *ctx, struct nft_data *data,
 
 		data->verdict.chain = chain;
 		break;
+	default:
+		return -EINVAL;
 	}
 
 	desc->len = sizeof(data->verdict);
diff --git net/netfilter/nft_byteorder.c net/netfilter/nft_byteorder.c
index dba16126c7ee..8c4ee49a80fb 100644
--- linux-4.14.336/net/netfilter/nft_byteorder.c
+++ linux-4.14.336/net/netfilter/nft_byteorder.c
@@ -41,19 +41,20 @@ static void nft_byteorder_eval(const struct nft_expr *expr,
 
 	switch (priv->size) {
 	case 8: {
+		u64 *dst64 = (void *)dst;
 		u64 src64;
 
 		switch (priv->op) {
 		case NFT_BYTEORDER_NTOH:
 			for (i = 0; i < priv->len / 8; i++) {
 				src64 = get_unaligned((u64 *)&src[i]);
-				put_unaligned_be64(src64, &dst[i]);
+				put_unaligned_be64(src64, &dst64[i]);
 			}
 			break;
 		case NFT_BYTEORDER_HTON:
 			for (i = 0; i < priv->len / 8; i++) {
 				src64 = get_unaligned_be64(&src[i]);
-				put_unaligned(src64, (u64 *)&dst[i]);
+				put_unaligned(src64, &dst64[i]);
 			}
 			break;
 		}
diff --git net/netfilter/nft_compat.c net/netfilter/nft_compat.c
index 8281656808ae..b87b7338266c 100644
--- linux-4.14.336/net/netfilter/nft_compat.c
+++ linux-4.14.336/net/netfilter/nft_compat.c
@@ -214,6 +214,7 @@ static const struct nla_policy nft_rule_compat_policy[NFTA_RULE_COMPAT_MAX + 1]
 static int nft_parse_compat(const struct nlattr *attr, u16 *proto, bool *inv)
 {
 	struct nlattr *tb[NFTA_RULE_COMPAT_MAX+1];
+	u32 l4proto;
 	u32 flags;
 	int err;
 
@@ -226,12 +227,18 @@ static int nft_parse_compat(const struct nlattr *attr, u16 *proto, bool *inv)
 		return -EINVAL;
 
 	flags = ntohl(nla_get_be32(tb[NFTA_RULE_COMPAT_FLAGS]));
-	if (flags & ~NFT_RULE_COMPAT_F_MASK)
+	if (flags & NFT_RULE_COMPAT_F_UNUSED ||
+	    flags & ~NFT_RULE_COMPAT_F_MASK)
 		return -EINVAL;
 	if (flags & NFT_RULE_COMPAT_F_INV)
 		*inv = true;
 
-	*proto = ntohl(nla_get_be32(tb[NFTA_RULE_COMPAT_PROTO]));
+	l4proto = ntohl(nla_get_be32(tb[NFTA_RULE_COMPAT_PROTO]));
+	if (l4proto > U16_MAX)
+		return -EINVAL;
+
+	*proto = l4proto;
+
 	return 0;
 }
 
diff --git net/netlabel/netlabel_calipso.c net/netlabel/netlabel_calipso.c
index d177dd066504..e0d63fb927bd 100644
--- linux-4.14.336/net/netlabel/netlabel_calipso.c
+++ linux-4.14.336/net/netlabel/netlabel_calipso.c
@@ -68,6 +68,28 @@ static const struct nla_policy calipso_genl_policy[NLBL_CALIPSO_A_MAX + 1] = {
 	[NLBL_CALIPSO_A_MTYPE] = { .type = NLA_U32 },
 };
 
+static const struct netlbl_calipso_ops *calipso_ops;
+
+/**
+ * netlbl_calipso_ops_register - Register the CALIPSO operations
+ * @ops: ops to register
+ *
+ * Description:
+ * Register the CALIPSO packet engine operations.
+ *
+ */
+const struct netlbl_calipso_ops *
+netlbl_calipso_ops_register(const struct netlbl_calipso_ops *ops)
+{
+	return xchg(&calipso_ops, ops);
+}
+EXPORT_SYMBOL(netlbl_calipso_ops_register);
+
+static const struct netlbl_calipso_ops *netlbl_calipso_ops_get(void)
+{
+	return ACCESS_ONCE(calipso_ops);
+}
+
 /* NetLabel Command Handlers
  */
 /**
@@ -110,16 +132,19 @@ static int netlbl_calipso_add_pass(struct genl_info *info,
  *
  */
 static int netlbl_calipso_add(struct sk_buff *skb, struct genl_info *info)
-
 {
 	int ret_val = -EINVAL;
 	struct netlbl_audit audit_info;
+	const struct netlbl_calipso_ops *ops = netlbl_calipso_ops_get();
 
 	if (!info->attrs[NLBL_CALIPSO_A_DOI] ||
 	    !info->attrs[NLBL_CALIPSO_A_MTYPE])
 		return -EINVAL;
 
-	netlbl_netlink_auditinfo(skb, &audit_info);
+	if (!ops)
+		return -EOPNOTSUPP;
+
+	netlbl_netlink_auditinfo(&audit_info);
 	switch (nla_get_u32(info->attrs[NLBL_CALIPSO_A_MTYPE])) {
 	case CALIPSO_MAP_PASS:
 		ret_val = netlbl_calipso_add_pass(info, &audit_info);
@@ -301,7 +326,7 @@ static int netlbl_calipso_remove(struct sk_buff *skb, struct genl_info *info)
 	if (!info->attrs[NLBL_CALIPSO_A_DOI])
 		return -EINVAL;
 
-	netlbl_netlink_auditinfo(skb, &audit_info);
+	netlbl_netlink_auditinfo(&audit_info);
 	cb_arg.doi = nla_get_u32(info->attrs[NLBL_CALIPSO_A_DOI]);
 	cb_arg.audit_info = &audit_info;
 	ret_val = netlbl_domhsh_walk(&skip_bkt, &skip_chain,
@@ -375,27 +400,6 @@ int __init netlbl_calipso_genl_init(void)
 	return genl_register_family(&netlbl_calipso_gnl_family);
 }
 
-static const struct netlbl_calipso_ops *calipso_ops;
-
-/**
- * netlbl_calipso_ops_register - Register the CALIPSO operations
- *
- * Description:
- * Register the CALIPSO packet engine operations.
- *
- */
-const struct netlbl_calipso_ops *
-netlbl_calipso_ops_register(const struct netlbl_calipso_ops *ops)
-{
-	return xchg(&calipso_ops, ops);
-}
-EXPORT_SYMBOL(netlbl_calipso_ops_register);
-
-static const struct netlbl_calipso_ops *netlbl_calipso_ops_get(void)
-{
-	return ACCESS_ONCE(calipso_ops);
-}
-
 /**
  * calipso_doi_add - Add a new DOI to the CALIPSO protocol engine
  * @doi_def: the DOI structure
diff --git net/netlabel/netlabel_cipso_v4.c net/netlabel/netlabel_cipso_v4.c
index e252f62bb8c2..a0a145db3fc7 100644
--- linux-4.14.336/net/netlabel/netlabel_cipso_v4.c
+++ linux-4.14.336/net/netlabel/netlabel_cipso_v4.c
@@ -420,7 +420,7 @@ static int netlbl_cipsov4_add(struct sk_buff *skb, struct genl_info *info)
 	    !info->attrs[NLBL_CIPSOV4_A_MTYPE])
 		return -EINVAL;
 
-	netlbl_netlink_auditinfo(skb, &audit_info);
+	netlbl_netlink_auditinfo(&audit_info);
 	switch (nla_get_u32(info->attrs[NLBL_CIPSOV4_A_MTYPE])) {
 	case CIPSO_V4_MAP_TRANS:
 		ret_val = netlbl_cipsov4_add_std(info, &audit_info);
@@ -715,7 +715,7 @@ static int netlbl_cipsov4_remove(struct sk_buff *skb, struct genl_info *info)
 	if (!info->attrs[NLBL_CIPSOV4_A_DOI])
 		return -EINVAL;
 
-	netlbl_netlink_auditinfo(skb, &audit_info);
+	netlbl_netlink_auditinfo(&audit_info);
 	cb_arg.doi = nla_get_u32(info->attrs[NLBL_CIPSOV4_A_DOI]);
 	cb_arg.audit_info = &audit_info;
 	ret_val = netlbl_domhsh_walk(&skip_bkt, &skip_chain,
diff --git net/netlabel/netlabel_mgmt.c net/netlabel/netlabel_mgmt.c
index 71ba69cb50c9..43c51242dcd2 100644
--- linux-4.14.336/net/netlabel/netlabel_mgmt.c
+++ linux-4.14.336/net/netlabel/netlabel_mgmt.c
@@ -447,7 +447,7 @@ static int netlbl_mgmt_add(struct sk_buff *skb, struct genl_info *info)
 	     (info->attrs[NLBL_MGMT_A_IPV6MASK] != NULL)))
 		return -EINVAL;
 
-	netlbl_netlink_auditinfo(skb, &audit_info);
+	netlbl_netlink_auditinfo(&audit_info);
 
 	return netlbl_mgmt_add_common(info, &audit_info);
 }
@@ -470,7 +470,7 @@ static int netlbl_mgmt_remove(struct sk_buff *skb, struct genl_info *info)
 	if (!info->attrs[NLBL_MGMT_A_DOMAIN])
 		return -EINVAL;
 
-	netlbl_netlink_auditinfo(skb, &audit_info);
+	netlbl_netlink_auditinfo(&audit_info);
 
 	domain = nla_data(info->attrs[NLBL_MGMT_A_DOMAIN]);
 	return netlbl_domhsh_remove(domain, AF_UNSPEC, &audit_info);
@@ -570,7 +570,7 @@ static int netlbl_mgmt_adddef(struct sk_buff *skb, struct genl_info *info)
 	     (info->attrs[NLBL_MGMT_A_IPV6MASK] != NULL)))
 		return -EINVAL;
 
-	netlbl_netlink_auditinfo(skb, &audit_info);
+	netlbl_netlink_auditinfo(&audit_info);
 
 	return netlbl_mgmt_add_common(info, &audit_info);
 }
@@ -589,7 +589,7 @@ static int netlbl_mgmt_removedef(struct sk_buff *skb, struct genl_info *info)
 {
 	struct netlbl_audit audit_info;
 
-	netlbl_netlink_auditinfo(skb, &audit_info);
+	netlbl_netlink_auditinfo(&audit_info);
 
 	return netlbl_domhsh_remove_default(AF_UNSPEC, &audit_info);
 }
diff --git net/netlabel/netlabel_unlabeled.c net/netlabel/netlabel_unlabeled.c
index 0067f472367b..ff52ff2278ed 100644
--- linux-4.14.336/net/netlabel/netlabel_unlabeled.c
+++ linux-4.14.336/net/netlabel/netlabel_unlabeled.c
@@ -827,7 +827,7 @@ static int netlbl_unlabel_accept(struct sk_buff *skb, struct genl_info *info)
 	if (info->attrs[NLBL_UNLABEL_A_ACPTFLG]) {
 		value = nla_get_u8(info->attrs[NLBL_UNLABEL_A_ACPTFLG]);
 		if (value == 1 || value == 0) {
-			netlbl_netlink_auditinfo(skb, &audit_info);
+			netlbl_netlink_auditinfo(&audit_info);
 			netlbl_unlabel_acceptflg_set(value, &audit_info);
 			return 0;
 		}
@@ -910,7 +910,7 @@ static int netlbl_unlabel_staticadd(struct sk_buff *skb,
 	       !info->attrs[NLBL_UNLABEL_A_IPV6MASK])))
 		return -EINVAL;
 
-	netlbl_netlink_auditinfo(skb, &audit_info);
+	netlbl_netlink_auditinfo(&audit_info);
 
 	ret_val = netlbl_unlabel_addrinfo_get(info, &addr, &mask, &addr_len);
 	if (ret_val != 0)
@@ -960,7 +960,7 @@ static int netlbl_unlabel_staticadddef(struct sk_buff *skb,
 	       !info->attrs[NLBL_UNLABEL_A_IPV6MASK])))
 		return -EINVAL;
 
-	netlbl_netlink_auditinfo(skb, &audit_info);
+	netlbl_netlink_auditinfo(&audit_info);
 
 	ret_val = netlbl_unlabel_addrinfo_get(info, &addr, &mask, &addr_len);
 	if (ret_val != 0)
@@ -1007,7 +1007,7 @@ static int netlbl_unlabel_staticremove(struct sk_buff *skb,
 	       !info->attrs[NLBL_UNLABEL_A_IPV6MASK])))
 		return -EINVAL;
 
-	netlbl_netlink_auditinfo(skb, &audit_info);
+	netlbl_netlink_auditinfo(&audit_info);
 
 	ret_val = netlbl_unlabel_addrinfo_get(info, &addr, &mask, &addr_len);
 	if (ret_val != 0)
@@ -1047,7 +1047,7 @@ static int netlbl_unlabel_staticremovedef(struct sk_buff *skb,
 	       !info->attrs[NLBL_UNLABEL_A_IPV6MASK])))
 		return -EINVAL;
 
-	netlbl_netlink_auditinfo(skb, &audit_info);
+	netlbl_netlink_auditinfo(&audit_info);
 
 	ret_val = netlbl_unlabel_addrinfo_get(info, &addr, &mask, &addr_len);
 	if (ret_val != 0)
diff --git net/netlabel/netlabel_user.h net/netlabel/netlabel_user.h
index 4a397cde1a48..2c608677b43b 100644
--- linux-4.14.336/net/netlabel/netlabel_user.h
+++ linux-4.14.336/net/netlabel/netlabel_user.h
@@ -42,11 +42,9 @@
 
 /**
  * netlbl_netlink_auditinfo - Fetch the audit information from a NETLINK msg
- * @skb: the packet
  * @audit_info: NetLabel audit information
  */
-static inline void netlbl_netlink_auditinfo(struct sk_buff *skb,
-					    struct netlbl_audit *audit_info)
+static inline void netlbl_netlink_auditinfo(struct netlbl_audit *audit_info)
 {
 	security_task_getsecid(current, &audit_info->secid);
 	audit_info->loginuid = audit_get_loginuid(current);
diff --git net/netlink/af_netlink.c net/netlink/af_netlink.c
index 89ece1f093e2..ee42244aada1 100644
--- linux-4.14.336/net/netlink/af_netlink.c
+++ linux-4.14.336/net/netlink/af_netlink.c
@@ -162,7 +162,7 @@ static inline u32 netlink_group_mask(u32 group)
 static struct sk_buff *netlink_to_full_skb(const struct sk_buff *skb,
 					   gfp_t gfp_mask)
 {
-	unsigned int len = skb_end_offset(skb);
+	unsigned int len = skb->len;
 	struct sk_buff *new;
 
 	new = alloc_skb(len, gfp_mask);
@@ -342,7 +342,7 @@ static void netlink_skb_destructor(struct sk_buff *skb)
 	if (is_vmalloc_addr(skb->head)) {
 		if (!skb->cloned ||
 		    !atomic_dec_return(&(skb_shinfo(skb)->dataref)))
-			vfree(skb->head);
+			vfree_atomic(skb->head);
 
 		skb->head = NULL;
 	}
diff --git net/nfc/nci/core.c net/nfc/nci/core.c
index d42c603dd635..2d9934dbbead 100644
--- linux-4.14.336/net/nfc/nci/core.c
+++ linux-4.14.336/net/nfc/nci/core.c
@@ -1209,6 +1209,10 @@ void nci_free_device(struct nci_dev *ndev)
 {
 	nfc_free_device(ndev->nfc_dev);
 	nci_hci_deallocate(ndev);
+
+	/* drop partial rx data packet if present */
+	if (ndev->rx_data_reassembly)
+		kfree_skb(ndev->rx_data_reassembly);
 	kfree(ndev);
 }
 EXPORT_SYMBOL(nci_free_device);
diff --git net/packet/af_packet.c net/packet/af_packet.c
index ea29453fcf7a..6a02cf8d7141 100644
--- linux-4.14.336/net/packet/af_packet.c
+++ linux-4.14.336/net/packet/af_packet.c
@@ -1890,7 +1890,7 @@ static int packet_rcv_spkt(struct sk_buff *skb, struct net_device *dev,
 	 */
 
 	spkt->spkt_family = dev->type;
-	strlcpy(spkt->spkt_device, dev->name, sizeof(spkt->spkt_device));
+	strscpy(spkt->spkt_device, dev->name, sizeof(spkt->spkt_device));
 	spkt->spkt_protocol = skb->protocol;
 
 	/*
@@ -3537,7 +3537,7 @@ static int packet_getname_spkt(struct socket *sock, struct sockaddr *uaddr,
 	rcu_read_lock();
 	dev = dev_get_by_index_rcu(sock_net(sk), READ_ONCE(pkt_sk(sk)->ifindex));
 	if (dev)
-		strlcpy(uaddr->sa_data, dev->name, sizeof(uaddr->sa_data));
+		strscpy(uaddr->sa_data, dev->name, sizeof(uaddr->sa_data));
 	rcu_read_unlock();
 	*uaddr_len = sizeof(*uaddr);
 
diff --git net/rds/af_rds.c net/rds/af_rds.c
index b405f77d664c..2628c1d3844e 100644
--- linux-4.14.336/net/rds/af_rds.c
+++ linux-4.14.336/net/rds/af_rds.c
@@ -315,7 +315,7 @@ static int rds_recv_track_latency(struct rds_sock *rs, char __user *optval,
 
 	rs->rs_rx_traces = trace.rx_traces;
 	for (i = 0; i < rs->rs_rx_traces; i++) {
-		if (trace.rx_trace_pos[i] > RDS_MSG_RX_DGRAM_TRACE_MAX) {
+		if (trace.rx_trace_pos[i] >= RDS_MSG_RX_DGRAM_TRACE_MAX) {
 			rs->rs_rx_traces = 0;
 			return -EFAULT;
 		}
diff --git net/rxrpc/conn_event.c net/rxrpc/conn_event.c
index 2432c118397f..8d14aebae621 100644
--- linux-4.14.336/net/rxrpc/conn_event.c
+++ linux-4.14.336/net/rxrpc/conn_event.c
@@ -48,6 +48,14 @@ static void rxrpc_conn_retransmit_call(struct rxrpc_connection *conn,
 
 	_enter("%d", conn->debug_id);
 
+	if (sp && sp->hdr.type == RXRPC_PACKET_TYPE_ACK) {
+		if (skb_copy_bits(skb, sizeof(struct rxrpc_wire_header),
+				  &pkt.ack, sizeof(pkt.ack)) < 0)
+			return;
+		if (pkt.ack.reason == RXRPC_ACK_PING_RESPONSE)
+			return;
+	}
+
 	chan = &conn->channels[sp->hdr.cid & RXRPC_CHANNELMASK];
 
 	/* If the last call got moved on whilst we were waiting to run, just
diff --git net/rxrpc/conn_service.c net/rxrpc/conn_service.c
index f6fcdb3130a1..7c5745997cd4 100644
--- linux-4.14.336/net/rxrpc/conn_service.c
+++ linux-4.14.336/net/rxrpc/conn_service.c
@@ -29,7 +29,7 @@ struct rxrpc_connection *rxrpc_find_service_conn_rcu(struct rxrpc_peer *peer,
 	struct rxrpc_conn_proto k;
 	struct rxrpc_skb_priv *sp = rxrpc_skb(skb);
 	struct rb_node *p;
-	unsigned int seq = 0;
+	unsigned int seq = 1;
 
 	k.epoch	= sp->hdr.epoch;
 	k.cid	= sp->hdr.cid & RXRPC_CIDMASK;
@@ -39,6 +39,7 @@ struct rxrpc_connection *rxrpc_find_service_conn_rcu(struct rxrpc_peer *peer,
 		 * under just the RCU read lock, so we have to check for
 		 * changes.
 		 */
+		seq++; /* 2 on the 1st/lockless path, otherwise odd */
 		read_seqbegin_or_lock(&peer->service_conn_lock, &seq);
 
 		p = rcu_dereference_raw(peer->service_conns.rb_node);
diff --git net/sched/Kconfig net/sched/Kconfig
index 782114a230ae..1a3ee928c57c 100644
--- linux-4.14.336/net/sched/Kconfig
+++ linux-4.14.336/net/sched/Kconfig
@@ -44,23 +44,6 @@ if NET_SCHED
 
 comment "Queueing/Scheduling"
 
-config NET_SCH_CBQ
-	tristate "Class Based Queueing (CBQ)"
-	---help---
-	  Say Y here if you want to use the Class-Based Queueing (CBQ) packet
-	  scheduling algorithm. This algorithm classifies the waiting packets
-	  into a tree-like hierarchy of classes; the leaves of this tree are
-	  in turn scheduled by separate algorithms.
-
-	  See the top of <file:net/sched/sch_cbq.c> for more details.
-
-	  CBQ is a commonly used scheduler, so if you're unsure, you should
-	  say Y here. Then say Y to all the queueing algorithms below that you
-	  want to use as leaf disciplines.
-
-	  To compile this code as a module, choose M here: the
-	  module will be called sch_cbq.
-
 config NET_SCH_HTB
 	tristate "Hierarchical Token Bucket (HTB)"
 	---help---
@@ -84,20 +67,6 @@ config NET_SCH_HFSC
 	  To compile this code as a module, choose M here: the
 	  module will be called sch_hfsc.
 
-config NET_SCH_ATM
-	tristate "ATM Virtual Circuits (ATM)"
-	depends on ATM
-	---help---
-	  Say Y here if you want to use the ATM pseudo-scheduler.  This
-	  provides a framework for invoking classifiers, which in turn
-	  select classes of this queuing discipline.  Each class maps
-	  the flow(s) it is handling to a given virtual circuit.
-
-	  See the top of <file:net/sched/sch_atm.c> for more details.
-
-	  To compile this code as a module, choose M here: the
-	  module will be called sch_atm.
-
 config NET_SCH_PRIO
 	tristate "Multi Band Priority Queueing (PRIO)"
 	---help---
@@ -183,17 +152,6 @@ config NET_SCH_GRED
 	  To compile this code as a module, choose M here: the
 	  module will be called sch_gred.
 
-config NET_SCH_DSMARK
-	tristate "Differentiated Services marker (DSMARK)"
-	---help---
-	  Say Y if you want to schedule packets according to the
-	  Differentiated Services architecture proposed in RFC 2475.
-	  Technical information on this method, with pointers to associated
-	  RFCs, is available at <http://www.gta.ufrj.br/diffserv/>.
-
-	  To compile this code as a module, choose M here: the
-	  module will be called sch_dsmark.
-
 config NET_SCH_NETEM
 	tristate "Network emulator (NETEM)"
 	---help---
diff --git net/sched/Makefile net/sched/Makefile
index c156c182f546..b2c2cea1fd91 100644
--- linux-4.14.336/net/sched/Makefile
+++ linux-4.14.336/net/sched/Makefile
@@ -28,20 +28,17 @@ obj-$(CONFIG_NET_IFE_SKBPRIO)	+= act_meta_skbprio.o
 obj-$(CONFIG_NET_IFE_SKBTCINDEX)	+= act_meta_skbtcindex.o
 obj-$(CONFIG_NET_ACT_TUNNEL_KEY)+= act_tunnel_key.o
 obj-$(CONFIG_NET_SCH_FIFO)	+= sch_fifo.o
-obj-$(CONFIG_NET_SCH_CBQ)	+= sch_cbq.o
 obj-$(CONFIG_NET_SCH_HTB)	+= sch_htb.o
 obj-$(CONFIG_NET_SCH_HFSC)	+= sch_hfsc.o
 obj-$(CONFIG_NET_SCH_RED)	+= sch_red.o
 obj-$(CONFIG_NET_SCH_GRED)	+= sch_gred.o
 obj-$(CONFIG_NET_SCH_INGRESS)	+= sch_ingress.o 
-obj-$(CONFIG_NET_SCH_DSMARK)	+= sch_dsmark.o
 obj-$(CONFIG_NET_SCH_SFB)	+= sch_sfb.o
 obj-$(CONFIG_NET_SCH_SFQ)	+= sch_sfq.o
 obj-$(CONFIG_NET_SCH_TBF)	+= sch_tbf.o
 obj-$(CONFIG_NET_SCH_TEQL)	+= sch_teql.o
 obj-$(CONFIG_NET_SCH_PRIO)	+= sch_prio.o
 obj-$(CONFIG_NET_SCH_MULTIQ)	+= sch_multiq.o
-obj-$(CONFIG_NET_SCH_ATM)	+= sch_atm.o
 obj-$(CONFIG_NET_SCH_NETEM)	+= sch_netem.o
 obj-$(CONFIG_NET_SCH_DRR)	+= sch_drr.o
 obj-$(CONFIG_NET_SCH_PLUG)	+= sch_plug.o
diff --git net/sched/sch_atm.c net/sched/sch_atm.c
deleted file mode 100644
index 184ce9050457..000000000000
--- linux-4.14.336/net/sched/sch_atm.c
+++ linux-4.14.336//dev/null
@@ -1,701 +0,0 @@
-/* net/sched/sch_atm.c - ATM VC selection "queueing discipline" */
-
-/* Written 1998-2000 by Werner Almesberger, EPFL ICA */
-
-#include <linux/module.h>
-#include <linux/slab.h>
-#include <linux/init.h>
-#include <linux/interrupt.h>
-#include <linux/string.h>
-#include <linux/errno.h>
-#include <linux/skbuff.h>
-#include <linux/atmdev.h>
-#include <linux/atmclip.h>
-#include <linux/rtnetlink.h>
-#include <linux/file.h>		/* for fput */
-#include <net/netlink.h>
-#include <net/pkt_sched.h>
-#include <net/pkt_cls.h>
-
-/*
- * The ATM queuing discipline provides a framework for invoking classifiers
- * (aka "filters"), which in turn select classes of this queuing discipline.
- * Each class maps the flow(s) it is handling to a given VC. Multiple classes
- * may share the same VC.
- *
- * When creating a class, VCs are specified by passing the number of the open
- * socket descriptor by which the calling process references the VC. The kernel
- * keeps the VC open at least until all classes using it are removed.
- *
- * In this file, most functions are named atm_tc_* to avoid confusion with all
- * the atm_* in net/atm. This naming convention differs from what's used in the
- * rest of net/sched.
- *
- * Known bugs:
- *  - sometimes messes up the IP stack
- *  - any manipulations besides the few operations described in the README, are
- *    untested and likely to crash the system
- *  - should lock the flow while there is data in the queue (?)
- */
-
-#define VCC2FLOW(vcc) ((struct atm_flow_data *) ((vcc)->user_back))
-
-struct atm_flow_data {
-	struct Qdisc_class_common common;
-	struct Qdisc		*q;	/* FIFO, TBF, etc. */
-	struct tcf_proto __rcu	*filter_list;
-	struct tcf_block	*block;
-	struct atm_vcc		*vcc;	/* VCC; NULL if VCC is closed */
-	void			(*old_pop)(struct atm_vcc *vcc,
-					   struct sk_buff *skb); /* chaining */
-	struct atm_qdisc_data	*parent;	/* parent qdisc */
-	struct socket		*sock;		/* for closing */
-	int			ref;		/* reference count */
-	struct gnet_stats_basic_packed	bstats;
-	struct gnet_stats_queue	qstats;
-	struct list_head	list;
-	struct atm_flow_data	*excess;	/* flow for excess traffic;
-						   NULL to set CLP instead */
-	int			hdr_len;
-	unsigned char		hdr[0];		/* header data; MUST BE LAST */
-};
-
-struct atm_qdisc_data {
-	struct atm_flow_data	link;		/* unclassified skbs go here */
-	struct list_head	flows;		/* NB: "link" is also on this
-						   list */
-	struct tasklet_struct	task;		/* dequeue tasklet */
-};
-
-/* ------------------------- Class/flow operations ------------------------- */
-
-static inline struct atm_flow_data *lookup_flow(struct Qdisc *sch, u32 classid)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct atm_flow_data *flow;
-
-	list_for_each_entry(flow, &p->flows, list) {
-		if (flow->common.classid == classid)
-			return flow;
-	}
-	return NULL;
-}
-
-static int atm_tc_graft(struct Qdisc *sch, unsigned long arg,
-			struct Qdisc *new, struct Qdisc **old)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct atm_flow_data *flow = (struct atm_flow_data *)arg;
-
-	pr_debug("atm_tc_graft(sch %p,[qdisc %p],flow %p,new %p,old %p)\n",
-		sch, p, flow, new, old);
-	if (list_empty(&flow->list))
-		return -EINVAL;
-	if (!new)
-		new = &noop_qdisc;
-	*old = flow->q;
-	flow->q = new;
-	if (*old)
-		qdisc_reset(*old);
-	return 0;
-}
-
-static struct Qdisc *atm_tc_leaf(struct Qdisc *sch, unsigned long cl)
-{
-	struct atm_flow_data *flow = (struct atm_flow_data *)cl;
-
-	pr_debug("atm_tc_leaf(sch %p,flow %p)\n", sch, flow);
-	return flow ? flow->q : NULL;
-}
-
-static unsigned long atm_tc_find(struct Qdisc *sch, u32 classid)
-{
-	struct atm_qdisc_data *p __maybe_unused = qdisc_priv(sch);
-	struct atm_flow_data *flow;
-
-	pr_debug("%s(sch %p,[qdisc %p],classid %x)\n", __func__, sch, p, classid);
-	flow = lookup_flow(sch, classid);
-	pr_debug("%s: flow %p\n", __func__, flow);
-	return (unsigned long)flow;
-}
-
-static unsigned long atm_tc_bind_filter(struct Qdisc *sch,
-					unsigned long parent, u32 classid)
-{
-	struct atm_qdisc_data *p __maybe_unused = qdisc_priv(sch);
-	struct atm_flow_data *flow;
-
-	pr_debug("%s(sch %p,[qdisc %p],classid %x)\n", __func__, sch, p, classid);
-	flow = lookup_flow(sch, classid);
-	if (flow)
-		flow->ref++;
-	pr_debug("%s: flow %p\n", __func__, flow);
-	return (unsigned long)flow;
-}
-
-/*
- * atm_tc_put handles all destructions, including the ones that are explicitly
- * requested (atm_tc_destroy, etc.). The assumption here is that we never drop
- * anything that still seems to be in use.
- */
-static void atm_tc_put(struct Qdisc *sch, unsigned long cl)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct atm_flow_data *flow = (struct atm_flow_data *)cl;
-
-	pr_debug("atm_tc_put(sch %p,[qdisc %p],flow %p)\n", sch, p, flow);
-	if (--flow->ref)
-		return;
-	pr_debug("atm_tc_put: destroying\n");
-	list_del_init(&flow->list);
-	pr_debug("atm_tc_put: qdisc %p\n", flow->q);
-	qdisc_destroy(flow->q);
-	tcf_block_put(flow->block);
-	if (flow->sock) {
-		pr_debug("atm_tc_put: f_count %ld\n",
-			file_count(flow->sock->file));
-		flow->vcc->pop = flow->old_pop;
-		sockfd_put(flow->sock);
-	}
-	if (flow->excess)
-		atm_tc_put(sch, (unsigned long)flow->excess);
-	if (flow != &p->link)
-		kfree(flow);
-	/*
-	 * If flow == &p->link, the qdisc no longer works at this point and
-	 * needs to be removed. (By the caller of atm_tc_put.)
-	 */
-}
-
-static void sch_atm_pop(struct atm_vcc *vcc, struct sk_buff *skb)
-{
-	struct atm_qdisc_data *p = VCC2FLOW(vcc)->parent;
-
-	pr_debug("sch_atm_pop(vcc %p,skb %p,[qdisc %p])\n", vcc, skb, p);
-	VCC2FLOW(vcc)->old_pop(vcc, skb);
-	tasklet_schedule(&p->task);
-}
-
-static const u8 llc_oui_ip[] = {
-	0xaa,			/* DSAP: non-ISO */
-	0xaa,			/* SSAP: non-ISO */
-	0x03,			/* Ctrl: Unnumbered Information Command PDU */
-	0x00,			/* OUI: EtherType */
-	0x00, 0x00,
-	0x08, 0x00
-};				/* Ethertype IP (0800) */
-
-static const struct nla_policy atm_policy[TCA_ATM_MAX + 1] = {
-	[TCA_ATM_FD]		= { .type = NLA_U32 },
-	[TCA_ATM_EXCESS]	= { .type = NLA_U32 },
-};
-
-static int atm_tc_change(struct Qdisc *sch, u32 classid, u32 parent,
-			 struct nlattr **tca, unsigned long *arg)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct atm_flow_data *flow = (struct atm_flow_data *)*arg;
-	struct atm_flow_data *excess = NULL;
-	struct nlattr *opt = tca[TCA_OPTIONS];
-	struct nlattr *tb[TCA_ATM_MAX + 1];
-	struct socket *sock;
-	int fd, error, hdr_len;
-	void *hdr;
-
-	pr_debug("atm_tc_change(sch %p,[qdisc %p],classid %x,parent %x,"
-		"flow %p,opt %p)\n", sch, p, classid, parent, flow, opt);
-	/*
-	 * The concept of parents doesn't apply for this qdisc.
-	 */
-	if (parent && parent != TC_H_ROOT && parent != sch->handle)
-		return -EINVAL;
-	/*
-	 * ATM classes cannot be changed. In order to change properties of the
-	 * ATM connection, that socket needs to be modified directly (via the
-	 * native ATM API. In order to send a flow to a different VC, the old
-	 * class needs to be removed and a new one added. (This may be changed
-	 * later.)
-	 */
-	if (flow)
-		return -EBUSY;
-	if (opt == NULL)
-		return -EINVAL;
-
-	error = nla_parse_nested(tb, TCA_ATM_MAX, opt, atm_policy, NULL);
-	if (error < 0)
-		return error;
-
-	if (!tb[TCA_ATM_FD])
-		return -EINVAL;
-	fd = nla_get_u32(tb[TCA_ATM_FD]);
-	pr_debug("atm_tc_change: fd %d\n", fd);
-	if (tb[TCA_ATM_HDR]) {
-		hdr_len = nla_len(tb[TCA_ATM_HDR]);
-		hdr = nla_data(tb[TCA_ATM_HDR]);
-	} else {
-		hdr_len = RFC1483LLC_LEN;
-		hdr = NULL;	/* default LLC/SNAP for IP */
-	}
-	if (!tb[TCA_ATM_EXCESS])
-		excess = NULL;
-	else {
-		excess = (struct atm_flow_data *)
-			atm_tc_find(sch, nla_get_u32(tb[TCA_ATM_EXCESS]));
-		if (!excess)
-			return -ENOENT;
-	}
-	pr_debug("atm_tc_change: type %d, payload %d, hdr_len %d\n",
-		 opt->nla_type, nla_len(opt), hdr_len);
-	sock = sockfd_lookup(fd, &error);
-	if (!sock)
-		return error;	/* f_count++ */
-	pr_debug("atm_tc_change: f_count %ld\n", file_count(sock->file));
-	if (sock->ops->family != PF_ATMSVC && sock->ops->family != PF_ATMPVC) {
-		error = -EPROTOTYPE;
-		goto err_out;
-	}
-	/* @@@ should check if the socket is really operational or we'll crash
-	   on vcc->send */
-	if (classid) {
-		if (TC_H_MAJ(classid ^ sch->handle)) {
-			pr_debug("atm_tc_change: classid mismatch\n");
-			error = -EINVAL;
-			goto err_out;
-		}
-	} else {
-		int i;
-		unsigned long cl;
-
-		for (i = 1; i < 0x8000; i++) {
-			classid = TC_H_MAKE(sch->handle, 0x8000 | i);
-			cl = atm_tc_find(sch, classid);
-			if (!cl)
-				break;
-		}
-	}
-	pr_debug("atm_tc_change: new id %x\n", classid);
-	flow = kzalloc(sizeof(struct atm_flow_data) + hdr_len, GFP_KERNEL);
-	pr_debug("atm_tc_change: flow %p\n", flow);
-	if (!flow) {
-		error = -ENOBUFS;
-		goto err_out;
-	}
-
-	error = tcf_block_get(&flow->block, &flow->filter_list);
-	if (error) {
-		kfree(flow);
-		goto err_out;
-	}
-
-	flow->q = qdisc_create_dflt(sch->dev_queue, &pfifo_qdisc_ops, classid);
-	if (!flow->q)
-		flow->q = &noop_qdisc;
-	pr_debug("atm_tc_change: qdisc %p\n", flow->q);
-	flow->sock = sock;
-	flow->vcc = ATM_SD(sock);	/* speedup */
-	flow->vcc->user_back = flow;
-	pr_debug("atm_tc_change: vcc %p\n", flow->vcc);
-	flow->old_pop = flow->vcc->pop;
-	flow->parent = p;
-	flow->vcc->pop = sch_atm_pop;
-	flow->common.classid = classid;
-	flow->ref = 1;
-	flow->excess = excess;
-	list_add(&flow->list, &p->link.list);
-	flow->hdr_len = hdr_len;
-	if (hdr)
-		memcpy(flow->hdr, hdr, hdr_len);
-	else
-		memcpy(flow->hdr, llc_oui_ip, sizeof(llc_oui_ip));
-	*arg = (unsigned long)flow;
-	return 0;
-err_out:
-	sockfd_put(sock);
-	return error;
-}
-
-static int atm_tc_delete(struct Qdisc *sch, unsigned long arg)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct atm_flow_data *flow = (struct atm_flow_data *)arg;
-
-	pr_debug("atm_tc_delete(sch %p,[qdisc %p],flow %p)\n", sch, p, flow);
-	if (list_empty(&flow->list))
-		return -EINVAL;
-	if (rcu_access_pointer(flow->filter_list) || flow == &p->link)
-		return -EBUSY;
-	/*
-	 * Reference count must be 2: one for "keepalive" (set at class
-	 * creation), and one for the reference held when calling delete.
-	 */
-	if (flow->ref < 2) {
-		pr_err("atm_tc_delete: flow->ref == %d\n", flow->ref);
-		return -EINVAL;
-	}
-	if (flow->ref > 2)
-		return -EBUSY;	/* catch references via excess, etc. */
-	atm_tc_put(sch, arg);
-	return 0;
-}
-
-static void atm_tc_walk(struct Qdisc *sch, struct qdisc_walker *walker)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct atm_flow_data *flow;
-
-	pr_debug("atm_tc_walk(sch %p,[qdisc %p],walker %p)\n", sch, p, walker);
-	if (walker->stop)
-		return;
-	list_for_each_entry(flow, &p->flows, list) {
-		if (walker->count >= walker->skip &&
-		    walker->fn(sch, (unsigned long)flow, walker) < 0) {
-			walker->stop = 1;
-			break;
-		}
-		walker->count++;
-	}
-}
-
-static struct tcf_block *atm_tc_tcf_block(struct Qdisc *sch, unsigned long cl)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct atm_flow_data *flow = (struct atm_flow_data *)cl;
-
-	pr_debug("atm_tc_find_tcf(sch %p,[qdisc %p],flow %p)\n", sch, p, flow);
-	return flow ? flow->block : p->link.block;
-}
-
-/* --------------------------- Qdisc operations ---------------------------- */
-
-static int atm_tc_enqueue(struct sk_buff *skb, struct Qdisc *sch,
-			  struct sk_buff **to_free)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct atm_flow_data *flow;
-	struct tcf_result res;
-	int result;
-	int ret = NET_XMIT_SUCCESS | __NET_XMIT_BYPASS;
-
-	pr_debug("atm_tc_enqueue(skb %p,sch %p,[qdisc %p])\n", skb, sch, p);
-	result = TC_ACT_OK;	/* be nice to gcc */
-	flow = NULL;
-	if (TC_H_MAJ(skb->priority) != sch->handle ||
-	    !(flow = (struct atm_flow_data *)atm_tc_find(sch, skb->priority))) {
-		struct tcf_proto *fl;
-
-		list_for_each_entry(flow, &p->flows, list) {
-			fl = rcu_dereference_bh(flow->filter_list);
-			if (fl) {
-				result = tcf_classify(skb, fl, &res, true);
-				if (result < 0)
-					continue;
-				if (result == TC_ACT_SHOT)
-					goto done;
-
-				flow = (struct atm_flow_data *)res.class;
-				if (!flow)
-					flow = lookup_flow(sch, res.classid);
-				goto drop;
-			}
-		}
-		flow = NULL;
-done:
-		;
-	}
-	if (!flow) {
-		flow = &p->link;
-	} else {
-		if (flow->vcc)
-			ATM_SKB(skb)->atm_options = flow->vcc->atm_options;
-		/*@@@ looks good ... but it's not supposed to work :-) */
-#ifdef CONFIG_NET_CLS_ACT
-		switch (result) {
-		case TC_ACT_QUEUED:
-		case TC_ACT_STOLEN:
-		case TC_ACT_TRAP:
-			__qdisc_drop(skb, to_free);
-			return NET_XMIT_SUCCESS | __NET_XMIT_STOLEN;
-		case TC_ACT_SHOT:
-			__qdisc_drop(skb, to_free);
-			goto drop;
-		case TC_ACT_RECLASSIFY:
-			if (flow->excess)
-				flow = flow->excess;
-			else
-				ATM_SKB(skb)->atm_options |= ATM_ATMOPT_CLP;
-			break;
-		}
-#endif
-	}
-
-	ret = qdisc_enqueue(skb, flow->q, to_free);
-	if (ret != NET_XMIT_SUCCESS) {
-drop: __maybe_unused
-		if (net_xmit_drop_count(ret)) {
-			qdisc_qstats_drop(sch);
-			if (flow)
-				flow->qstats.drops++;
-		}
-		return ret;
-	}
-	/*
-	 * Okay, this may seem weird. We pretend we've dropped the packet if
-	 * it goes via ATM. The reason for this is that the outer qdisc
-	 * expects to be able to q->dequeue the packet later on if we return
-	 * success at this place. Also, sch->q.qdisc needs to reflect whether
-	 * there is a packet egligible for dequeuing or not. Note that the
-	 * statistics of the outer qdisc are necessarily wrong because of all
-	 * this. There's currently no correct solution for this.
-	 */
-	if (flow == &p->link) {
-		sch->q.qlen++;
-		return NET_XMIT_SUCCESS;
-	}
-	tasklet_schedule(&p->task);
-	return NET_XMIT_SUCCESS | __NET_XMIT_BYPASS;
-}
-
-/*
- * Dequeue packets and send them over ATM. Note that we quite deliberately
- * avoid checking net_device's flow control here, simply because sch_atm
- * uses its own channels, which have nothing to do with any CLIP/LANE/or
- * non-ATM interfaces.
- */
-
-static void sch_atm_dequeue(unsigned long data)
-{
-	struct Qdisc *sch = (struct Qdisc *)data;
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct atm_flow_data *flow;
-	struct sk_buff *skb;
-
-	pr_debug("sch_atm_dequeue(sch %p,[qdisc %p])\n", sch, p);
-	list_for_each_entry(flow, &p->flows, list) {
-		if (flow == &p->link)
-			continue;
-		/*
-		 * If traffic is properly shaped, this won't generate nasty
-		 * little bursts. Otherwise, it may ... (but that's okay)
-		 */
-		while ((skb = flow->q->ops->peek(flow->q))) {
-			if (!atm_may_send(flow->vcc, skb->truesize))
-				break;
-
-			skb = qdisc_dequeue_peeked(flow->q);
-			if (unlikely(!skb))
-				break;
-
-			qdisc_bstats_update(sch, skb);
-			bstats_update(&flow->bstats, skb);
-			pr_debug("atm_tc_dequeue: sending on class %p\n", flow);
-			/* remove any LL header somebody else has attached */
-			skb_pull(skb, skb_network_offset(skb));
-			if (skb_headroom(skb) < flow->hdr_len) {
-				struct sk_buff *new;
-
-				new = skb_realloc_headroom(skb, flow->hdr_len);
-				dev_kfree_skb(skb);
-				if (!new)
-					continue;
-				skb = new;
-			}
-			pr_debug("sch_atm_dequeue: ip %p, data %p\n",
-				 skb_network_header(skb), skb->data);
-			ATM_SKB(skb)->vcc = flow->vcc;
-			memcpy(skb_push(skb, flow->hdr_len), flow->hdr,
-			       flow->hdr_len);
-			refcount_add(skb->truesize,
-				   &sk_atm(flow->vcc)->sk_wmem_alloc);
-			/* atm.atm_options are already set by atm_tc_enqueue */
-			flow->vcc->send(flow->vcc, skb);
-		}
-	}
-}
-
-static struct sk_buff *atm_tc_dequeue(struct Qdisc *sch)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct sk_buff *skb;
-
-	pr_debug("atm_tc_dequeue(sch %p,[qdisc %p])\n", sch, p);
-	tasklet_schedule(&p->task);
-	skb = qdisc_dequeue_peeked(p->link.q);
-	if (skb)
-		sch->q.qlen--;
-	return skb;
-}
-
-static struct sk_buff *atm_tc_peek(struct Qdisc *sch)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-
-	pr_debug("atm_tc_peek(sch %p,[qdisc %p])\n", sch, p);
-
-	return p->link.q->ops->peek(p->link.q);
-}
-
-static int atm_tc_init(struct Qdisc *sch, struct nlattr *opt)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	int err;
-
-	pr_debug("atm_tc_init(sch %p,[qdisc %p],opt %p)\n", sch, p, opt);
-	INIT_LIST_HEAD(&p->flows);
-	INIT_LIST_HEAD(&p->link.list);
-	list_add(&p->link.list, &p->flows);
-	p->link.q = qdisc_create_dflt(sch->dev_queue,
-				      &pfifo_qdisc_ops, sch->handle);
-	if (!p->link.q)
-		p->link.q = &noop_qdisc;
-	pr_debug("atm_tc_init: link (%p) qdisc %p\n", &p->link, p->link.q);
-	p->link.vcc = NULL;
-	p->link.sock = NULL;
-	p->link.common.classid = sch->handle;
-	p->link.ref = 1;
-
-	err = tcf_block_get(&p->link.block, &p->link.filter_list);
-	if (err)
-		return err;
-
-	tasklet_init(&p->task, sch_atm_dequeue, (unsigned long)sch);
-	return 0;
-}
-
-static void atm_tc_reset(struct Qdisc *sch)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct atm_flow_data *flow;
-
-	pr_debug("atm_tc_reset(sch %p,[qdisc %p])\n", sch, p);
-	list_for_each_entry(flow, &p->flows, list)
-		qdisc_reset(flow->q);
-	sch->q.qlen = 0;
-}
-
-static void atm_tc_destroy(struct Qdisc *sch)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct atm_flow_data *flow, *tmp;
-
-	pr_debug("atm_tc_destroy(sch %p,[qdisc %p])\n", sch, p);
-	list_for_each_entry(flow, &p->flows, list) {
-		tcf_block_put(flow->block);
-		flow->block = NULL;
-	}
-
-	list_for_each_entry_safe(flow, tmp, &p->flows, list) {
-		if (flow->ref > 1)
-			pr_err("atm_destroy: %p->ref = %d\n", flow, flow->ref);
-		atm_tc_put(sch, (unsigned long)flow);
-	}
-	tasklet_kill(&p->task);
-}
-
-static int atm_tc_dump_class(struct Qdisc *sch, unsigned long cl,
-			     struct sk_buff *skb, struct tcmsg *tcm)
-{
-	struct atm_qdisc_data *p = qdisc_priv(sch);
-	struct atm_flow_data *flow = (struct atm_flow_data *)cl;
-	struct nlattr *nest;
-
-	pr_debug("atm_tc_dump_class(sch %p,[qdisc %p],flow %p,skb %p,tcm %p)\n",
-		sch, p, flow, skb, tcm);
-	if (list_empty(&flow->list))
-		return -EINVAL;
-	tcm->tcm_handle = flow->common.classid;
-	tcm->tcm_info = flow->q->handle;
-
-	nest = nla_nest_start(skb, TCA_OPTIONS);
-	if (nest == NULL)
-		goto nla_put_failure;
-
-	if (nla_put(skb, TCA_ATM_HDR, flow->hdr_len, flow->hdr))
-		goto nla_put_failure;
-	if (flow->vcc) {
-		struct sockaddr_atmpvc pvc;
-		int state;
-
-		memset(&pvc, 0, sizeof(pvc));
-		pvc.sap_family = AF_ATMPVC;
-		pvc.sap_addr.itf = flow->vcc->dev ? flow->vcc->dev->number : -1;
-		pvc.sap_addr.vpi = flow->vcc->vpi;
-		pvc.sap_addr.vci = flow->vcc->vci;
-		if (nla_put(skb, TCA_ATM_ADDR, sizeof(pvc), &pvc))
-			goto nla_put_failure;
-		state = ATM_VF2VS(flow->vcc->flags);
-		if (nla_put_u32(skb, TCA_ATM_STATE, state))
-			goto nla_put_failure;
-	}
-	if (flow->excess) {
-		if (nla_put_u32(skb, TCA_ATM_EXCESS, flow->common.classid))
-			goto nla_put_failure;
-	} else {
-		if (nla_put_u32(skb, TCA_ATM_EXCESS, 0))
-			goto nla_put_failure;
-	}
-	return nla_nest_end(skb, nest);
-
-nla_put_failure:
-	nla_nest_cancel(skb, nest);
-	return -1;
-}
-static int
-atm_tc_dump_class_stats(struct Qdisc *sch, unsigned long arg,
-			struct gnet_dump *d)
-{
-	struct atm_flow_data *flow = (struct atm_flow_data *)arg;
-
-	if (gnet_stats_copy_basic(qdisc_root_sleeping_running(sch),
-				  d, NULL, &flow->bstats) < 0 ||
-	    gnet_stats_copy_queue(d, NULL, &flow->qstats, flow->q->q.qlen) < 0)
-		return -1;
-
-	return 0;
-}
-
-static int atm_tc_dump(struct Qdisc *sch, struct sk_buff *skb)
-{
-	return 0;
-}
-
-static const struct Qdisc_class_ops atm_class_ops = {
-	.graft		= atm_tc_graft,
-	.leaf		= atm_tc_leaf,
-	.find		= atm_tc_find,
-	.change		= atm_tc_change,
-	.delete		= atm_tc_delete,
-	.walk		= atm_tc_walk,
-	.tcf_block	= atm_tc_tcf_block,
-	.bind_tcf	= atm_tc_bind_filter,
-	.unbind_tcf	= atm_tc_put,
-	.dump		= atm_tc_dump_class,
-	.dump_stats	= atm_tc_dump_class_stats,
-};
-
-static struct Qdisc_ops atm_qdisc_ops __read_mostly = {
-	.cl_ops		= &atm_class_ops,
-	.id		= "atm",
-	.priv_size	= sizeof(struct atm_qdisc_data),
-	.enqueue	= atm_tc_enqueue,
-	.dequeue	= atm_tc_dequeue,
-	.peek		= atm_tc_peek,
-	.init		= atm_tc_init,
-	.reset		= atm_tc_reset,
-	.destroy	= atm_tc_destroy,
-	.dump		= atm_tc_dump,
-	.owner		= THIS_MODULE,
-};
-
-static int __init atm_init(void)
-{
-	return register_qdisc(&atm_qdisc_ops);
-}
-
-static void __exit atm_exit(void)
-{
-	unregister_qdisc(&atm_qdisc_ops);
-}
-
-module_init(atm_init)
-module_exit(atm_exit)
-MODULE_LICENSE("GPL");
diff --git net/sched/sch_cbq.c net/sched/sch_cbq.c
deleted file mode 100644
index 92ff508367e8..000000000000
--- linux-4.14.336/net/sched/sch_cbq.c
+++ linux-4.14.336//dev/null
@@ -1,1794 +0,0 @@
-/*
- * net/sched/sch_cbq.c	Class-Based Queueing discipline.
- *
- *		This program is free software; you can redistribute it and/or
- *		modify it under the terms of the GNU General Public License
- *		as published by the Free Software Foundation; either version
- *		2 of the License, or (at your option) any later version.
- *
- * Authors:	Alexey Kuznetsov, <kuznet@ms2.inr.ac.ru>
- *
- */
-
-#include <linux/module.h>
-#include <linux/slab.h>
-#include <linux/types.h>
-#include <linux/kernel.h>
-#include <linux/string.h>
-#include <linux/errno.h>
-#include <linux/skbuff.h>
-#include <net/netlink.h>
-#include <net/pkt_sched.h>
-#include <net/pkt_cls.h>
-
-
-/*	Class-Based Queueing (CBQ) algorithm.
-	=======================================
-
-	Sources: [1] Sally Floyd and Van Jacobson, "Link-sharing and Resource
-		 Management Models for Packet Networks",
-		 IEEE/ACM Transactions on Networking, Vol.3, No.4, 1995
-
-		 [2] Sally Floyd, "Notes on CBQ and Guaranteed Service", 1995
-
-		 [3] Sally Floyd, "Notes on Class-Based Queueing: Setting
-		 Parameters", 1996
-
-		 [4] Sally Floyd and Michael Speer, "Experimental Results
-		 for Class-Based Queueing", 1998, not published.
-
-	-----------------------------------------------------------------------
-
-	Algorithm skeleton was taken from NS simulator cbq.cc.
-	If someone wants to check this code against the LBL version,
-	he should take into account that ONLY the skeleton was borrowed,
-	the implementation is different. Particularly:
-
-	--- The WRR algorithm is different. Our version looks more
-	reasonable (I hope) and works when quanta are allowed to be
-	less than MTU, which is always the case when real time classes
-	have small rates. Note, that the statement of [3] is
-	incomplete, delay may actually be estimated even if class
-	per-round allotment is less than MTU. Namely, if per-round
-	allotment is W*r_i, and r_1+...+r_k = r < 1
-
-	delay_i <= ([MTU/(W*r_i)]*W*r + W*r + k*MTU)/B
-
-	In the worst case we have IntServ estimate with D = W*r+k*MTU
-	and C = MTU*r. The proof (if correct at all) is trivial.
-
-
-	--- It seems that cbq-2.0 is not very accurate. At least, I cannot
-	interpret some places, which look like wrong translations
-	from NS. Anyone is advised to find these differences
-	and explain to me, why I am wrong 8).
-
-	--- Linux has no EOI event, so that we cannot estimate true class
-	idle time. Workaround is to consider the next dequeue event
-	as sign that previous packet is finished. This is wrong because of
-	internal device queueing, but on a permanently loaded link it is true.
-	Moreover, combined with clock integrator, this scheme looks
-	very close to an ideal solution.  */
-
-struct cbq_sched_data;
-
-
-struct cbq_class {
-	struct Qdisc_class_common common;
-	struct cbq_class	*next_alive;	/* next class with backlog in this priority band */
-
-/* Parameters */
-	unsigned char		priority;	/* class priority */
-	unsigned char		priority2;	/* priority to be used after overlimit */
-	unsigned char		ewma_log;	/* time constant for idle time calculation */
-
-	u32			defmap;
-
-	/* Link-sharing scheduler parameters */
-	long			maxidle;	/* Class parameters: see below. */
-	long			offtime;
-	long			minidle;
-	u32			avpkt;
-	struct qdisc_rate_table	*R_tab;
-
-	/* General scheduler (WRR) parameters */
-	long			allot;
-	long			quantum;	/* Allotment per WRR round */
-	long			weight;		/* Relative allotment: see below */
-
-	struct Qdisc		*qdisc;		/* Ptr to CBQ discipline */
-	struct cbq_class	*split;		/* Ptr to split node */
-	struct cbq_class	*share;		/* Ptr to LS parent in the class tree */
-	struct cbq_class	*tparent;	/* Ptr to tree parent in the class tree */
-	struct cbq_class	*borrow;	/* NULL if class is bandwidth limited;
-						   parent otherwise */
-	struct cbq_class	*sibling;	/* Sibling chain */
-	struct cbq_class	*children;	/* Pointer to children chain */
-
-	struct Qdisc		*q;		/* Elementary queueing discipline */
-
-
-/* Variables */
-	unsigned char		cpriority;	/* Effective priority */
-	unsigned char		delayed;
-	unsigned char		level;		/* level of the class in hierarchy:
-						   0 for leaf classes, and maximal
-						   level of children + 1 for nodes.
-						 */
-
-	psched_time_t		last;		/* Last end of service */
-	psched_time_t		undertime;
-	long			avgidle;
-	long			deficit;	/* Saved deficit for WRR */
-	psched_time_t		penalized;
-	struct gnet_stats_basic_packed bstats;
-	struct gnet_stats_queue qstats;
-	struct net_rate_estimator __rcu *rate_est;
-	struct tc_cbq_xstats	xstats;
-
-	struct tcf_proto __rcu	*filter_list;
-	struct tcf_block	*block;
-
-	int			filters;
-
-	struct cbq_class	*defaults[TC_PRIO_MAX + 1];
-};
-
-struct cbq_sched_data {
-	struct Qdisc_class_hash	clhash;			/* Hash table of all classes */
-	int			nclasses[TC_CBQ_MAXPRIO + 1];
-	unsigned int		quanta[TC_CBQ_MAXPRIO + 1];
-
-	struct cbq_class	link;
-
-	unsigned int		activemask;
-	struct cbq_class	*active[TC_CBQ_MAXPRIO + 1];	/* List of all classes
-								   with backlog */
-
-#ifdef CONFIG_NET_CLS_ACT
-	struct cbq_class	*rx_class;
-#endif
-	struct cbq_class	*tx_class;
-	struct cbq_class	*tx_borrowed;
-	int			tx_len;
-	psched_time_t		now;		/* Cached timestamp */
-	unsigned int		pmask;
-
-	struct hrtimer		delay_timer;
-	struct qdisc_watchdog	watchdog;	/* Watchdog timer,
-						   started when CBQ has
-						   backlog, but cannot
-						   transmit just now */
-	psched_tdiff_t		wd_expires;
-	int			toplevel;
-	u32			hgenerator;
-};
-
-
-#define L2T(cl, len)	qdisc_l2t((cl)->R_tab, len)
-
-static inline struct cbq_class *
-cbq_class_lookup(struct cbq_sched_data *q, u32 classid)
-{
-	struct Qdisc_class_common *clc;
-
-	clc = qdisc_class_find(&q->clhash, classid);
-	if (clc == NULL)
-		return NULL;
-	return container_of(clc, struct cbq_class, common);
-}
-
-#ifdef CONFIG_NET_CLS_ACT
-
-static struct cbq_class *
-cbq_reclassify(struct sk_buff *skb, struct cbq_class *this)
-{
-	struct cbq_class *cl;
-
-	for (cl = this->tparent; cl; cl = cl->tparent) {
-		struct cbq_class *new = cl->defaults[TC_PRIO_BESTEFFORT];
-
-		if (new != NULL && new != this)
-			return new;
-	}
-	return NULL;
-}
-
-#endif
-
-/* Classify packet. The procedure is pretty complicated, but
- * it allows us to combine link sharing and priority scheduling
- * transparently.
- *
- * Namely, you can put link sharing rules (f.e. route based) at root of CBQ,
- * so that it resolves to split nodes. Then packets are classified
- * by logical priority, or a more specific classifier may be attached
- * to the split node.
- */
-
-static struct cbq_class *
-cbq_classify(struct sk_buff *skb, struct Qdisc *sch, int *qerr)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct cbq_class *head = &q->link;
-	struct cbq_class **defmap;
-	struct cbq_class *cl = NULL;
-	u32 prio = skb->priority;
-	struct tcf_proto *fl;
-	struct tcf_result res;
-
-	/*
-	 *  Step 1. If skb->priority points to one of our classes, use it.
-	 */
-	if (TC_H_MAJ(prio ^ sch->handle) == 0 &&
-	    (cl = cbq_class_lookup(q, prio)) != NULL)
-		return cl;
-
-	*qerr = NET_XMIT_SUCCESS | __NET_XMIT_BYPASS;
-	for (;;) {
-		int result = 0;
-		defmap = head->defaults;
-
-		fl = rcu_dereference_bh(head->filter_list);
-		/*
-		 * Step 2+n. Apply classifier.
-		 */
-		result = tcf_classify(skb, fl, &res, true);
-		if (!fl || result < 0)
-			goto fallback;
-		if (result == TC_ACT_SHOT)
-			return NULL;
-
-		cl = (void *)res.class;
-		if (!cl) {
-			if (TC_H_MAJ(res.classid))
-				cl = cbq_class_lookup(q, res.classid);
-			else if ((cl = defmap[res.classid & TC_PRIO_MAX]) == NULL)
-				cl = defmap[TC_PRIO_BESTEFFORT];
-
-			if (cl == NULL)
-				goto fallback;
-		}
-		if (cl->level >= head->level)
-			goto fallback;
-#ifdef CONFIG_NET_CLS_ACT
-		switch (result) {
-		case TC_ACT_QUEUED:
-		case TC_ACT_STOLEN:
-		case TC_ACT_TRAP:
-			*qerr = NET_XMIT_SUCCESS | __NET_XMIT_STOLEN;
-		case TC_ACT_RECLASSIFY:
-			return cbq_reclassify(skb, cl);
-		}
-#endif
-		if (cl->level == 0)
-			return cl;
-
-		/*
-		 * Step 3+n. If classifier selected a link sharing class,
-		 *	   apply agency specific classifier.
-		 *	   Repeat this procdure until we hit a leaf node.
-		 */
-		head = cl;
-	}
-
-fallback:
-	cl = head;
-
-	/*
-	 * Step 4. No success...
-	 */
-	if (TC_H_MAJ(prio) == 0 &&
-	    !(cl = head->defaults[prio & TC_PRIO_MAX]) &&
-	    !(cl = head->defaults[TC_PRIO_BESTEFFORT]))
-		return head;
-
-	return cl;
-}
-
-/*
- * A packet has just been enqueued on the empty class.
- * cbq_activate_class adds it to the tail of active class list
- * of its priority band.
- */
-
-static inline void cbq_activate_class(struct cbq_class *cl)
-{
-	struct cbq_sched_data *q = qdisc_priv(cl->qdisc);
-	int prio = cl->cpriority;
-	struct cbq_class *cl_tail;
-
-	cl_tail = q->active[prio];
-	q->active[prio] = cl;
-
-	if (cl_tail != NULL) {
-		cl->next_alive = cl_tail->next_alive;
-		cl_tail->next_alive = cl;
-	} else {
-		cl->next_alive = cl;
-		q->activemask |= (1<<prio);
-	}
-}
-
-/*
- * Unlink class from active chain.
- * Note that this same procedure is done directly in cbq_dequeue*
- * during round-robin procedure.
- */
-
-static void cbq_deactivate_class(struct cbq_class *this)
-{
-	struct cbq_sched_data *q = qdisc_priv(this->qdisc);
-	int prio = this->cpriority;
-	struct cbq_class *cl;
-	struct cbq_class *cl_prev = q->active[prio];
-
-	do {
-		cl = cl_prev->next_alive;
-		if (cl == this) {
-			cl_prev->next_alive = cl->next_alive;
-			cl->next_alive = NULL;
-
-			if (cl == q->active[prio]) {
-				q->active[prio] = cl_prev;
-				if (cl == q->active[prio]) {
-					q->active[prio] = NULL;
-					q->activemask &= ~(1<<prio);
-					return;
-				}
-			}
-			return;
-		}
-	} while ((cl_prev = cl) != q->active[prio]);
-}
-
-static void
-cbq_mark_toplevel(struct cbq_sched_data *q, struct cbq_class *cl)
-{
-	int toplevel = q->toplevel;
-
-	if (toplevel > cl->level) {
-		psched_time_t now = psched_get_time();
-
-		do {
-			if (cl->undertime < now) {
-				q->toplevel = cl->level;
-				return;
-			}
-		} while ((cl = cl->borrow) != NULL && toplevel > cl->level);
-	}
-}
-
-static int
-cbq_enqueue(struct sk_buff *skb, struct Qdisc *sch,
-	    struct sk_buff **to_free)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	int ret;
-	struct cbq_class *cl = cbq_classify(skb, sch, &ret);
-
-#ifdef CONFIG_NET_CLS_ACT
-	q->rx_class = cl;
-#endif
-	if (cl == NULL) {
-		if (ret & __NET_XMIT_BYPASS)
-			qdisc_qstats_drop(sch);
-		__qdisc_drop(skb, to_free);
-		return ret;
-	}
-
-	ret = qdisc_enqueue(skb, cl->q, to_free);
-	if (ret == NET_XMIT_SUCCESS) {
-		sch->q.qlen++;
-		cbq_mark_toplevel(q, cl);
-		if (!cl->next_alive)
-			cbq_activate_class(cl);
-		return ret;
-	}
-
-	if (net_xmit_drop_count(ret)) {
-		qdisc_qstats_drop(sch);
-		cbq_mark_toplevel(q, cl);
-		cl->qstats.drops++;
-	}
-	return ret;
-}
-
-/* Overlimit action: penalize leaf class by adding offtime */
-static void cbq_overlimit(struct cbq_class *cl)
-{
-	struct cbq_sched_data *q = qdisc_priv(cl->qdisc);
-	psched_tdiff_t delay = cl->undertime - q->now;
-
-	if (!cl->delayed) {
-		delay += cl->offtime;
-
-		/*
-		 * Class goes to sleep, so that it will have no
-		 * chance to work avgidle. Let's forgive it 8)
-		 *
-		 * BTW cbq-2.0 has a crap in this
-		 * place, apparently they forgot to shift it by cl->ewma_log.
-		 */
-		if (cl->avgidle < 0)
-			delay -= (-cl->avgidle) - ((-cl->avgidle) >> cl->ewma_log);
-		if (cl->avgidle < cl->minidle)
-			cl->avgidle = cl->minidle;
-		if (delay <= 0)
-			delay = 1;
-		cl->undertime = q->now + delay;
-
-		cl->xstats.overactions++;
-		cl->delayed = 1;
-	}
-	if (q->wd_expires == 0 || q->wd_expires > delay)
-		q->wd_expires = delay;
-
-	/* Dirty work! We must schedule wakeups based on
-	 * real available rate, rather than leaf rate,
-	 * which may be tiny (even zero).
-	 */
-	if (q->toplevel == TC_CBQ_MAXLEVEL) {
-		struct cbq_class *b;
-		psched_tdiff_t base_delay = q->wd_expires;
-
-		for (b = cl->borrow; b; b = b->borrow) {
-			delay = b->undertime - q->now;
-			if (delay < base_delay) {
-				if (delay <= 0)
-					delay = 1;
-				base_delay = delay;
-			}
-		}
-
-		q->wd_expires = base_delay;
-	}
-}
-
-static psched_tdiff_t cbq_undelay_prio(struct cbq_sched_data *q, int prio,
-				       psched_time_t now)
-{
-	struct cbq_class *cl;
-	struct cbq_class *cl_prev = q->active[prio];
-	psched_time_t sched = now;
-
-	if (cl_prev == NULL)
-		return 0;
-
-	do {
-		cl = cl_prev->next_alive;
-		if (now - cl->penalized > 0) {
-			cl_prev->next_alive = cl->next_alive;
-			cl->next_alive = NULL;
-			cl->cpriority = cl->priority;
-			cl->delayed = 0;
-			cbq_activate_class(cl);
-
-			if (cl == q->active[prio]) {
-				q->active[prio] = cl_prev;
-				if (cl == q->active[prio]) {
-					q->active[prio] = NULL;
-					return 0;
-				}
-			}
-
-			cl = cl_prev->next_alive;
-		} else if (sched - cl->penalized > 0)
-			sched = cl->penalized;
-	} while ((cl_prev = cl) != q->active[prio]);
-
-	return sched - now;
-}
-
-static enum hrtimer_restart cbq_undelay(struct hrtimer *timer)
-{
-	struct cbq_sched_data *q = container_of(timer, struct cbq_sched_data,
-						delay_timer);
-	struct Qdisc *sch = q->watchdog.qdisc;
-	psched_time_t now;
-	psched_tdiff_t delay = 0;
-	unsigned int pmask;
-
-	now = psched_get_time();
-
-	pmask = q->pmask;
-	q->pmask = 0;
-
-	while (pmask) {
-		int prio = ffz(~pmask);
-		psched_tdiff_t tmp;
-
-		pmask &= ~(1<<prio);
-
-		tmp = cbq_undelay_prio(q, prio, now);
-		if (tmp > 0) {
-			q->pmask |= 1<<prio;
-			if (tmp < delay || delay == 0)
-				delay = tmp;
-		}
-	}
-
-	if (delay) {
-		ktime_t time;
-
-		time = 0;
-		time = ktime_add_ns(time, PSCHED_TICKS2NS(now + delay));
-		hrtimer_start(&q->delay_timer, time, HRTIMER_MODE_ABS_PINNED);
-	}
-
-	__netif_schedule(qdisc_root(sch));
-	return HRTIMER_NORESTART;
-}
-
-/*
- * It is mission critical procedure.
- *
- * We "regenerate" toplevel cutoff, if transmitting class
- * has backlog and it is not regulated. It is not part of
- * original CBQ description, but looks more reasonable.
- * Probably, it is wrong. This question needs further investigation.
- */
-
-static inline void
-cbq_update_toplevel(struct cbq_sched_data *q, struct cbq_class *cl,
-		    struct cbq_class *borrowed)
-{
-	if (cl && q->toplevel >= borrowed->level) {
-		if (cl->q->q.qlen > 1) {
-			do {
-				if (borrowed->undertime == PSCHED_PASTPERFECT) {
-					q->toplevel = borrowed->level;
-					return;
-				}
-			} while ((borrowed = borrowed->borrow) != NULL);
-		}
-#if 0
-	/* It is not necessary now. Uncommenting it
-	   will save CPU cycles, but decrease fairness.
-	 */
-		q->toplevel = TC_CBQ_MAXLEVEL;
-#endif
-	}
-}
-
-static void
-cbq_update(struct cbq_sched_data *q)
-{
-	struct cbq_class *this = q->tx_class;
-	struct cbq_class *cl = this;
-	int len = q->tx_len;
-	psched_time_t now;
-
-	q->tx_class = NULL;
-	/* Time integrator. We calculate EOS time
-	 * by adding expected packet transmission time.
-	 */
-	now = q->now + L2T(&q->link, len);
-
-	for ( ; cl; cl = cl->share) {
-		long avgidle = cl->avgidle;
-		long idle;
-
-		cl->bstats.packets++;
-		cl->bstats.bytes += len;
-
-		/*
-		 * (now - last) is total time between packet right edges.
-		 * (last_pktlen/rate) is "virtual" busy time, so that
-		 *
-		 *	idle = (now - last) - last_pktlen/rate
-		 */
-
-		idle = now - cl->last;
-		if ((unsigned long)idle > 128*1024*1024) {
-			avgidle = cl->maxidle;
-		} else {
-			idle -= L2T(cl, len);
-
-		/* true_avgidle := (1-W)*true_avgidle + W*idle,
-		 * where W=2^{-ewma_log}. But cl->avgidle is scaled:
-		 * cl->avgidle == true_avgidle/W,
-		 * hence:
-		 */
-			avgidle += idle - (avgidle>>cl->ewma_log);
-		}
-
-		if (avgidle <= 0) {
-			/* Overlimit or at-limit */
-
-			if (avgidle < cl->minidle)
-				avgidle = cl->minidle;
-
-			cl->avgidle = avgidle;
-
-			/* Calculate expected time, when this class
-			 * will be allowed to send.
-			 * It will occur, when:
-			 * (1-W)*true_avgidle + W*delay = 0, i.e.
-			 * idle = (1/W - 1)*(-true_avgidle)
-			 * or
-			 * idle = (1 - W)*(-cl->avgidle);
-			 */
-			idle = (-avgidle) - ((-avgidle) >> cl->ewma_log);
-
-			/*
-			 * That is not all.
-			 * To maintain the rate allocated to the class,
-			 * we add to undertime virtual clock,
-			 * necessary to complete transmitted packet.
-			 * (len/phys_bandwidth has been already passed
-			 * to the moment of cbq_update)
-			 */
-
-			idle -= L2T(&q->link, len);
-			idle += L2T(cl, len);
-
-			cl->undertime = now + idle;
-		} else {
-			/* Underlimit */
-
-			cl->undertime = PSCHED_PASTPERFECT;
-			if (avgidle > cl->maxidle)
-				cl->avgidle = cl->maxidle;
-			else
-				cl->avgidle = avgidle;
-		}
-		if ((s64)(now - cl->last) > 0)
-			cl->last = now;
-	}
-
-	cbq_update_toplevel(q, this, q->tx_borrowed);
-}
-
-static inline struct cbq_class *
-cbq_under_limit(struct cbq_class *cl)
-{
-	struct cbq_sched_data *q = qdisc_priv(cl->qdisc);
-	struct cbq_class *this_cl = cl;
-
-	if (cl->tparent == NULL)
-		return cl;
-
-	if (cl->undertime == PSCHED_PASTPERFECT || q->now >= cl->undertime) {
-		cl->delayed = 0;
-		return cl;
-	}
-
-	do {
-		/* It is very suspicious place. Now overlimit
-		 * action is generated for not bounded classes
-		 * only if link is completely congested.
-		 * Though it is in agree with ancestor-only paradigm,
-		 * it looks very stupid. Particularly,
-		 * it means that this chunk of code will either
-		 * never be called or result in strong amplification
-		 * of burstiness. Dangerous, silly, and, however,
-		 * no another solution exists.
-		 */
-		cl = cl->borrow;
-		if (!cl) {
-			this_cl->qstats.overlimits++;
-			cbq_overlimit(this_cl);
-			return NULL;
-		}
-		if (cl->level > q->toplevel)
-			return NULL;
-	} while (cl->undertime != PSCHED_PASTPERFECT && q->now < cl->undertime);
-
-	cl->delayed = 0;
-	return cl;
-}
-
-static inline struct sk_buff *
-cbq_dequeue_prio(struct Qdisc *sch, int prio)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct cbq_class *cl_tail, *cl_prev, *cl;
-	struct sk_buff *skb;
-	int deficit;
-
-	cl_tail = cl_prev = q->active[prio];
-	cl = cl_prev->next_alive;
-
-	do {
-		deficit = 0;
-
-		/* Start round */
-		do {
-			struct cbq_class *borrow = cl;
-
-			if (cl->q->q.qlen &&
-			    (borrow = cbq_under_limit(cl)) == NULL)
-				goto skip_class;
-
-			if (cl->deficit <= 0) {
-				/* Class exhausted its allotment per
-				 * this round. Switch to the next one.
-				 */
-				deficit = 1;
-				cl->deficit += cl->quantum;
-				goto next_class;
-			}
-
-			skb = cl->q->dequeue(cl->q);
-
-			/* Class did not give us any skb :-(
-			 * It could occur even if cl->q->q.qlen != 0
-			 * f.e. if cl->q == "tbf"
-			 */
-			if (skb == NULL)
-				goto skip_class;
-
-			cl->deficit -= qdisc_pkt_len(skb);
-			q->tx_class = cl;
-			q->tx_borrowed = borrow;
-			if (borrow != cl) {
-#ifndef CBQ_XSTATS_BORROWS_BYTES
-				borrow->xstats.borrows++;
-				cl->xstats.borrows++;
-#else
-				borrow->xstats.borrows += qdisc_pkt_len(skb);
-				cl->xstats.borrows += qdisc_pkt_len(skb);
-#endif
-			}
-			q->tx_len = qdisc_pkt_len(skb);
-
-			if (cl->deficit <= 0) {
-				q->active[prio] = cl;
-				cl = cl->next_alive;
-				cl->deficit += cl->quantum;
-			}
-			return skb;
-
-skip_class:
-			if (cl->q->q.qlen == 0 || prio != cl->cpriority) {
-				/* Class is empty or penalized.
-				 * Unlink it from active chain.
-				 */
-				cl_prev->next_alive = cl->next_alive;
-				cl->next_alive = NULL;
-
-				/* Did cl_tail point to it? */
-				if (cl == cl_tail) {
-					/* Repair it! */
-					cl_tail = cl_prev;
-
-					/* Was it the last class in this band? */
-					if (cl == cl_tail) {
-						/* Kill the band! */
-						q->active[prio] = NULL;
-						q->activemask &= ~(1<<prio);
-						if (cl->q->q.qlen)
-							cbq_activate_class(cl);
-						return NULL;
-					}
-
-					q->active[prio] = cl_tail;
-				}
-				if (cl->q->q.qlen)
-					cbq_activate_class(cl);
-
-				cl = cl_prev;
-			}
-
-next_class:
-			cl_prev = cl;
-			cl = cl->next_alive;
-		} while (cl_prev != cl_tail);
-	} while (deficit);
-
-	q->active[prio] = cl_prev;
-
-	return NULL;
-}
-
-static inline struct sk_buff *
-cbq_dequeue_1(struct Qdisc *sch)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct sk_buff *skb;
-	unsigned int activemask;
-
-	activemask = q->activemask & 0xFF;
-	while (activemask) {
-		int prio = ffz(~activemask);
-		activemask &= ~(1<<prio);
-		skb = cbq_dequeue_prio(sch, prio);
-		if (skb)
-			return skb;
-	}
-	return NULL;
-}
-
-static struct sk_buff *
-cbq_dequeue(struct Qdisc *sch)
-{
-	struct sk_buff *skb;
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	psched_time_t now;
-
-	now = psched_get_time();
-
-	if (q->tx_class)
-		cbq_update(q);
-
-	q->now = now;
-
-	for (;;) {
-		q->wd_expires = 0;
-
-		skb = cbq_dequeue_1(sch);
-		if (skb) {
-			qdisc_bstats_update(sch, skb);
-			sch->q.qlen--;
-			return skb;
-		}
-
-		/* All the classes are overlimit.
-		 *
-		 * It is possible, if:
-		 *
-		 * 1. Scheduler is empty.
-		 * 2. Toplevel cutoff inhibited borrowing.
-		 * 3. Root class is overlimit.
-		 *
-		 * Reset 2d and 3d conditions and retry.
-		 *
-		 * Note, that NS and cbq-2.0 are buggy, peeking
-		 * an arbitrary class is appropriate for ancestor-only
-		 * sharing, but not for toplevel algorithm.
-		 *
-		 * Our version is better, but slower, because it requires
-		 * two passes, but it is unavoidable with top-level sharing.
-		 */
-
-		if (q->toplevel == TC_CBQ_MAXLEVEL &&
-		    q->link.undertime == PSCHED_PASTPERFECT)
-			break;
-
-		q->toplevel = TC_CBQ_MAXLEVEL;
-		q->link.undertime = PSCHED_PASTPERFECT;
-	}
-
-	/* No packets in scheduler or nobody wants to give them to us :-(
-	 * Sigh... start watchdog timer in the last case.
-	 */
-
-	if (sch->q.qlen) {
-		qdisc_qstats_overlimit(sch);
-		if (q->wd_expires)
-			qdisc_watchdog_schedule(&q->watchdog,
-						now + q->wd_expires);
-	}
-	return NULL;
-}
-
-/* CBQ class maintanance routines */
-
-static void cbq_adjust_levels(struct cbq_class *this)
-{
-	if (this == NULL)
-		return;
-
-	do {
-		int level = 0;
-		struct cbq_class *cl;
-
-		cl = this->children;
-		if (cl) {
-			do {
-				if (cl->level > level)
-					level = cl->level;
-			} while ((cl = cl->sibling) != this->children);
-		}
-		this->level = level + 1;
-	} while ((this = this->tparent) != NULL);
-}
-
-static void cbq_normalize_quanta(struct cbq_sched_data *q, int prio)
-{
-	struct cbq_class *cl;
-	unsigned int h;
-
-	if (q->quanta[prio] == 0)
-		return;
-
-	for (h = 0; h < q->clhash.hashsize; h++) {
-		hlist_for_each_entry(cl, &q->clhash.hash[h], common.hnode) {
-			/* BUGGGG... Beware! This expression suffer of
-			 * arithmetic overflows!
-			 */
-			if (cl->priority == prio) {
-				cl->quantum = (cl->weight*cl->allot*q->nclasses[prio])/
-					q->quanta[prio];
-			}
-			if (cl->quantum <= 0 ||
-			    cl->quantum > 32*qdisc_dev(cl->qdisc)->mtu) {
-				pr_warn("CBQ: class %08x has bad quantum==%ld, repaired.\n",
-					cl->common.classid, cl->quantum);
-				cl->quantum = qdisc_dev(cl->qdisc)->mtu/2 + 1;
-			}
-		}
-	}
-}
-
-static void cbq_sync_defmap(struct cbq_class *cl)
-{
-	struct cbq_sched_data *q = qdisc_priv(cl->qdisc);
-	struct cbq_class *split = cl->split;
-	unsigned int h;
-	int i;
-
-	if (split == NULL)
-		return;
-
-	for (i = 0; i <= TC_PRIO_MAX; i++) {
-		if (split->defaults[i] == cl && !(cl->defmap & (1<<i)))
-			split->defaults[i] = NULL;
-	}
-
-	for (i = 0; i <= TC_PRIO_MAX; i++) {
-		int level = split->level;
-
-		if (split->defaults[i])
-			continue;
-
-		for (h = 0; h < q->clhash.hashsize; h++) {
-			struct cbq_class *c;
-
-			hlist_for_each_entry(c, &q->clhash.hash[h],
-					     common.hnode) {
-				if (c->split == split && c->level < level &&
-				    c->defmap & (1<<i)) {
-					split->defaults[i] = c;
-					level = c->level;
-				}
-			}
-		}
-	}
-}
-
-static void cbq_change_defmap(struct cbq_class *cl, u32 splitid, u32 def, u32 mask)
-{
-	struct cbq_class *split = NULL;
-
-	if (splitid == 0) {
-		split = cl->split;
-		if (!split)
-			return;
-		splitid = split->common.classid;
-	}
-
-	if (split == NULL || split->common.classid != splitid) {
-		for (split = cl->tparent; split; split = split->tparent)
-			if (split->common.classid == splitid)
-				break;
-	}
-
-	if (split == NULL)
-		return;
-
-	if (cl->split != split) {
-		cl->defmap = 0;
-		cbq_sync_defmap(cl);
-		cl->split = split;
-		cl->defmap = def & mask;
-	} else
-		cl->defmap = (cl->defmap & ~mask) | (def & mask);
-
-	cbq_sync_defmap(cl);
-}
-
-static void cbq_unlink_class(struct cbq_class *this)
-{
-	struct cbq_class *cl, **clp;
-	struct cbq_sched_data *q = qdisc_priv(this->qdisc);
-
-	qdisc_class_hash_remove(&q->clhash, &this->common);
-
-	if (this->tparent) {
-		clp = &this->sibling;
-		cl = *clp;
-		do {
-			if (cl == this) {
-				*clp = cl->sibling;
-				break;
-			}
-			clp = &cl->sibling;
-		} while ((cl = *clp) != this->sibling);
-
-		if (this->tparent->children == this) {
-			this->tparent->children = this->sibling;
-			if (this->sibling == this)
-				this->tparent->children = NULL;
-		}
-	} else {
-		WARN_ON(this->sibling != this);
-	}
-}
-
-static void cbq_link_class(struct cbq_class *this)
-{
-	struct cbq_sched_data *q = qdisc_priv(this->qdisc);
-	struct cbq_class *parent = this->tparent;
-
-	this->sibling = this;
-	qdisc_class_hash_insert(&q->clhash, &this->common);
-
-	if (parent == NULL)
-		return;
-
-	if (parent->children == NULL) {
-		parent->children = this;
-	} else {
-		this->sibling = parent->children->sibling;
-		parent->children->sibling = this;
-	}
-}
-
-static void
-cbq_reset(struct Qdisc *sch)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct cbq_class *cl;
-	int prio;
-	unsigned int h;
-
-	q->activemask = 0;
-	q->pmask = 0;
-	q->tx_class = NULL;
-	q->tx_borrowed = NULL;
-	qdisc_watchdog_cancel(&q->watchdog);
-	hrtimer_cancel(&q->delay_timer);
-	q->toplevel = TC_CBQ_MAXLEVEL;
-	q->now = psched_get_time();
-
-	for (prio = 0; prio <= TC_CBQ_MAXPRIO; prio++)
-		q->active[prio] = NULL;
-
-	for (h = 0; h < q->clhash.hashsize; h++) {
-		hlist_for_each_entry(cl, &q->clhash.hash[h], common.hnode) {
-			qdisc_reset(cl->q);
-
-			cl->next_alive = NULL;
-			cl->undertime = PSCHED_PASTPERFECT;
-			cl->avgidle = cl->maxidle;
-			cl->deficit = cl->quantum;
-			cl->cpriority = cl->priority;
-		}
-	}
-	sch->q.qlen = 0;
-}
-
-
-static int cbq_set_lss(struct cbq_class *cl, struct tc_cbq_lssopt *lss)
-{
-	if (lss->change & TCF_CBQ_LSS_FLAGS) {
-		cl->share = (lss->flags & TCF_CBQ_LSS_ISOLATED) ? NULL : cl->tparent;
-		cl->borrow = (lss->flags & TCF_CBQ_LSS_BOUNDED) ? NULL : cl->tparent;
-	}
-	if (lss->change & TCF_CBQ_LSS_EWMA)
-		cl->ewma_log = lss->ewma_log;
-	if (lss->change & TCF_CBQ_LSS_AVPKT)
-		cl->avpkt = lss->avpkt;
-	if (lss->change & TCF_CBQ_LSS_MINIDLE)
-		cl->minidle = -(long)lss->minidle;
-	if (lss->change & TCF_CBQ_LSS_MAXIDLE) {
-		cl->maxidle = lss->maxidle;
-		cl->avgidle = lss->maxidle;
-	}
-	if (lss->change & TCF_CBQ_LSS_OFFTIME)
-		cl->offtime = lss->offtime;
-	return 0;
-}
-
-static void cbq_rmprio(struct cbq_sched_data *q, struct cbq_class *cl)
-{
-	q->nclasses[cl->priority]--;
-	q->quanta[cl->priority] -= cl->weight;
-	cbq_normalize_quanta(q, cl->priority);
-}
-
-static void cbq_addprio(struct cbq_sched_data *q, struct cbq_class *cl)
-{
-	q->nclasses[cl->priority]++;
-	q->quanta[cl->priority] += cl->weight;
-	cbq_normalize_quanta(q, cl->priority);
-}
-
-static int cbq_set_wrr(struct cbq_class *cl, struct tc_cbq_wrropt *wrr)
-{
-	struct cbq_sched_data *q = qdisc_priv(cl->qdisc);
-
-	if (wrr->allot)
-		cl->allot = wrr->allot;
-	if (wrr->weight)
-		cl->weight = wrr->weight;
-	if (wrr->priority) {
-		cl->priority = wrr->priority - 1;
-		cl->cpriority = cl->priority;
-		if (cl->priority >= cl->priority2)
-			cl->priority2 = TC_CBQ_MAXPRIO - 1;
-	}
-
-	cbq_addprio(q, cl);
-	return 0;
-}
-
-static int cbq_set_fopt(struct cbq_class *cl, struct tc_cbq_fopt *fopt)
-{
-	cbq_change_defmap(cl, fopt->split, fopt->defmap, fopt->defchange);
-	return 0;
-}
-
-static const struct nla_policy cbq_policy[TCA_CBQ_MAX + 1] = {
-	[TCA_CBQ_LSSOPT]	= { .len = sizeof(struct tc_cbq_lssopt) },
-	[TCA_CBQ_WRROPT]	= { .len = sizeof(struct tc_cbq_wrropt) },
-	[TCA_CBQ_FOPT]		= { .len = sizeof(struct tc_cbq_fopt) },
-	[TCA_CBQ_OVL_STRATEGY]	= { .len = sizeof(struct tc_cbq_ovl) },
-	[TCA_CBQ_RATE]		= { .len = sizeof(struct tc_ratespec) },
-	[TCA_CBQ_RTAB]		= { .type = NLA_BINARY, .len = TC_RTAB_SIZE },
-	[TCA_CBQ_POLICE]	= { .len = sizeof(struct tc_cbq_police) },
-};
-
-static int cbq_opt_parse(struct nlattr *tb[TCA_CBQ_MAX + 1], struct nlattr *opt)
-{
-	int err;
-
-	if (!opt)
-		return -EINVAL;
-
-	err = nla_parse_nested(tb, TCA_CBQ_MAX, opt, cbq_policy, NULL);
-	if (err < 0)
-		return err;
-
-	if (tb[TCA_CBQ_WRROPT]) {
-		const struct tc_cbq_wrropt *wrr = nla_data(tb[TCA_CBQ_WRROPT]);
-
-		if (wrr->priority > TC_CBQ_MAXPRIO)
-			err = -EINVAL;
-	}
-	return err;
-}
-
-static int cbq_init(struct Qdisc *sch, struct nlattr *opt)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct nlattr *tb[TCA_CBQ_MAX + 1];
-	struct tc_ratespec *r;
-	int err;
-
-	qdisc_watchdog_init(&q->watchdog, sch);
-	hrtimer_init(&q->delay_timer, CLOCK_MONOTONIC, HRTIMER_MODE_ABS_PINNED);
-	q->delay_timer.function = cbq_undelay;
-
-	err = cbq_opt_parse(tb, opt);
-	if (err < 0)
-		return err;
-
-	if (tb[TCA_CBQ_RTAB] == NULL || tb[TCA_CBQ_RATE] == NULL)
-		return -EINVAL;
-
-	r = nla_data(tb[TCA_CBQ_RATE]);
-
-	if ((q->link.R_tab = qdisc_get_rtab(r, tb[TCA_CBQ_RTAB])) == NULL)
-		return -EINVAL;
-
-	err = tcf_block_get(&q->link.block, &q->link.filter_list);
-	if (err)
-		goto put_rtab;
-
-	err = qdisc_class_hash_init(&q->clhash);
-	if (err < 0)
-		goto put_block;
-
-	q->link.sibling = &q->link;
-	q->link.common.classid = sch->handle;
-	q->link.qdisc = sch;
-	q->link.q = qdisc_create_dflt(sch->dev_queue, &pfifo_qdisc_ops,
-				      sch->handle);
-	if (!q->link.q)
-		q->link.q = &noop_qdisc;
-	else
-		qdisc_hash_add(q->link.q, true);
-
-	q->link.priority = TC_CBQ_MAXPRIO - 1;
-	q->link.priority2 = TC_CBQ_MAXPRIO - 1;
-	q->link.cpriority = TC_CBQ_MAXPRIO - 1;
-	q->link.allot = psched_mtu(qdisc_dev(sch));
-	q->link.quantum = q->link.allot;
-	q->link.weight = q->link.R_tab->rate.rate;
-
-	q->link.ewma_log = TC_CBQ_DEF_EWMA;
-	q->link.avpkt = q->link.allot/2;
-	q->link.minidle = -0x7FFFFFFF;
-
-	q->toplevel = TC_CBQ_MAXLEVEL;
-	q->now = psched_get_time();
-
-	cbq_link_class(&q->link);
-
-	if (tb[TCA_CBQ_LSSOPT])
-		cbq_set_lss(&q->link, nla_data(tb[TCA_CBQ_LSSOPT]));
-
-	cbq_addprio(q, &q->link);
-	return 0;
-
-put_block:
-	tcf_block_put(q->link.block);
-
-put_rtab:
-	qdisc_put_rtab(q->link.R_tab);
-	return err;
-}
-
-static int cbq_dump_rate(struct sk_buff *skb, struct cbq_class *cl)
-{
-	unsigned char *b = skb_tail_pointer(skb);
-
-	if (nla_put(skb, TCA_CBQ_RATE, sizeof(cl->R_tab->rate), &cl->R_tab->rate))
-		goto nla_put_failure;
-	return skb->len;
-
-nla_put_failure:
-	nlmsg_trim(skb, b);
-	return -1;
-}
-
-static int cbq_dump_lss(struct sk_buff *skb, struct cbq_class *cl)
-{
-	unsigned char *b = skb_tail_pointer(skb);
-	struct tc_cbq_lssopt opt;
-
-	opt.flags = 0;
-	if (cl->borrow == NULL)
-		opt.flags |= TCF_CBQ_LSS_BOUNDED;
-	if (cl->share == NULL)
-		opt.flags |= TCF_CBQ_LSS_ISOLATED;
-	opt.ewma_log = cl->ewma_log;
-	opt.level = cl->level;
-	opt.avpkt = cl->avpkt;
-	opt.maxidle = cl->maxidle;
-	opt.minidle = (u32)(-cl->minidle);
-	opt.offtime = cl->offtime;
-	opt.change = ~0;
-	if (nla_put(skb, TCA_CBQ_LSSOPT, sizeof(opt), &opt))
-		goto nla_put_failure;
-	return skb->len;
-
-nla_put_failure:
-	nlmsg_trim(skb, b);
-	return -1;
-}
-
-static int cbq_dump_wrr(struct sk_buff *skb, struct cbq_class *cl)
-{
-	unsigned char *b = skb_tail_pointer(skb);
-	struct tc_cbq_wrropt opt;
-
-	memset(&opt, 0, sizeof(opt));
-	opt.flags = 0;
-	opt.allot = cl->allot;
-	opt.priority = cl->priority + 1;
-	opt.cpriority = cl->cpriority + 1;
-	opt.weight = cl->weight;
-	if (nla_put(skb, TCA_CBQ_WRROPT, sizeof(opt), &opt))
-		goto nla_put_failure;
-	return skb->len;
-
-nla_put_failure:
-	nlmsg_trim(skb, b);
-	return -1;
-}
-
-static int cbq_dump_fopt(struct sk_buff *skb, struct cbq_class *cl)
-{
-	unsigned char *b = skb_tail_pointer(skb);
-	struct tc_cbq_fopt opt;
-
-	if (cl->split || cl->defmap) {
-		opt.split = cl->split ? cl->split->common.classid : 0;
-		opt.defmap = cl->defmap;
-		opt.defchange = ~0;
-		if (nla_put(skb, TCA_CBQ_FOPT, sizeof(opt), &opt))
-			goto nla_put_failure;
-	}
-	return skb->len;
-
-nla_put_failure:
-	nlmsg_trim(skb, b);
-	return -1;
-}
-
-static int cbq_dump_attr(struct sk_buff *skb, struct cbq_class *cl)
-{
-	if (cbq_dump_lss(skb, cl) < 0 ||
-	    cbq_dump_rate(skb, cl) < 0 ||
-	    cbq_dump_wrr(skb, cl) < 0 ||
-	    cbq_dump_fopt(skb, cl) < 0)
-		return -1;
-	return 0;
-}
-
-static int cbq_dump(struct Qdisc *sch, struct sk_buff *skb)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct nlattr *nest;
-
-	nest = nla_nest_start(skb, TCA_OPTIONS);
-	if (nest == NULL)
-		goto nla_put_failure;
-	if (cbq_dump_attr(skb, &q->link) < 0)
-		goto nla_put_failure;
-	return nla_nest_end(skb, nest);
-
-nla_put_failure:
-	nla_nest_cancel(skb, nest);
-	return -1;
-}
-
-static int
-cbq_dump_stats(struct Qdisc *sch, struct gnet_dump *d)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-
-	q->link.xstats.avgidle = q->link.avgidle;
-	return gnet_stats_copy_app(d, &q->link.xstats, sizeof(q->link.xstats));
-}
-
-static int
-cbq_dump_class(struct Qdisc *sch, unsigned long arg,
-	       struct sk_buff *skb, struct tcmsg *tcm)
-{
-	struct cbq_class *cl = (struct cbq_class *)arg;
-	struct nlattr *nest;
-
-	if (cl->tparent)
-		tcm->tcm_parent = cl->tparent->common.classid;
-	else
-		tcm->tcm_parent = TC_H_ROOT;
-	tcm->tcm_handle = cl->common.classid;
-	tcm->tcm_info = cl->q->handle;
-
-	nest = nla_nest_start(skb, TCA_OPTIONS);
-	if (nest == NULL)
-		goto nla_put_failure;
-	if (cbq_dump_attr(skb, cl) < 0)
-		goto nla_put_failure;
-	return nla_nest_end(skb, nest);
-
-nla_put_failure:
-	nla_nest_cancel(skb, nest);
-	return -1;
-}
-
-static int
-cbq_dump_class_stats(struct Qdisc *sch, unsigned long arg,
-	struct gnet_dump *d)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct cbq_class *cl = (struct cbq_class *)arg;
-
-	cl->xstats.avgidle = cl->avgidle;
-	cl->xstats.undertime = 0;
-
-	if (cl->undertime != PSCHED_PASTPERFECT)
-		cl->xstats.undertime = cl->undertime - q->now;
-
-	if (gnet_stats_copy_basic(qdisc_root_sleeping_running(sch),
-				  d, NULL, &cl->bstats) < 0 ||
-	    gnet_stats_copy_rate_est(d, &cl->rate_est) < 0 ||
-	    gnet_stats_copy_queue(d, NULL, &cl->qstats, cl->q->q.qlen) < 0)
-		return -1;
-
-	return gnet_stats_copy_app(d, &cl->xstats, sizeof(cl->xstats));
-}
-
-static int cbq_graft(struct Qdisc *sch, unsigned long arg, struct Qdisc *new,
-		     struct Qdisc **old)
-{
-	struct cbq_class *cl = (struct cbq_class *)arg;
-
-	if (new == NULL) {
-		new = qdisc_create_dflt(sch->dev_queue,
-					&pfifo_qdisc_ops, cl->common.classid);
-		if (new == NULL)
-			return -ENOBUFS;
-	}
-
-	*old = qdisc_replace(sch, new, &cl->q);
-	return 0;
-}
-
-static struct Qdisc *cbq_leaf(struct Qdisc *sch, unsigned long arg)
-{
-	struct cbq_class *cl = (struct cbq_class *)arg;
-
-	return cl->q;
-}
-
-static void cbq_qlen_notify(struct Qdisc *sch, unsigned long arg)
-{
-	struct cbq_class *cl = (struct cbq_class *)arg;
-
-	cbq_deactivate_class(cl);
-}
-
-static unsigned long cbq_find(struct Qdisc *sch, u32 classid)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-
-	return (unsigned long)cbq_class_lookup(q, classid);
-}
-
-static void cbq_destroy_class(struct Qdisc *sch, struct cbq_class *cl)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-
-	WARN_ON(cl->filters);
-
-	tcf_block_put(cl->block);
-	qdisc_destroy(cl->q);
-	qdisc_put_rtab(cl->R_tab);
-	gen_kill_estimator(&cl->rate_est);
-	if (cl != &q->link)
-		kfree(cl);
-}
-
-static void cbq_destroy(struct Qdisc *sch)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct hlist_node *next;
-	struct cbq_class *cl;
-	unsigned int h;
-
-#ifdef CONFIG_NET_CLS_ACT
-	q->rx_class = NULL;
-#endif
-	/*
-	 * Filters must be destroyed first because we don't destroy the
-	 * classes from root to leafs which means that filters can still
-	 * be bound to classes which have been destroyed already. --TGR '04
-	 */
-	for (h = 0; h < q->clhash.hashsize; h++) {
-		hlist_for_each_entry(cl, &q->clhash.hash[h], common.hnode) {
-			tcf_block_put(cl->block);
-			cl->block = NULL;
-		}
-	}
-	for (h = 0; h < q->clhash.hashsize; h++) {
-		hlist_for_each_entry_safe(cl, next, &q->clhash.hash[h],
-					  common.hnode)
-			cbq_destroy_class(sch, cl);
-	}
-	qdisc_class_hash_destroy(&q->clhash);
-}
-
-static int
-cbq_change_class(struct Qdisc *sch, u32 classid, u32 parentid, struct nlattr **tca,
-		 unsigned long *arg)
-{
-	int err;
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct cbq_class *cl = (struct cbq_class *)*arg;
-	struct nlattr *opt = tca[TCA_OPTIONS];
-	struct nlattr *tb[TCA_CBQ_MAX + 1];
-	struct cbq_class *parent;
-	struct qdisc_rate_table *rtab = NULL;
-
-	err = cbq_opt_parse(tb, opt);
-	if (err < 0)
-		return err;
-
-	if (tb[TCA_CBQ_OVL_STRATEGY] || tb[TCA_CBQ_POLICE])
-		return -EOPNOTSUPP;
-
-	if (cl) {
-		/* Check parent */
-		if (parentid) {
-			if (cl->tparent &&
-			    cl->tparent->common.classid != parentid)
-				return -EINVAL;
-			if (!cl->tparent && parentid != TC_H_ROOT)
-				return -EINVAL;
-		}
-
-		if (tb[TCA_CBQ_RATE]) {
-			rtab = qdisc_get_rtab(nla_data(tb[TCA_CBQ_RATE]),
-					      tb[TCA_CBQ_RTAB]);
-			if (rtab == NULL)
-				return -EINVAL;
-		}
-
-		if (tca[TCA_RATE]) {
-			err = gen_replace_estimator(&cl->bstats, NULL,
-						    &cl->rate_est,
-						    NULL,
-						    qdisc_root_sleeping_running(sch),
-						    tca[TCA_RATE]);
-			if (err) {
-				qdisc_put_rtab(rtab);
-				return err;
-			}
-		}
-
-		/* Change class parameters */
-		sch_tree_lock(sch);
-
-		if (cl->next_alive != NULL)
-			cbq_deactivate_class(cl);
-
-		if (rtab) {
-			qdisc_put_rtab(cl->R_tab);
-			cl->R_tab = rtab;
-		}
-
-		if (tb[TCA_CBQ_LSSOPT])
-			cbq_set_lss(cl, nla_data(tb[TCA_CBQ_LSSOPT]));
-
-		if (tb[TCA_CBQ_WRROPT]) {
-			cbq_rmprio(q, cl);
-			cbq_set_wrr(cl, nla_data(tb[TCA_CBQ_WRROPT]));
-		}
-
-		if (tb[TCA_CBQ_FOPT])
-			cbq_set_fopt(cl, nla_data(tb[TCA_CBQ_FOPT]));
-
-		if (cl->q->q.qlen)
-			cbq_activate_class(cl);
-
-		sch_tree_unlock(sch);
-
-		return 0;
-	}
-
-	if (parentid == TC_H_ROOT)
-		return -EINVAL;
-
-	if (tb[TCA_CBQ_WRROPT] == NULL || tb[TCA_CBQ_RATE] == NULL ||
-	    tb[TCA_CBQ_LSSOPT] == NULL)
-		return -EINVAL;
-
-	rtab = qdisc_get_rtab(nla_data(tb[TCA_CBQ_RATE]), tb[TCA_CBQ_RTAB]);
-	if (rtab == NULL)
-		return -EINVAL;
-
-	if (classid) {
-		err = -EINVAL;
-		if (TC_H_MAJ(classid ^ sch->handle) ||
-		    cbq_class_lookup(q, classid))
-			goto failure;
-	} else {
-		int i;
-		classid = TC_H_MAKE(sch->handle, 0x8000);
-
-		for (i = 0; i < 0x8000; i++) {
-			if (++q->hgenerator >= 0x8000)
-				q->hgenerator = 1;
-			if (cbq_class_lookup(q, classid|q->hgenerator) == NULL)
-				break;
-		}
-		err = -ENOSR;
-		if (i >= 0x8000)
-			goto failure;
-		classid = classid|q->hgenerator;
-	}
-
-	parent = &q->link;
-	if (parentid) {
-		parent = cbq_class_lookup(q, parentid);
-		err = -EINVAL;
-		if (parent == NULL)
-			goto failure;
-	}
-
-	err = -ENOBUFS;
-	cl = kzalloc(sizeof(*cl), GFP_KERNEL);
-	if (cl == NULL)
-		goto failure;
-
-	err = tcf_block_get(&cl->block, &cl->filter_list);
-	if (err) {
-		kfree(cl);
-		goto failure;
-	}
-
-	if (tca[TCA_RATE]) {
-		err = gen_new_estimator(&cl->bstats, NULL, &cl->rate_est,
-					NULL,
-					qdisc_root_sleeping_running(sch),
-					tca[TCA_RATE]);
-		if (err) {
-			tcf_block_put(cl->block);
-			kfree(cl);
-			goto failure;
-		}
-	}
-
-	cl->R_tab = rtab;
-	rtab = NULL;
-	cl->q = qdisc_create_dflt(sch->dev_queue, &pfifo_qdisc_ops, classid);
-	if (!cl->q)
-		cl->q = &noop_qdisc;
-	else
-		qdisc_hash_add(cl->q, true);
-
-	cl->common.classid = classid;
-	cl->tparent = parent;
-	cl->qdisc = sch;
-	cl->allot = parent->allot;
-	cl->quantum = cl->allot;
-	cl->weight = cl->R_tab->rate.rate;
-
-	sch_tree_lock(sch);
-	cbq_link_class(cl);
-	cl->borrow = cl->tparent;
-	if (cl->tparent != &q->link)
-		cl->share = cl->tparent;
-	cbq_adjust_levels(parent);
-	cl->minidle = -0x7FFFFFFF;
-	cbq_set_lss(cl, nla_data(tb[TCA_CBQ_LSSOPT]));
-	cbq_set_wrr(cl, nla_data(tb[TCA_CBQ_WRROPT]));
-	if (cl->ewma_log == 0)
-		cl->ewma_log = q->link.ewma_log;
-	if (cl->maxidle == 0)
-		cl->maxidle = q->link.maxidle;
-	if (cl->avpkt == 0)
-		cl->avpkt = q->link.avpkt;
-	if (tb[TCA_CBQ_FOPT])
-		cbq_set_fopt(cl, nla_data(tb[TCA_CBQ_FOPT]));
-	sch_tree_unlock(sch);
-
-	qdisc_class_hash_grow(sch, &q->clhash);
-
-	*arg = (unsigned long)cl;
-	return 0;
-
-failure:
-	qdisc_put_rtab(rtab);
-	return err;
-}
-
-static int cbq_delete(struct Qdisc *sch, unsigned long arg)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct cbq_class *cl = (struct cbq_class *)arg;
-	unsigned int qlen, backlog;
-
-	if (cl->filters || cl->children || cl == &q->link)
-		return -EBUSY;
-
-	sch_tree_lock(sch);
-
-	qlen = cl->q->q.qlen;
-	backlog = cl->q->qstats.backlog;
-	qdisc_reset(cl->q);
-	qdisc_tree_reduce_backlog(cl->q, qlen, backlog);
-
-	if (cl->next_alive)
-		cbq_deactivate_class(cl);
-
-	if (q->tx_borrowed == cl)
-		q->tx_borrowed = q->tx_class;
-	if (q->tx_class == cl) {
-		q->tx_class = NULL;
-		q->tx_borrowed = NULL;
-	}
-#ifdef CONFIG_NET_CLS_ACT
-	if (q->rx_class == cl)
-		q->rx_class = NULL;
-#endif
-
-	cbq_unlink_class(cl);
-	cbq_adjust_levels(cl->tparent);
-	cl->defmap = 0;
-	cbq_sync_defmap(cl);
-
-	cbq_rmprio(q, cl);
-	sch_tree_unlock(sch);
-
-	cbq_destroy_class(sch, cl);
-	return 0;
-}
-
-static struct tcf_block *cbq_tcf_block(struct Qdisc *sch, unsigned long arg)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct cbq_class *cl = (struct cbq_class *)arg;
-
-	if (cl == NULL)
-		cl = &q->link;
-
-	return cl->block;
-}
-
-static unsigned long cbq_bind_filter(struct Qdisc *sch, unsigned long parent,
-				     u32 classid)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct cbq_class *p = (struct cbq_class *)parent;
-	struct cbq_class *cl = cbq_class_lookup(q, classid);
-
-	if (cl) {
-		if (p && p->level <= cl->level)
-			return 0;
-		cl->filters++;
-		return (unsigned long)cl;
-	}
-	return 0;
-}
-
-static void cbq_unbind_filter(struct Qdisc *sch, unsigned long arg)
-{
-	struct cbq_class *cl = (struct cbq_class *)arg;
-
-	cl->filters--;
-}
-
-static void cbq_walk(struct Qdisc *sch, struct qdisc_walker *arg)
-{
-	struct cbq_sched_data *q = qdisc_priv(sch);
-	struct cbq_class *cl;
-	unsigned int h;
-
-	if (arg->stop)
-		return;
-
-	for (h = 0; h < q->clhash.hashsize; h++) {
-		hlist_for_each_entry(cl, &q->clhash.hash[h], common.hnode) {
-			if (arg->count < arg->skip) {
-				arg->count++;
-				continue;
-			}
-			if (arg->fn(sch, (unsigned long)cl, arg) < 0) {
-				arg->stop = 1;
-				return;
-			}
-			arg->count++;
-		}
-	}
-}
-
-static const struct Qdisc_class_ops cbq_class_ops = {
-	.graft		=	cbq_graft,
-	.leaf		=	cbq_leaf,
-	.qlen_notify	=	cbq_qlen_notify,
-	.find		=	cbq_find,
-	.change		=	cbq_change_class,
-	.delete		=	cbq_delete,
-	.walk		=	cbq_walk,
-	.tcf_block	=	cbq_tcf_block,
-	.bind_tcf	=	cbq_bind_filter,
-	.unbind_tcf	=	cbq_unbind_filter,
-	.dump		=	cbq_dump_class,
-	.dump_stats	=	cbq_dump_class_stats,
-};
-
-static struct Qdisc_ops cbq_qdisc_ops __read_mostly = {
-	.next		=	NULL,
-	.cl_ops		=	&cbq_class_ops,
-	.id		=	"cbq",
-	.priv_size	=	sizeof(struct cbq_sched_data),
-	.enqueue	=	cbq_enqueue,
-	.dequeue	=	cbq_dequeue,
-	.peek		=	qdisc_peek_dequeued,
-	.init		=	cbq_init,
-	.reset		=	cbq_reset,
-	.destroy	=	cbq_destroy,
-	.change		=	NULL,
-	.dump		=	cbq_dump,
-	.dump_stats	=	cbq_dump_stats,
-	.owner		=	THIS_MODULE,
-};
-
-static int __init cbq_module_init(void)
-{
-	return register_qdisc(&cbq_qdisc_ops);
-}
-static void __exit cbq_module_exit(void)
-{
-	unregister_qdisc(&cbq_qdisc_ops);
-}
-module_init(cbq_module_init)
-module_exit(cbq_module_exit)
-MODULE_LICENSE("GPL");
diff --git net/sched/sch_dsmark.c net/sched/sch_dsmark.c
deleted file mode 100644
index b972d50828ca..000000000000
--- linux-4.14.336/net/sched/sch_dsmark.c
+++ linux-4.14.336//dev/null
@@ -1,514 +0,0 @@
-/* net/sched/sch_dsmark.c - Differentiated Services field marker */
-
-/* Written 1998-2000 by Werner Almesberger, EPFL ICA */
-
-
-#include <linux/module.h>
-#include <linux/init.h>
-#include <linux/slab.h>
-#include <linux/types.h>
-#include <linux/string.h>
-#include <linux/errno.h>
-#include <linux/skbuff.h>
-#include <linux/rtnetlink.h>
-#include <linux/bitops.h>
-#include <net/pkt_sched.h>
-#include <net/pkt_cls.h>
-#include <net/dsfield.h>
-#include <net/inet_ecn.h>
-#include <asm/byteorder.h>
-
-/*
- * classid	class		marking
- * -------	-----		-------
- *   n/a	  0		n/a
- *   x:0	  1		use entry [0]
- *   ...	 ...		...
- *   x:y y>0	 y+1		use entry [y]
- *   ...	 ...		...
- * x:indices-1	indices		use entry [indices-1]
- *   ...	 ...		...
- *   x:y	 y+1		use entry [y & (indices-1)]
- *   ...	 ...		...
- * 0xffff	0x10000		use entry [indices-1]
- */
-
-
-#define NO_DEFAULT_INDEX	(1 << 16)
-
-struct mask_value {
-	u8			mask;
-	u8			value;
-};
-
-struct dsmark_qdisc_data {
-	struct Qdisc		*q;
-	struct tcf_proto __rcu	*filter_list;
-	struct tcf_block	*block;
-	struct mask_value	*mv;
-	u16			indices;
-	u8			set_tc_index;
-	u32			default_index;	/* index range is 0...0xffff */
-#define DSMARK_EMBEDDED_SZ	16
-	struct mask_value	embedded[DSMARK_EMBEDDED_SZ];
-};
-
-static inline int dsmark_valid_index(struct dsmark_qdisc_data *p, u16 index)
-{
-	return index <= p->indices && index > 0;
-}
-
-/* ------------------------- Class/flow operations ------------------------- */
-
-static int dsmark_graft(struct Qdisc *sch, unsigned long arg,
-			struct Qdisc *new, struct Qdisc **old)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-
-	pr_debug("%s(sch %p,[qdisc %p],new %p,old %p)\n",
-		 __func__, sch, p, new, old);
-
-	if (new == NULL) {
-		new = qdisc_create_dflt(sch->dev_queue, &pfifo_qdisc_ops,
-					sch->handle);
-		if (new == NULL)
-			new = &noop_qdisc;
-	}
-
-	*old = qdisc_replace(sch, new, &p->q);
-	return 0;
-}
-
-static struct Qdisc *dsmark_leaf(struct Qdisc *sch, unsigned long arg)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-	return p->q;
-}
-
-static unsigned long dsmark_find(struct Qdisc *sch, u32 classid)
-{
-	return TC_H_MIN(classid) + 1;
-}
-
-static unsigned long dsmark_bind_filter(struct Qdisc *sch,
-					unsigned long parent, u32 classid)
-{
-	pr_debug("%s(sch %p,[qdisc %p],classid %x)\n",
-		 __func__, sch, qdisc_priv(sch), classid);
-
-	return dsmark_find(sch, classid);
-}
-
-static void dsmark_unbind_filter(struct Qdisc *sch, unsigned long cl)
-{
-}
-
-static const struct nla_policy dsmark_policy[TCA_DSMARK_MAX + 1] = {
-	[TCA_DSMARK_INDICES]		= { .type = NLA_U16 },
-	[TCA_DSMARK_DEFAULT_INDEX]	= { .type = NLA_U16 },
-	[TCA_DSMARK_SET_TC_INDEX]	= { .type = NLA_FLAG },
-	[TCA_DSMARK_MASK]		= { .type = NLA_U8 },
-	[TCA_DSMARK_VALUE]		= { .type = NLA_U8 },
-};
-
-static int dsmark_change(struct Qdisc *sch, u32 classid, u32 parent,
-			 struct nlattr **tca, unsigned long *arg)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-	struct nlattr *opt = tca[TCA_OPTIONS];
-	struct nlattr *tb[TCA_DSMARK_MAX + 1];
-	int err = -EINVAL;
-
-	pr_debug("%s(sch %p,[qdisc %p],classid %x,parent %x), arg 0x%lx\n",
-		 __func__, sch, p, classid, parent, *arg);
-
-	if (!dsmark_valid_index(p, *arg)) {
-		err = -ENOENT;
-		goto errout;
-	}
-
-	if (!opt)
-		goto errout;
-
-	err = nla_parse_nested(tb, TCA_DSMARK_MAX, opt, dsmark_policy, NULL);
-	if (err < 0)
-		goto errout;
-
-	if (tb[TCA_DSMARK_VALUE])
-		p->mv[*arg - 1].value = nla_get_u8(tb[TCA_DSMARK_VALUE]);
-
-	if (tb[TCA_DSMARK_MASK])
-		p->mv[*arg - 1].mask = nla_get_u8(tb[TCA_DSMARK_MASK]);
-
-	err = 0;
-
-errout:
-	return err;
-}
-
-static int dsmark_delete(struct Qdisc *sch, unsigned long arg)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-
-	if (!dsmark_valid_index(p, arg))
-		return -EINVAL;
-
-	p->mv[arg - 1].mask = 0xff;
-	p->mv[arg - 1].value = 0;
-
-	return 0;
-}
-
-static void dsmark_walk(struct Qdisc *sch, struct qdisc_walker *walker)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-	int i;
-
-	pr_debug("%s(sch %p,[qdisc %p],walker %p)\n",
-		 __func__, sch, p, walker);
-
-	if (walker->stop)
-		return;
-
-	for (i = 0; i < p->indices; i++) {
-		if (p->mv[i].mask == 0xff && !p->mv[i].value)
-			goto ignore;
-		if (walker->count >= walker->skip) {
-			if (walker->fn(sch, i + 1, walker) < 0) {
-				walker->stop = 1;
-				break;
-			}
-		}
-ignore:
-		walker->count++;
-	}
-}
-
-static struct tcf_block *dsmark_tcf_block(struct Qdisc *sch, unsigned long cl)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-
-	return p->block;
-}
-
-/* --------------------------- Qdisc operations ---------------------------- */
-
-static int dsmark_enqueue(struct sk_buff *skb, struct Qdisc *sch,
-			  struct sk_buff **to_free)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-	int err;
-
-	pr_debug("%s(skb %p,sch %p,[qdisc %p])\n", __func__, skb, sch, p);
-
-	if (p->set_tc_index) {
-		int wlen = skb_network_offset(skb);
-
-		switch (tc_skb_protocol(skb)) {
-		case htons(ETH_P_IP):
-			wlen += sizeof(struct iphdr);
-			if (!pskb_may_pull(skb, wlen) ||
-			    skb_try_make_writable(skb, wlen))
-				goto drop;
-
-			skb->tc_index = ipv4_get_dsfield(ip_hdr(skb))
-				& ~INET_ECN_MASK;
-			break;
-
-		case htons(ETH_P_IPV6):
-			wlen += sizeof(struct ipv6hdr);
-			if (!pskb_may_pull(skb, wlen) ||
-			    skb_try_make_writable(skb, wlen))
-				goto drop;
-
-			skb->tc_index = ipv6_get_dsfield(ipv6_hdr(skb))
-				& ~INET_ECN_MASK;
-			break;
-		default:
-			skb->tc_index = 0;
-			break;
-		}
-	}
-
-	if (TC_H_MAJ(skb->priority) == sch->handle)
-		skb->tc_index = TC_H_MIN(skb->priority);
-	else {
-		struct tcf_result res;
-		struct tcf_proto *fl = rcu_dereference_bh(p->filter_list);
-		int result = tcf_classify(skb, fl, &res, false);
-
-		pr_debug("result %d class 0x%04x\n", result, res.classid);
-
-		switch (result) {
-#ifdef CONFIG_NET_CLS_ACT
-		case TC_ACT_QUEUED:
-		case TC_ACT_STOLEN:
-		case TC_ACT_TRAP:
-			__qdisc_drop(skb, to_free);
-			return NET_XMIT_SUCCESS | __NET_XMIT_STOLEN;
-
-		case TC_ACT_SHOT:
-			goto drop;
-#endif
-		case TC_ACT_OK:
-			skb->tc_index = TC_H_MIN(res.classid);
-			break;
-
-		default:
-			if (p->default_index != NO_DEFAULT_INDEX)
-				skb->tc_index = p->default_index;
-			break;
-		}
-	}
-
-	err = qdisc_enqueue(skb, p->q, to_free);
-	if (err != NET_XMIT_SUCCESS) {
-		if (net_xmit_drop_count(err))
-			qdisc_qstats_drop(sch);
-		return err;
-	}
-
-	qdisc_qstats_backlog_inc(sch, skb);
-	sch->q.qlen++;
-
-	return NET_XMIT_SUCCESS;
-
-drop:
-	qdisc_drop(skb, sch, to_free);
-	return NET_XMIT_SUCCESS | __NET_XMIT_BYPASS;
-}
-
-static struct sk_buff *dsmark_dequeue(struct Qdisc *sch)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-	struct sk_buff *skb;
-	u32 index;
-
-	pr_debug("%s(sch %p,[qdisc %p])\n", __func__, sch, p);
-
-	skb = qdisc_dequeue_peeked(p->q);
-	if (skb == NULL)
-		return NULL;
-
-	qdisc_bstats_update(sch, skb);
-	qdisc_qstats_backlog_dec(sch, skb);
-	sch->q.qlen--;
-
-	index = skb->tc_index & (p->indices - 1);
-	pr_debug("index %d->%d\n", skb->tc_index, index);
-
-	switch (tc_skb_protocol(skb)) {
-	case htons(ETH_P_IP):
-		ipv4_change_dsfield(ip_hdr(skb), p->mv[index].mask,
-				    p->mv[index].value);
-			break;
-	case htons(ETH_P_IPV6):
-		ipv6_change_dsfield(ipv6_hdr(skb), p->mv[index].mask,
-				    p->mv[index].value);
-			break;
-	default:
-		/*
-		 * Only complain if a change was actually attempted.
-		 * This way, we can send non-IP traffic through dsmark
-		 * and don't need yet another qdisc as a bypass.
-		 */
-		if (p->mv[index].mask != 0xff || p->mv[index].value)
-			pr_warn("%s: unsupported protocol %d\n",
-				__func__, ntohs(tc_skb_protocol(skb)));
-		break;
-	}
-
-	return skb;
-}
-
-static struct sk_buff *dsmark_peek(struct Qdisc *sch)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-
-	pr_debug("%s(sch %p,[qdisc %p])\n", __func__, sch, p);
-
-	return p->q->ops->peek(p->q);
-}
-
-static int dsmark_init(struct Qdisc *sch, struct nlattr *opt)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-	struct nlattr *tb[TCA_DSMARK_MAX + 1];
-	int err = -EINVAL;
-	u32 default_index = NO_DEFAULT_INDEX;
-	u16 indices;
-	int i;
-
-	pr_debug("%s(sch %p,[qdisc %p],opt %p)\n", __func__, sch, p, opt);
-
-	if (!opt)
-		goto errout;
-
-	err = tcf_block_get(&p->block, &p->filter_list);
-	if (err)
-		return err;
-
-	err = nla_parse_nested(tb, TCA_DSMARK_MAX, opt, dsmark_policy, NULL);
-	if (err < 0)
-		goto errout;
-
-	err = -EINVAL;
-	if (!tb[TCA_DSMARK_INDICES])
-		goto errout;
-	indices = nla_get_u16(tb[TCA_DSMARK_INDICES]);
-
-	if (hweight32(indices) != 1)
-		goto errout;
-
-	if (tb[TCA_DSMARK_DEFAULT_INDEX])
-		default_index = nla_get_u16(tb[TCA_DSMARK_DEFAULT_INDEX]);
-
-	if (indices <= DSMARK_EMBEDDED_SZ)
-		p->mv = p->embedded;
-	else
-		p->mv = kmalloc_array(indices, sizeof(*p->mv), GFP_KERNEL);
-	if (!p->mv) {
-		err = -ENOMEM;
-		goto errout;
-	}
-	for (i = 0; i < indices; i++) {
-		p->mv[i].mask = 0xff;
-		p->mv[i].value = 0;
-	}
-	p->indices = indices;
-	p->default_index = default_index;
-	p->set_tc_index = nla_get_flag(tb[TCA_DSMARK_SET_TC_INDEX]);
-
-	p->q = qdisc_create_dflt(sch->dev_queue, &pfifo_qdisc_ops, sch->handle);
-	if (p->q == NULL)
-		p->q = &noop_qdisc;
-	else
-		qdisc_hash_add(p->q, true);
-
-	pr_debug("%s: qdisc %p\n", __func__, p->q);
-
-	err = 0;
-errout:
-	return err;
-}
-
-static void dsmark_reset(struct Qdisc *sch)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-
-	pr_debug("%s(sch %p,[qdisc %p])\n", __func__, sch, p);
-	if (p->q)
-		qdisc_reset(p->q);
-	sch->qstats.backlog = 0;
-	sch->q.qlen = 0;
-}
-
-static void dsmark_destroy(struct Qdisc *sch)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-
-	pr_debug("%s(sch %p,[qdisc %p])\n", __func__, sch, p);
-
-	tcf_block_put(p->block);
-	qdisc_destroy(p->q);
-	if (p->mv != p->embedded)
-		kfree(p->mv);
-}
-
-static int dsmark_dump_class(struct Qdisc *sch, unsigned long cl,
-			     struct sk_buff *skb, struct tcmsg *tcm)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-	struct nlattr *opts = NULL;
-
-	pr_debug("%s(sch %p,[qdisc %p],class %ld\n", __func__, sch, p, cl);
-
-	if (!dsmark_valid_index(p, cl))
-		return -EINVAL;
-
-	tcm->tcm_handle = TC_H_MAKE(TC_H_MAJ(sch->handle), cl - 1);
-	tcm->tcm_info = p->q->handle;
-
-	opts = nla_nest_start(skb, TCA_OPTIONS);
-	if (opts == NULL)
-		goto nla_put_failure;
-	if (nla_put_u8(skb, TCA_DSMARK_MASK, p->mv[cl - 1].mask) ||
-	    nla_put_u8(skb, TCA_DSMARK_VALUE, p->mv[cl - 1].value))
-		goto nla_put_failure;
-
-	return nla_nest_end(skb, opts);
-
-nla_put_failure:
-	nla_nest_cancel(skb, opts);
-	return -EMSGSIZE;
-}
-
-static int dsmark_dump(struct Qdisc *sch, struct sk_buff *skb)
-{
-	struct dsmark_qdisc_data *p = qdisc_priv(sch);
-	struct nlattr *opts = NULL;
-
-	opts = nla_nest_start(skb, TCA_OPTIONS);
-	if (opts == NULL)
-		goto nla_put_failure;
-	if (nla_put_u16(skb, TCA_DSMARK_INDICES, p->indices))
-		goto nla_put_failure;
-
-	if (p->default_index != NO_DEFAULT_INDEX &&
-	    nla_put_u16(skb, TCA_DSMARK_DEFAULT_INDEX, p->default_index))
-		goto nla_put_failure;
-
-	if (p->set_tc_index &&
-	    nla_put_flag(skb, TCA_DSMARK_SET_TC_INDEX))
-		goto nla_put_failure;
-
-	return nla_nest_end(skb, opts);
-
-nla_put_failure:
-	nla_nest_cancel(skb, opts);
-	return -EMSGSIZE;
-}
-
-static const struct Qdisc_class_ops dsmark_class_ops = {
-	.graft		=	dsmark_graft,
-	.leaf		=	dsmark_leaf,
-	.find		=	dsmark_find,
-	.change		=	dsmark_change,
-	.delete		=	dsmark_delete,
-	.walk		=	dsmark_walk,
-	.tcf_block	=	dsmark_tcf_block,
-	.bind_tcf	=	dsmark_bind_filter,
-	.unbind_tcf	=	dsmark_unbind_filter,
-	.dump		=	dsmark_dump_class,
-};
-
-static struct Qdisc_ops dsmark_qdisc_ops __read_mostly = {
-	.next		=	NULL,
-	.cl_ops		=	&dsmark_class_ops,
-	.id		=	"dsmark",
-	.priv_size	=	sizeof(struct dsmark_qdisc_data),
-	.enqueue	=	dsmark_enqueue,
-	.dequeue	=	dsmark_dequeue,
-	.peek		=	dsmark_peek,
-	.init		=	dsmark_init,
-	.reset		=	dsmark_reset,
-	.destroy	=	dsmark_destroy,
-	.change		=	NULL,
-	.dump		=	dsmark_dump,
-	.owner		=	THIS_MODULE,
-};
-
-static int __init dsmark_module_init(void)
-{
-	return register_qdisc(&dsmark_qdisc_ops);
-}
-
-static void __exit dsmark_module_exit(void)
-{
-	unregister_qdisc(&dsmark_qdisc_ops);
-}
-
-module_init(dsmark_module_init)
-module_exit(dsmark_module_exit)
-
-MODULE_LICENSE("GPL");
diff --git net/sunrpc/xprtmultipath.c net/sunrpc/xprtmultipath.c
index e2d64c7138c3..699d5ba128fa 100644
--- linux-4.14.336/net/sunrpc/xprtmultipath.c
+++ linux-4.14.336/net/sunrpc/xprtmultipath.c
@@ -235,8 +235,9 @@ struct rpc_xprt *xprt_iter_current_entry(struct rpc_xprt_iter *xpi)
 	return xprt_switch_find_current_entry(head, xpi->xpi_cursor);
 }
 
-bool rpc_xprt_switch_has_addr(struct rpc_xprt_switch *xps,
-			      const struct sockaddr *sap)
+static
+bool __rpc_xprt_switch_has_addr(struct rpc_xprt_switch *xps,
+				const struct sockaddr *sap)
 {
 	struct list_head *head;
 	struct rpc_xprt *pos;
@@ -255,6 +256,18 @@ bool rpc_xprt_switch_has_addr(struct rpc_xprt_switch *xps,
 	return false;
 }
 
+bool rpc_xprt_switch_has_addr(struct rpc_xprt_switch *xps,
+			      const struct sockaddr *sap)
+{
+	bool res;
+
+	rcu_read_lock();
+	res = __rpc_xprt_switch_has_addr(xps, sap);
+	rcu_read_unlock();
+
+	return res;
+}
+
 static
 struct rpc_xprt *xprt_switch_find_next_entry(struct list_head *head,
 		const struct rpc_xprt *cur)
diff --git net/tipc/bearer.c net/tipc/bearer.c
index 506cbd1b2223..db21e00806f5 100644
--- linux-4.14.336/net/tipc/bearer.c
+++ linux-4.14.336/net/tipc/bearer.c
@@ -931,6 +931,12 @@ int tipc_nl_bearer_add(struct sk_buff *skb, struct genl_info *info)
 
 #ifdef CONFIG_TIPC_MEDIA_UDP
 	if (attrs[TIPC_NLA_BEARER_UDP_OPTS]) {
+		if (b->media->type_id != TIPC_MEDIA_TYPE_UDP) {
+			rtnl_unlock();
+			NL_SET_ERR_MSG(info->extack, "UDP option is unsupported");
+			return -EINVAL;
+		}
+
 		err = tipc_udp_nl_bearer_add(b,
 					     attrs[TIPC_NLA_BEARER_UDP_OPTS]);
 		if (err) {
diff --git net/unix/af_unix.c net/unix/af_unix.c
index 8d25d50f916e..b1855778acd0 100644
--- linux-4.14.336/net/unix/af_unix.c
+++ linux-4.14.336/net/unix/af_unix.c
@@ -1127,13 +1127,11 @@ static void unix_state_double_lock(struct sock *sk1, struct sock *sk2)
 		unix_state_lock(sk1);
 		return;
 	}
-	if (sk1 < sk2) {
-		unix_state_lock(sk1);
-		unix_state_lock_nested(sk2);
-	} else {
-		unix_state_lock(sk2);
-		unix_state_lock_nested(sk1);
-	}
+	if (sk1 > sk2)
+		swap(sk1, sk2);
+
+	unix_state_lock(sk1);
+	unix_state_lock_nested(sk2, U_LOCK_SECOND);
 }
 
 static void unix_state_double_unlock(struct sock *sk1, struct sock *sk2)
@@ -1352,7 +1350,7 @@ restart:
 		goto out_unlock;
 	}
 
-	unix_state_lock_nested(sk);
+	unix_state_lock_nested(sk, U_LOCK_SECOND);
 
 	if (sk->sk_state != st) {
 		unix_state_unlock(sk);
diff --git net/unix/diag.c net/unix/diag.c
index 3183d9b8ab33..d6ceac688def 100644
--- linux-4.14.336/net/unix/diag.c
+++ linux-4.14.336/net/unix/diag.c
@@ -80,7 +80,7 @@ static int sk_diag_dump_icons(struct sock *sk, struct sk_buff *nlskb)
 			 * queue lock. With the other's queue locked it's
 			 * OK to lock the state.
 			 */
-			unix_state_lock_nested(req);
+			unix_state_lock_nested(req, U_LOCK_DIAG);
 			peer = unix_sk(req)->peer;
 			buf[i++] = (peer ? sock_i_ino(peer) : 0);
 			unix_state_unlock(req);
diff --git net/wireless/nl80211.c net/wireless/nl80211.c
index b4b564182db0..4f43f4dfb996 100644
--- linux-4.14.336/net/wireless/nl80211.c
+++ linux-4.14.336/net/wireless/nl80211.c
@@ -2717,6 +2717,7 @@ static int nl80211_dump_interface(struct sk_buff *skb, struct netlink_callback *
 			if_idx++;
 		}
 
+		if_start = 0;
 		wp_idx++;
 	}
  out:
@@ -2896,6 +2897,8 @@ static int nl80211_set_interface(struct sk_buff *skb, struct genl_info *info)
 
 		if (ntype != NL80211_IFTYPE_MESH_POINT)
 			return -EINVAL;
+		if (otype != NL80211_IFTYPE_MESH_POINT)
+			return -EINVAL;
 		if (netif_running(dev))
 			return -EBUSY;
 
diff --git net/wireless/scan.c net/wireless/scan.c
index 8bbcdcf5c829..88fe0e8e8b18 100644
--- linux-4.14.336/net/wireless/scan.c
+++ linux-4.14.336/net/wireless/scan.c
@@ -1015,8 +1015,12 @@ cfg80211_bss_update(struct cfg80211_registered_device *rdev,
 				list_add(&new->hidden_list,
 					 &hidden->hidden_list);
 				hidden->refcount++;
+
+				ies = (void *)rcu_access_pointer(new->pub.beacon_ies);
 				rcu_assign_pointer(new->pub.beacon_ies,
 						   hidden->pub.beacon_ies);
+				if (ies)
+					kfree_rcu(ies, rcu_head);
 			}
 		} else {
 			/*
diff --git security/apparmor/policy_unpack.c security/apparmor/policy_unpack.c
index 2cef8d4404cc..4f41aa6ff897 100644
--- linux-4.14.336/security/apparmor/policy_unpack.c
+++ linux-4.14.336/security/apparmor/policy_unpack.c
@@ -604,6 +604,10 @@ static struct aa_profile *unpack_profile(struct aa_ext *e, char **ns_name)
 
 	tmpname = aa_splitn_fqname(name, strlen(name), &tmpns, &ns_len);
 	if (tmpns) {
+		if (!tmpname) {
+			info = "empty profile name";
+			goto fail;
+		}
 		*ns_name = kstrndup(tmpns, ns_len, GFP_KERNEL);
 		if (!*ns_name) {
 			info = "out of memory";
diff --git security/security.c security/security.c
index b5e3d7a91b33..90c2094380e2 100644
--- linux-4.14.336/security/security.c
+++ linux-4.14.336/security/security.c
@@ -884,6 +884,23 @@ int security_file_ioctl(struct file *file, unsigned int cmd, unsigned long arg)
 	return call_int_hook(file_ioctl, 0, file, cmd, arg);
 }
 
+/**
+ * security_file_ioctl_compat() - Check if an ioctl is allowed in compat mode
+ * @file: associated file
+ * @cmd: ioctl cmd
+ * @arg: ioctl arguments
+ *
+ * Compat version of security_file_ioctl() that correctly handles 32-bit
+ * processes running on 64-bit kernels.
+ *
+ * Return: Returns 0 if permission is granted.
+ */
+int security_file_ioctl_compat(struct file *file, unsigned int cmd,
+			       unsigned long arg)
+{
+	return call_int_hook(file_ioctl_compat, 0, file, cmd, arg);
+}
+
 static inline unsigned long mmap_prot(struct file *file, unsigned long prot)
 {
 	/*
diff --git security/selinux/hooks.c security/selinux/hooks.c
index 38a4db1f3aaa..a1613e22a734 100644
--- linux-4.14.336/security/selinux/hooks.c
+++ linux-4.14.336/security/selinux/hooks.c
@@ -3571,6 +3571,33 @@ static int selinux_file_ioctl(struct file *file, unsigned int cmd,
 	return error;
 }
 
+static int selinux_file_ioctl_compat(struct file *file, unsigned int cmd,
+			      unsigned long arg)
+{
+	/*
+	 * If we are in a 64-bit kernel running 32-bit userspace, we need to
+	 * make sure we don't compare 32-bit flags to 64-bit flags.
+	 */
+	switch (cmd) {
+	case FS_IOC32_GETFLAGS:
+		cmd = FS_IOC_GETFLAGS;
+		break;
+	case FS_IOC32_SETFLAGS:
+		cmd = FS_IOC_SETFLAGS;
+		break;
+	case FS_IOC32_GETVERSION:
+		cmd = FS_IOC_GETVERSION;
+		break;
+	case FS_IOC32_SETVERSION:
+		cmd = FS_IOC_SETVERSION;
+		break;
+	default:
+		break;
+	}
+
+	return selinux_file_ioctl(file, cmd, arg);
+}
+
 static int default_noexec;
 
 static int file_map_prot_check(struct file *file, unsigned long prot, int shared)
@@ -6377,6 +6404,7 @@ static struct security_hook_list selinux_hooks[] __lsm_ro_after_init = {
 	LSM_HOOK_INIT(file_alloc_security, selinux_file_alloc_security),
 	LSM_HOOK_INIT(file_free_security, selinux_file_free_security),
 	LSM_HOOK_INIT(file_ioctl, selinux_file_ioctl),
+	LSM_HOOK_INIT(file_ioctl_compat, selinux_file_ioctl_compat),
 	LSM_HOOK_INIT(mmap_file, selinux_mmap_file),
 	LSM_HOOK_INIT(mmap_addr, selinux_mmap_addr),
 	LSM_HOOK_INIT(file_mprotect, selinux_file_mprotect),
diff --git security/smack/smack_lsm.c security/smack/smack_lsm.c
index fe070669dc18..a6e81ef73b42 100644
--- linux-4.14.336/security/smack/smack_lsm.c
+++ linux-4.14.336/security/smack/smack_lsm.c
@@ -4651,6 +4651,7 @@ static struct security_hook_list smack_hooks[] __lsm_ro_after_init = {
 	LSM_HOOK_INIT(file_alloc_security, smack_file_alloc_security),
 	LSM_HOOK_INIT(file_free_security, smack_file_free_security),
 	LSM_HOOK_INIT(file_ioctl, smack_file_ioctl),
+	LSM_HOOK_INIT(file_ioctl_compat, smack_file_ioctl),
 	LSM_HOOK_INIT(file_lock, smack_file_lock),
 	LSM_HOOK_INIT(file_fcntl, smack_file_fcntl),
 	LSM_HOOK_INIT(mmap_file, smack_mmap_file),
diff --git security/tomoyo/tomoyo.c security/tomoyo/tomoyo.c
index 213b8c593668..195f9b706926 100644
--- linux-4.14.336/security/tomoyo/tomoyo.c
+++ linux-4.14.336/security/tomoyo/tomoyo.c
@@ -516,6 +516,7 @@ static struct security_hook_list tomoyo_hooks[] __lsm_ro_after_init = {
 	LSM_HOOK_INIT(path_rename, tomoyo_path_rename),
 	LSM_HOOK_INIT(inode_getattr, tomoyo_inode_getattr),
 	LSM_HOOK_INIT(file_ioctl, tomoyo_file_ioctl),
+	LSM_HOOK_INIT(file_ioctl_compat, tomoyo_file_ioctl),
 	LSM_HOOK_INIT(path_chmod, tomoyo_path_chmod),
 	LSM_HOOK_INIT(path_chown, tomoyo_path_chown),
 	LSM_HOOK_INIT(path_chroot, tomoyo_path_chroot),
diff --git sound/core/Makefile sound/core/Makefile
index ee4a4a6b99ba..753bf1a0dbf3 100644
--- linux-4.14.336/sound/core/Makefile
+++ linux-4.14.336/sound/core/Makefile
@@ -30,7 +30,6 @@ snd-pcm-dmaengine-objs := pcm_dmaengine.o
 snd-rawmidi-objs  := rawmidi.o
 snd-timer-objs    := timer.o
 snd-hrtimer-objs  := hrtimer.o
-snd-rtctimer-objs := rtctimer.o
 snd-hwdep-objs    := hwdep.o
 snd-seq-device-objs := seq_device.o
 
diff --git sound/pci/hda/hda_intel.c sound/pci/hda/hda_intel.c
index 978719fc4cd3..bb76b9c26da8 100644
--- linux-4.14.336/sound/pci/hda/hda_intel.c
+++ linux-4.14.336/sound/pci/hda/hda_intel.c
@@ -2545,6 +2545,12 @@ static const struct pci_device_id azx_ids[] = {
 	/* Cannonlake */
 	{ PCI_DEVICE(0x8086, 0x9dc8),
 	  .driver_data = AZX_DRIVER_SKL | AZX_DCAPS_INTEL_SKYLAKE},
+	/* Icelake */
+	{ PCI_DEVICE(0x8086, 0x34c8),
+	  .driver_data = AZX_DRIVER_SKL | AZX_DCAPS_INTEL_SKYLAKE},
+	/* Arrow Lake */
+	{ PCI_DEVICE(0x8086, 0x7728),
+	  .driver_data = AZX_DRIVER_SKL | AZX_DCAPS_INTEL_SKYLAKE},
 	/* Broxton-P(Apollolake) */
 	{ PCI_DEVICE(0x8086, 0x5a98),
 	  .driver_data = AZX_DRIVER_SKL | AZX_DCAPS_INTEL_BROXTON },
diff --git sound/pci/hda/patch_conexant.c sound/pci/hda/patch_conexant.c
index 9263cb56df7d..6215d85428c7 100644
--- linux-4.14.336/sound/pci/hda/patch_conexant.c
+++ linux-4.14.336/sound/pci/hda/patch_conexant.c
@@ -263,6 +263,7 @@ enum {
 	CXT_FIXUP_MUTE_LED_GPIO,
 	CXT_FIXUP_HEADSET_MIC,
 	CXT_FIXUP_HP_MIC_NO_PRESENCE,
+	CXT_PINCFG_SWS_JS201D,
 };
 
 /* for hda_fixup_thinkpad_acpi() */
@@ -754,6 +755,17 @@ static const struct hda_pintbl cxt_pincfg_lemote[] = {
 	{}
 };
 
+/* SuoWoSi/South-holding JS201D with sn6140 */
+static const struct hda_pintbl cxt_pincfg_sws_js201d[] = {
+	{ 0x16, 0x03211040 }, /* hp out */
+	{ 0x17, 0x91170110 }, /* SPK/Class_D */
+	{ 0x18, 0x95a70130 }, /* Internal mic */
+	{ 0x19, 0x03a11020 }, /* Headset Mic */
+	{ 0x1a, 0x40f001f0 }, /* Not used */
+	{ 0x21, 0x40f001f0 }, /* Not used */
+	{}
+};
+
 static const struct hda_fixup cxt_fixups[] = {
 	[CXT_PINCFG_LENOVO_X200] = {
 		.type = HDA_FIXUP_PINS,
@@ -905,6 +917,10 @@ static const struct hda_fixup cxt_fixups[] = {
 		.chained = true,
 		.chain_id = CXT_FIXUP_HEADSET_MIC,
 	},
+	[CXT_PINCFG_SWS_JS201D] = {
+		.type = HDA_FIXUP_PINS,
+		.v.pins = cxt_pincfg_sws_js201d,
+	},
 };
 
 static const struct snd_pci_quirk cxt5045_fixups[] = {
@@ -973,6 +989,7 @@ static const struct snd_pci_quirk cxt5066_fixups[] = {
 	SND_PCI_QUIRK(0x103c, 0x8402, "HP ProBook 645 G4", CXT_FIXUP_MUTE_LED_GPIO),
 	SND_PCI_QUIRK(0x103c, 0x8455, "HP Z2 G4", CXT_FIXUP_HP_MIC_NO_PRESENCE),
 	SND_PCI_QUIRK(0x1043, 0x138d, "Asus", CXT_FIXUP_HEADPHONE_MIC_PIN),
+	SND_PCI_QUIRK(0x14f1, 0x0265, "SWS JS201D", CXT_PINCFG_SWS_JS201D),
 	SND_PCI_QUIRK(0x152d, 0x0833, "OLPC XO-1.5", CXT_FIXUP_OLPC_XO),
 	SND_PCI_QUIRK(0x17aa, 0x20f2, "Lenovo T400", CXT_PINCFG_LENOVO_TP410),
 	SND_PCI_QUIRK(0x17aa, 0x215e, "Lenovo T410", CXT_PINCFG_LENOVO_TP410),
@@ -1011,6 +1028,7 @@ static const struct hda_model_fixup cxt5066_fixup_models[] = {
 	{ .id = CXT_FIXUP_HP_DOCK, .name = "hp-dock" },
 	{ .id = CXT_FIXUP_MUTE_LED_GPIO, .name = "mute-led-gpio" },
 	{ .id = CXT_PINCFG_LENOVO_NOTEBOOK, .name = "lenovo-20149" },
+	{ .id = CXT_PINCFG_SWS_JS201D, .name = "sws-js201d" },
 	{}
 };
 
diff --git sound/pci/oxygen/oxygen_mixer.c sound/pci/oxygen/oxygen_mixer.c
index 4ca12665ff73..64a82688d7fb 100644
--- linux-4.14.336/sound/pci/oxygen/oxygen_mixer.c
+++ linux-4.14.336/sound/pci/oxygen/oxygen_mixer.c
@@ -730,7 +730,7 @@ static int ac97_fp_rec_volume_put(struct snd_kcontrol *ctl,
 	oldreg = oxygen_read_ac97(chip, 1, AC97_REC_GAIN);
 	newreg = oldreg & ~0x0707;
 	newreg = newreg | (value->value.integer.value[0] & 7);
-	newreg = newreg | ((value->value.integer.value[0] & 7) << 8);
+	newreg = newreg | ((value->value.integer.value[1] & 7) << 8);
 	change = newreg != oldreg;
 	if (change)
 		oxygen_write_ac97(chip, 1, AC97_REC_GAIN, newreg);
diff --git sound/soc/codecs/cs35l33.c sound/soc/codecs/cs35l33.c
index e2c1194ea61a..32048c4c7e71 100644
--- linux-4.14.336/sound/soc/codecs/cs35l33.c
+++ linux-4.14.336/sound/soc/codecs/cs35l33.c
@@ -26,13 +26,11 @@
 #include <sound/soc-dapm.h>
 #include <sound/initval.h>
 #include <sound/tlv.h>
-#include <linux/gpio.h>
 #include <linux/gpio/consumer.h>
 #include <sound/cs35l33.h>
 #include <linux/pm_runtime.h>
 #include <linux/regulator/consumer.h>
 #include <linux/regulator/machine.h>
-#include <linux/of_gpio.h>
 #include <linux/of.h>
 #include <linux/of_device.h>
 #include <linux/of_irq.h>
@@ -1173,7 +1171,7 @@ static int cs35l33_i2c_probe(struct i2c_client *i2c_client,
 
 	/* We could issue !RST or skip it based on AMP topology */
 	cs35l33->reset_gpio = devm_gpiod_get_optional(&i2c_client->dev,
-			"reset-gpios", GPIOD_OUT_HIGH);
+			"reset", GPIOD_OUT_HIGH);
 	if (IS_ERR(cs35l33->reset_gpio)) {
 		dev_err(&i2c_client->dev, "%s ERROR: Can't get reset GPIO\n",
 			__func__);
diff --git sound/soc/codecs/cs35l34.c sound/soc/codecs/cs35l34.c
index 1e05026bedca..8a0ca34d828e 100644
--- linux-4.14.336/sound/soc/codecs/cs35l34.c
+++ linux-4.14.336/sound/soc/codecs/cs35l34.c
@@ -24,14 +24,12 @@
 #include <linux/regulator/machine.h>
 #include <linux/pm_runtime.h>
 #include <linux/of_device.h>
-#include <linux/of_gpio.h>
 #include <linux/of_irq.h>
 #include <sound/core.h>
 #include <sound/pcm.h>
 #include <sound/pcm_params.h>
 #include <sound/soc.h>
 #include <sound/soc-dapm.h>
-#include <linux/gpio.h>
 #include <linux/gpio/consumer.h>
 #include <sound/initval.h>
 #include <sound/tlv.h>
@@ -1068,7 +1066,7 @@ static int cs35l34_i2c_probe(struct i2c_client *i2c_client,
 		dev_err(&i2c_client->dev, "Failed to request IRQ: %d\n", ret);
 
 	cs35l34->reset_gpio = devm_gpiod_get_optional(&i2c_client->dev,
-				"reset-gpios", GPIOD_OUT_LOW);
+				"reset", GPIOD_OUT_LOW);
 	if (IS_ERR(cs35l34->reset_gpio))
 		return PTR_ERR(cs35l34->reset_gpio);
 
diff --git sound/soc/codecs/cs43130.c sound/soc/codecs/cs43130.c
index 643e37fc218e..ad5d527e6e52 100644
--- linux-4.14.336/sound/soc/codecs/cs43130.c
+++ linux-4.14.336/sound/soc/codecs/cs43130.c
@@ -581,7 +581,7 @@ static int cs43130_set_sp_fmt(int dai_id, unsigned int bitwidth_sclk,
 		break;
 	case SND_SOC_DAIFMT_LEFT_J:
 		hi_size = bitwidth_sclk;
-		frm_delay = 2;
+		frm_delay = 0;
 		frm_phase = 1;
 		break;
 	case SND_SOC_DAIFMT_DSP_A:
@@ -1675,7 +1675,7 @@ static ssize_t cs43130_show_dc_r(struct device *dev,
 	return cs43130_show_dc(dev, buf, HP_RIGHT);
 }
 
-static u16 const cs43130_ac_freq[CS43130_AC_FREQ] = {
+static const u16 cs43130_ac_freq[CS43130_AC_FREQ] = {
 	24,
 	43,
 	93,
@@ -2351,7 +2351,7 @@ static const struct regmap_config cs43130_regmap = {
 	.use_single_rw		= true, /* needed for regcache_sync */
 };
 
-static u16 const cs43130_dc_threshold[CS43130_DC_THRESHOLD] = {
+static const u16 cs43130_dc_threshold[CS43130_DC_THRESHOLD] = {
 	50,
 	120,
 };
diff --git sound/soc/codecs/da7219-aad.c sound/soc/codecs/da7219-aad.c
index 793c8768f7c4..5a31a4db1e23 100644
--- linux-4.14.336/sound/soc/codecs/da7219-aad.c
+++ linux-4.14.336/sound/soc/codecs/da7219-aad.c
@@ -650,7 +650,7 @@ static struct da7219_aad_pdata *da7219_aad_fw_to_pdata(struct snd_soc_codec *cod
 		aad_pdata->mic_det_thr =
 			da7219_aad_fw_mic_det_thr(codec, fw_val32);
 	else
-		aad_pdata->mic_det_thr = DA7219_AAD_MIC_DET_THR_500_OHMS;
+		aad_pdata->mic_det_thr = DA7219_AAD_MIC_DET_THR_200_OHMS;
 
 	if (fwnode_property_read_u32(aad_np, "dlg,jack-ins-deb", &fw_val32) >= 0)
 		aad_pdata->jack_ins_deb =
diff --git sound/soc/codecs/rt5645.c sound/soc/codecs/rt5645.c
index 822c42101c3f..536a33820265 100644
--- linux-4.14.336/sound/soc/codecs/rt5645.c
+++ linux-4.14.336/sound/soc/codecs/rt5645.c
@@ -417,6 +417,7 @@ struct rt5645_priv {
 	struct regulator_bulk_data supplies[ARRAY_SIZE(rt5645_supply_names)];
 	struct rt5645_eq_param_s *eq_param;
 	struct timer_list btn_check_timer;
+	struct mutex jd_mutex;
 
 	int codec_type;
 	int sysclk;
@@ -3158,6 +3159,8 @@ static int rt5645_jack_detect(struct snd_soc_codec *codec, int jack_insert)
 				rt5645_enable_push_button_irq(codec, true);
 			}
 		} else {
+			if (rt5645->en_button_func)
+				rt5645_enable_push_button_irq(codec, false);
 			snd_soc_dapm_disable_pin(dapm, "Mic Det Power");
 			snd_soc_dapm_sync(dapm);
 			rt5645->jack_type = SND_JACK_HEADPHONE;
@@ -3238,6 +3241,8 @@ static void rt5645_jack_detect_work(struct work_struct *work)
 	if (!rt5645->codec)
 		return;
 
+	mutex_lock(&rt5645->jd_mutex);
+
 	switch (rt5645->pdata.jd_mode) {
 	case 0: /* Not using rt5645 JD */
 		if (rt5645->gpiod_hp_det) {
@@ -3250,6 +3255,7 @@ static void rt5645_jack_detect_work(struct work_struct *work)
 				    report, SND_JACK_HEADPHONE);
 		snd_soc_jack_report(rt5645->mic_jack,
 				    report, SND_JACK_MICROPHONE);
+		mutex_unlock(&rt5645->jd_mutex);
 		return;
 	default: /* read rt5645 jd1_1 status */
 		val = snd_soc_read(rt5645->codec, RT5645_INT_IRQ_ST) & 0x1000;
@@ -3259,7 +3265,7 @@ static void rt5645_jack_detect_work(struct work_struct *work)
 
 	if (!val && (rt5645->jack_type == 0)) { /* jack in */
 		report = rt5645_jack_detect(rt5645->codec, 1);
-	} else if (!val && rt5645->jack_type != 0) {
+	} else if (!val && rt5645->jack_type == SND_JACK_HEADSET) {
 		/* for push button and jack out */
 		btn_type = 0;
 		if (snd_soc_read(rt5645->codec, RT5645_INT_IRQ_ST) & 0x4) {
@@ -3315,6 +3321,8 @@ static void rt5645_jack_detect_work(struct work_struct *work)
 		rt5645_jack_detect(rt5645->codec, 0);
 	}
 
+	mutex_unlock(&rt5645->jd_mutex);
+
 	snd_soc_jack_report(rt5645->hp_jack, report, SND_JACK_HEADPHONE);
 	snd_soc_jack_report(rt5645->mic_jack, report, SND_JACK_MICROPHONE);
 	if (rt5645->en_button_func)
@@ -3939,6 +3947,7 @@ static int rt5645_i2c_probe(struct i2c_client *i2c,
 	setup_timer(&rt5645->btn_check_timer,
 		rt5645_btn_check_callback, (unsigned long)rt5645);
 
+	mutex_init(&rt5645->jd_mutex);
 	INIT_DELAYED_WORK(&rt5645->jack_detect_work, rt5645_jack_detect_work);
 	INIT_DELAYED_WORK(&rt5645->rcclock_work, rt5645_rcclock_work);
 
diff --git tools/lib/subcmd/help.c tools/lib/subcmd/help.c
index 2859f107abc8..4260c8b4257b 100644
--- linux-4.14.336/tools/lib/subcmd/help.c
+++ linux-4.14.336/tools/lib/subcmd/help.c
@@ -50,11 +50,21 @@ void uniq(struct cmdnames *cmds)
 	if (!cmds->cnt)
 		return;
 
-	for (i = j = 1; i < cmds->cnt; i++)
-		if (strcmp(cmds->names[i]->name, cmds->names[i-1]->name))
-			cmds->names[j++] = cmds->names[i];
-
+	for (i = 1; i < cmds->cnt; i++) {
+		if (!strcmp(cmds->names[i]->name, cmds->names[i-1]->name))
+			zfree(&cmds->names[i - 1]);
+	}
+	for (i = 0, j = 0; i < cmds->cnt; i++) {
+		if (cmds->names[i]) {
+			if (i == j)
+				j++;
+			else
+				cmds->names[j++] = cmds->names[i];
+		}
+	}
 	cmds->cnt = j;
+	while (j < i)
+		cmds->names[j++] = NULL;
 }
 
 void exclude_cmds(struct cmdnames *cmds, struct cmdnames *excludes)
diff --git tools/testing/selftests/powerpc/math/fpu_preempt.c tools/testing/selftests/powerpc/math/fpu_preempt.c
index 0f85b79d883d..c91f3b36e884 100644
--- linux-4.14.336/tools/testing/selftests/powerpc/math/fpu_preempt.c
+++ linux-4.14.336/tools/testing/selftests/powerpc/math/fpu_preempt.c
@@ -41,19 +41,20 @@ __thread double darray[] = {0.1, 0.2, 0.3, 0.4, 0.5, 0.6, 0.7, 0.8, 0.9, 1.0,
 int threads_starting;
 int running;
 
-extern void preempt_fpu(double *darray, int *threads_starting, int *running);
+extern int preempt_fpu(double *darray, int *threads_starting, int *running);
 
 void *preempt_fpu_c(void *p)
 {
+	long rc;
 	int i;
+
 	srand(pthread_self());
 	for (i = 0; i < 21; i++)
 		darray[i] = rand();
 
-	/* Test failed if it ever returns */
-	preempt_fpu(darray, &threads_starting, &running);
+	rc = preempt_fpu(darray, &threads_starting, &running);
 
-	return p;
+	return (void *)rc;
 }
 
 int test_preempt_fpu(void)
diff --git tools/testing/selftests/powerpc/math/vmx_preempt.c tools/testing/selftests/powerpc/math/vmx_preempt.c
index 9ef376c55b13..7ba95ceaaa50 100644
--- linux-4.14.336/tools/testing/selftests/powerpc/math/vmx_preempt.c
+++ linux-4.14.336/tools/testing/selftests/powerpc/math/vmx_preempt.c
@@ -41,19 +41,21 @@ __thread vector int varray[] = {{1, 2, 3, 4}, {5, 6, 7, 8}, {9, 10,11,12},
 int threads_starting;
 int running;
 
-extern void preempt_vmx(vector int *varray, int *threads_starting, int *running);
+extern int preempt_vmx(vector int *varray, int *threads_starting, int *running);
 
 void *preempt_vmx_c(void *p)
 {
 	int i, j;
+	long rc;
+
 	srand(pthread_self());
 	for (i = 0; i < 12; i++)
 		for (j = 0; j < 4; j++)
 			varray[i][j] = rand();
 
-	/* Test fails if it ever returns */
-	preempt_vmx(varray, &threads_starting, &running);
-	return p;
+	rc = preempt_vmx(varray, &threads_starting, &running);
+
+	return (void *)rc;
 }
 
 int test_preempt_vmx(void)
diff --git virt/kvm/arm/vgic/vgic-its.c virt/kvm/arm/vgic/vgic-its.c
index fd25c2161060..a4398f58a830 100644
--- linux-4.14.336/virt/kvm/arm/vgic/vgic-its.c
+++ linux-4.14.336/virt/kvm/arm/vgic/vgic-its.c
@@ -424,6 +424,9 @@ static int its_sync_lpi_pending_table(struct kvm_vcpu *vcpu)
 		}
 
 		irq = vgic_get_irq(vcpu->kvm, NULL, intids[i]);
+		if (!irq)
+			continue;
+
 		spin_lock(&irq->irq_lock);
 		irq->pending_latch = pendmask & (1U << bit_nr);
 		vgic_queue_irq_unlock(vcpu->kvm, irq);
